Function	Function Call	Call Count	Percent of Total	Max Displacement (bits)
#% BEGIN STATIC GRAPH
__start	out	4	in	0
	out	4	100%
	_exit	1	25%	0	0	0
	___ghs_ind_crt0	1	25%	0	241	0
	___ghs_initial_dotsyscall	1	25%	0	23	0
	___dotsyscall	1	25%	0	0	0
	in	0	100%
___ghs_multicore_wait_for_init	out	0	in	0
	out	0	100%
	in	0	100%
___ghs_multicore_init_done	out	0	in	0
	out	0	100%
	in	0	100%
_PWN_Init	out	1	in	1
	out	1	100%
	_TimerB_PWM_Init	1	100%	0	7	0
	in	1	100%
	_BSP_PWM_Init	1	100%	0	341	0
_PWM_Channel_Init	out	2	in	1
	out	2	100%
	_TimerB_PWM_Channel_Start	1	50%	0	53	0
	_TimerB_PWM_Channel_Init	1	50%	0	47	0
	in	1	100%
	_BSP_PWM_Init	1	100%	0	357	0
_PWM_Channel_Set_Freq	out	1	in	1
	out	1	100%
	_TimerB_PWM_Channel_Fre_Set	1	100%	0	85	0
	in	1	100%
	_BSP_PWM_Init	1	100%	0	367	0
_PWM_Channel_Set_Duty	out	1	in	2
	out	1	100%
	_TimerB_PWM_Channel_Duty_Set	1	100%	0	111	0
	in	2	100%
	_BSP_PWM_Init	1	50%	0	377	0
	_BSP_SetBL_Brightness_PWM	1	50%	0	2041	0
_PWM_Channel_Stop	out	1	in	0
	out	1	100%
	_TimerB_PWM_Channel_Stop	1	100%	0	131	0
	in	0	100%
_WDT_Clear	out	1	in	2
	out	1	100%
	_WDT__Clear	1	100%	0	7	0
	in	2	100%
	_main	1	50%	0	77	0
	_BSP_WDT_Clear	1	50%	0	7	0
_WDT_Reset_Init	out	0	in	0
	out	0	100%
	in	0	100%
_Internal_EEPROM_OPEN	out	1	in	2
	out	1	100%
	_FDL_Open	1	100%	0	7	0
	in	2	100%
	_Internal_EEL_Read	1	50%	0	285	0
	_Internal_EEL_Write	1	50%	0	181	0
_Internal_EEPROM_CLOSE	out	1	in	2
	out	1	100%
	_FDL_Close	1	100%	0	25	0
	in	2	100%
	_Internal_EEL_Read	1	50%	0	337	18
	_Internal_EEL_Write	1	50%	0	223	18
_Internal_EEL_Init	out	6	in	2
	out	7	100%
	_SampleApp_EEL_HdrLoop	1	14%	0	93	0
	_SampleApp_EEL_ErrorHdr	1	14%	0	121	0
	_EX_EE_INIT	2	28%	0	97	0
	_R_EEL_GetDriverStatus	1	14%	0	133	0
	_R_EEL_Execute	1	14%	0	85	0
	_R_EEL_Handler	1	14%	0	125	0
	in	2	100%
	_Internal_EEL_Read	1	50%	0	289	36
	_Internal_EEL_Write	1	50%	0	185	36
_Internal_EEL_Write	out	6	in	1
	out	6	100%
	_Internal_EEPROM_OPEN	1	16%	0	181	0
	_Internal_EEPROM_CLOSE	1	16%	0	223	18
	_Internal_EEL_Init	1	16%	0	185	36
	_Internal_EEL_DEINIT	1	16%	0	219	370
	_SampleApp_EEL_HdrLoop	1	16%	0	215	0
	_R_EEL_Execute	1	16%	0	207	0
	in	1	100%
	_DFlash_WriteData	1	100%	0	51	0
_Internal_EEL_Read	out	6	in	1
	out	6	100%
	_Internal_EEPROM_OPEN	1	16%	0	285	0
	_Internal_EEPROM_CLOSE	1	16%	0	337	18
	_Internal_EEL_Init	1	16%	0	289	36
	_Internal_EEL_DEINIT	1	16%	0	333	370
	_SampleApp_EEL_HdrLoop	1	16%	0	329	0
	_R_EEL_Execute	1	16%	0	321	0
	in	1	100%
	_DFlash_ReadData	1	100%	0	17	0
_Internal_EEL_DEINIT	out	4	in	2
	out	5	100%
	_SampleApp_EEL_ErrorHdr	2	40%	0	429	0
	_R_EEL_GetDriverStatus	1	20%	0	413	0
	_R_EEL_Handler	1	20%	0	405	0
	_R_EEL_ShutDown	1	20%	0	377	0
	in	2	100%
	_Internal_EEL_Read	1	50%	0	333	370
	_Internal_EEL_Write	1	50%	0	219	370
_DFlash_ReadData	out	1	in	1
	out	1	100%
	_Internal_EEL_Read	1	100%	0	17	0
	in	1	100%
	_ReadDFlashData	1	100%	0	827	0
_DFlash_WriteData	out	1	in	1
	out	1	100%
	_Internal_EEL_Write	1	100%	0	51	0
	in	1	100%
	_WriteDFlashData	1	100%	0	857	0
_FCL_Ctrl1	out	5	in	0
	out	10	100%
	_R_FCL_CopySections	1	10%	0	25	0
	_R_FCL_Init	1	10%	0	15	0
	_R_FCL_Execute	6	60%	0	523	0
	_FCLUser_Open	1	10%	0	89	0
	_FCLUser_Close	1	10%	0	635	0
	in	0	100%
_Internal_FCL_OPEN	out	3	in	3
	out	3	100%
	_R_FCL_CopySections	1	33%	0	673	0
	_R_FCL_Init	1	33%	0	663	0
	_FCLUser_Open	1	33%	0	737	0
	in	3	100%
	_OTA_FLASH_Write	1	33%	0	177	0
	_OTA_FLASH_Erase	1	33%	0	17	0
	_RTE_FCL_OP	1	33%	0	67	0
_Internal_FCL_CLOSE	out	1	in	3
	out	1	100%
	_FCLUser_Close	1	100%	0	757	0
	in	3	100%
	_OTA_FLASH_Write	1	33%	0	199	0
	_OTA_FLASH_Erase	1	33%	0	35	0
	_RTE_FCL_OP	1	33%	0	83	0
_Internal_FCL_Init	out	1	in	3
	out	1	100%
	_R_FCL_Execute	1	100%	0	791	0
	in	3	100%
	_OTA_FLASH_Write	1	33%	0	181	0
	_OTA_FLASH_Erase	1	33%	0	21	0
	_RTE_FCL_OP	1	33%	0	71	0
_Internal_FCL_Unlock	out	1	in	2
	out	1	100%
	_R_FCL_Execute	1	100%	0	843	0
	in	2	100%
	_OTA_FLASH_Erase	1	50%	0	25	0
	_RTE_FCL_OP	1	50%	0	75	0
_Internal_FCL_Erase	out	1	in	1
	out	1	100%
	_R_FCL_Execute	1	100%	0	931	0
	in	1	100%
	_OTA_FLASH_Erase	1	100%	0	31	0
_Internal_FCL_Write	out	1	in	1
	out	1	100%
	_R_FCL_Execute	1	100%	0	1029	0
	in	1	100%
	_OTA_FLASH_Write	1	100%	0	195	0
_Internal_FCL_Read32	out	0	in	1
	out	0	100%
	in	1	100%
	_RTE_FLASH_Read32	1	100%	0	235	0
_OptionByte_Handle	out	1	in	1
	out	2	100%
	_R_FCL_Execute	2	100%	0	1295	0
	in	1	100%
	_RTE_FCL_OP	1	100%	0	79	0
_Clock_Run_Mode_Init	out	0	in	1
	out	0	100%
	in	1	100%
	_Sys_Startup_Pre_Init	1	100%	0	7	0
_Clock_Sleep_Mode_Init	out	0	in	0
	out	0	100%
	in	0	100%
_Clock_Get_Main_OSC_Status	out	0	in	0
	out	0	100%
	in	0	100%
_WDT_Init	out	0	in	1
	out	0	100%
	in	1	100%
	_Sys_Startup_Init	1	100%	0	45	0
_WDT_Enable	out	0	in	0
	out	0	100%
	in	0	100%
_WDT_Disable	out	0	in	0
	out	0	100%
	in	0	100%
_WDT__Clear	out	0	in	1
	out	0	100%
	in	1	100%
	_WDT_Clear	1	100%	0	7	0
_RH850_Software_Reset	out	0	in	0
	out	0	100%
	in	0	100%
_RH850_Hardware_Reset	out	0	in	1
	out	0	100%
	in	1	100%
	_OTA_SystemReset	1	100%	0	1159	0
_RH850_Peripheral_IRQ_Enable	out	0	in	7
	out	0	100%
	in	32	100%
	_Sys_Tick_Timer_Start	1	3%	0	63	0
	_TimerB_Input_Channel_Init	2	6%	0	1125	0
	_RSCAN0_CH_Init	12	37%	0	2387	0
	_UART_Init	8	25%	0	741	0
	_RIIC0_Init	4	12%	0	835	0
	_RIIC1_Init	4	12%	0	4267	0
	_touch_IRQ_Enable	1	3%	0	879	0
_RH850_Peripheral_IRQ_Disable	out	0	in	3
	out	0	100%
	in	9	100%
	_Sys_Tick_Timer_Stop	1	11%	0	93	0
	_RIIC0_Init	4	44%	0	301	0
	_RIIC1_Init	4	44%	0	3733	0
_RH850_Peripheral_IRQ_Flag_Clear	out	0	in	3
	out	0	100%
	in	3	100%
	_Sys_Tick_Timer_ISR	1	33%	0	167	0
	_BSP_FTM0_IRQHandler	1	33%	0	263	0
	_BSP_TOUCH_IRQHandler	1	33%	0	921	0
_RH850_Enter_Idle_Mode	out	0	in	0
	out	0	100%
	in	0	100%
_RH850_Enter_Stop_Mode	out	0	in	0
	out	0	100%
	in	0	100%
_RH850_Get_startup_mode	out	0	in	0
	out	0	100%
	in	0	100%
_Sys_Tick_Timer_Start	out	1	in	1
	out	1	100%
	_RH850_Peripheral_IRQ_Enable	1	100%	0	63	0
	in	1	100%
	_Sys_Startup_Init	1	100%	0	49	0
_Sys_Tick_Timer_Stop	out	1	in	0
	out	1	100%
	_RH850_Peripheral_IRQ_Disable	1	100%	0	93	0
	in	0	100%
_Sys_Tick_Timer_Call_Back_Reg	out	0	in	0
	out	0	100%
	in	0	100%
_Sys_Tick_Timer_ISR	out	1	in	0
	out	1	100%
	_RH850_Peripheral_IRQ_Flag_Clear	1	100%	0	167	0
	in	0	100%
_ADC_Get_Physical_Channel..Z.3A.5CD.5Ctest.5CFX12_test.5Cghs.5Cobj.5CADC.	out	0	in	0
	out	0	100%
	in	0	100%
_ADC_Get_Channel_Result..Z.3A.5CD.5Ctest.5CFX12_test.5Cghs.5Cobj.5CADC.	out	0	in	0
	out	0	100%
	in	0	100%
_ADC_Virtual_Channel_Config..Z.3A.5CD.5Ctest.5CFX12_test.5Cghs.5Cobj.5CADC.	out	0	in	0
	out	0	100%
	in	0	100%
_ADC_Init	out	0	in	1
	out	0	100%
	in	1	100%
	_Analog_Signal_Conv_Init	1	100%	0	47	0
_ADC_DeInit	out	0	in	1
	out	0	100%
	in	1	100%
	_Analog_Signal_Conv_Stop	1	100%	0	171	0
_ADC_Start_Conversion	out	0	in	2
	out	0	100%
	in	4	100%
	_Analog_Signal_Conv_Service	3	75%	0	1197	0
	_ADC_Conv_Single_Channel	1	25%	0	1385	0
_ADC_Stop_Conversion	out	0	in	2
	out	0	100%
	in	4	100%
	_Analog_Signal_Conv_Init	1	25%	0	15	0
	_Analog_Signal_Conv_Service	3	75%	0	1247	0
_ADC_Get_Conversion_Status	out	0	in	4
	out	0	100%
	in	7	100%
	_ADC_Get_Conversion_Result	1	14%	0	381	310
	_Analog_Signal_Conv_Init	1	14%	0	19	0
	_Analog_Signal_Conv_Service	3	42%	0	1225	0
	_ADC_Conv_Single_Channel	2	28%	0	1393	0
_ADC_Get_Conversion_Result	out	1	in	2
	out	1	100%
	_ADC_Get_Conversion_Status	1	100%	0	381	310
	in	2	100%
	_Analog_Signal_Conv_Service	1	50%	0	517	0
	_ADC_Conv_Single_Channel	1	50%	0	1425	0
_ADC_Input_Voltage_Calc	out	0	in	2
	out	0	100%
	in	3	100%
	_Analog_Signal_Conv_Service	1	33%	0	671	0
	_ADC_Conv_Single_Channel	2	66%	0	1635	0
_ADC_VRef_Calibrate	out	0	in	0
	out	0	100%
	in	0	100%
_ADC_Data_Calibrate	out	0	in	2
	out	0	100%
	in	3	100%
	_Analog_Signal_Conv_Service	1	33%	0	1065	0
	_ADC_Conv_Single_Channel	2	66%	0	1895	0
_ADC_Voltage_Calc_Circuit101	out	0	in	0
	out	0	100%
	in	0	100%
_ADC_Voltage_Calc_Circuit102	out	2	in	0
	out	3	100%
	___gh_udiv64	2	66%	0	277	0
	___gh_mul64	1	33%	0	231	0
	in	0	100%
_ADC_Res_Calc_Circuit101	out	2	in	0
	out	2	100%
	___gh_udiv64	1	50%	0	449	0
	___gh_mul64	1	50%	0	427	0
	in	0	100%
_ADC_Res_Calc_Circuit102	out	2	in	0
	out	5	100%
	___gh_udiv64	1	20%	0	807	0
	___gh_mul64	4	80%	0	777	0
	in	0	100%
_ADC_Res_Calc_Circuit103	out	2	in	0
	out	7	100%
	___gh_udiv64	2	28%	0	1269	0
	___gh_mul64	5	71%	0	1239	0
	in	0	100%
_ADC_Res_Calc_Circuit201	out	2	in	0
	out	2	100%
	___gh_udiv64	1	50%	0	1509	0
	___gh_mul64	1	50%	0	1487	0
	in	0	100%
_ADC_Res_Calc_Circuit202	out	2	in	0
	out	4	100%
	___gh_udiv64	2	50%	0	1823	0
	___gh_mul64	2	50%	0	1801	0
	in	0	100%
_ADC_Res_Calc_Circuit203	out	2	in	0
	out	6	100%
	___gh_udiv64	3	50%	0	2239	0
	___gh_mul64	3	50%	0	2223	0
	in	0	100%
_ADC_Res_Calc_Circuit301	out	0	in	0
	out	0	100%
	in	0	100%
_ADC_Res_Calc_Circuit302	out	0	in	0
	out	0	100%
	in	0	100%
_ADC_Res_Calc_Circuit303	out	2	in	0
	out	3	100%
	___gh_udiv64	1	33%	0	2663	0
	___gh_mul64	2	66%	0	2681	0
	in	0	100%
_Analog_Signal_Conv_Init	out	3	in	1
	out	3	100%
	_ADC_Stop_Conversion	1	33%	0	15	0
	_ADC_Get_Conversion_Status	1	33%	0	19	0
	_ADC_Init	1	33%	0	47	0
	in	1	100%
	_Analog_Signal_Conv_Service	1	100%	0	1253	0
_Analog_Signal_Conv_Stop	out	1	in	0
	out	1	100%
	_ADC_DeInit	1	100%	0	171	0
	in	0	100%
_Analog_Signal_Conv_Service	out	9	in	0
	out	15	100%
	_ADC_Get_Conversion_Result	1	6%	0	517	0
	_ADC_Stop_Conversion	3	20%	0	1247	0
	_ADC_Start_Conversion	3	20%	0	1197	0
	_ADC_Get_Conversion_Status	3	20%	0	1225	0
	_ADC_Data_Calibrate	1	6%	0	1065	0
	_ADC_Input_Voltage_Calc	1	6%	0	671	0
	_Analog_Signal_Conv_Init	1	6%	0	1253	0
	_ADC_Read_Signal_Valid	1	6%	0	837	1302
	_ADC_Read_Signal	1	6%	0	805	1272
	in	0	100%
_ADC_Read_Signal	out	0	in	1
	out	0	100%
	in	1	100%
	_Analog_Signal_Conv_Service	1	100%	0	805	1272
_ADC_Read_Signal_Valid	out	0	in	1
	out	0	100%
	in	1	100%
	_Analog_Signal_Conv_Service	1	100%	0	837	1302
_ADC_Conv_Single_Channel	out	5	in	0
	out	8	100%
	_ADC_Get_Conversion_Result	1	12%	0	1425	0
	_ADC_Start_Conversion	1	12%	0	1385	0
	_ADC_Get_Conversion_Status	2	25%	0	1393	0
	_ADC_Data_Calibrate	2	25%	0	1895	0
	_ADC_Input_Voltage_Calc	2	25%	0	1635	0
	in	0	100%
_TimerB_PWM_Init	out	0	in	1
	out	0	100%
	in	1	100%
	_PWN_Init	1	100%	0	7	0
_TimerB_PWM_Master_Channel_Init..Z.3A.5CD.5Ctest.5CFX12_test.5Cghs.5Cobj.5CTimerB.	out	0	in	0
	out	0	100%
	in	0	100%
_TimerB_PWM_Slave_Channel_Init..Z.3A.5CD.5Ctest.5CFX12_test.5Cghs.5Cobj.5CTimerB.	out	0	in	0
	out	0	100%
	in	0	100%
_TimerB_PWM_Channel_Init	out	0	in	1
	out	0	100%
	in	1	100%
	_PWM_Channel_Init	1	100%	0	47	0
_TimerB_PWM_Channel_Fre_Set	out	0	in	1
	out	0	100%
	in	1	100%
	_PWM_Channel_Set_Freq	1	100%	0	85	0
_TimerB_PWM_Channel_Duty_Set	out	0	in	1
	out	0	100%
	in	1	100%
	_PWM_Channel_Set_Duty	1	100%	0	111	0
_TimerB_PWM_Channel_Start	out	0	in	1
	out	0	100%
	in	1	100%
	_PWM_Channel_Init	1	100%	0	53	0
_TimerB_PWM_Channel_Stop	out	0	in	1
	out	0	100%
	in	1	100%
	_PWM_Channel_Stop	1	100%	0	131	0
_TimerB_PWM_Channel_Sleep	out	0	in	0
	out	0	100%
	in	0	100%
_TimerB_Input_Capture_Channel_Init..Z.3A.5CD.5Ctest.5CFX12_test.5Cghs.5Cobj.5CTimerB.	out	0	in	0
	out	0	100%
	in	0	100%
_TimerB_Interval_Timer_Channel_Init..Z.3A.5CD.5Ctest.5CFX12_test.5Cghs.5Cobj.5CTimerB.	out	0	in	0
	out	0	100%
	in	0	100%
_TimerB_Input_Channel_Init	out	1	in	0
	out	2	100%
	_RH850_Peripheral_IRQ_Enable	2	100%	0	1125	0
	in	0	100%
_TimerB_Input_Channel_Start	out	0	in	0
	out	0	100%
	in	0	100%
_TimerB_Input_Channel_Stop	out	0	in	0
	out	0	100%
	in	0	100%
_TimerB_Input_Isr	out	1	in	0
	out	1	100%
	_TimerB_Cal_Fre	1	100%	0	1339	1352
	in	0	100%
_TimerB_Overflow_Isr	out	0	in	0
	out	0	100%
	in	0	100%
_TimerB_Cal_Fre	out	0	in	1
	out	0	100%
	in	1	100%
	_TimerB_Input_Isr	1	100%	0	1339	1352
_RSCAN0_CH_Baud_Rate_Cal..Z.3A.5CD.5Ctest.5CFX12_test.5Cghs.5Cobj.5CRSCAN.	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH_Init	out	1	in	0
	out	12	100%
	_RH850_Peripheral_IRQ_Enable	12	100%	0	2387	0
	in	0	100%
_RSCAN0_CH0_Receive	out	0	in	1
	out	0	100%
	in	1	100%
	_RSCAN0_CH0_RX_ISR	1	100%	0	7445	3092
_RSCAN0_CH1_Receive	out	0	in	1
	out	0	100%
	in	1	100%
	_RSCAN0_CH1_RX_ISR	1	100%	0	7599	3150
_RSCAN0_CH2_Receive	out	0	in	1
	out	0	100%
	in	1	100%
	_RSCAN0_CH2_RX_ISR	1	100%	0	7753	3208
_RSCAN0_CH3_Receive	out	0	in	1
	out	0	100%
	in	1	100%
	_RSCAN0_CH3_RX_ISR	1	100%	0	7907	3266
_RSCAN0_CH4_Receive	out	0	in	1
	out	0	100%
	in	1	100%
	_RSCAN0_CH4_RX_ISR	1	100%	0	8061	3324
_RSCAN0_CH5_Receive	out	0	in	1
	out	0	100%
	in	1	100%
	_RSCAN0_CH5_RX_ISR	1	100%	0	8215	3382
_RSCAN0_CH0_Set_FIFO0_Data	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH1_Set_FIFO0_Data	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH2_Set_FIFO0_Data	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH3_Set_FIFO0_Data	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH4_Set_FIFO0_Data	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH5_Set_FIFO0_Data	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH0_Set_TXBUF_Data	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH1_Set_TXBUF_Data	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH2_Set_TXBUF_Data	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH3_Set_TXBUF_Data	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH4_Set_TXBUF_Data	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH5_Set_TXBUF_Data	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH0_Get_Busoff_Status	out	0	in	1
	out	0	100%
	in	1	100%
	_RSCAN0_CH0_Busoff_Recover	1	100%	0	5953	5814
_RSCAN0_CH1_Get_Busoff_Status	out	0	in	1
	out	0	100%
	in	1	100%
	_RSCAN0_CH1_Busoff_Recover	1	100%	0	6023	5836
_RSCAN0_CH2_Get_Busoff_Status	out	0	in	1
	out	0	100%
	in	1	100%
	_RSCAN0_CH2_Busoff_Recover	1	100%	0	6093	5858
_RSCAN0_CH3_Get_Busoff_Status	out	0	in	1
	out	0	100%
	in	1	100%
	_RSCAN0_CH3_Busoff_Recover	1	100%	0	6163	5880
_RSCAN0_CH4_Get_Busoff_Status	out	0	in	1
	out	0	100%
	in	1	100%
	_RSCAN0_CH4_Busoff_Recover	1	100%	0	6233	5902
_RSCAN0_CH5_Get_Busoff_Status	out	0	in	1
	out	0	100%
	in	1	100%
	_RSCAN0_CH5_Busoff_Recover	1	100%	0	6303	5924
_RSCAN0_CH0_Busoff_Recover	out	1	in	0
	out	1	100%
	_RSCAN0_CH0_Get_Busoff_Status	1	100%	0	5953	5814
	in	0	100%
_RSCAN0_CH1_Busoff_Recover	out	1	in	0
	out	1	100%
	_RSCAN0_CH1_Get_Busoff_Status	1	100%	0	6023	5836
	in	0	100%
_RSCAN0_CH2_Busoff_Recover	out	1	in	0
	out	1	100%
	_RSCAN0_CH2_Get_Busoff_Status	1	100%	0	6093	5858
	in	0	100%
_RSCAN0_CH3_Busoff_Recover	out	1	in	0
	out	1	100%
	_RSCAN0_CH3_Get_Busoff_Status	1	100%	0	6163	5880
	in	0	100%
_RSCAN0_CH4_Busoff_Recover	out	1	in	0
	out	1	100%
	_RSCAN0_CH4_Get_Busoff_Status	1	100%	0	6233	5902
	in	0	100%
_RSCAN0_CH5_Busoff_Recover	out	1	in	0
	out	1	100%
	_RSCAN0_CH5_Get_Busoff_Status	1	100%	0	6303	5924
	in	0	100%
_RSCAN0_CH0_Abort	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH1_Abort	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH2_Abort	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH3_Abort	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH4_Abort	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH5_Abort	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH0_Sleep_Init	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH1_Sleep_Init	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH2_Sleep_Init	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH3_Sleep_Init	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH4_Sleep_Init	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH5_Sleep_Init	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_Sleep_Init	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH0_TX_Error_Count	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH1_TX_Error_Count	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH2_TX_Error_Count	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH3_TX_Error_Count	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH4_TX_Error_Count	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH5_TX_Error_Count	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH0_RX_Error_Count	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH1_RX_Error_Count	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH2_RX_Error_Count	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH3_RX_Error_Count	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH4_RX_Error_Count	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH5_RX_Error_Count	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH0_RX_ISR	out	1	in	0
	out	1	100%
	_RSCAN0_CH0_Receive	1	100%	0	7445	3092
	in	0	100%
_RSCAN0_CH1_RX_ISR	out	1	in	0
	out	1	100%
	_RSCAN0_CH1_Receive	1	100%	0	7599	3150
	in	0	100%
_RSCAN0_CH2_RX_ISR	out	1	in	0
	out	1	100%
	_RSCAN0_CH2_Receive	1	100%	0	7753	3208
	in	0	100%
_RSCAN0_CH3_RX_ISR	out	1	in	0
	out	1	100%
	_RSCAN0_CH3_Receive	1	100%	0	7907	3266
	in	0	100%
_RSCAN0_CH4_RX_ISR	out	1	in	0
	out	1	100%
	_RSCAN0_CH4_Receive	1	100%	0	8061	3324
	in	0	100%
_RSCAN0_CH5_RX_ISR	out	1	in	0
	out	1	100%
	_RSCAN0_CH5_Receive	1	100%	0	8215	3382
	in	0	100%
_RSCAN0_CH0_TX_ISR	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH1_TX_ISR	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH2_TX_ISR	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH3_TX_ISR	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH4_TX_ISR	out	0	in	0
	out	0	100%
	in	0	100%
_RSCAN0_CH5_TX_ISR	out	0	in	0
	out	0	100%
	in	0	100%
_GPIO_PIN_Init..Z.3A.5CD.5Ctest.5Cc928_test.5Cghs.5Cobj.5CGPIO.	out	0	in	0
	out	0	100%
	in	0	100%
_GPIO_Init	out	0	in	1
	out	0	100%
	in	1	100%
	_Sys_Startup_Init	1	100%	0	37	0
_GPIO_Get_Wake_Bit..Z.3A.5CD.5Ctest.5Cc928_test.5Cghs.5Cobj.5CGPIO.	out	0	in	0
	out	0	100%
	in	0	100%
_GPIO_Wakeup_PIN_Set	out	0	in	0
	out	0	100%
	in	0	100%
_GPIO_Register_Address_Cal..Z.3A.5CD.5Ctest.5Cc928_test.5Cghs.5Cobj.5CGPIO.	out	0	in	0
	out	0	100%
	in	0	100%
_GPIO_Config	out	0	in	0
	out	0	100%
	in	0	100%
_GPIO_SET_KEPP	out	0	in	0
	out	0	100%
	in	0	100%
_UART_Variate_Init..Z.3A.5CD.5Ctest.5CFX12_test.5Cghs.5Cobj.5CUART.	out	0	in	0
	out	0	100%
	in	0	100%
_UART_Init	out	1	in	1
	out	8	100%
	_RH850_Peripheral_IRQ_Enable	8	100%	0	741	0
	in	1	100%
	_BSP_InitUSART	1	100%	0	581	0
_UART_Sleep_Init	out	0	in	0
	out	0	100%
	in	0	100%
_UART_Ch0_Get_TX_Busy_Flag	out	0	in	2
	out	0	100%
	in	2	100%
	_UART_Ch0_Send_Multiple_Byte	1	50%	0	995	830
	_BSP_SendString	1	50%	0	411	0
_UART_Ch1_Get_TX_Busy_Flag	out	0	in	2
	out	0	100%
	in	2	100%
	_UART_Ch1_Send_Multiple_Byte	1	50%	0	1103	866
	_Get_Uart_BusyFlash	1	50%	0	2135	866
_UART_Ch2_Get_TX_Busy_Flag	out	0	in	1
	out	0	100%
	in	1	100%
	_UART_Ch2_Send_Multiple_Byte	1	100%	0	1217	902
_UART_Ch3_Get_TX_Busy_Flag	out	0	in	1
	out	0	100%
	in	1	100%
	_UART_Ch3_Send_Multiple_Byte	1	100%	0	1323	938
_UART_Ch0_Send_Multiple_Byte	out	1	in	1
	out	1	100%
	_UART_Ch0_Get_TX_Busy_Flag	1	100%	0	995	830
	in	1	100%
	_BSP_SendString	1	100%	0	407	0
_UART_Ch1_Send_Multiple_Byte	out	1	in	0
	out	1	100%
	_UART_Ch1_Get_TX_Busy_Flag	1	100%	0	1103	866
	in	0	100%
_UART_Ch2_Send_Multiple_Byte	out	1	in	0
	out	1	100%
	_UART_Ch2_Get_TX_Busy_Flag	1	100%	0	1217	902
	in	0	100%
_UART_Ch3_Send_Multiple_Byte	out	1	in	0
	out	1	100%
	_UART_Ch3_Get_TX_Busy_Flag	1	100%	0	1323	938
	in	0	100%
_UART_CH0_RX_ISR	out	0	in	1
	out	0	100%
	in	1	100%
	_INTRLIN30UR1	1	100%	0	285	0
_UART_CH1_RX_ISR	out	0	in	0
	out	0	100%
	in	0	100%
_UART_CH2_RX_ISR	out	0	in	0
	out	0	100%
	in	0	100%
_UART_CH3_RX_ISR	out	0	in	0
	out	0	100%
	in	0	100%
_UART_CH0_TX_ISR	out	0	in	1
	out	0	100%
	in	1	100%
	_INTRLIN30UR0	1	100%	0	169	0
_UART_CH1_TX_ISR	out	0	in	0
	out	0	100%
	in	0	100%
_UART_CH2_TX_ISR	out	0	in	0
	out	0	100%
	in	0	100%
_UART_CH3_TX_ISR	out	0	in	0
	out	0	100%
	in	0	100%
_Get_Uart_BusyFlash	out	1	in	0
	out	1	100%
	_UART_Ch1_Get_TX_Busy_Flag	1	100%	0	2135	866
	in	0	100%
_RIIC0_Default_Mode_Status..Z.3A.5CD.5Ctest.5CFX12_test.5Cghs.5Cobj.5CRIIC.	out	0	in	0
	out	0	100%
	in	0	100%
_RIIC0_IsBusy	out	0	in	6
	out	0	100%
	in	6	100%
	_RIIC0_WaitForBusy_Block	1	16%	0	163	92
	_RIIC0_Master_SendMultiByte_Interrupt	1	16%	0	2523	92
	_RIIC0_Master_SendRecvMultiByte_Interrupt	1	16%	0	2921	92
	_RIIC0_Slave_RecvMultiByte	1	16%	0	3241	92
	_RIIC0_Master_RecvMultiByte_Interrupt	1	16%	0	2715	92
	_RIIC0_Slave_SendMultiByte	1	16%	0	3119	92
_RIIC0_WaitForBusy_Block	out	1	in	3
	out	1	100%
	_RIIC0_IsBusy	1	100%	0	163	92
	in	4	100%
	_AIM951_i2c_sendreceive	1	25%	0	1057	0
	_AIM951_i2c_send	1	25%	0	1007	0
	_fx12_test_server	2	50%	0	1885	0
_RIIC0_GPIO_Init..Z.3A.5CD.5Ctest.5CFX12_test.5Cghs.5Cobj.5CRIIC.	out	0	in	0
	out	0	100%
	in	0	100%
_RIIC0_Init	out	2	in	1
	out	8	100%
	_RH850_Peripheral_IRQ_Enable	4	50%	0	835	0
	_RH850_Peripheral_IRQ_Disable	4	50%	0	301	0
	in	1	100%
	_BSP_I2C0_INIT	1	100%	0	685	0
_RIIC0_Event_ISR	out	0	in	1
	out	0	100%
	in	1	100%
	_INTRIIC0EE	1	100%	0	1605	0
_RIIC0_TX_ISR	out	0	in	1
	out	0	100%
	in	1	100%
	_INTRIIC0TI	1	100%	0	1489	0
_RIIC0_TX_End_ISR	out	0	in	1
	out	0	100%
	in	1	100%
	_INTRIIC0TEI	1	100%	0	1837	0
_RIIC0_RX_End_ISR	out	0	in	1
	out	0	100%
	in	1	100%
	_INTRIIC0RI	1	100%	0	1721	0
_RIIC0_Master_SendMultiByte_Interrupt	out	1	in	2
	out	1	100%
	_RIIC0_IsBusy	1	100%	0	2523	92
	in	2	100%
	_AIM951_i2c_send	1	50%	0	1003	0
	_fx12_test_server	1	50%	0	1929	0
_RIIC0_Master_RecvMultiByte_Interrupt	out	1	in	1
	out	1	100%
	_RIIC0_IsBusy	1	100%	0	2715	92
	in	1	100%
	_fx12_test_server	1	100%	0	1881	0
_RIIC0_Master_SendRecvMultiByte_Interrupt	out	1	in	1
	out	1	100%
	_RIIC0_IsBusy	1	100%	0	2921	92
	in	1	100%
	_AIM951_i2c_sendreceive	1	100%	0	1053	0
_RIIC0_Slave_SendMultiByte	out	1	in	0
	out	1	100%
	_RIIC0_IsBusy	1	100%	0	3119	92
	in	0	100%
_RIIC0_Slave_RecvMultiByte	out	1	in	0
	out	1	100%
	_RIIC0_IsBusy	1	100%	0	3241	92
	in	0	100%
_RIIC0_Slave_Recv_Flag	out	0	in	0
	out	0	100%
	in	0	100%
_RIIC0_Slave_Recv_Flag_Reset	out	0	in	0
	out	0	100%
	in	0	100%
_RIIC0_Slave_Recv_Count	out	0	in	0
	out	0	100%
	in	0	100%
_RIIC0_Slave_Send_Flag	out	0	in	0
	out	0	100%
	in	0	100%
_RIIC0_Slave_Send_Flag_Reset	out	0	in	0
	out	0	100%
	in	0	100%
_RIIC0_Slave_Send_Count	out	0	in	0
	out	0	100%
	in	0	100%
_RIIC1_Default_Mode_Status..Z.3A.5CD.5Ctest.5CFX12_test.5Cghs.5Cobj.5CRIIC.	out	0	in	0
	out	0	100%
	in	0	100%
_RIIC1_IsBusy	out	0	in	6
	out	0	100%
	in	6	100%
	_RIIC1_WaitForBusy_Block	1	16%	0	3603	3532
	_RIIC1_Master_RecvMultiByte_Interrupt	1	16%	0	6147	3532
	_RIIC1_Master_SendMultiByte_Interrupt	1	16%	0	5955	3532
	_RIIC1_Master_SendRecvMultiByte_Interrupt	1	16%	0	6353	3532
	_RIIC1_Slave_RecvMultiByte	1	16%	0	6673	3532
	_RIIC1_Slave_SendMultiByte	1	16%	0	6551	3532
_RIIC1_WaitForBusy_Block	out	1	in	0
	out	1	100%
	_RIIC1_IsBusy	1	100%	0	3603	3532
	in	0	100%
_RIIC1_GPIO_Init..Z.3A.5CD.5Ctest.5CFX12_test.5Cghs.5Cobj.5CRIIC.	out	0	in	0
	out	0	100%
	in	0	100%
_RIIC1_Init	out	2	in	0
	out	8	100%
	_RH850_Peripheral_IRQ_Enable	4	50%	0	4267	0
	_RH850_Peripheral_IRQ_Disable	4	50%	0	3733	0
	in	0	100%
_RIIC1_Event_ISR	out	0	in	1
	out	0	100%
	in	1	100%
	_INTRIIC1EE	1	100%	0	2069	0
_RIIC1_TX_ISR	out	0	in	1
	out	0	100%
	in	1	100%
	_INTRIIC1TI	1	100%	0	1953	0
_RIIC1_TX_End_ISR	out	0	in	1
	out	0	100%
	in	1	100%
	_INTRIIC1TEI	1	100%	0	2301	0
_RIIC1_RX_End_ISR	out	0	in	1
	out	0	100%
	in	1	100%
	_INTRIIC1RI	1	100%	0	2185	0
_RIIC1_Master_SendMultiByte_Interrupt	out	1	in	0
	out	1	100%
	_RIIC1_IsBusy	1	100%	0	5955	3532
	in	0	100%
_RIIC1_Master_RecvMultiByte_Interrupt	out	1	in	0
	out	1	100%
	_RIIC1_IsBusy	1	100%	0	6147	3532
	in	0	100%
_RIIC1_Master_SendRecvMultiByte_Interrupt	out	1	in	0
	out	1	100%
	_RIIC1_IsBusy	1	100%	0	6353	3532
	in	0	100%
_RIIC1_Slave_SendMultiByte	out	1	in	0
	out	1	100%
	_RIIC1_IsBusy	1	100%	0	6551	3532
	in	0	100%
_RIIC1_Slave_RecvMultiByte	out	1	in	0
	out	1	100%
	_RIIC1_IsBusy	1	100%	0	6673	3532
	in	0	100%
_RIIC1_Slave_Recv_Flag	out	0	in	0
	out	0	100%
	in	0	100%
_RIIC1_Slave_Recv_Flag_Reset	out	0	in	0
	out	0	100%
	in	0	100%
_RIIC1_Slave_Recv_Count	out	0	in	0
	out	0	100%
	in	0	100%
_RIIC1_Slave_Send_Flag	out	0	in	1
	out	0	100%
	in	2	100%
	_I2C1_Send_End	2	100%	0	621	0
_RIIC1_Slave_Send_Flag_Reset	out	0	in	1
	out	0	100%
	in	2	100%
	_I2C1_Send_End	2	100%	0	629	0
_RIIC1_Slave_Send_Count	out	0	in	1
	out	0	100%
	in	1	100%
	_I2C1_Send_End	1	100%	0	609	0
_SIM_8080_P_OUT_DATA	out	0	in	4
	out	0	100%
	in	6	100%
	_Sim_8080_Data_Write	2	33%	0	663	0
	_Sim_8080_Init	1	16%	0	297	0
	_Sim_8080_Command_Write	2	33%	0	481	0
	_Sim_8080_Data_Read	1	16%	0	871	0
_Sim_8080_Init	out	1	in	1
	out	1	100%
	_SIM_8080_P_OUT_DATA	1	100%	0	297	0
	in	1	100%
	_LCD_Init	1	100%	0	11	0
_Sim_8080_Command_Write	out	1	in	5
	out	2	100%
	_SIM_8080_P_OUT_DATA	2	100%	0	481	0
	in	25	100%
	_LCD_Init	19	76%	0	671	0
	_LCD_Start_Data_Writing	1	4%	0	949	0
	_LCD_Start_Data_Reading	1	4%	0	999	0
	_LCD_Shutdown	2	8%	0	741	0
	_LCD_Set_Window	2	8%	0	885	0
_Sim_8080_Data_Write	out	1	in	6
	out	2	100%
	_SIM_8080_P_OUT_DATA	2	100%	0	663	0
	in	78	100%
	_LCD_Init	65	83%	0	689	0
	_LCD_Start_Data_Writing	1	1%	0	957	0
	_LCD_Start_Data_Reading	1	1%	0	1007	0
	_LCD_Shutdown	2	2%	0	749	0
	_LCD_Write_Data	1	1%	0	977	0
	_LCD_Set_Window	8	10%	0	909	0
_Sim_8080_Data_Read	out	1	in	1
	out	1	100%
	_SIM_8080_P_OUT_DATA	1	100%	0	871	0
	in	1	100%
	_LCD_Read_Data	1	100%	0	1025	0
_TFT_LCD_Startup	out	1	in	1
	out	1	100%
	_LCD_Init	1	100%	0	7	0
	in	1	100%
	_Sys_Startup_Init	1	100%	0	113	0
_TFT_LCD_Shutdown	out	1	in	0
	out	1	100%
	_LCD_Shutdown	1	100%	0	107	0
	in	0	100%
_TFT_LCD_Set_Brightness	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Busy_Check	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Display_Update_Service	out	0	in	1
	out	0	100%
	in	1	100%
	_main	1	100%	0	33	0
_TFT_LCD_Cls	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Draw_Bmp	out	0	in	3
	out	0	100%
	in	29	100%
	_Display_Init	7	24%	0	551	0
	_fx12_test_server	12	41%	0	1847	0
	_ver_Display	10	34%	0	363	0
_TFT_LCD_Draw_NEAR_Bmp	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Draw_Traffic_Bmp	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Draw_Transparent_Bmp	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Draw_Pixel	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Draw_Horizontal_Line	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Draw_Vertical_Line	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Draw_Box	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Cls_Handler..Z.3A.5CD.5Ctest.5C393_TEST.5Cghs.5Cobj.5CTFT_LCD.	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Direct_Draw_Bmp_Handler..Z.3A.5CD.5Ctest.5C393_TEST.5Cghs.5Cobj.5CTFT_LCD.	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Insert_Draw_Bmp_Handler..Z.3A.5CD.5Ctest.5C393_TEST.5Cghs.5Cobj.5CTFT_LCD.	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Direct_Draw_Transparent_Bmp_Handler..Z.3A.5CD.5Ctest.5C393_TEST.5Cghs.5Cobj.5CTFT_LCD.	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Insert_Draw_Transparent_Bmp_Handler..Z.3A.5CD.5Ctest.5C393_TEST.5Cghs.5Cobj.5CTFT_LCD.	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Draw_Pixel_Handler..Z.3A.5CD.5Ctest.5C393_TEST.5Cghs.5Cobj.5CTFT_LCD.	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Draw_Horizontal_Line_Handler..Z.3A.5CD.5Ctest.5C393_TEST.5Cghs.5Cobj.5CTFT_LCD.	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Draw_Vertical_Line_Handler..Z.3A.5CD.5Ctest.5C393_TEST.5Cghs.5Cobj.5CTFT_LCD.	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Draw_Box_Border_Handler..Z.3A.5CD.5Ctest.5C393_TEST.5Cghs.5Cobj.5CTFT_LCD.	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Direct_Draw_Full_Box_Handler..Z.3A.5CD.5Ctest.5C393_TEST.5Cghs.5Cobj.5CTFT_LCD.	out	0	in	0
	out	0	100%
	in	0	100%
_TFT_LCD_Insert_Draw_Full_Box_Handler..Z.3A.5CD.5Ctest.5C393_TEST.5Cghs.5Cobj.5CTFT_LCD.	out	0	in	0
	out	0	100%
	in	0	100%
_LCD_Init	out	4	in	1
	out	89	100%
	_Sim_8080_Data_Write	65	73%	0	689	0
	_Sim_8080_Init	1	1%	0	11	0
	_Sim_8080_Command_Write	19	21%	0	671	0
	_BSP_Delay_ms	4	4%	0	577	0
	in	1	100%
	_TFT_LCD_Startup	1	100%	0	7	0
_LCD_Shutdown	out	3	in	1
	out	6	100%
	_Sim_8080_Data_Write	2	33%	0	749	0
	_Sim_8080_Command_Write	2	33%	0	741	0
	_BSP_Delay_ms	2	33%	0	779	0
	in	1	100%
	_TFT_LCD_Shutdown	1	100%	0	107	0
_LCD_Set_Window	out	2	in	11
	out	10	100%
	_Sim_8080_Data_Write	8	80%	0	909	0
	_Sim_8080_Command_Write	2	20%	0	885	0
	in	50	100%
	.static000030ee	1	2%	0	5829	0
	.static00003103	1	2%	0	5985	0
	.static0000311c	5	10%	0	6843	0
	.static00003160	2	4%	0	7185	0
	.static0000318d	2	4%	0	7631	0
	.static000031e9	2	4%	0	8747	0
	.static00003200	2	4%	0	8945	0
	.static0000322e	7	14%	0	9771	0
	.static00003283	18	36%	0	11941	0
	.static0000337c	3	6%	0	12359	0
	.static000033b8	7	14%	0	13559	0
_LCD_Start_Data_Writing	out	2	in	11
	out	2	100%
	_Sim_8080_Data_Write	1	50%	0	957	0
	_Sim_8080_Command_Write	1	50%	0	949	0
	in	29	100%
	.static000030ee	1	3%	0	5833	0
	.static00003103	1	3%	0	5989	0
	.static0000311c	3	10%	0	6847	0
	.static00003160	1	3%	0	7189	0
	.static0000318d	1	3%	0	7635	0
	.static000031e9	1	3%	0	8751	0
	.static00003200	1	3%	0	8949	0
	.static0000322e	4	13%	0	9775	0
	.static00003283	10	34%	0	11945	0
	.static0000337c	2	6%	0	12363	0
	.static000033b8	4	13%	0	13563	0
_LCD_Write_Data	out	1	in	11
	out	1	100%
	_Sim_8080_Data_Write	1	100%	0	977	0
	in	66	100%
	.static000030ee	1	1%	0	5851	0
	.static00003103	1	1%	0	6055	0
	.static0000311c	3	4%	0	6909	0
	.static00003160	3	4%	0	7385	0
	.static0000318d	9	13%	0	8433	0
	.static000031e9	1	1%	0	8757	0
	.static00003200	3	4%	0	9083	0
	.static0000322e	9	13%	0	9839	0
	.static00003283	24	36%	0	12009	0
	.static0000337c	3	4%	0	12457	0
	.static000033b8	9	13%	0	13697	0
_LCD_Start_Data_Reading	out	2	in	9
	out	2	100%
	_Sim_8080_Data_Write	1	50%	0	1007	0
	_Sim_8080_Command_Write	1	50%	0	999	0
	in	21	100%
	.static0000311c	2	9%	0	6781	0
	.static00003160	1	4%	0	7129	0
	.static0000318d	1	4%	0	7575	0
	.static000031e9	1	4%	0	8633	0
	.static00003200	1	4%	0	8889	0
	.static0000322e	3	14%	0	9735	0
	.static00003283	8	38%	0	11905	0
	.static0000337c	1	4%	0	12165	0
	.static000033b8	3	14%	0	13503	0
_LCD_Read_Data	out	1	in	9
	out	1	100%
	_Sim_8080_Data_Read	1	100%	0	1025	0
	in	42	100%
	.static0000311c	4	9%	0	6805	0
	.static00003160	2	4%	0	7153	0
	.static0000318d	2	4%	0	7599	0
	.static000031e9	2	4%	0	8643	0
	.static00003200	2	4%	0	8913	0
	.static0000322e	6	14%	0	9747	0
	.static00003283	16	38%	0	11917	0
	.static0000337c	2	4%	0	12189	0
	.static000033b8	6	14%	0	13527	0
_R_CLKC_PllInit	out	0	in	0
	out	0	100%
	in	0	100%
_R_CLKC_SetRscanClockDomain	out	0	in	0
	out	0	100%
	in	0	100%
_R_CLKC_SetAdca0ClockDomain	out	0	in	0
	out	0	100%
	in	0	100%
_R_CLKC_SetTaujClockDomain	out	0	in	0
	out	0	100%
	in	0	100%
_R_CLKC_SetAdca0StopMask	out	0	in	0
	out	0	100%
	in	0	100%
_R_CLKC_ResetAdca0StopMask	out	0	in	0
	out	0	100%
	in	0	100%
_R_CLKC_SetTaujStopMask	out	0	in	0
	out	0	100%
	in	0	100%
_R_CLKC_ResetTaujStopMask	out	0	in	0
	out	0	100%
	in	0	100%
_FCL_Ctrl	out	3	in	0
	out	8	100%
	_R_FCL_Execute	6	75%	0	335	0
	_FCLUser_Open	1	12%	0	67	0
	_FCLUser_Close	1	12%	0	339	0
	in	0	100%
_Sys_Startup_Pre_Init	out	1	in	0
	out	1	100%
	_Clock_Run_Mode_Init	1	100%	0	7	0
	in	0	100%
_Sys_Startup_Init	out	16	in	1
	out	19	100%
	_WDT_Init	1	5%	0	45	0
	_Sys_Tick_Timer_Start	1	5%	0	49	0
	_GPIO_Init	1	5%	0	37	0
	_TFT_LCD_Startup	1	5%	0	113	0
	_BSP_GPIO_96751_1V8_EN	1	5%	0	75	0
	_BSP_GPIO_TFT_EN	1	5%	0	87	0
	_BSP_GPIO_96751_1V_EN	1	5%	0	63	0
	_BSP_GPIO_96751_PDB_EN	1	5%	0	101	0
	_BSP_Delay_ms	4	21%	0	109	0
	_BSP_InitUSART	1	5%	0	53	0
	_BSP_PWM_Init	1	5%	0	121	0
	_BSP_I2C0_INIT	1	5%	0	57	0
	_touch_IRQ_Enable	1	5%	0	41	0
	_init_951	1	5%	0	125	0
	_RTE_FCL_OP	1	5%	0	27	0
	_Display_Init	1	5%	0	117	0
	in	1	100%
	_main	1	100%	0	9	0
_INTOSTM0	out	1	in	0
	out	1	100%
	_BSP_FTM0_IRQHandler	1	100%	0	53	0
	in	0	100%
_INTRLIN30UR0	out	1	in	0
	out	1	100%
	_UART_CH0_TX_ISR	1	100%	0	169	0
	in	0	100%
_INTRLIN30UR1	out	1	in	0
	out	1	100%
	_UART_CH0_RX_ISR	1	100%	0	285	0
	in	0	100%
_INTTAUB0I0	out	0	in	0
	out	0	100%
	in	0	100%
_INTTAUB0I1	out	0	in	0
	out	0	100%
	in	0	100%
_INTTAUB0I2	out	0	in	0
	out	0	100%
	in	0	100%
_INTTAUB0I3	out	0	in	0
	out	0	100%
	in	0	100%
_INTTAUB0I4	out	0	in	0
	out	0	100%
	in	0	100%
_INTTAUB0I5	out	0	in	0
	out	0	100%
	in	0	100%
_INTTAUB0I6	out	0	in	0
	out	0	100%
	in	0	100%
_INTTAUB0I7	out	0	in	0
	out	0	100%
	in	0	100%
_INTTAUB0I8	out	0	in	0
	out	0	100%
	in	0	100%
_INTTAUB0I9	out	0	in	0
	out	0	100%
	in	0	100%
_INTTAUB0I10	out	0	in	0
	out	0	100%
	in	0	100%
_INTTAUB0I11	out	0	in	0
	out	0	100%
	in	0	100%
_INTTAUB0I12	out	0	in	0
	out	0	100%
	in	0	100%
_INTTAUB0I13	out	0	in	0
	out	0	100%
	in	0	100%
_INTTAUB0I14	out	0	in	0
	out	0	100%
	in	0	100%
_INTTAUB0I15	out	0	in	0
	out	0	100%
	in	0	100%
_INTRIIC0TI	out	1	in	0
	out	1	100%
	_RIIC0_TX_ISR	1	100%	0	1489	0
	in	0	100%
_INTRIIC0EE	out	1	in	0
	out	1	100%
	_RIIC0_Event_ISR	1	100%	0	1605	0
	in	0	100%
_INTRIIC0RI	out	1	in	0
	out	1	100%
	_RIIC0_RX_End_ISR	1	100%	0	1721	0
	in	0	100%
_INTRIIC0TEI	out	1	in	0
	out	1	100%
	_RIIC0_TX_End_ISR	1	100%	0	1837	0
	in	0	100%
_INTRIIC1TI	out	1	in	0
	out	1	100%
	_RIIC1_TX_ISR	1	100%	0	1953	0
	in	0	100%
_INTRIIC1EE	out	1	in	0
	out	1	100%
	_RIIC1_Event_ISR	1	100%	0	2069	0
	in	0	100%
_INTRIIC1RI	out	1	in	0
	out	1	100%
	_RIIC1_RX_End_ISR	1	100%	0	2185	0
	in	0	100%
_INTRIIC1TEI	out	1	in	0
	out	1	100%
	_RIIC1_TX_End_ISR	1	100%	0	2301	0
	in	0	100%
_INTP2	out	1	in	0
	out	1	100%
	_BSP_TOUCH_IRQHandler	1	100%	0	2417	0
	in	0	100%
_main	out	8	in	1
	out	9	100%
	_WDT_Clear	1	11%	0	77	0
	_TFT_LCD_Display_Update_Service	1	11%	0	33	0
	_Sys_Startup_Init	1	11%	0	9	0
	_uart1_printf	1	11%	0	19	0
	_TimeStamp_Reset	2	22%	0	73	0
	_TimeStamp_Update	1	11%	0	47	0
	_TimeStamp_GetCntTime	1	11%	0	57	0
	_fx12_test_server	1	11%	0	37	0
	in	1	100%
	___ghs_ind_crt1	1	100%	0	189	0
.intvect..Z.3A.5CD.5Ctest.5CFX12_test.5Cghs.5Cobj.5Cdr7f701684_startup.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_I_read_memory_u32..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_I_read_memory_u16..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_I_read_memory_u08..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_I_write_unaligned_memory_u32..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_I_write_memory_u32..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_I_write_memory_u16..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_I_write_memory_u08	out	0	in	9
	out	0	100%
	in	28	100%
	.static00003f52	4	14%	0	99	132
	.static00003fcc	1	3%	0	919	132
	.static00003fe1	2	7%	0	1121	132
	.static00004045	1	3%	0	1679	132
	_R_FCL_FCUFct_GetConfigArea	1	3%	0	1563	132
	_R_FCL_FCUFct_PrepareEnvironment	3	10%	0	2157	132
	_R_FCL_FCUFct_HandleMultiOperation	14	50%	0	4947	132
	_R_FCL_FCUFct_GetDeviceName	1	3%	0	1057	132
	_R_FCL_Init	1	3%	0	627	0
_R_FCL_I_GetCPUCorePid..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_FCUFct_VerifyID..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_FCUFct_Clear_Cache..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_FCUFct_Chk_DBFull..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_FCUFct_SetFrequency..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_FCUFct_SwitchMode_Start	out	0	in	3
	out	0	100%
	in	7	100%
	_R_FCL_FCUFct_PrepareEnvironment	2	28%	0	2131	676
	_R_FCL_FCUFct_HandleMultiOperation	4	57%	0	6385	676
	.static000046d0	1	14%	0	93	0
_R_FCL_FCUFct_SwitchMode_Check	out	0	in	3
	out	0	100%
	in	5	100%
	_R_FCL_FCUFct_PrepareEnvironment	2	40%	0	2177	844
	_R_FCL_FCUFct_HandleMultiOperation	2	40%	0	6005	844
	.static000046d0	1	20%	0	125	0
_R_FCL_FCUFct_ForcedStop..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_FCUFct_ChkSuspended..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_FCUFct_ClearStatus..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_FCUFct_RestoreLastState..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_FCUFct_GetResult..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_FCUFct_GetConfigArea	out	1	in	2
	out	1	100%
	_R_FCL_I_write_memory_u08	1	100%	0	1563	132
	in	2	100%
	_R_FCL_Fct_CallFromRAM	1	50%	0	41	1396
	_R_FCL_CopySections	1	50%	0	256	0
_R_FCL_FCUFct_PrepareEnvironment_IntErr..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_FCUFct_PrepareEnvironment	out	3	in	1
	out	7	100%
	_R_FCL_I_write_memory_u08	3	42%	0	2157	132
	_R_FCL_FCUFct_SwitchMode_Start	2	28%	0	2131	676
	_R_FCL_FCUFct_SwitchMode_Check	2	28%	0	2177	844
	in	1	100%
	.static000046d0	1	100%	0	215	0
_R_FCL_FCUFct_GetDeviceInfo..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_FCUFct_HandleMultiOperation_IntErr..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_FCUFct_HandleMultiOperation	out	3	in	1
	out	20	100%
	_R_FCL_I_write_memory_u08	14	70%	0	4947	132
	_R_FCL_FCUFct_SwitchMode_Start	4	20%	0	6385	676
	_R_FCL_FCUFct_SwitchMode_Check	2	10%	0	6005	844
	in	1	100%
	.static000046d0	1	100%	0	221	0
_R_FCL_Fct_CallFromRAM	out	1	in	1
	out	1	100%
	_R_FCL_FCUFct_GetConfigArea	1	100%	0	41	1396
	in	3	100%
	_R_FCL_Execute	3	100%	0	477	0
_R_FCL_FCUFct_CheckMode	out	0	in	5
	out	0	100%
	in	5	100%
	_R_FCL_FCUFct_SetConfigArea	1	20%	0	109	56
	_R_FCL_FCUFct_Erase	1	20%	0	1565	56
	_R_FCL_FCUFct_Write	1	20%	0	2157	56
	_R_FCL_FCUFct_HandleLockBit	1	20%	0	2681	56
	_R_FCL_Execute	1	20%	0	45	0
_R_FCL_FCUFct_SetConfigArea	out	1	in	1
	out	1	100%
	_R_FCL_FCUFct_CheckMode	1	100%	0	109	56
	in	4	100%
	_R_FCL_Execute	4	100%	0	567	0
_R_FCL_FCUFct_GetSecurityFlag	out	0	in	1
	out	0	100%
	in	1	100%
	_R_FCL_Execute	1	100%	0	733	0
_R_FCL_FCUFct_GetBlockCnt	out	0	in	1
	out	0	100%
	in	1	100%
	_R_FCL_Execute	1	100%	0	631	0
_R_FCL_FCUFct_GetDeviceName	out	1	in	1
	out	1	100%
	_R_FCL_I_write_memory_u08	1	100%	0	1057	132
	in	1	100%
	_R_FCL_Execute	1	100%	0	599	0
_R_FCL_FCUFct_GetBlockEndAddr	out	0	in	1
	out	0	100%
	in	1	100%
	_R_FCL_Execute	1	100%	0	663	0
_R_FCL_FCUFct_Erase	out	1	in	1
	out	1	100%
	_R_FCL_FCUFct_CheckMode	1	100%	0	1565	56
	in	1	100%
	_R_FCL_Execute	1	100%	0	185	0
_R_FCL_FCUFct_Write	out	1	in	1
	out	1	100%
	_R_FCL_FCUFct_CheckMode	1	100%	0	2157	56
	in	1	100%
	_R_FCL_Execute	1	100%	0	219	0
_R_FCL_FCUFct_HandleLockBit	out	1	in	1
	out	1	100%
	_R_FCL_FCUFct_CheckMode	1	100%	0	2681	56
	in	2	100%
	_R_FCL_Execute	2	100%	0	269	0
_R_FCL_FCUFct_LockBitMode	out	0	in	1
	out	0	100%
	in	2	100%
	_R_FCL_Execute	2	100%	0	305	0
_R_FCL_CopySections	out	2	in	3
	out	3	100%
	_R_FCL_FCUFct_GetConfigArea	1	33%	0	256	0
	_R_FCL_CalcFctAddr	2	66%	0	281	316
	in	3	100%
	_FCL_Ctrl1	1	33%	0	25	0
	_Internal_FCL_OPEN	1	33%	0	673	0
	_FCL_Init_ALL	1	33%	0	213	0
_R_FCL_CalcFctAddr	out	0	in	1
	out	0	100%
	in	2	100%
	_R_FCL_CopySections	2	100%	0	281	316
_R_FCL_GetVersionString	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_Init	out	1	in	3
	out	1	100%
	_R_FCL_I_write_memory_u08	1	100%	0	627	0
	in	3	100%
	_FCL_Ctrl1	1	33%	0	15	0
	_Internal_FCL_OPEN	1	33%	0	663	0
	_FCL_Init_ALL	1	33%	0	203	0
_R_FCL_Handler..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_user_if.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FCL_Fct_Handler..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fcl_user_if.	out	0	in	0
	out	0	100%
	in	0	100%
_FCL_Return_HandleStatus	out	0	in	1
	out	0	100%
	in	1	100%
	_FCL_Init	1	100%	0	23	0
_R_FCL_Execute	out	11	in	8
	out	18	100%
	_R_FCL_FCUFct_SetConfigArea	4	22%	0	567	0
	_R_FCL_Fct_CallFromRAM	3	16%	0	477	0
	_R_FCL_FCUFct_CheckMode	1	5%	0	45	0
	_R_FCL_FCUFct_GetBlockCnt	1	5%	0	631	0
	_R_FCL_FCUFct_GetSecurityFlag	1	5%	0	733	0
	_R_FCL_FCUFct_GetDeviceName	1	5%	0	599	0
	_R_FCL_FCUFct_Erase	1	5%	0	185	0
	_R_FCL_FCUFct_Write	1	5%	0	219	0
	_R_FCL_FCUFct_GetBlockEndAddr	1	5%	0	663	0
	_R_FCL_FCUFct_HandleLockBit	2	11%	0	269	0
	_R_FCL_FCUFct_LockBitMode	2	11%	0	305	0
	in	19	100%
	_Internal_FCL_Init	1	5%	0	791	0
	_OptionByte_Handle	2	10%	0	1295	0
	_Internal_FCL_Erase	1	5%	0	931	0
	_Internal_FCL_Unlock	1	5%	0	843	0
	_Internal_FCL_Write	1	5%	0	1029	0
	_FCL_Ctrl1	6	31%	0	523	0
	_FCL_Ctrl	6	31%	0	335	0
	_FCL_Init	1	5%	0	17	0
_FCL_Init	out	2	in	1
	out	2	100%
	_FCL_Return_HandleStatus	1	50%	0	23	0
	_R_FCL_Execute	1	50%	0	17	0
	in	1	100%
	_FCL_Init_ALL	1	100%	0	223	0
_FCLUser_Open	out	0	in	4
	out	0	100%
	in	4	100%
	_FCL_Ctrl1	1	25%	0	89	0
	_Internal_FCL_OPEN	1	25%	0	737	0
	_FCL_Ctrl	1	25%	0	67	0
	_FCL_Init_ALL	1	25%	0	219	48
_FCLUser_Close	out	0	in	3
	out	0	100%
	in	3	100%
	_FCL_Ctrl1	1	33%	0	635	0
	_Internal_FCL_CLOSE	1	33%	0	757	0
	_FCL_Ctrl	1	33%	0	339	0
_FCL_Init_ALL	out	4	in	0
	out	4	100%
	_R_FCL_CopySections	1	25%	0	213	0
	_R_FCL_Init	1	25%	0	203	0
	_FCL_Init	1	25%	0	223	0
	_FCLUser_Open	1	25%	0	219	48
	in	0	100%
_FDL_User_CriticalSetionBegin	out	0	in	0
	out	0	100%
	in	0	100%
_FDL_User_CriticalSetionEnd	out	0	in	0
	out	0	100%
	in	0	100%
_FDL_Open	out	0	in	1
	out	0	100%
	in	1	100%
	_Internal_EEPROM_OPEN	1	100%	0	7	0
_FDL_Close	out	0	in	1
	out	0	100%
	in	1	100%
	_Internal_EEPROM_CLOSE	1	100%	0	25	0
_R_FDL_IFct_ReadMemoryU32_TS..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_IFct_ReadMemoryU08_TS..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_IFct_ReadMemoryU16_TS..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_IFct_WriteMemoryU08_TS	out	0	in	6
	out	0	100%
	in	12	100%
	_R_FDL_InitVariables	1	8%	0	35	0
	_R_FDL_FCUFct_ForcedStop	1	8%	0	367	18
	_R_FDL_FCUFct_Switch_FAEINT	2	16%	0	559	18
	_R_FDL_FCUFct_ClearStatus	2	16%	0	511	18
	_R_FDL_FCUFct_StartBCEraseOperation	2	16%	0	1987	18
	_R_FDL_FCUFct_ReadOperation	4	33%	0	2275	18
_R_FDL_IFct_WriteMemoryU16_TS..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_IFct_WriteMemoryU32_TS..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_IFct_CalcFOpUnitCnt_BC	out	0	in	2
	out	0	100%
	in	2	100%
	.static00004f54	1	50%	0	3679	0
	.static00004e88	1	50%	0	2021	0
_R_FDL_IFct_ChkAccessBoundaries	out	0	in	2
	out	0	100%
	in	2	100%
	.static00004f54	1	50%	0	3759	0
	.static00004a2b	1	50%	0	289	66
_R_FDL_IFct_ChkAccessRight..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_FCUFct_ChkReg_Asm	out	0	in	1
	out	0	100%
	in	1	100%
	_R_FDL_FCUFct_ForcedStop	1	100%	0	415	324
_R_FDL_FCUFct_ForcedStop	out	2	in	4
	out	2	100%
	_R_FDL_FCUFct_ChkReg_Asm	1	50%	0	415	324
	_R_FDL_IFct_WriteMemoryU08_TS	1	50%	0	367	18
	in	5	100%
	_R_FDL_FCUFct_StartWriteOperation	1	20%	0	1857	352
	_R_FDL_FCUFct_StartBCEraseOperation	1	20%	0	1993	352
	.static00004e0e	1	20%	0	653	0
	.static00004ea6	2	40%	0	2503	0
_R_FDL_FCUFct_ClearStatus	out	1	in	4
	out	2	100%
	_R_FDL_IFct_WriteMemoryU08_TS	2	100%	0	511	18
	in	4	100%
	_R_FDL_FCUFct_SwitchMode_Start	1	25%	0	1263	442
	.static00004e6d	1	25%	0	1473	0
	.static00004e5c	1	25%	0	1367	0
	.static00004ea6	1	25%	0	2509	0
_R_FDL_FCUFct_Switch_FAEINT	out	1	in	1
	out	2	100%
	_R_FDL_IFct_WriteMemoryU08_TS	2	100%	0	559	18
	in	3	100%
	.static00004ea6	3	100%	0	2521	0
_R_FDL_IFct_GetFWParam..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_hw_access.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_FCUFct_GetDFSize	out	0	in	1
	out	0	100%
	in	1	100%
	.static00004ea6	1	100%	0	2605	0
_R_FDL_FCUFct_SetFrequency	out	0	in	1
	out	0	100%
	in	1	100%
	.static00004ea6	1	100%	0	2649	0
_R_FDL_FCUFct_VerifyChecksum	out	0	in	1
	out	0	100%
	in	1	100%
	.static00004ea6	1	100%	0	2577	0
_R_FDL_FCUFct_InitRAM	out	0	in	1
	out	0	100%
	in	1	100%
	.static00004ea6	1	100%	0	2429	0
_R_FDL_FCUFct_SwitchMode_Start	out	1	in	10
	out	1	100%
	_R_FDL_FCUFct_ClearStatus	1	100%	0	1263	442
	in	14	100%
	.static00004f54	2	14%	0	4023	0
	_R_FDL_Execute	1	7%	0	355	0
	.static00004e34	2	14%	0	1077	0
	.static00004e0e	1	7%	0	675	0
	.static00004e6d	1	7%	0	1553	0
	.static00004e5c	1	7%	0	1373	0
	.static00004e88	1	7%	0	2113	0
	.static00004ea6	3	21%	0	2515	0
	_R_FDL_Handler	1	7%	0	2999	0
	_R_FDL_CancelRequest	1	7%	0	3459	0
_R_FDL_FCUFct_SwitchMode_Check_TS	out	0	in	9
	out	0	100%
	in	10	100%
	.static00004f54	1	10%	0	3857	0
	_R_FDL_FCUFct_StandBy_Processing	2	20%	0	2749	1398
	_R_FDL_FCUFct_WakeUp_Processing	1	10%	0	2973	1398
	.static00004e0e	1	10%	0	629	0
	.static00004e6d	1	10%	0	1559	0
	.static00004e5c	1	10%	0	1379	0
	.static00004e88	1	10%	0	2119	0
	.static00004ea6	1	10%	0	2235	0
	_R_FDL_Handler	1	10%	0	3005	0
_R_FDL_FCUFct_GetStat	out	0	in	1
	out	0	100%
	in	1	100%
	.static00004e6d	1	100%	0	1465	0
_R_FDL_FCUFct_StartWriteOperation	out	1	in	2
	out	1	100%
	_R_FDL_FCUFct_ForcedStop	1	100%	0	1857	352
	in	2	100%
	.static00004f54	1	50%	0	3933	0
	.static00004e88	1	50%	0	1837	0
_R_FDL_FCUFct_StartBCEraseOperation	out	2	in	2
	out	3	100%
	_R_FDL_IFct_WriteMemoryU08_TS	2	66%	0	1987	18
	_R_FDL_FCUFct_ForcedStop	1	33%	0	1993	352
	in	3	100%
	.static00004f54	1	33%	0	3911	0
	.static00004e88	2	66%	0	2069	0
_R_FDL_FCUFct_ReadOperation	out	1	in	1
	out	4	100%
	_R_FDL_IFct_WriteMemoryU08_TS	4	100%	0	2275	18
	in	1	100%
	.static00004f54	1	100%	0	3803	0
_R_FDL_FCUFct_ChkStartable	out	0	in	1
	out	0	100%
	in	1	100%
	_R_FDL_Execute	1	100%	0	483	0
_R_FDL_FCUFct_ChkSuspendable_TS	out	0	in	2
	out	0	100%
	in	2	100%
	_R_FDL_FCUFct_StandBy_Processing	1	50%	0	2831	2388
	.static00004e29	1	50%	0	851	0
_R_FDL_FCUFct_Suspend_TS	out	0	in	2
	out	0	100%
	in	2	100%
	_R_FDL_FCUFct_StandBy_Processing	1	50%	0	2839	2432
	.static00004e29	1	50%	0	859	0
_R_FDL_FCUFct_ResumeChkNeed_TS	out	0	in	1
	out	0	100%
	in	1	100%
	_R_FDL_FCUFct_WakeUp_Processing	1	100%	0	2995	2458
_R_FDL_FCUFct_Resume_TS	out	0	in	2
	out	0	100%
	in	2	100%
	_R_FDL_FCUFct_WakeUp_Processing	1	50%	0	3003	2500
	.static00004ea6	1	50%	0	2693	0
_R_FDL_FCUFct_ChkReady_TS	out	0	in	2
	out	0	100%
	in	2	100%
	_R_FDL_FCUFct_StandBy_Processing	1	50%	0	2809	2526
	_R_FDL_Handler	1	50%	0	2945	0
_R_FDL_FCUFct_CheckFatalError	out	0	in	1
	out	0	100%
	in	1	100%
	.static00004e5c	1	100%	0	1357	0
_R_FDL_FCUFct_StandBy_Processing	out	4	in	1
	out	5	100%
	_R_FDL_FCUFct_SwitchMode_Check_TS	2	40%	0	2749	1398
	_R_FDL_FCUFct_ChkSuspendable_TS	1	20%	0	2831	2388
	_R_FDL_FCUFct_Suspend_TS	1	20%	0	2839	2432
	_R_FDL_FCUFct_ChkReady_TS	1	20%	0	2809	2526
	in	1	100%
	_R_FDL_StandBy	1	100%	0	3325	0
_R_FDL_FCUFct_WakeUp_Processing	out	3	in	1
	out	3	100%
	_R_FDL_FCUFct_SwitchMode_Check_TS	1	33%	0	2973	1398
	_R_FDL_FCUFct_ResumeChkNeed_TS	1	33%	0	2995	2458
	_R_FDL_FCUFct_Resume_TS	1	33%	0	3003	2500
	in	1	100%
	_R_FDL_WakeUp	1	100%	0	3351	0
_R_FDL_InitVariables	out	1	in	1
	out	1	100%
	_R_FDL_IFct_WriteMemoryU08_TS	1	100%	0	35	0
	in	1	100%
	_R_FDL_Init	1	100%	0	7	0
_R_FDL_Execute	out	2	in	6
	out	2	100%
	_R_FDL_FCUFct_SwitchMode_Start	1	50%	0	355	0
	_R_FDL_FCUFct_ChkStartable	1	50%	0	483	0
	in	6	100%
	.static0000522b	1	16%	0	107	0
	.static00005343	1	16%	0	209	0
	.static00005353	1	16%	0	409	0
	.static0000532d	1	16%	0	55	0
	.static0000538b	1	16%	0	831	0
	.static0000537f	1	16%	0	677	0
_R_FDL_Handler_CancelReq..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_user_if.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_Handler_BusyAndSuspendPossible..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_user_if.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_Handler_ChkResume..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_user_if.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_Handler_ReactOnFatalErrors..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_user_if.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_Handler_StatusCheckAndSuspendOnReady..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_user_if.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_Handler_MultiOperation..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_user_if.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_Handler_OperationStates..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_user_if.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_Handler	out	3	in	3
	out	3	100%
	_R_FDL_FCUFct_SwitchMode_Check_TS	1	33%	0	3005	0
	_R_FDL_FCUFct_SwitchMode_Start	1	33%	0	2999	0
	_R_FDL_FCUFct_ChkReady_TS	1	33%	0	2945	0
	in	4	100%
	.static0000522b	1	25%	0	113	0
	.static0000532d	1	25%	0	65	0
	_R_EEL_FDLIF_Handler	2	50%	0	951	0
_R_FDL_GetVersionString	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_SuspendRequest	out	0	in	1
	out	0	100%
	in	1	100%
	_R_EEL_FDLIF_EraseSuspendRequest	1	100%	0	509	0
_R_FDL_ResumeRequest	out	0	in	1
	out	0	100%
	in	1	100%
	.static00005375	1	100%	0	543	0
_R_FDL_StandBy	out	1	in	0
	out	1	100%
	_R_FDL_FCUFct_StandBy_Processing	1	100%	0	3325	0
	in	0	100%
_R_FDL_WakeUp	out	1	in	0
	out	1	100%
	_R_FDL_FCUFct_WakeUp_Processing	1	100%	0	3351	0
	in	0	100%
_R_FDL_CancelRequest	out	1	in	0
	out	1	100%
	_R_FDL_FCUFct_SwitchMode_Start	1	100%	0	3459	0
	in	0	100%
_R_FDL_UFct_FlashOpStart..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_user_if.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_UFct_EndCurrentOperation..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_user_if.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_UFct_StateOperational..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_fdl_user_if.	out	0	in	0
	out	0	100%
	in	0	100%
_R_FDL_Init	out	1	in	1
	out	1	100%
	_R_FDL_InitVariables	1	100%	0	7	0
	in	1	100%
	.static0000522b	1	100%	0	73	0
_SampleApp_EEL_ErrorHdr	out	0	in	4
	out	0	100%
	in	9	100%
	_Internal_EEL_Init	1	11%	0	121	0
	_Internal_EEL_DEINIT	2	22%	0	429	0
	.static0000522b	2	22%	0	159	0
	_SampleApp_EEL_Control	4	44%	0	581	0
_SampleApp_EEL_HdrLoop	out	1	in	4
	out	1	100%
	_R_EEL_Handler	1	100%	0	29	0
	in	8	100%
	_Internal_EEL_Init	1	12%	0	93	0
	_Internal_EEL_Read	1	12%	0	329	0
	_Internal_EEL_Write	1	12%	0	215	0
	_SampleApp_EEL_Control	5	62%	0	543	14
_SampleApp_EEL_Init..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Ceelapp_control.	out	0	in	0
	out	0	100%
	in	0	100%
_SampleApp_EEL_Control	out	6	in	0
	out	19	100%
	_SampleApp_EEL_HdrLoop	5	26%	0	543	14
	_SampleApp_EEL_ErrorHdr	4	21%	0	581	0
	_R_EEL_GetDriverStatus	2	10%	0	565	0
	_R_EEL_Execute	5	26%	0	535	0
	_R_EEL_Handler	2	10%	0	557	0
	_R_EEL_ShutDown	1	5%	0	547	0
	in	0	100%
_EX_EE_INIT	out	0	in	1
	out	0	100%
	in	2	100%
	_Internal_EEL_Init	2	100%	0	97	0
_R_EEL_FDLIF_BlankCheck..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_FDLIF_Read..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_FDLIF_Write..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_FDLIF_WriteTag..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_FDLIF_EraseSuspendRequest	out	1	in	1
	out	1	100%
	_R_FDL_SuspendRequest	1	100%	0	509	0
	in	1	100%
	_R_EEL_Execute	1	100%	0	1013	0
_R_EEL_FDLIF_EraseResume..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_FDLIF_Erase..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_FDLIF_BitCheck..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_FDLIF_Handler	out	1	in	2
	out	2	100%
	_R_FDL_Handler	2	100%	0	951	0
	in	2	100%
	_R_EEL_SM_Prepare_EraseResume	1	50%	0	12351	884
	_R_EEL_Handler	1	50%	0	1313	0
_R_EEL_PFct_CastU32Ptr2Add..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_CastU08Ptr2Add	out	0	in	3
	out	0	100%
	in	3	100%
	_R_EEL_SM_WriteInc_Start	1	33%	0	8787	978
	_R_EEL_SM_Read_Start	1	33%	0	8455	978
	.static000063a0	1	33%	0	239	0
_R_EEL_PFct_ReadDFlashU32..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_BlankCheckDFlash..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_ReadDFlash_cmpPat..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_ReadDFlash_cmpPatBC..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_ReadDFlash_BCcmpPat..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_ReadDataFromAddU08..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_WriteDataToAddU08	out	0	in	2
	out	0	100%
	in	4	100%
	.static0000551f	3	75%	0	3365	1426
	_R_EEL_Init	1	25%	0	1523	0
_R_EEL_PFct_Calc_Add2vBlk..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_Calc_vBlkBaseAdd..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_Calc_vBlkTopAdd..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_Calc_vBlkDataAdd..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_Calc_BlkFreeSpace..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_ConvertTidx2RefAdd..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_ConvertRefAdd2WIdx..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_Get_RefAdd2DataAdd..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_Get_RefAdd2DataAdd_Rel..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_Chk_DSInvalidated_InvFlg..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_Chk_DSInvalidated..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_Chk_EELPoolSpaceForDS..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_ConvertId2TIdx	out	0	in	4
	out	0	100%
	in	4	100%
	.static000058a2	1	25%	0	10813	1960
	.static0000550a	1	25%	0	3013	1960
	.static000063a0	1	25%	0	193	0
	.static000063bc	1	25%	0	391	0
_R_EEL_PFct_ConvertId2TIdxSorted..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_ConvertTIdx2Len	out	0	in	6
	out	0	100%
	in	6	100%
	.static00005788	1	16%	0	8151	2094
	.static000058a2	1	16%	0	11059	2094
	_R_EEL_SM_WriteInc_Start	1	16%	0	8743	2094
	.static000063a0	1	16%	0	229	0
	.static000063bc	1	16%	0	421	0
	_R_EEL_Init	1	16%	0	1781	0
_R_EEL_PFct_ConvertTIdx2Id	out	0	in	2
	out	0	100%
	in	2	100%
	_R_EEL_SM_WriteInc_Start	1	50%	0	8639	2120
	_R_EEL_Init	1	50%	0	1799	0
_R_EEL_PFct_Get_RefAdd2ID..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_RoundUpToWriteGranularity..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_Pfct_AdjustByteCnt_ExtFeatures..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_PrepLoopLimitReset..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_Chk_ProcessActive	out	0	in	2
	out	0	100%
	in	2	100%
	.static000063a0	1	50%	0	171	0
	.static000063bc	1	50%	0	371	0
_R_EEL_PFct_Calc_BlockRWP..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_Calc_BlockEC..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_Read_BlkHeaderData24bit..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_PFct_Calc_BlkSpace	out	0	in	3
	out	0	100%
	in	3	100%
	_R_EEL_SFct_Calc_FreeSpace	1	33%	0	4657	2338
	_R_EEL_GetSpace	1	33%	0	2703	0
	_R_EEL_Init	1	33%	0	1835	0
_R_EEL_SFct_ChkBlockElder..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_SearchDS..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_Chk_DSValid..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_FindValidDS..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_FindValidDS_NoIdxTab..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_Read_Chk_Data..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_SetChecksum_8Bit_from_24bit..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_SetDriverStatus	out	3	in	14
	out	3	100%
	_R_EEL_SFct_ProcessErrorUpdate	1	33%	0	3723	4144
	_R_EEL_SFct_ErrStatCheckError	1	33%	0	3579	3860
	_R_EEL_SM_Supv_Run	1	33%	0	3712	15212
	in	20	100%
	.static00005742	4	20%	0	7795	3494
	.static0000588f	2	10%	0	10563	3494
	.static000059bb	1	5%	0	12921	3494
	.static00005a5a	1	5%	0	14537	3494
	.static00005a86	1	5%	0	15133	3494
	_R_EEL_SM_Read_Start	1	5%	0	8549	3494
	_R_EEL_SM_Supv_Run	2	10%	0	15341	3494
	_R_EEL_Execute	1	5%	0	1157	0
	_R_EEL_Handler	2	10%	0	1399	0
	_R_EEL_Init	1	5%	0	1653	0
	_R_EEL_Startup	1	5%	0	2181	0
	_R_EEL_ShutDown	1	5%	0	2267	0
	_R_EEL_SuspendRequest	1	5%	0	2441	0
	_R_EEL_ResumeRequest	1	5%	0	2527	0
_R_EEL_SFct_ErrStatCheckError_CurProc..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_ErrStatCheckError	out	0	in	6
	out	0	100%
	in	6	100%
	.static000058a2	1	16%	0	10645	3860
	.static00005574	1	16%	0	3845	3860
	.static000059a9	1	16%	0	12687	3860
	_R_EEL_SFct_SetDriverStatus	1	16%	0	3579	3860
	_R_EEL_SFct_ProcessErrorUpdate	1	16%	0	4215	3860
	_R_EEL_GetDriverStatus	1	16%	0	2621	0
_R_EEL_SFct_FlashConvertWriteStatus2ProcessStatus..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_FlashOpResultCheck_Write..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_FlashConvertEraseStatus2ProcessStatus..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_FlashConvertBitCheckStat2ProcessStat..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_FlashOpResultCheck_BitCheck..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_ProcessErrorReset	out	0	in	5
	out	0	100%
	in	6	100%
	.static000056d1	1	16%	0	6429	4110
	.static000059bb	1	16%	0	12913	4110
	_R_EEL_SFct_ActivateProcess	1	16%	0	4487	4110
	_R_EEL_GetDriverStatus	1	16%	0	2633	0
	_R_EEL_Init	2	33%	0	1645	0
_R_EEL_SFct_ProcessErrorUpdate	out	1	in	4
	out	1	100%
	_R_EEL_SFct_ErrStatCheckError	1	100%	0	4215	3860
	in	4	100%
	.static000055d1	1	25%	0	4427	4144
	_R_EEL_SFct_SetDriverStatus	1	25%	0	3723	4144
	_R_EEL_Execute	1	25%	0	1135	0
	_R_EEL_Init	1	25%	0	2079	0
_R_EEL_SFct_ProcessErrorUpdate_CurProcDefaultErrState..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_ActivateProcess	out	1	in	6
	out	1	100%
	_R_EEL_SFct_ProcessErrorReset	1	100%	0	4487	4110
	in	6	100%
	.static00005788	1	16%	0	8213	4442
	.static000058a2	1	16%	0	11143	4442
	.static00005680	1	16%	0	5417	4442
	.static000056d1	1	16%	0	6495	4442
	_R_EEL_Execute	1	16%	0	1109	0
	_R_EEL_Startup	1	16%	0	2173	0
_R_EEL_SFct_ConvertProcID2WriteProcID	out	0	in	2
	out	0	100%
	in	2	100%
	_R_EEL_SMachine_Main	1	50%	0	15507	4498
	.static000063a0	1	50%	0	253	0
_R_EEL_SFct_ConvertProcessID2CommandNo..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_Calc_FreeSpace	out	1	in	2
	out	1	100%
	_R_EEL_PFct_Calc_BlkSpace	1	100%	0	4657	2338
	in	2	100%
	.static0000545b	1	50%	0	1909	4562
	_R_EEL_GetSpace	1	50%	0	2697	0
_R_EEL_SFct_Calc_BlkStat..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_Init_BlkStatCnt..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_SetBlkStat..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_Calc_NextBlk_Any..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_Calc_NextBlk_DedicatedStatus..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_Calc_NextBlk_ActPrep	out	0	in	2
	out	0	100%
	in	4	100%
	.static00005742	3	75%	0	7977	5286
	_R_EEL_Execute	1	25%	0	835	0
_R_EEL_SFct_Prepare_StartProcess..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_Write_InitProcess	out	0	in	3
	out	0	100%
	in	3	100%
	.static00005788	1	33%	0	8201	5428
	.static000058a2	1	33%	0	11131	5428
	.static000063a0	1	33%	0	277	0
_R_EEL_SFct_Write_UpdateRpWp..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_Write_UpdateIDXTable..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_ForwardRpWp_DSWrite..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_Refresh_StartProcess..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_Get_RefAdd_2_DSLen_LimMode..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_SetActive_StartProcess..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_SetInvalid_StartProcess..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_Supv_Judge_Blk_Stat..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_Supv_Run..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_Supv_Ensure_DS_Margin..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SFct_ForwardSUPVProcessState..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Read_Start	out	2	in	2
	out	2	100%
	_R_EEL_PFct_CastU08Ptr2Add	1	50%	0	8455	978
	_R_EEL_SFct_SetDriverStatus	1	50%	0	8549	3494
	in	2	100%
	.static000055d1	1	50%	0	4320	8298
	_R_EEL_Execute	1	50%	0	536	0
_R_EEL_SM_WriteInc_Start	out	4	in	1
	out	4	100%
	_R_EEL_PFct_CastU08Ptr2Add	1	25%	0	8787	978
	_R_EEL_PFct_ConvertTIdx2Id	1	25%	0	8639	2120
	_R_EEL_PFct_ConvertTIdx2Len	1	25%	0	8743	2094
	_R_EEL_SM_Write_Start	1	25%	0	8852	8872
	in	2	100%
	_R_EEL_Execute	2	100%	0	730	0
_R_EEL_SM_Write_Start	out	0	in	6
	out	0	100%
	in	9	100%
	.static00005788	1	11%	0	8206	8872
	.static000057fb	1	11%	0	9162	8872
	.static00005817	1	11%	0	9498	8872
	.static000058a2	1	11%	0	11136	8872
	_R_EEL_SM_WriteInc_Start	1	11%	0	8852	8872
	_R_EEL_Execute	4	44%	0	782	0
_R_EEL_SM_Write_SOR..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Write_DRP..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Write_SetActiveError..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Write_Data..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Write_CmpData..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Write_EOR0..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Write_EOR1..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Write_Wait_Finish..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Write_Finish..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Refresh_Start..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Refresh_Finish..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Set_Active_A0..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Set_Active_RWP..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Set_Active_A1..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Set_Active_WaitEnd..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Set_Active_End..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Set_Invalid_I0..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Set_Invalid_I1..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Set_Invalid_WaitEnd..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Set_Invalid_End..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Prepare_Start..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Prepare_Chk_Erase_Result..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Prepare_SetPrep_WriteEC..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Prepare_SetPrep_WriteP..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Prepare_EraseResume	out	1	in	1
	out	1	100%
	_R_EEL_FDLIF_Handler	1	100%	0	12351	884
	in	1	100%
	_R_EEL_Execute	1	100%	0	1006	0
_R_EEL_SM_Prepare_Wait_Finish..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Prepare_Finish..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Format_Start	out	0	in	1
	out	0	100%
	in	1	100%
	_R_EEL_Execute	1	100%	0	952	0
_R_EEL_SM_Format_NextBlock..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Format_Finish..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Supv_Start	out	0	in	1
	out	0	100%
	in	1	100%
	_R_EEL_Startup	1	100%	0	2166	0
_R_EEL_SM_SUPV_Get_Blk_Stat1..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_SUPV_Get_Blk_Stat2..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_SUPV_Chk_Blk_Consistency..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_SUPV_Chk_Pool_Full..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_SUPV_Get_Pointers..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_SUPV_Get_Ram_Table..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_basic_fct.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_SM_Supv_Run	out	1	in	8
	out	2	100%
	_R_EEL_SFct_SetDriverStatus	2	100%	0	15341	3494
	in	8	100%
	.static000055d1	1	12%	0	4412	15212
	.static000059cd	1	12%	0	13196	15212
	.static000059eb	1	12%	0	13500	15212
	.static00005a38	1	12%	0	14172	15212
	.static00005a86	1	12%	0	15138	15212
	_R_EEL_SFct_SetDriverStatus	1	12%	0	3712	15212
	_R_EEL_Execute	1	12%	0	896	0
	_R_EEL_Init	1	12%	0	2072	0
_R_EEL_SMachine_GetActiveProcess	out	0	in	2
	out	0	100%
	in	2	100%
	_R_EEL_SMachine_Main	1	50%	0	15419	15352
	_R_EEL_Handler	1	50%	0	1371	0
_R_EEL_SMachine_Main	out	2	in	1
	out	2	100%
	_R_EEL_SFct_ConvertProcID2WriteProcID	1	50%	0	15507	4498
	_R_EEL_SMachine_GetActiveProcess	1	50%	0	15419	15352
	in	1	100%
	_R_EEL_Handler	1	100%	0	1367	0
_R_EEL_UFct_ChkLibraryInitialized..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_user_if.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_UFct_Write..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_user_if.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_UFct_Read..Z.3A.5CD.5Cproject.5CFX12.5C.B4.F8.C6.C1.B9.A4.D7.B0.B0.E5.5CFX12_test.5Cghs.5Cobj.5Cr_eel_user_if.	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_Execute	out	11	in	4
	out	15	100%
	_R_EEL_SFct_Calc_NextBlk_ActPrep	1	6%	0	835	0
	_R_EEL_FDLIF_EraseSuspendRequest	1	6%	0	1013	0
	_R_EEL_SFct_SetDriverStatus	1	6%	0	1157	0
	_R_EEL_SFct_ProcessErrorUpdate	1	6%	0	1135	0
	_R_EEL_SFct_ActivateProcess	1	6%	0	1109	0
	_R_EEL_SM_WriteInc_Start	2	13%	0	730	0
	_R_EEL_SM_Read_Start	1	6%	0	536	0
	_R_EEL_SM_Write_Start	4	26%	0	782	0
	_R_EEL_SM_Format_Start	1	6%	0	952	0
	_R_EEL_SM_Prepare_EraseResume	1	6%	0	1006	0
	_R_EEL_SM_Supv_Run	1	6%	0	896	0
	in	8	100%
	_Internal_EEL_Init	1	12%	0	85	0
	_Internal_EEL_Read	1	12%	0	321	0
	_Internal_EEL_Write	1	12%	0	207	0
	_SampleApp_EEL_Control	5	62%	0	535	0
_R_EEL_Handler	out	4	in	5
	out	5	100%
	_R_EEL_FDLIF_Handler	1	20%	0	1313	0
	_R_EEL_SFct_SetDriverStatus	2	40%	0	1399	0
	_R_EEL_SMachine_GetActiveProcess	1	20%	0	1371	0
	_R_EEL_SMachine_Main	1	20%	0	1367	0
	in	6	100%
	_Internal_EEL_Init	1	16%	0	125	0
	_Internal_EEL_DEINIT	1	16%	0	405	0
	.static0000522b	1	16%	0	163	0
	_SampleApp_EEL_HdrLoop	1	16%	0	29	0
	_SampleApp_EEL_Control	2	33%	0	557	0
_R_EEL_Init	out	8	in	1
	out	9	100%
	_R_EEL_PFct_WriteDataToAddU08	1	11%	0	1523	0
	_R_EEL_PFct_ConvertTIdx2Id	1	11%	0	1799	0
	_R_EEL_PFct_ConvertTIdx2Len	1	11%	0	1781	0
	_R_EEL_PFct_Calc_BlkSpace	1	11%	0	1835	0
	_R_EEL_SFct_SetDriverStatus	1	11%	0	1653	0
	_R_EEL_SFct_ProcessErrorReset	2	22%	0	1645	0
	_R_EEL_SFct_ProcessErrorUpdate	1	11%	0	2079	0
	_R_EEL_SM_Supv_Run	1	11%	0	2072	0
	in	1	100%
	.static0000522b	1	100%	0	143	0
_R_EEL_Startup	out	3	in	1
	out	3	100%
	_R_EEL_SFct_SetDriverStatus	1	33%	0	2181	0
	_R_EEL_SFct_ActivateProcess	1	33%	0	2173	0
	_R_EEL_SM_Supv_Start	1	33%	0	2166	0
	in	1	100%
	.static0000522b	1	100%	0	153	0
_R_EEL_ShutDown	out	1	in	2
	out	1	100%
	_R_EEL_SFct_SetDriverStatus	1	100%	0	2267	0
	in	2	100%
	_Internal_EEL_DEINIT	1	50%	0	377	0
	_SampleApp_EEL_Control	1	50%	0	547	0
_R_EEL_SuspendRequest	out	2	in	0
	out	2	100%
	_R_EEL_SFct_SetDriverStatus	1	50%	0	2441	0
	_R_EEL_GetDriverStatus	1	50%	0	2433	2546
	in	0	100%
_R_EEL_ResumeRequest	out	1	in	0
	out	1	100%
	_R_EEL_SFct_SetDriverStatus	1	100%	0	2527	0
	in	0	100%
_R_EEL_GetDriverStatus	out	2	in	5
	out	2	100%
	_R_EEL_SFct_ProcessErrorReset	1	50%	0	2633	0
	_R_EEL_SFct_ErrStatCheckError	1	50%	0	2621	0
	in	6	100%
	_Internal_EEL_Init	1	16%	0	133	0
	_Internal_EEL_DEINIT	1	16%	0	413	0
	.static0000522b	1	16%	0	171	0
	_SampleApp_EEL_Control	2	33%	0	565	0
	_R_EEL_SuspendRequest	1	16%	0	2433	2546
_R_EEL_GetSpace	out	2	in	1
	out	2	100%
	_R_EEL_SFct_Calc_FreeSpace	1	50%	0	2697	0
	_R_EEL_PFct_Calc_BlkSpace	1	50%	0	2703	0
	in	1	100%
	.static0000545b	1	100%	0	1923	0
_R_EEL_GetEraseCounter	out	0	in	0
	out	0	100%
	in	0	100%
_R_EEL_GetVersionString	out	0	in	0
	out	0	100%
	in	0	100%
_BSP_WDT_Clear	out	1	in	4
	out	1	100%
	_WDT_Clear	1	100%	0	7	0
	in	4	100%
	_BSP_Delay_ms	1	25%	0	305	0
	_AIM951_i2c_sendreceive	1	25%	0	1061	0
	_AIM951_i2c_send	1	25%	0	1011	0
	_OTA_EraseAll_APP	1	25%	0	1123	0
_BSP_GPIO_96751_1V_EN	out	0	in	1
	out	0	100%
	in	1	100%
	_Sys_Startup_Init	1	100%	0	63	0
_BSP_GPIO_96751_1V8_EN	out	0	in	1
	out	0	100%
	in	1	100%
	_Sys_Startup_Init	1	100%	0	75	0
_BSP_GPIO_TFT_EN	out	0	in	1
	out	0	100%
	in	1	100%
	_Sys_Startup_Init	1	100%	0	87	0
_BSP_GPIO_96751_PDB_EN	out	0	in	1
	out	0	100%
	in	1	100%
	_Sys_Startup_Init	1	100%	0	101	0
_BSP_GPIO_Get_948_lock	out	0	in	0
	out	0	100%
	in	0	100%
_BSP_FTM0_IRQHandler	out	2	in	1
	out	2	100%
	_RH850_Peripheral_IRQ_Flag_Clear	1	50%	0	263	0
	_TimeStamp_TimeCntCallback	1	50%	0	255	0
	in	1	100%
	_INTOSTM0	1	100%	0	53	0
_BSP_Delay_ms	out	4	in	6
	out	4	100%
	_BSP_WDT_Clear	1	25%	0	305	0
	_TimeStamp_Reset	1	25%	0	291	0
	_TimeStamp_Update	1	25%	0	301	0
	_TimeStamp_GetCntTime	1	25%	0	313	0
	in	93	100%
	_LCD_Init	4	4%	0	577	0
	_LCD_Shutdown	2	2%	0	779	0
	_Sys_Startup_Init	4	4%	0	109	0
	_switch_951_init	67	72%	0	2507	274
	_switch_951_Color	15	16%	0	2845	274
	_fx12_test_server	1	1%	0	1915	0
_BSP_PWM_Init	out	4	in	1
	out	4	100%
	_PWM_Channel_Set_Duty	1	25%	0	377	0
	_PWM_Channel_Init	1	25%	0	357	0
	_PWM_Channel_Set_Freq	1	25%	0	367	0
	_PWN_Init	1	25%	0	341	0
	in	1	100%
	_Sys_Startup_Init	1	100%	0	121	0
_BSP_SendString	out	2	in	1
	out	2	100%
	_UART_Ch0_Send_Multiple_Byte	1	50%	0	407	0
	_UART_Ch0_Get_TX_Busy_Flag	1	50%	0	411	0
	in	1	100%
	_uart1_printf	1	100%	0	525	388
_uart1_printf	out	3	in	1
	out	3	100%
	_BSP_SendString	1	33%	0	525	388
	_vsprintf	1	33%	0	517	0
	_memset	1	33%	0	497	0
	in	1	100%
	_main	1	100%	0	19	0
_BSP_InitUSART	out	1	in	1
	out	1	100%
	_UART_Init	1	100%	0	581	0
	in	1	100%
	_Sys_Startup_Init	1	100%	0	53	0
_I2C1_Send_End	out	3	in	0
	out	5	100%
	_RIIC1_Slave_Send_Flag_Reset	2	40%	0	629	0
	_RIIC1_Slave_Send_Flag	2	40%	0	621	0
	_RIIC1_Slave_Send_Count	1	20%	0	609	0
	in	0	100%
_BSP_I2C0_INIT	out	1	in	1
	out	1	100%
	_RIIC0_Init	1	100%	0	685	0
	in	1	100%
	_Sys_Startup_Init	1	100%	0	57	0
_gpio_get_key1	out	0	in	1
	out	0	100%
	in	1	100%
	_fx12_test_server	1	100%	0	619	0
_gpio_get_key2	out	0	in	1
	out	0	100%
	in	1	100%
	_fx12_test_server	1	100%	0	1095	0
_gpio_get_key3	out	0	in	1
	out	0	100%
	in	1	100%
	_fx12_test_server	1	100%	0	1321	0
_gpio_get_key4	out	0	in	0
	out	0	100%
	in	0	100%
_gpio_get_key5	out	0	in	1
	out	0	100%
	in	1	100%
	_fx12_test_server	1	100%	0	783	0
_gpio_get_key6	out	0	in	1
	out	0	100%
	in	1	100%
	_fx12_test_server	1	100%	0	905	0
_gpio_get_96751_lock	out	0	in	1
	out	0	100%
	in	1	100%
	_fx12_test_server	1	100%	0	1399	0
_touch_IRQ_Enable	out	1	in	1
	out	1	100%
	_RH850_Peripheral_IRQ_Enable	1	100%	0	879	0
	in	1	100%
	_Sys_Startup_Init	1	100%	0	41	0
_BSP_TOUCH_IRQHandler	out	1	in	1
	out	1	100%
	_RH850_Peripheral_IRQ_Flag_Clear	1	100%	0	921	0
	in	1	100%
	_INTP2	1	100%	0	2417	0
_GET_TOUCH_IRQHandler_flag	out	0	in	1
	out	0	100%
	in	1	100%
	_fx12_test_server	1	100%	0	1857	0
_Clear_TOUCH_IRQHandler_flag	out	0	in	1
	out	0	100%
	in	1	100%
	_fx12_test_server	1	100%	0	2017	0
_AIM951_i2c_send	out	3	in	2
	out	3	100%
	_RIIC0_WaitForBusy_Block	1	33%	0	1007	0
	_RIIC0_Master_SendMultiByte_Interrupt	1	33%	0	1003	0
	_BSP_WDT_Clear	1	33%	0	1011	0
	in	109	100%
	_switch_951_init	94	86%	0	2501	968
	_switch_951_Color	15	13%	0	2839	968
_AIM951_i2c_sendreceive	out	3	in	1
	out	3	100%
	_RIIC0_WaitForBusy_Block	1	33%	0	1057	0
	_RIIC0_Master_SendRecvMultiByte_Interrupt	1	33%	0	1053	0
	_BSP_WDT_Clear	1	33%	0	1061	0
	in	1	100%
	_fx12_test_server	1	100%	0	1695	0
_switch_951_init	out	2	in	2
	out	161	100%
	_BSP_Delay_ms	67	41%	0	2507	274
	_AIM951_i2c_send	94	58%	0	2501	968
	in	2	100%
	_init_951	1	50%	0	2865	1072
	_fx12_test_server	1	50%	0	767	0
_get_auto_color_flag	out	0	in	0
	out	0	100%
	in	0	100%
_get_color_flag	out	0	in	0
	out	0	100%
	in	0	100%
_switch_951_Color	out	2	in	1
	out	30	100%
	_BSP_Delay_ms	15	50%	0	2845	274
	_AIM951_i2c_send	15	50%	0	2839	968
	in	2	100%
	_fx12_test_server	2	100%	0	1643	0
_init_951	out	1	in	1
	out	1	100%
	_switch_951_init	1	100%	0	2865	1072
	in	1	100%
	_Sys_Startup_Init	1	100%	0	125	0
_TimeStamp_TimeCntCallback	out	0	in	1
	out	0	100%
	in	1	100%
	_BSP_FTM0_IRQHandler	1	100%	0	255	0
_TimeStamp_Reset	out	0	in	4
	out	0	100%
	in	7	100%
	_main	2	28%	0	73	0
	_BSP_Delay_ms	1	14%	0	291	0
	_Display_Init	1	14%	0	561	0
	_fx12_test_server	3	42%	0	1685	0
_TimeStamp_Update	out	0	in	3
	out	0	100%
	in	4	100%
	_main	1	25%	0	47	0
	_BSP_Delay_ms	1	25%	0	301	0
	_fx12_test_server	2	50%	0	1653	0
_TimeStamp_GetCntTime	out	0	in	3
	out	0	100%
	in	4	100%
	_main	1	25%	0	57	0
	_BSP_Delay_ms	1	25%	0	313	0
	_fx12_test_server	2	50%	0	1663	0
_OTA_FLASH_Erase	out	5	in	1
	out	5	100%
	_Internal_FCL_Init	1	20%	0	21	0
	_Internal_FCL_Erase	1	20%	0	31	0
	_Internal_FCL_Unlock	1	20%	0	25	0
	_Internal_FCL_OPEN	1	20%	0	17	0
	_Internal_FCL_CLOSE	1	20%	0	35	0
	in	1	100%
	_OTA_EraseAll_APP	1	100%	0	1129	0
_RTE_FCL_OP	out	5	in	1
	out	5	100%
	_Internal_FCL_Init	1	20%	0	71	0
	_OptionByte_Handle	1	20%	0	79	0
	_Internal_FCL_Unlock	1	20%	0	75	0
	_Internal_FCL_OPEN	1	20%	0	67	0
	_Internal_FCL_CLOSE	1	20%	0	83	0
	in	1	100%
	_Sys_Startup_Init	1	100%	0	27	0
_OTA_FLASH_Write	out	4	in	2
	out	4	100%
	_Internal_FCL_Init	1	25%	0	181	0
	_Internal_FCL_Write	1	25%	0	195	0
	_Internal_FCL_OPEN	1	25%	0	177	0
	_Internal_FCL_CLOSE	1	25%	0	199	0
	in	3	100%
	_OTA_Write	2	66%	0	1621	98
	_OTA_END_Write	1	33%	0	1759	98
_OTA_FCL_Read8	out	0	in	0
	out	0	100%
	in	0	100%
_RTE_FLASH_Read32	out	1	in	2
	out	1	100%
	_Internal_FCL_Read32	1	100%	0	235	0
	in	3	100%
	_BootReadCrcBlockInfo	1	33%	0	319	228
	_UDS_CheckProgDependence	2	66%	0	607	228
_CalculateAPPCRC32ForFF01	out	0	in	1
	out	0	100%
	in	4	100%
	_UDS_CheckProgDependence	4	100%	0	691	246
_BootReadCrcBlockInfo	out	2	in	1
	out	2	100%
	_BuildUint32_t	1	50%	0	367	382
	_RTE_FLASH_Read32	1	50%	0	319	228
	in	1	100%
	_OTA_CRC	1	100%	0	1849	312
_BuildUint32_t	out	0	in	2
	out	0	100%
	in	2	100%
	_BootReadCrcBlockInfo	1	50%	0	367	382
	_UDS_CheckProgDependence	1	50%	0	523	382
_UDS_CheckProgDependence	out	3	in	1
	out	7	100%
	_CalculateAPPCRC32ForFF01	4	57%	0	691	246
	_BuildUint32_t	1	14%	0	523	382
	_RTE_FLASH_Read32	2	28%	0	607	228
	in	1	100%
	_OTA_CRC	1	100%	0	1817	428
_OTA_EEL_Read	out	1	in	1
	out	1	100%
	_ReadProgramVaildStatus	1	100%	0	781	922
	in	2	100%
	_OTA_BOOT_init	2	100%	0	1091	774
_OTA_EEL_Write	out	1	in	1
	out	1	100%
	_WriteProgramVaildStatus	1	100%	0	803	972
	in	2	100%
	_OTA_CRC	2	100%	0	1907	796
_ReadDFlashData	out	1	in	1
	out	1	100%
	_DFlash_ReadData	1	100%	0	827	0
	in	1	100%
	_ReadProgramVaildStatus	1	100%	0	951	814
_WriteDFlashData	out	1	in	1
	out	1	100%
	_DFlash_WriteData	1	100%	0	857	0
	in	1	100%
	_WriteProgramVaildStatus	1	100%	0	1023	842
_AllFlagInit	out	0	in	1
	out	0	100%
	in	1	100%
	_ReadProgramVaildStatus	1	100%	0	940	872
_ReadProgramVaildStatus	out	2	in	1
	out	2	100%
	_ReadDFlashData	1	50%	0	951	814
	_AllFlagInit	1	50%	0	940	872
	in	1	100%
	_OTA_EEL_Read	1	100%	0	781	922
_WriteProgramVaildStatus	out	1	in	1
	out	1	100%
	_WriteDFlashData	1	100%	0	1023	842
	in	1	100%
	_OTA_EEL_Write	1	100%	0	803	972
_OTA_BOOT_init	out	4	in	0
	out	6	100%
	_OTA_EEL_Read	2	33%	0	1091	774
	_JumpToUserApplication	2	33%	0	1087	1170
	_Update_buffer_init	1	16%	0	1097	1204
	_OTA_CRC	1	16%	0	1079	1808
	in	0	100%
_OTA_EraseAll_APP	out	2	in	0
	out	2	100%
	_BSP_WDT_Clear	1	50%	0	1123	0
	_OTA_FLASH_Erase	1	50%	0	1129	0
	in	0	100%
_OTA_SystemReset	out	1	in	0
	out	1	100%
	_RH850_Hardware_Reset	1	100%	0	1159	0
	in	0	100%
_JumpToUserApplication	out	0	in	1
	out	0	100%
	in	2	100%
	_OTA_BOOT_init	2	100%	0	1087	1170
_Update_buffer_init	out	0	in	2
	out	0	100%
	in	2	100%
	_OTA_BOOT_init	1	50%	0	1097	1204
	_OTA_END_Write	1	50%	0	1763	1204
_OTA_Write	out	1	in	0
	out	2	100%
	_OTA_FLASH_Write	2	100%	0	1621	98
	in	0	100%
_OTA_END_Write	out	2	in	0
	out	2	100%
	_OTA_FLASH_Write	1	50%	0	1759	98
	_Update_buffer_init	1	50%	0	1763	1204
	in	0	100%
_S19_Checksum	out	0	in	0
	out	0	100%
	in	0	100%
_OTA_CRC	out	3	in	2
	out	4	100%
	_BootReadCrcBlockInfo	1	25%	0	1849	312
	_UDS_CheckProgDependence	1	25%	0	1817	428
	_OTA_EEL_Write	2	50%	0	1907	796
	in	2	100%
	_OTA_BOOT_init	1	50%	0	1079	1808
	_OTA_test	1	50%	0	1929	1808
_OTA_test	out	1	in	0
	out	1	100%
	_OTA_CRC	1	100%	0	1929	1808
	in	0	100%
_ver_Display	out	1	in	2
	out	10	100%
	_TFT_LCD_Draw_Bmp	10	100%	0	363	0
	in	3	100%
	_Display_Init	1	33%	0	467	0
	_fx12_test_server	2	66%	0	2013	0
_Display_Init	out	3	in	1
	out	9	100%
	_TFT_LCD_Draw_Bmp	7	77%	0	551	0
	_TimeStamp_Reset	1	11%	0	561	0
	_ver_Display	1	11%	0	467	0
	in	1	100%
	_Sys_Startup_Init	1	100%	0	117	0
_fx12_test_server	out	21	in	1
	out	39	100%
	_RIIC0_WaitForBusy_Block	2	5%	0	1885	0
	_RIIC0_Master_SendMultiByte_Interrupt	1	2%	0	1929	0
	_RIIC0_Master_RecvMultiByte_Interrupt	1	2%	0	1881	0
	_TFT_LCD_Draw_Bmp	12	30%	0	1847	0
	_BSP_Delay_ms	1	2%	0	1915	0
	_gpio_get_key2	1	2%	0	1095	0
	_AIM951_i2c_sendreceive	1	2%	0	1695	0
	_gpio_get_96751_lock	1	2%	0	1399	0
	_Clear_TOUCH_IRQHandler_flag	1	2%	0	2017	0
	_switch_951_init	1	2%	0	767	0
	_gpio_get_key3	1	2%	0	1321	0
	_gpio_get_key6	1	2%	0	905	0
	_gpio_get_key5	1	2%	0	783	0
	_GET_TOUCH_IRQHandler_flag	1	2%	0	1857	0
	_gpio_get_key1	1	2%	0	619	0
	_switch_951_Color	2	5%	0	1643	0
	_TimeStamp_Reset	3	7%	0	1685	0
	_TimeStamp_Update	2	5%	0	1653	0
	_TimeStamp_GetCntTime	2	5%	0	1663	0
	_ver_Display	2	5%	0	2013	0
	_BSP_SetBL_Brightness_PWM	1	2%	0	1091	2030
	in	1	100%
	_main	1	100%	0	37	0
_BSP_SetBL_Brightness_PWM	out	1	in	1
	out	1	100%
	_PWM_Channel_Set_Duty	1	100%	0	2041	0
	in	1	100%
	_fx12_test_server	1	100%	0	1091	2030
_sputc..trg.2Frh850.2Fobjs.2Flibs.2Flibansi.2Fccsprntf.	out	0	in	0
	out	0	100%
	in	0	100%
_vsprintf	out	1	in	2
	out	1	100%
	___gh_vsprintf	1	100%	0	75	0
	in	2	100%
	_uart1_printf	1	50%	0	517	0
	_sprintf	1	50%	0	135	22
_sprintf	out	1	in	0
	out	1	100%
	_vsprintf	1	100%	0	135	22
	in	0	100%
_exit	out	1	in	2
	out	1	100%
	__Exit	1	100%	0	79	0
	in	2	100%
	__start	1	50%	0	0	0
	___ghs_ind_crt1	1	50%	0	195	0
___gh_xxdecout	out	0	in	2
	out	0	100%
	in	2	100%
	.static000070c0	1	50%	0	7	0
	.static00007036	1	50%	0	657	0
___gh_outchars	out	2	in	2
	out	2	100%
	___ghsload25	1	50%	0	65	0
	___ghssave25a	1	50%	0	33	0
	in	3	100%
	___gh_strout	2	66%	0	593	32
	___gh_outspaces	1	33%	0	73	32
___gh_outspaces	out	1	in	1
	out	1	100%
	___gh_outchars	1	100%	0	73	32
	in	2	100%
	___gh_strout	2	100%	0	623	68
___gh_strout	out	8	in	5
	out	12	100%
	___gh_outchars	2	16%	0	593	32
	___gh_outspaces	2	16%	0	623	68
	___ghsload20	1	8%	0	633	0
	___gh_wctomb	2	16%	0	531	0
	_strnlen	1	8%	0	225	0
	_strlen	2	16%	0	249	0
	___ghs_u32tomb	1	8%	0	137	0
	___ghssave20	1	8%	0	79	0
	in	7	100%
	___gh_octhexout	1	14%	0	807	78
	___gh_vsprintf	3	42%	0	1949	78
	.static000070c5	1	14%	0	219	0
	___gh_uns_long_long_printf	1	14%	0	389	0
	.static00007036	1	14%	0	681	78
_unsout..trg.2Frh850.2Fobjs.2Flibs.2Flibansi.2Fccvsprnt.	out	0	in	0
	out	0	100%
	in	0	100%
___gh_hexout	out	0	in	2
	out	0	100%
	in	3	100%
	___gh_octhexout	1	33%	0	799	692
	___gh_uns_long_long_printf	2	66%	0	381	0
___gh_octhexout	out	4	in	1
	out	4	100%
	___gh_strout	1	25%	0	807	78
	___gh_hexout	1	25%	0	799	692
	___ghsload29	1	25%	0	815	0
	___ghssave29	1	25%	0	759	0
	in	1	100%
	___gh_vsprintf	1	100%	0	1567	758
___gh_vsprintf	out	4	in	1
	out	10	100%
	___gh_strout	3	30%	0	1949	78
	___gh_octhexout	1	10%	0	1567	758
	___gh_long_long_printf	3	30%	0	1469	0
	___gh_uns_long_long_printf	3	30%	0	1647	0
	in	1	100%
	_vsprintf	1	100%	0	75	0
_xxdecout..trg.2Frh850.2Fobjs.2Flibs.2Flibansi.2Fccllout.	out	0	in	0
	out	0	100%
	in	0	100%
_xdecout..trg.2Frh850.2Fobjs.2Flibs.2Flibansi.2Fccllout.	out	0	in	0
	out	0	100%
	in	0	100%
___gh_long_long_printf	out	0	in	1
	out	0	100%
	in	3	100%
	___gh_vsprintf	3	100%	0	1469	0
___gh_uns_long_long_printf	out	4	in	1
	out	5	100%
	___gh_strout	1	20%	0	389	0
	___gh_hexout	2	40%	0	381	0
	___ghsload28	1	20%	0	397	0
	___ghssave28	1	20%	0	259	0
	in	3	100%
	___gh_vsprintf	3	100%	0	1647	0
_strnlen	out	0	in	1
	out	0	100%
	in	1	100%
	___gh_strout	1	100%	0	225	0
___ghs_strlen	out	0	in	0
	out	0	100%
	in	0	100%
_strlen	out	0	in	1
	out	0	100%
	in	2	100%
	___gh_strout	2	100%	0	249	0
___gh_store_wc	out	0	in	0
	out	0	100%
	in	0	100%
___gh_wctomb	out	1	in	1
	out	1	100%
	_wctomb	1	100%	0	41	0
	in	2	100%
	___gh_strout	2	100%	0	531	0
___ghs_u32tomb	out	0	in	2
	out	0	100%
	in	2	100%
	___gh_strout	1	50%	0	137	0
	_wctomb	1	50%	0	73	0
_wctomb	out	1	in	1
	out	1	100%
	___ghs_u32tomb	1	100%	0	73	0
	in	1	100%
	___gh_wctomb	1	100%	0	41	0
_memset	out	0	in	2
	out	0	100%
	in	3	100%
	_uart1_printf	1	33%	0	497	0
	___ghs_ind_crt0	2	66%	0	64	0
___ghs_ind_crt0	out	3	in	1
	out	6	100%
	_memset	2	33%	0	64	0
	_memcpy	2	33%	0	68	0
	___ghs_ind_crt1	2	33%	0	60	0
	in	1	100%
	__start	1	100%	0	241	0
_memcpy..trg.2Frh850.2Fobjs.2Flibs.2Flibstartup.2Find_mcpy.	out	0	in	0
	out	0	100%
	in	0	100%
_memcpy	out	0	in	1
	out	0	100%
	in	2	100%
	___ghs_ind_crt0	2	100%	0	68	0
___mcopy	out	0	in	0
	out	0	100%
	in	0	100%
__exit	out	0	in	0
	out	0	100%
	in	0	100%
__Exit	out	3	in	1
	out	3	100%
	___ghs_syscall	1	33%	0	101	0
	___ghsLock	1	33%	0	39	0
	___ghsUnlock	1	33%	0	93	0
	in	1	100%
	_exit	1	100%	0	79	0
___ghs_at_exit	out	2	in	0
	out	2	100%
	___ghsLock	1	50%	0	133	0
	___ghsUnlock	1	50%	0	149	0
	in	0	100%
___ghs_initial_dotsyscall	out	0	in	1
	out	0	100%
	in	1	100%
	__start	1	100%	0	23	0
___dotsyscall	out	0	in	2
	out	0	100%
	in	2	100%
	__start	1	50%	0	0	0
	___ghs_syscall	1	50%	0	12	0
___ghs_syscall	out	2	in	1
	out	2	100%
	___dotsyscall	1	50%	0	12	0
	___gh_set_errno	1	50%	0	21	0
	in	1	100%
	__Exit	1	100%	0	101	0
___ghs_ind_crt1	out	3	in	1
	out	3	100%
	_main	1	33%	0	189	0
	_exit	1	33%	0	195	0
	___gh_lock_init	1	33%	0	57	0
	in	2	100%
	___ghs_ind_crt0	2	100%	0	60	0
___ghsLock	out	0	in	2
	out	0	100%
	in	2	100%
	__Exit	1	50%	0	39	0
	___ghs_at_exit	1	50%	0	133	0
___ghsUnlock	out	0	in	2
	out	0	100%
	in	2	100%
	__Exit	1	50%	0	93	0
	___ghs_at_exit	1	50%	0	149	0
___gh_lock_init	out	0	in	1
	out	0	100%
	in	1	100%
	___ghs_ind_crt1	1	100%	0	57	0
___gh_set_errno	out	0	in	1
	out	0	100%
	in	1	100%
	___ghs_syscall	1	100%	0	21	0
___gh_errno_ptr	out	0	in	0
	out	0	100%
	in	0	100%
___gh_get_errno	out	0	in	0
	out	0	100%
	in	0	100%
___gh_udiv64_core	out	1	in	1
	out	1	100%
	___gh_shrl_64_32	1	100%	0	95	0
	in	1	100%
	___gh_udiv64	1	100%	0	1125	0
___gh_udiv64	out	1	in	8
	out	1	100%
	___gh_udiv64_core	1	100%	0	1125	0
	in	13	100%
	_ADC_Res_Calc_Circuit103	2	15%	0	1269	0
	_ADC_Voltage_Calc_Circuit102	2	15%	0	277	0
	_ADC_Res_Calc_Circuit102	1	7%	0	807	0
	_ADC_Res_Calc_Circuit101	1	7%	0	449	0
	_ADC_Res_Calc_Circuit202	2	15%	0	1823	0
	_ADC_Res_Calc_Circuit203	3	23%	0	2239	0
	_ADC_Res_Calc_Circuit201	1	7%	0	1509	0
	_ADC_Res_Calc_Circuit303	1	7%	0	2663	0
___gh_mul64	out	0	in	8
	out	0	100%
	in	19	100%
	_ADC_Res_Calc_Circuit103	5	26%	0	1239	0
	_ADC_Voltage_Calc_Circuit102	1	5%	0	231	0
	_ADC_Res_Calc_Circuit102	4	21%	0	777	0
	_ADC_Res_Calc_Circuit101	1	5%	0	427	0
	_ADC_Res_Calc_Circuit202	2	10%	0	1801	0
	_ADC_Res_Calc_Circuit203	3	15%	0	2223	0
	_ADC_Res_Calc_Circuit201	1	5%	0	1487	0
	_ADC_Res_Calc_Circuit303	2	10%	0	2681	0
___ghssave29a	out	0	in	1
	out	0	100%
	in	1	100%
	.static000070c0	1	100%	0	1	0
___ghssave28a	out	1	in	0
	out	1	100%
	___ghs_save27a	1	100%	0	6	16
	in	0	100%
___ghssave27a	out	1	in	0
	out	1	100%
	___ghs_save27a	1	100%	0	12	16
	in	0	100%
___ghs_save27a	out	1	in	4
	out	1	100%
	___ghs_save27a	1	100%	0	16	16
	in	4	100%
	___ghs_save23a	1	25%	0	43	0
	___ghssave28a	1	25%	0	6	16
	___ghs_save27a	1	25%	0	16	16
	___ghssave27a	1	25%	0	12	16
___ghssave26a	out	0	in	0
	out	0	100%
	in	0	100%
___ghssave25a	out	1	in	1
	out	1	100%
	___ghs_save23a	1	100%	0	6	24
	in	1	100%
	___gh_outchars	1	100%	0	33	0
___ghssave24a	out	1	in	0
	out	1	100%
	___ghs_save23a	1	100%	0	12	24
	in	0	100%
___ghssave23a	out	1	in	0
	out	1	100%
	___ghs_save23a	1	100%	0	18	24
	in	0	100%
___ghs_save23a	out	2	in	4
	out	2	100%
	___ghs_save23a	1	50%	0	24	24
	___ghs_save27a	1	50%	0	43	0
	in	4	100%
	___ghs_save23a	1	25%	0	24	24
	___ghssave25a	1	25%	0	6	24
	___ghssave24a	1	25%	0	12	24
	___ghssave23a	1	25%	0	18	24
___ghssavelp	out	0	in	0
	out	0	100%
	in	0	100%
___ghssave29	out	1	in	1
	out	1	100%
	___ghs_save27	1	100%	0	6	22
	in	1	100%
	___gh_octhexout	1	100%	0	759	0
___ghssave28	out	1	in	2
	out	1	100%
	___ghs_save27	1	100%	0	12	22
	in	2	100%
	___gh_uns_long_long_printf	1	50%	0	259	0
	.static00007036	1	50%	0	639	0
___ghssave27	out	1	in	0
	out	1	100%
	___ghs_save27	1	100%	0	18	22
	in	0	100%
___ghs_save27	out	1	in	5
	out	1	100%
	___ghs_save27	1	100%	0	22	22
	in	5	100%
	___ghs_save23	1	20%	0	43	0
	___ghs_save27	1	20%	0	22	22
	___ghssave29	1	20%	0	6	22
	___ghssave27	1	20%	0	18	22
	___ghssave28	1	20%	0	12	22
___ghssave26	out	0	in	0
	out	0	100%
	in	0	100%
___ghssave25	out	1	in	1
	out	1	100%
	___ghs_save23	1	100%	0	6	24
	in	1	100%
	.static000070c5	1	100%	0	37	0
___ghssave24	out	1	in	0
	out	1	100%
	___ghs_save23	1	100%	0	12	24
	in	0	100%
___ghssave23	out	1	in	0
	out	1	100%
	___ghs_save23	1	100%	0	18	24
	in	0	100%
___ghs_save23	out	2	in	5
	out	2	100%
	___ghs_save23	1	50%	0	24	24
	___ghs_save27	1	50%	0	43	0
	in	5	100%
	___ghs_save23	1	20%	0	24	24
	___ghssave25	1	20%	0	6	24
	___ghssave24	1	20%	0	12	24
	___ghssave23	1	20%	0	18	24
	___ghssave20	1	20%	0	31	0
___ghssave22	out	0	in	0
	out	0	100%
	in	0	100%
___ghssave21	out	1	in	0
	out	1	100%
	___ghssave20	1	100%	0	6	12
	in	0	100%
___ghssave20	out	2	in	3
	out	2	100%
	___ghs_save23	1	50%	0	31	0
	___ghssave20	1	50%	0	12	12
	in	3	100%
	___gh_strout	1	33%	0	79	0
	___ghssave20	1	33%	0	12	12
	___ghssave21	1	33%	0	6	12
___ghsload29	out	0	in	2
	out	0	100%
	in	2	100%
	___gh_octhexout	1	50%	0	815	0
	.static000070c0	1	50%	0	31	0
___ghsload28	out	1	in	2
	out	1	100%
	___ghs_load27	1	100%	0	4	10
	in	2	100%
	___gh_uns_long_long_printf	1	50%	0	397	0
	.static00007036	1	50%	0	689	0
___ghsload27	out	1	in	0
	out	1	100%
	___ghs_load27	1	100%	0	8	10
	in	0	100%
___ghs_load27	out	1	in	4
	out	1	100%
	___ghs_load27	1	100%	0	10	10
	in	4	100%
	___ghs_load27	1	25%	0	10	10
	___ghsload27	1	25%	0	8	10
	___ghsload28	1	25%	0	4	10
	___ghs_load23	1	25%	0	31	0
___ghsload26	out	0	in	0
	out	0	100%
	in	0	100%
___ghsload25	out	1	in	2
	out	1	100%
	___ghs_load23	1	100%	0	4	14
	in	2	100%
	___gh_outchars	1	50%	0	65	0
	.static000070c5	1	50%	0	227	0
___ghsload24	out	1	in	0
	out	1	100%
	___ghs_load23	1	100%	0	8	14
	in	0	100%
___ghsload23	out	1	in	0
	out	1	100%
	___ghs_load23	1	100%	0	12	14
	in	0	100%
___ghs_load23	out	2	in	5
	out	2	100%
	___ghs_load27	1	50%	0	31	0
	___ghs_load23	1	50%	0	14	14
	in	5	100%
	___ghsload24	1	20%	0	8	14
	___ghsload20	1	20%	0	23	0
	___ghs_load23	1	20%	0	14	14
	___ghsload25	1	20%	0	4	14
	___ghsload23	1	20%	0	12	14
___ghsload22	out	0	in	0
	out	0	100%
	in	0	100%
___ghsload21	out	1	in	0
	out	1	100%
	___ghsload20	1	100%	0	4	8
	in	0	100%
___ghsload20	out	2	in	3
	out	2	100%
	___ghsload20	1	50%	0	8	8
	___ghs_load23	1	50%	0	23	0
	in	3	100%
	___gh_strout	1	33%	0	633	0
	___ghsload21	1	33%	0	4	8
	___ghsload20	1	33%	0	8	8
___gh_shrl_64_32	out	0	in	2
	out	0	100%
	in	2	100%
	___gh_shrl_64_64	1	50%	0	61	0
	___gh_udiv64_core	1	50%	0	95	0
___gh_shrl_64_64	out	1	in	0
	out	1	100%
	___gh_shrl_64_32	1	100%	0	61	0
	in	0	100%
.static000030ee	out	3	in	0
	out	3	100%
	_LCD_Start_Data_Writing	1	33%	0	5833	0
	_LCD_Write_Data	1	33%	0	5851	0
	_LCD_Set_Window	1	33%	0	5829	0
	in	0	100%
.static00003103	out	3	in	0
	out	3	100%
	_LCD_Start_Data_Writing	1	33%	0	5989	0
	_LCD_Write_Data	1	33%	0	6055	0
	_LCD_Set_Window	1	33%	0	5985	0
	in	0	100%
.static0000311c	out	5	in	0
	out	17	100%
	_LCD_Start_Data_Writing	3	17%	0	6847	0
	_LCD_Start_Data_Reading	2	11%	0	6781	0
	_LCD_Write_Data	3	17%	0	6909	0
	_LCD_Read_Data	4	23%	0	6805	0
	_LCD_Set_Window	5	29%	0	6843	0
	in	0	100%
.static00003160	out	5	in	0
	out	9	100%
	_LCD_Start_Data_Writing	1	11%	0	7189	0
	_LCD_Start_Data_Reading	1	11%	0	7129	0
	_LCD_Write_Data	3	33%	0	7385	0
	_LCD_Read_Data	2	22%	0	7153	0
	_LCD_Set_Window	2	22%	0	7185	0
	in	0	100%
.static0000318d	out	5	in	0
	out	15	100%
	_LCD_Start_Data_Writing	1	6%	0	7635	0
	_LCD_Start_Data_Reading	1	6%	0	7575	0
	_LCD_Write_Data	9	60%	0	8433	0
	_LCD_Read_Data	2	13%	0	7599	0
	_LCD_Set_Window	2	13%	0	7631	0
	in	0	100%
.static000031e9	out	5	in	0
	out	7	100%
	_LCD_Start_Data_Writing	1	14%	0	8751	0
	_LCD_Start_Data_Reading	1	14%	0	8633	0
	_LCD_Write_Data	1	14%	0	8757	0
	_LCD_Read_Data	2	28%	0	8643	0
	_LCD_Set_Window	2	28%	0	8747	0
	in	0	100%
.static00003200	out	5	in	0
	out	9	100%
	_LCD_Start_Data_Writing	1	11%	0	8949	0
	_LCD_Start_Data_Reading	1	11%	0	8889	0
	_LCD_Write_Data	3	33%	0	9083	0
	_LCD_Read_Data	2	22%	0	8913	0
	_LCD_Set_Window	2	22%	0	8945	0
	in	0	100%
.static0000322e	out	5	in	0
	out	29	100%
	_LCD_Start_Data_Writing	4	13%	0	9775	0
	_LCD_Start_Data_Reading	3	10%	0	9735	0
	_LCD_Write_Data	9	31%	0	9839	0
	_LCD_Read_Data	6	20%	0	9747	0
	_LCD_Set_Window	7	24%	0	9771	0
	in	0	100%
.static00003283	out	5	in	0
	out	76	100%
	_LCD_Start_Data_Writing	10	13%	0	11945	0
	_LCD_Start_Data_Reading	8	10%	0	11905	0
	_LCD_Write_Data	24	31%	0	12009	0
	_LCD_Read_Data	16	21%	0	11917	0
	_LCD_Set_Window	18	23%	0	11941	0
	in	0	100%
.static0000337c	out	5	in	0
	out	11	100%
	_LCD_Start_Data_Writing	2	18%	0	12363	0
	_LCD_Start_Data_Reading	1	9%	0	12165	0
	_LCD_Write_Data	3	27%	0	12457	0
	_LCD_Read_Data	2	18%	0	12189	0
	_LCD_Set_Window	3	27%	0	12359	0
	in	0	100%
.static000033b8	out	5	in	0
	out	29	100%
	_LCD_Start_Data_Writing	4	13%	0	13563	0
	_LCD_Start_Data_Reading	3	10%	0	13503	0
	_LCD_Write_Data	9	31%	0	13697	0
	_LCD_Read_Data	6	20%	0	13527	0
	_LCD_Set_Window	7	24%	0	13559	0
	in	0	100%
.static00003f52	out	1	in	0
	out	4	100%
	_R_FCL_I_write_memory_u08	4	100%	0	99	132
	in	0	100%
.static00003fcc	out	1	in	0
	out	1	100%
	_R_FCL_I_write_memory_u08	1	100%	0	919	132
	in	0	100%
.static00003fe1	out	1	in	0
	out	2	100%
	_R_FCL_I_write_memory_u08	2	100%	0	1121	132
	in	0	100%
.static00004045	out	1	in	0
	out	1	100%
	_R_FCL_I_write_memory_u08	1	100%	0	1679	132
	in	0	100%
.static000046d0	out	4	in	0
	out	4	100%
	_R_FCL_FCUFct_SwitchMode_Start	1	25%	0	93	0
	_R_FCL_FCUFct_SwitchMode_Check	1	25%	0	125	0
	_R_FCL_FCUFct_PrepareEnvironment	1	25%	0	215	0
	_R_FCL_FCUFct_HandleMultiOperation	1	25%	0	221	0
	in	0	100%
.static00004f54	out	7	in	0
	out	8	100%
	_R_FDL_IFct_CalcFOpUnitCnt_BC	1	12%	0	3679	0
	_R_FDL_IFct_ChkAccessBoundaries	1	12%	0	3759	0
	_R_FDL_FCUFct_SwitchMode_Check_TS	1	12%	0	3857	0
	_R_FDL_FCUFct_StartWriteOperation	1	12%	0	3933	0
	_R_FDL_FCUFct_SwitchMode_Start	2	25%	0	4023	0
	_R_FDL_FCUFct_StartBCEraseOperation	1	12%	0	3911	0
	_R_FDL_FCUFct_ReadOperation	1	12%	0	3803	0
	in	0	100%
.static00004a2b	out	1	in	0
	out	1	100%
	_R_FDL_IFct_ChkAccessBoundaries	1	100%	0	289	66
	in	0	100%
.static00004e29	out	2	in	0
	out	2	100%
	_R_FDL_FCUFct_ChkSuspendable_TS	1	50%	0	851	0
	_R_FDL_FCUFct_Suspend_TS	1	50%	0	859	0
	in	0	100%
.static00004e34	out	1	in	0
	out	2	100%
	_R_FDL_FCUFct_SwitchMode_Start	2	100%	0	1077	0
	in	0	100%
.static00004e0e	out	3	in	0
	out	3	100%
	_R_FDL_FCUFct_ForcedStop	1	33%	0	653	0
	_R_FDL_FCUFct_SwitchMode_Check_TS	1	33%	0	629	0
	_R_FDL_FCUFct_SwitchMode_Start	1	33%	0	675	0
	in	0	100%
.static00004e6d	out	4	in	0
	out	4	100%
	_R_FDL_FCUFct_ClearStatus	1	25%	0	1473	0
	_R_FDL_FCUFct_SwitchMode_Check_TS	1	25%	0	1559	0
	_R_FDL_FCUFct_SwitchMode_Start	1	25%	0	1553	0
	_R_FDL_FCUFct_GetStat	1	25%	0	1465	0
	in	0	100%
.static00004e5c	out	4	in	0
	out	4	100%
	_R_FDL_FCUFct_ClearStatus	1	25%	0	1367	0
	_R_FDL_FCUFct_SwitchMode_Check_TS	1	25%	0	1379	0
	_R_FDL_FCUFct_SwitchMode_Start	1	25%	0	1373	0
	_R_FDL_FCUFct_CheckFatalError	1	25%	0	1357	0
	in	0	100%
.static00004e88	out	5	in	0
	out	6	100%
	_R_FDL_IFct_CalcFOpUnitCnt_BC	1	16%	0	2021	0
	_R_FDL_FCUFct_SwitchMode_Check_TS	1	16%	0	2119	0
	_R_FDL_FCUFct_StartWriteOperation	1	16%	0	1837	0
	_R_FDL_FCUFct_SwitchMode_Start	1	16%	0	2113	0
	_R_FDL_FCUFct_StartBCEraseOperation	2	33%	0	2069	0
	in	0	100%
.static00004ea6	out	10	in	0
	out	15	100%
	_R_FDL_FCUFct_ForcedStop	2	13%	0	2503	0
	_R_FDL_FCUFct_Switch_FAEINT	3	20%	0	2521	0
	_R_FDL_FCUFct_ClearStatus	1	6%	0	2509	0
	_R_FDL_FCUFct_SetFrequency	1	6%	0	2649	0
	_R_FDL_FCUFct_GetDFSize	1	6%	0	2605	0
	_R_FDL_FCUFct_VerifyChecksum	1	6%	0	2577	0
	_R_FDL_FCUFct_SwitchMode_Check_TS	1	6%	0	2235	0
	_R_FDL_FCUFct_SwitchMode_Start	3	20%	0	2515	0
	_R_FDL_FCUFct_InitRAM	1	6%	0	2429	0
	_R_FDL_FCUFct_Resume_TS	1	6%	0	2693	0
	in	0	100%
.static00005742	out	2	in	0
	out	7	100%
	_R_EEL_SFct_Calc_NextBlk_ActPrep	3	42%	0	7977	5286
	_R_EEL_SFct_SetDriverStatus	4	57%	0	7795	3494
	in	0	100%
.static00005788	out	4	in	0
	out	4	100%
	_R_EEL_SFct_Write_InitProcess	1	25%	0	8201	5428
	_R_EEL_PFct_ConvertTIdx2Len	1	25%	0	8151	2094
	_R_EEL_SFct_ActivateProcess	1	25%	0	8213	4442
	_R_EEL_SM_Write_Start	1	25%	0	8206	8872
	in	0	100%
.static000057fb	out	1	in	0
	out	1	100%
	_R_EEL_SM_Write_Start	1	100%	0	9162	8872
	in	0	100%
.static00005817	out	1	in	0
	out	1	100%
	_R_EEL_SM_Write_Start	1	100%	0	9498	8872
	in	0	100%
.static0000588f	out	1	in	0
	out	2	100%
	_R_EEL_SFct_SetDriverStatus	2	100%	0	10563	3494
	in	0	100%
.static000058a2	out	6	in	0
	out	6	100%
	_R_EEL_SFct_Write_InitProcess	1	16%	0	11131	5428
	_R_EEL_PFct_ConvertId2TIdx	1	16%	0	10813	1960
	_R_EEL_PFct_ConvertTIdx2Len	1	16%	0	11059	2094
	_R_EEL_SFct_ErrStatCheckError	1	16%	0	10645	3860
	_R_EEL_SFct_ActivateProcess	1	16%	0	11143	4442
	_R_EEL_SM_Write_Start	1	16%	0	11136	8872
	in	0	100%
.static0000522b	out	8	in	0
	out	9	100%
	_R_FDL_Execute	1	11%	0	107	0
	_R_FDL_Handler	1	11%	0	113	0
	_R_FDL_Init	1	11%	0	73	0
	_SampleApp_EEL_ErrorHdr	2	22%	0	159	0
	_R_EEL_GetDriverStatus	1	11%	0	171	0
	_R_EEL_Handler	1	11%	0	163	0
	_R_EEL_Init	1	11%	0	143	0
	_R_EEL_Startup	1	11%	0	153	0
	in	0	100%
.static00005343	out	1	in	0
	out	1	100%
	_R_FDL_Execute	1	100%	0	209	0
	in	0	100%
.static00005353	out	1	in	0
	out	1	100%
	_R_FDL_Execute	1	100%	0	409	0
	in	0	100%
.static0000532d	out	2	in	0
	out	2	100%
	_R_FDL_Execute	1	50%	0	55	0
	_R_FDL_Handler	1	50%	0	65	0
	in	0	100%
.static0000538b	out	1	in	0
	out	1	100%
	_R_FDL_Execute	1	100%	0	831	0
	in	0	100%
.static0000537f	out	1	in	0
	out	1	100%
	_R_FDL_Execute	1	100%	0	677	0
	in	0	100%
.static00005375	out	1	in	0
	out	1	100%
	_R_FDL_ResumeRequest	1	100%	0	543	0
	in	0	100%
.static0000545b	out	2	in	0
	out	2	100%
	_R_EEL_SFct_Calc_FreeSpace	1	50%	0	1909	4562
	_R_EEL_GetSpace	1	50%	0	1923	0
	in	0	100%
.static0000550a	out	1	in	0
	out	1	100%
	_R_EEL_PFct_ConvertId2TIdx	1	100%	0	3013	1960
	in	0	100%
.static0000551f	out	1	in	0
	out	3	100%
	_R_EEL_PFct_WriteDataToAddU08	3	100%	0	3365	1426
	in	0	100%
.static00005574	out	1	in	0
	out	1	100%
	_R_EEL_SFct_ErrStatCheckError	1	100%	0	3845	3860
	in	0	100%
.static000055d1	out	3	in	0
	out	3	100%
	_R_EEL_SFct_ProcessErrorUpdate	1	33%	0	4427	4144
	_R_EEL_SM_Read_Start	1	33%	0	4320	8298
	_R_EEL_SM_Supv_Run	1	33%	0	4412	15212
	in	0	100%
.static00005680	out	1	in	0
	out	1	100%
	_R_EEL_SFct_ActivateProcess	1	100%	0	5417	4442
	in	0	100%
.static000056d1	out	2	in	0
	out	2	100%
	_R_EEL_SFct_ProcessErrorReset	1	50%	0	6429	4110
	_R_EEL_SFct_ActivateProcess	1	50%	0	6495	4442
	in	0	100%
.static000059bb	out	2	in	0
	out	2	100%
	_R_EEL_SFct_SetDriverStatus	1	50%	0	12921	3494
	_R_EEL_SFct_ProcessErrorReset	1	50%	0	12913	4110
	in	0	100%
.static000059a9	out	1	in	0
	out	1	100%
	_R_EEL_SFct_ErrStatCheckError	1	100%	0	12687	3860
	in	0	100%
.static000059cd	out	1	in	0
	out	1	100%
	_R_EEL_SM_Supv_Run	1	100%	0	13196	15212
	in	0	100%
.static000059eb	out	1	in	0
	out	1	100%
	_R_EEL_SM_Supv_Run	1	100%	0	13500	15212
	in	0	100%
.static00005a38	out	1	in	0
	out	1	100%
	_R_EEL_SM_Supv_Run	1	100%	0	14172	15212
	in	0	100%
.static00005a5a	out	1	in	0
	out	1	100%
	_R_EEL_SFct_SetDriverStatus	1	100%	0	14537	3494
	in	0	100%
.static00005a86	out	2	in	0
	out	2	100%
	_R_EEL_SFct_SetDriverStatus	1	50%	0	15133	3494
	_R_EEL_SM_Supv_Run	1	50%	0	15138	15212
	in	0	100%
.static000063a0	out	6	in	0
	out	6	100%
	_R_EEL_SFct_Write_InitProcess	1	16%	0	277	0
	_R_EEL_PFct_CastU08Ptr2Add	1	16%	0	239	0
	_R_EEL_PFct_ConvertId2TIdx	1	16%	0	193	0
	_R_EEL_PFct_ConvertTIdx2Len	1	16%	0	229	0
	_R_EEL_PFct_Chk_ProcessActive	1	16%	0	171	0
	_R_EEL_SFct_ConvertProcID2WriteProcID	1	16%	0	253	0
	in	0	100%
.static000063bc	out	3	in	0
	out	3	100%
	_R_EEL_PFct_ConvertId2TIdx	1	33%	0	391	0
	_R_EEL_PFct_ConvertTIdx2Len	1	33%	0	421	0
	_R_EEL_PFct_Chk_ProcessActive	1	33%	0	371	0
	in	0	100%
.static000070c5	out	3	in	0
	out	3	100%
	___gh_strout	1	33%	0	219	0
	___ghsload25	1	33%	0	227	0
	___ghssave25	1	33%	0	37	0
	in	0	100%
.static000070c0	out	3	in	0
	out	3	100%
	___gh_xxdecout	1	33%	0	7	0
	___ghsload29	1	33%	0	31	0
	___ghssave29a	1	33%	0	1	0
	in	0	100%
.static00007036	out	4	in	0
	out	4	100%
	___gh_strout	1	25%	0	681	78
	___gh_xxdecout	1	25%	0	657	0
	___ghsload28	1	25%	0	689	0
	___ghssave28	1	25%	0	639	0
	in	0	100%
#% END STATIC GRAPH
