<<Reserved symbol>>
LCDB

<<LCDB_LockUnlockLcd>>
LCDB_LockUnlockLcd
LCDB_LOCKUNLOCKLCD
LCDB_LockUnlockLcd_LockUnlockLcd
LCDB_LOCKUNLOCKLCD_LOCKUNLOCKLCD

<<LCDB_LockStatusLcd>>
LCDB_LockStatusLcd
LCDB_LOCKSTATUSLCD
LCDB_LockStatusLcd_LockStatusLcd
LCDB_LockStatusLcd_PrivilegeStatusLcd
LCDB_LockStatusLcd_FreezeStatusLcd
LCDB_LOCKSTATUSLCD_LOCKSTATUSLCD
LCDB_LOCKSTATUSLCD_PRIVILEGESTATUSLCD
LCDB_LOCKSTATUSLCD_FREEZESTATUSLCD

<<LCDB_InterfaceConfig>>
LCDB_InterfaceConfig
LCDB_INTERFACECONFIG
LCDB_InterfaceConfig_InterfaceType
LCDB_InterfaceConfig_InterfaceWidth
LCDB_InterfaceConfig_CsPolarity
LCDB_InterfaceConfig_WrPolarity
LCDB_InterfaceConfig_RdPolarity
LCDB_InterfaceConfig_RsPolarity
LCDB_InterfaceConfig_DataPolarity
LCDB_InterfaceConfig_TePolarity
LCDB_INTERFACECONFIG_INTERFACETYPE
LCDB_INTERFACECONFIG_INTERFACEWIDTH
LCDB_INTERFACECONFIG_CSPOLARITY
LCDB_INTERFACECONFIG_WRPOLARITY
LCDB_INTERFACECONFIG_RDPOLARITY
LCDB_INTERFACECONFIG_RSPOLARITY
LCDB_INTERFACECONFIG_DATAPOLARITY
LCDB_INTERFACECONFIG_TEPOLARITY

<<LCDB_WriteTimingConfig>>
LCDB_WriteTimingConfig
LCDB_WRITETIMINGCONFIG
LCDB_WriteTimingConfig_WriteSetupCycles
LCDB_WriteTimingConfig_WriteActiveCycles
LCDB_WriteTimingConfig_WriteHoldCycles
LCDB_WRITETIMINGCONFIG_WRITESETUPCYCLES
LCDB_WRITETIMINGCONFIG_WRITEACTIVECYCLES
LCDB_WRITETIMINGCONFIG_WRITEHOLDCYCLES

<<LCDB_ReadTimingConfig>>
LCDB_ReadTimingConfig
LCDB_READTIMINGCONFIG
LCDB_ReadTimingConfig_ReadSetupCycles
LCDB_ReadTimingConfig_ReadActiveCycles
LCDB_ReadTimingConfig_ReadHoldCycles
LCDB_READTIMINGCONFIG_READSETUPCYCLES
LCDB_READTIMINGCONFIG_READACTIVECYCLES
LCDB_READTIMINGCONFIG_READHOLDCYCLES

<<LCDB_CommandTransferMapping0>>
LCDB_CommandTransferMapping0
LCDB_COMMANDTRANSFERMAPPING0
LCDB_CommandTransferMapping0_CommandTransfer0Bits
LCDB_CommandTransferMapping0_CommandTransfer0SrcLsb
LCDB_CommandTransferMapping0_CommandTransfer0DstLsb
LCDB_CommandTransferMapping0_CommandTransfer0Next
LCDB_COMMANDTRANSFERMAPPING0_COMMANDTRANSFER0BITS
LCDB_COMMANDTRANSFERMAPPING0_COMMANDTRANSFER0SRCLSB
LCDB_COMMANDTRANSFERMAPPING0_COMMANDTRANSFER0DSTLSB
LCDB_COMMANDTRANSFERMAPPING0_COMMANDTRANSFER0NEXT

<<LCDB_CommandTransferMapping1>>
LCDB_CommandTransferMapping1
LCDB_COMMANDTRANSFERMAPPING1
LCDB_CommandTransferMapping1_CommandTransfer1Bits
LCDB_CommandTransferMapping1_CommandTransfer1SrcLsb
LCDB_CommandTransferMapping1_CommandTransfer1DstLsb
LCDB_CommandTransferMapping1_CommandTransfer1Next
LCDB_COMMANDTRANSFERMAPPING1_COMMANDTRANSFER1BITS
LCDB_COMMANDTRANSFERMAPPING1_COMMANDTRANSFER1SRCLSB
LCDB_COMMANDTRANSFERMAPPING1_COMMANDTRANSFER1DSTLSB
LCDB_COMMANDTRANSFERMAPPING1_COMMANDTRANSFER1NEXT

<<LCDB_CommandTransferMapping2>>
LCDB_CommandTransferMapping2
LCDB_COMMANDTRANSFERMAPPING2
LCDB_CommandTransferMapping2_CommandTransfer2Bits
LCDB_CommandTransferMapping2_CommandTransfer2SrcLsb
LCDB_CommandTransferMapping2_CommandTransfer2DstLsb
LCDB_COMMANDTRANSFERMAPPING2_COMMANDTRANSFER2BITS
LCDB_COMMANDTRANSFERMAPPING2_COMMANDTRANSFER2SRCLSB
LCDB_COMMANDTRANSFERMAPPING2_COMMANDTRANSFER2DSTLSB

<<LCDB_DataTransferMapping0>>
LCDB_DataTransferMapping0
LCDB_DATATRANSFERMAPPING0
LCDB_DataTransferMapping0_DataTransfer0Bits
LCDB_DataTransferMapping0_DataTransfer0SrcLsb
LCDB_DataTransferMapping0_DataTransfer0DstLsb
LCDB_DataTransferMapping0_DataTransfer0Next
LCDB_DATATRANSFERMAPPING0_DATATRANSFER0BITS
LCDB_DATATRANSFERMAPPING0_DATATRANSFER0SRCLSB
LCDB_DATATRANSFERMAPPING0_DATATRANSFER0DSTLSB
LCDB_DATATRANSFERMAPPING0_DATATRANSFER0NEXT

<<LCDB_DataTransferMapping1>>
LCDB_DataTransferMapping1
LCDB_DATATRANSFERMAPPING1
LCDB_DataTransferMapping1_DataTransfer1Bits
LCDB_DataTransferMapping1_DataTransfer1SrcLsb
LCDB_DataTransferMapping1_DataTransfer1DstLsb
LCDB_DataTransferMapping1_DataTransfer1Next
LCDB_DATATRANSFERMAPPING1_DATATRANSFER1BITS
LCDB_DATATRANSFERMAPPING1_DATATRANSFER1SRCLSB
LCDB_DATATRANSFERMAPPING1_DATATRANSFER1DSTLSB
LCDB_DATATRANSFERMAPPING1_DATATRANSFER1NEXT

<<LCDB_DataTransferMapping2>>
LCDB_DataTransferMapping2
LCDB_DATATRANSFERMAPPING2
LCDB_DataTransferMapping2_DataTransfer2Bits
LCDB_DataTransferMapping2_DataTransfer2SrcLsb
LCDB_DataTransferMapping2_DataTransfer2DstLsb
LCDB_DATATRANSFERMAPPING2_DATATRANSFER2BITS
LCDB_DATATRANSFERMAPPING2_DATATRANSFER2SRCLSB
LCDB_DATATRANSFERMAPPING2_DATATRANSFER2DSTLSB

<<LCDB_ColorComponentBits>>
LCDB_ColorComponentBits
LCDB_COLORCOMPONENTBITS
LCDB_ColorComponentBits_ComponentBitsBlue
LCDB_ColorComponentBits_ComponentBitsGreen
LCDB_ColorComponentBits_ComponentBitsRed
LCDB_COLORCOMPONENTBITS_COMPONENTBITSBLUE
LCDB_COLORCOMPONENTBITS_COMPONENTBITSGREEN
LCDB_COLORCOMPONENTBITS_COMPONENTBITSRED

<<LCDB_ColorComponentShift>>
LCDB_ColorComponentShift
LCDB_COLORCOMPONENTSHIFT
LCDB_ColorComponentShift_ComponentShiftBlue
LCDB_ColorComponentShift_ComponentShiftGreen
LCDB_ColorComponentShift_ComponentShiftRed
LCDB_COLORCOMPONENTSHIFT_COMPONENTSHIFTBLUE
LCDB_COLORCOMPONENTSHIFT_COMPONENTSHIFTGREEN
LCDB_COLORCOMPONENTSHIFT_COMPONENTSHIFTRED

<<LCDB_DestinationAttributes>>
LCDB_DestinationAttributes
LCDB_DESTINATIONATTRIBUTES
LCDB_DestinationAttributes_BitsPerTransfer
LCDB_DestinationAttributes_BitsPerPixel
LCDB_DESTINATIONATTRIBUTES_BITSPERTRANSFER
LCDB_DESTINATIONATTRIBUTES_BITSPERPIXEL

<<LCDB_LockUnlockControl>>
LCDB_LockUnlockControl
LCDB_LOCKUNLOCKCONTROL
LCDB_LockUnlockControl_LockUnlockControl
LCDB_LOCKUNLOCKCONTROL_LOCKUNLOCKCONTROL

<<LCDB_LockStatusControl>>
LCDB_LockStatusControl
LCDB_LOCKSTATUSCONTROL
LCDB_LockStatusControl_LockStatusControl
LCDB_LockStatusControl_PrivilegeStatusControl
LCDB_LockStatusControl_FreezeStatusControl
LCDB_LOCKSTATUSCONTROL_LOCKSTATUSCONTROL
LCDB_LOCKSTATUSCONTROL_PRIVILEGESTATUSCONTROL
LCDB_LOCKSTATUSCONTROL_FREEZESTATUSCONTROL

<<LCDB_SequencerConfig>>
LCDB_SequencerConfig
LCDB_SEQUENCERCONFIG
LCDB_SequencerConfig_InstructionTimeout
LCDB_SequencerConfig_InstructionTimeoutEnable
LCDB_SEQUENCERCONFIG_INSTRUCTIONTIMEOUT
LCDB_SEQUENCERCONFIG_INSTRUCTIONTIMEOUTENABLE

<<LCDB_InstructionFifoConfig>>
LCDB_InstructionFifoConfig
LCDB_INSTRUCTIONFIFOCONFIG
LCDB_InstructionFifoConfig_InstrThresholdLow
LCDB_InstructionFifoConfig_InstrThresholdHigh
LCDB_InstructionFifoConfig_InstrThresholdTrigger
LCDB_INSTRUCTIONFIFOCONFIG_INSTRTHRESHOLDLOW
LCDB_INSTRUCTIONFIFOCONFIG_INSTRTHRESHOLDHIGH
LCDB_INSTRUCTIONFIFOCONFIG_INSTRTHRESHOLDTRIGGER

<<LCDB_ReceptionFifoConfig>>
LCDB_ReceptionFifoConfig
LCDB_RECEPTIONFIFOCONFIG
LCDB_ReceptionFifoConfig_RxThresholdLow
LCDB_ReceptionFifoConfig_RxThresholdHigh
LCDB_ReceptionFifoConfig_RxThresholdTrigger
LCDB_RECEPTIONFIFOCONFIG_RXTHRESHOLDLOW
LCDB_RECEPTIONFIFOCONFIG_RXTHRESHOLDHIGH
LCDB_RECEPTIONFIFOCONFIG_RXTHRESHOLDTRIGGER

<<LCDB_SoftwareReset>>
LCDB_SoftwareReset
LCDB_SOFTWARERESET
LCDB_SoftwareReset_SoftwareReset
LCDB_SOFTWARERESET_SOFTWARERESET

<<LCDB_RxFifoControl>>
LCDB_RxFifoControl
LCDB_RXFIFOCONTROL
LCDB_RxFifoControl_RxClear
LCDB_RXFIFOCONTROL_RXCLEAR

<<LCDB_SequencerSync>>
LCDB_SequencerSync
LCDB_SEQUENCERSYNC
LCDB_SequencerSync_SequencerAck
LCDB_SEQUENCERSYNC_SEQUENCERACK

<<LCDB_SequencerStatus>>
LCDB_SequencerStatus
LCDB_SEQUENCERSTATUS
LCDB_SequencerStatus_OperationState
LCDB_SequencerStatus_WaitAck
LCDB_SequencerStatus_ErrorCode
LCDB_SequencerStatus_InstructionCounter
LCDB_SequencerStatus_InstructionRegister
LCDB_SequencerStatus_IrisInterfaceStatus
LCDB_SequencerStatus_LcdInterfaceState
LCDB_SEQUENCERSTATUS_OPERATIONSTATE
LCDB_SEQUENCERSTATUS_WAITACK
LCDB_SEQUENCERSTATUS_ERRORCODE
LCDB_SEQUENCERSTATUS_INSTRUCTIONCOUNTER
LCDB_SEQUENCERSTATUS_INSTRUCTIONREGISTER
LCDB_SEQUENCERSTATUS_IRISINTERFACESTATUS
LCDB_SEQUENCERSTATUS_LCDINTERFACESTATE

<<LCDB_FifoStatus>>
LCDB_FifoStatus
LCDB_FIFOSTATUS
LCDB_FifoStatus_InstrSpace
LCDB_FifoStatus_InstrEmpty
LCDB_FifoStatus_InstrFull
LCDB_FifoStatus_RxLevel
LCDB_FifoStatus_RxEmpty
LCDB_FifoStatus_RxFull
LCDB_FIFOSTATUS_INSTRSPACE
LCDB_FIFOSTATUS_INSTREMPTY
LCDB_FIFOSTATUS_INSTRFULL
LCDB_FIFOSTATUS_RXLEVEL
LCDB_FIFOSTATUS_RXEMPTY
LCDB_FIFOSTATUS_RXFULL

<<LCDB_LockUnlockFifo>>
LCDB_LockUnlockFifo
LCDB_LOCKUNLOCKFIFO
LCDB_LockUnlockFifo_LockUnlockFifo
LCDB_LOCKUNLOCKFIFO_LOCKUNLOCKFIFO

<<LCDB_LockStatusFifo>>
LCDB_LockStatusFifo
LCDB_LOCKSTATUSFIFO
LCDB_LockStatusFifo_LockStatusFifo
LCDB_LockStatusFifo_PrivilegeStatusFifo
LCDB_LockStatusFifo_FreezeStatusFifo
LCDB_LOCKSTATUSFIFO_LOCKSTATUSFIFO
LCDB_LOCKSTATUSFIFO_PRIVILEGESTATUSFIFO
LCDB_LOCKSTATUSFIFO_FREEZESTATUSFIFO

<<LCDB_InstructionFifox>>
LCDB_InstructionFifo[0-31]
LCDB_INSTRUCTIONFIFO[0-31]
LCDB_InstructionFifo[0-31]_Instruction
LCDB_INSTRUCTIONFIFO[0-31]_INSTRUCTION

<<LCDB_RxFifox>>
LCDB_RxFifo[0-15]
LCDB_RXFIFO[0-15]
LCDB_RxFifo[0-15]_RxEntry
LCDB_RXFIFO[0-15]_RXENTRY

