/* logical s-record file */
OPENFILE "%ABS_FILE%.s19"
format=motorola
busWidth=1
origin=0
len=0x1000000
destination=0
SRECORD=Sx
SENDBYTE 1 "%ABS_FILE%"
CLOSE


/* physical s-record file */
OPENFILE "%ABS_FILE%.phy"
format = motorola
busWidth = 1
len = 0x4000

/* logical non banked flash at $4000 and $C000 to physical */
origin = 0x004000
destination = 0x0F8000
SENDBYTE 1 "%ABS_FILE%"

origin = 0x00C000
destination = 0x0FC000
SENDBYTE 1 "%ABS_FILE%"

/* physical FTS512K flash window to physical 
origin = 0x008000
destination = 0x080000 
SENDBYTE 1 "%ABS_FILE%"
*/

/* physical FTS256K parts flash window to physical 
origin = 0x008000
destination = 0x0C0000 
SENDBYTE 1 "%ABS_FILE%"
*/

/* physical FTS128K parts flash window to physical 
origin = 0x008000
destination = 0x0E0000 
SENDBYTE 1 "%ABS_FILE%"
*/

/* physical FTS64K parts flash window to physical 
origin = 0x008000
destination = 0x0F0000 
SENDBYTE 1 "%ABS_FILE%"
*/

/* physical FTS32K parts flash window to physical 
origin = 0x008000
destination = 0x0F8000 
SENDBYTE 1 "%ABS_FILE%"
*/

/* logical 512 kB banked flash to physical */
origin = 0x208000
destination = 0x080000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x218000
destination = 0x084000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x228000
destination = 0x088000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x238000
destination = 0x08C000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x248000
destination = 0x090000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x258000
destination = 0x094000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x268000
destination = 0x098000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x278000
destination = 0x09C000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x288000
destination = 0x0A0000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x298000
destination = 0x0A4000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x2A8000
destination = 0x0A8000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x2B8000
destination = 0x0AC000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x2C8000
destination = 0x0B0000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x2D8000
destination = 0x0B4000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x2E8000
destination = 0x0B8000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x2F8000
destination = 0x0BC000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x308000
destination = 0x0C0000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x318000
destination = 0x0C4000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x328000
destination = 0x0C8000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x338000
destination = 0x0CC000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x348000
destination = 0x0D0000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x358000
destination = 0x0D4000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x368000
destination = 0x0D8000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x378000
destination = 0x0DC000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x388000
destination = 0x0E0000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x398000
destination = 0x0E4000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x3A8000
destination = 0x0E8000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x3B8000
destination = 0x0EC000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x3C8000
destination = 0x0F0000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x3D8000
destination = 0x0F4000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x3E8000
destination = 0x0F8000
SENDBYTE 1 "%ABS_FILE%"
origin = 0x3F8000
destination = 0x0FC000
SENDBYTE 1 "%ABS_FILE%"

CLOSE

