{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet3 "],"not_rendered":{"charts":0,"images":9,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet3 ","index":0,"n_rows":17,"n_cols":7,"rows_kept":17,"cut":false,"hidden":false,"merged":[[0,0,0,6],[1,0,1,6],[2,1,2,2],[13,1,13,6],[14,0,14,6],[15,2,15,3],[15,4,15,6],[16,2,16,3],[16,4,16,6]]}
["RMR42E-60标准作业检测台应用"]
["注：上电仪表自扫完成后，所有灯及功能全都是0"]
["序号\n（点位）","指示灯",null,"1SOC\n（2）CAN_0x18200A20、CAN_0x18203220）","2SOC\n（CAN_0x18203220、0x18200A21）","挡位（CAN_0x125）","刀盘挡位（CAN_0x157）"]
[0,null,null,0,0,0,"无效"]
[1,"草满指示灯（PIN 15)",null,1,1,1,0]
[2,"刀盘过载指示灯(PIN19)",null,3,3,2,1]
[3,"座椅检测\n指示灯（CAN_0x125）",null,5,5,"P",2]
[4,"钥匙接入指示灯（CAN_0x18202922）",null,7,7,"P",3]
[5," Ready指示灯（CAN_0x18202922）",null,10,9,"P",3]
[6,"充电指示灯(CAN_0x125、0x18202922)",null,10,10,"P",3]
[7,"刀盘开关指示（CAN_0x157）",null,10,10,"P",3]
[8,"大灯灯光检测（PIN14）",null,10,10,"P",3]
[9,null,null,10,10,"P",3]
[10,"灯全亮、天有为清零策略后进入自扫，直到IG OFF。"]
["备注（非软件工程）"]
[1,"单次工作时间",null,null,"CAN控制"]
[2,"累计工作时长",null,null,"CAN控制"]