###############################################################################
#
# IAR ELF Linker V9.40.1.364/W64 for ARM                  05/Feb/2025  17:01:57
# Copyright 2007-2023 IAR Systems AB.
#
#    Output file  =
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Exe\Project.out
#    Map file     =
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\List\Project.map
#    Command line =
#        -f
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Exe\Project.out.rsp
#        (C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\User_7280784329937237312.dir\main.o
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal.o
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_can.o
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_cortex.o
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_dma.o
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_gpio.o
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\User_7280784329937237312.dir\py32f072_hal_msp.o
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_pwr.o
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_rcc.o
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_rcc_ex.o
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_uart.o
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\User_7280784329937237312.dir\py32f072_it.o
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\PY32F072xx_Start_Kit_1292202923306237531.dir\py32f072xx_Start_Kit.o
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\EWARM_7214922893274846302.dir\startup_py32f072xx.o
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\CMSIS_6603591812247902717.dir\system_py32f072.o
#        --no_out_extension -o
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Exe\Project.out
#        --map
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\List\Project.map
#        --config
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\py32f072xB_flash.icf
#        --semihosting --entry __iar_program_start --vfe --text_out locale
#        --cpu=Cortex-M0+ --fpu=None) --dependencies=n
#        C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Exe\Project.out.iar_deps
#
###############################################################################

*******************************************************************************
*** RUNTIME MODEL ATTRIBUTES
***

CppFlavor       = *
__CPP_Runtime   = 1
__SystemLibrary = DLib
__dlib_version  = 6


*******************************************************************************
*** HEAP SELECTION
***

The basic heap was selected because --advanced_heap
was not specified and the application did not appear to
be primarily optimized for speed.


*******************************************************************************
*** PLACEMENT SUMMARY
***

"A0":  place at address 0x800'0000 { ro section .intvec };
"P1":  place in [from 0x800'0000 to 0x801'ffff] { ro };
define block CSTACK with size = 1K, alignment = 8 { };
define block HEAP with size = 512, alignment = 8 { };
"P2":  place in [from 0x2000'0000 to 0x2000'3fff] {
          rw, block CSTACK, block HEAP };
initialize by copy { rw };

  Section            Kind         Address    Size  Object
  -------            ----         -------    ----  ------
"A0":                                        0xc0
  .intvec            ro code   0x800'0000    0xc0  startup_py32f072xx.o [2]
                             - 0x800'00c0    0xc0

"P1":                                      0x1be2
  .text              ro code   0x800'00c0   0x804  py32f072_hal_rcc.o [3]
  .text              ro code   0x800'08c4     0xc  py32f072_hal.o [3]
  .text              ro code   0x800'08d0    0x5c  py32f072_hal.o [3]
  .text              ro code   0x800'092c    0x34  ABImemcpy.o [7]
  .text              ro code   0x800'0960    0xae  I32DivModFast.o [7]
  .text              ro code   0x800'0a0e     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0a10    0xf0  py32f072_hal_cortex.o [3]
  .text              ro code   0x800'0b00     0x2  IntDivZer.o [7]
  .text              ro code   0x800'0b02     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0b04   0x3d4  py32f072_hal_uart.o [3]
  .text              ro code   0x800'0ed8     0x2  py32f072_hal_uart.o [3]
  .text              ro code   0x800'0eda     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0edc   0x3c4  py32f072_hal_can.o [3]
  .text              ro code   0x800'12a0    0xc4  py32f072_hal_msp.o [5]
  .text              ro code   0x800'1364    0x14  memset.o [7]
  .text              ro code   0x800'1378   0x1a0  main.o [5]
  .text              ro code   0x800'1518   0x1ac  py32f072_hal_gpio.o [3]
  .text              ro code   0x800'16c4    0x4e  ABImemset.o [7]
  .text              ro code   0x800'1712     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1714    0x1c  py32f072_hal.o [3]
  .text              ro code   0x800'1730    0xcc  py32f072xx_Start_Kit.o [4]
  .text              ro code   0x800'17fc    0x28  printf.o [6]
  .text              ro code   0x800'1824   0x17c  xprintftiny.o [6]
  .text              ro code   0x800'19a0     0xe  strlen.o [7]
  .text              ro code   0x800'19ae     0x2  startup_py32f072xx.o [2]
  .rodata            const     0x800'19b0    0x40  system_py32f072.o [1]
  .text              ro code   0x800'19f0    0x3c  system_py32f072.o [1]
  .text              ro code   0x800'1a2c    0x3c  zero_init3.o [7]
  .text              ro code   0x800'1a68    0x30  copy_init3.o [7]
  .text              ro code   0x800'1a98    0x28  data_init.o [7]
  .iar.init_table    const     0x800'1ac0    0x24  - Linker created -
  .rodata            const     0x800'1ae4    0x20  system_py32f072.o [1]
  .rodata            const     0x800'1b04    0x20  system_py32f072.o [1]
  Initializer bytes  const     0x800'1b24    0x20  <for P2-1>
  .text              ro code   0x800'1b44    0x1e  cmain.o [7]
  .text              ro code   0x800'1b62     0x4  low_level_init.o [6]
  .text              ro code   0x800'1b66     0x8  exit.o [6]
  .text              ro code   0x800'1b6e     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1b70     0xa  cexit.o [7]
  .text              ro code   0x800'1b7a     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1b7c    0x14  exit.o [8]
  .rodata            const     0x800'1b90    0x1c  main.o [5]
  .text              ro code   0x800'1bac    0x1c  cstartup_M.o [7]
  .rodata            const     0x800'1bc8    0x18  main.o [5]
  .text              ro code   0x800'1be0    0x18  py32f072_hal.o [3]
  .text              ro code   0x800'1bf8    0x16  xprout.o [6]
  .text              ro code   0x800'1c0e     0x2  startup_py32f072xx.o [2]
  .rodata            const     0x800'1c10    0x14  py32f072_hal_rcc.o [3]
  .text              ro code   0x800'1c24    0x12  py32f072_it.o [5]
  .text              ro code   0x800'1c36     0x2  startup_py32f072xx.o [2]
  .rodata            const     0x800'1c38    0x10  py32f072_hal_rcc.o [3]
  .text              ro code   0x800'1c48    0x10  startup_py32f072xx.o [2]
  .rodata            const     0x800'1c58     0xc  py32f072_hal_can.o [3]
  .rodata            const     0x800'1c64     0x8  py32f072_hal_rcc.o [3]
  .rodata            const     0x800'1c6c     0x8  py32f072_hal_rcc.o [3]
  .text              ro code   0x800'1c74     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c76     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c78     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c7a     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c7c     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c7e     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c80     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c82     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c84     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c86     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c88     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c8a     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c8c     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c8e     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c90     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c92     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c94     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c96     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c98     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c9a     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c9c     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1c9e     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1ca0     0x2  startup_py32f072xx.o [2]
  .rodata            const     0x800'1ca2     0x0  zero_init3.o [7]
  .rodata            const     0x800'1ca2     0x0  copy_init3.o [7]
                             - 0x800'1ca2  0x1be2

"P2", part 1 of 3:                           0x20
  P2-1                        0x2000'0000    0x20  <Init block>
    .data            inited   0x2000'0000     0x8  main.o [5]
    .data            inited   0x2000'0008     0xc  main.o [5]
    .data            inited   0x2000'0014     0x4  py32f072_hal.o [3]
    .data            inited   0x2000'0018     0x4  py32f072_hal.o [3]
    .data            inited   0x2000'001c     0x4  system_py32f072.o [1]
                            - 0x2000'0020    0x20

"P2", part 2 of 3:                           0xdc
  .bss               zero     0x2000'0020    0x4c  py32f072xx_Start_Kit.o [4]
  .bss               zero     0x2000'006c    0x30  main.o [5]
  .bss               zero     0x2000'009c    0x20  main.o [5]
  .bss               zero     0x2000'00bc    0x1c  main.o [5]
  .bss               zero     0x2000'00d8    0x18  main.o [5]
  .bss               zero     0x2000'00f0     0x8  main.o [5]
  .bss               zero     0x2000'00f8     0x4  py32f072_hal.o [3]
                            - 0x2000'00fc    0xdc

"P2", part 3 of 3:                          0x400
  CSTACK                      0x2000'0100   0x400  <Block>
    CSTACK           uninit   0x2000'0100   0x400  <Block tail>
                            - 0x2000'0500   0x400

Unused ranges:

         From           To      Size
         ----           --      ----
   0x800'1ca2   0x801'ffff  0x1'e35e
  0x2000'00fc  0x2000'00ff       0x4
  0x2000'0500  0x2000'3fff    0x3b00


*******************************************************************************
*** INIT TABLE
***

          Address      Size
          -------      ----
Zero (__iar_zero_init3)
    1 destination range, total size 0xdc:
          0x2000'0020  0xdc

Copy (__iar_copy_init3)
    1 source range, total size 0x20:
           0x800'1b24  0x20
    1 destination range, total size 0x20:
          0x2000'0000  0x20



*******************************************************************************
*** MODULE SUMMARY
***

    Module                  ro code  ro data  rw data
    ------                  -------  -------  -------
command line/config:
    -------------------------------------------------
    Total:

C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\CMSIS_6603591812247902717.dir: [1]
    system_py32f072.o            60      132        4
    -------------------------------------------------
    Total:                       60      132        4

C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\EWARM_7214922893274846302.dir: [2]
    startup_py32f072xx.o        272
    -------------------------------------------------
    Total:                      272

C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir: [3]
    py32f072_hal.o              156        8       12
    py32f072_hal_can.o          964       12
    py32f072_hal_cortex.o       240
    py32f072_hal_gpio.o         428
    py32f072_hal_rcc.o        2'052       52
    py32f072_hal_uart.o         982
    -------------------------------------------------
    Total:                    4'822       72       12

C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\PY32F072xx_Start_Kit_1292202923306237531.dir: [4]
    py32f072xx_Start_Kit.o      204                76
    -------------------------------------------------
    Total:                      204                76

C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\User_7280784329937237312.dir: [5]
    main.o                      416       72      160
    py32f072_hal_msp.o          196
    py32f072_it.o                18
    -------------------------------------------------
    Total:                      630       72      160

dl6M_tln.a: [6]
    exit.o                        8
    low_level_init.o              4
    printf.o                     40
    xprintftiny.o               380
    xprout.o                     22
    -------------------------------------------------
    Total:                      454

rt6M_tl.a: [7]
    ABImemcpy.o                  52
    ABImemset.o                  78
    I32DivModFast.o             174
    IntDivZer.o                   2
    cexit.o                      10
    cmain.o                      30
    copy_init3.o                 48
    cstartup_M.o                 28
    data_init.o                  40
    memset.o                     20
    strlen.o                     14
    zero_init3.o                 60
    -------------------------------------------------
    Total:                      556

shb_l.a: [8]
    exit.o                       20
    -------------------------------------------------
    Total:                       20

    Linker created                        36    1'024
-----------------------------------------------------
    Grand Total:              7'018      312    1'276


*******************************************************************************
*** ENTRY LIST
***

Entry                       Address   Size  Type      Object
-----                       -------   ----  ----      ------
.iar.init_table$$Base    0x800'1ac0          --   Gb  - Linker created -
.iar.init_table$$Limit   0x800'1ae4          --   Gb  - Linker created -
?main                    0x800'1b45         Code  Gb  cmain.o [7]
ADC_COMP_IRQHandler      0x800'1c7b         Code  Wk  startup_py32f072xx.o [2]
AHBPrescTable            0x800'19b0   0x40  Data  Gb  system_py32f072.o [1]
APBPrescTable            0x800'1ae4   0x20  Data  Gb  system_py32f072.o [1]
APP_ErrorHandler         0x800'1515    0x4  Code  Gb  main.o [5]
APP_SystemClockConfig    0x800'1467   0x74  Code  Lc  main.o [5]
BSP_USART_Config         0x800'1731   0xa4  Code  Gb  py32f072xx_Start_Kit.o [4]
CAN_CopyMessageToFifo    0x800'1225   0x76  Code  Lc  py32f072_hal_can.o [3]
CAN_IRQHandler           0x800'1c9f         Code  Wk  startup_py32f072xx.o [2]
CSTACK$$Base            0x2000'0100          --   Gb  - Linker created -
CSTACK$$Limit           0x2000'0500          --   Gb  - Linker created -
CanFilter               0x2000'00bc   0x1c  Data  Gb  main.o [5]
CanHandle               0x2000'006c   0x30  Data  Gb  main.o [5]
CanRxHeader             0x2000'009c   0x20  Data  Gb  main.o [5]
CanTxHeader             0x2000'00d8   0x18  Data  Gb  main.o [5]
DLCtoBytes              0x2000'0008    0xc  Data  Gb  main.o [5]
DLCtoBytes               0x800'1c58    0xc  Data  Lc  py32f072_hal_can.o [3]
DMA1_Channel1_IRQHandler
                         0x800'1c75         Code  Wk  startup_py32f072xx.o [2]
DMA1_Channel2_3_IRQHandler
                         0x800'1c77         Code  Wk  startup_py32f072xx.o [2]
DMA1_Channel4_5_6_7_IRQHandler
                         0x800'1c79         Code  Wk  startup_py32f072xx.o [2]
DebugUartHandle         0x2000'0020   0x4c  Data  Gb  py32f072xx_Start_Kit.o [4]
EXTI0_1_IRQHandler       0x800'1b6f         Code  Wk  startup_py32f072xx.o [2]
EXTI2_3_IRQHandler       0x800'1b7b         Code  Wk  startup_py32f072xx.o [2]
EXTI4_15_IRQHandler      0x800'1c0f         Code  Wk  startup_py32f072xx.o [2]
FLASH_IRQHandler         0x800'1713         Code  Wk  startup_py32f072xx.o [2]
HAL_CAN_ActivateTxRequest
                         0x800'108f   0x58  Code  Gb  py32f072_hal_can.o [3]
HAL_CAN_AddMessageToTxFifo
                         0x800'1003   0x8c  Code  Gb  py32f072_hal_can.o [3]
HAL_CAN_ConfigFilter     0x800'0f63   0xa0  Code  Gb  py32f072_hal_can.o [3]
HAL_CAN_GetRxMessage     0x800'10e7   0xa8  Code  Gb  py32f072_hal_can.o [3]
HAL_CAN_Init             0x800'0edd   0x86  Code  Gb  py32f072_hal_can.o [3]
HAL_CAN_MspInit          0x800'12cd   0x84  Code  Gb  py32f072_hal_msp.o [5]
HAL_CAN_Start            0x800'11a5   0x7c  Code  Gb  py32f072_hal_can.o [3]
HAL_GPIO_Init            0x800'1519  0x190  Code  Gb  py32f072_hal_gpio.o [3]
HAL_GetTick              0x800'08c5    0xc  Code  Wk  py32f072_hal.o [3]
HAL_IncTick              0x800'1be1   0x18  Code  Wk  py32f072_hal.o [3]
HAL_Init                 0x800'1715   0x1c  Code  Gb  py32f072_hal.o [3]
HAL_InitTick             0x800'08d1   0x5c  Code  Wk  py32f072_hal.o [3]
HAL_MspInit              0x800'12a1   0x2c  Code  Gb  py32f072_hal_msp.o [5]
HAL_NVIC_EnableIRQ       0x800'0ad5    0xa  Code  Gb  py32f072_hal_cortex.o [3]
HAL_NVIC_SetPriority     0x800'0acb    0xa  Code  Gb  py32f072_hal_cortex.o [3]
HAL_RCC_ClockConfig      0x800'05e9  0x176  Code  Gb  py32f072_hal_rcc.o [3]
HAL_RCC_GetHCLKFreq      0x800'0849    0x6  Code  Gb  py32f072_hal_rcc.o [3]
HAL_RCC_GetPCLK1Freq     0x800'0855   0x1e  Code  Gb  py32f072_hal_rcc.o [3]
HAL_RCC_GetSysClockFreq
                         0x800'0781   0xc8  Code  Gb  py32f072_hal_rcc.o [3]
HAL_RCC_OscConfig        0x800'00c1  0x508  Code  Gb  py32f072_hal_rcc.o [3]
HAL_SYSTICK_Config       0x800'0adf    0x8  Code  Gb  py32f072_hal_cortex.o [3]
HAL_UART_Init            0x800'0b05   0x84  Code  Gb  py32f072_hal_uart.o [3]
HAL_UART_MspInit         0x800'0ed9    0x2  Code  Wk  py32f072_hal_uart.o [3]
HAL_UART_Transmit        0x800'0b91   0xf0  Code  Gb  py32f072_hal_uart.o [3]
HSIFreqTable             0x800'1b04   0x20  Data  Gb  system_py32f072.o [1]
HardFault_Handler        0x800'1c27    0x4  Code  Gb  py32f072_it.o [5]
I2C1_IRQHandler          0x800'1c91         Code  Wk  startup_py32f072xx.o [2]
I2C2_IRQHandler          0x800'1c93         Code  Wk  startup_py32f072xx.o [2]
LCD_IRQHandler           0x800'1c37         Code  Wk  startup_py32f072xx.o [2]
NMI_Handler              0x800'1c25    0x2  Code  Gb  py32f072_it.o [5]
PVD_IRQHandler           0x800'0b03         Code  Wk  startup_py32f072xx.o [2]
PendSV_Handler           0x800'1c2d    0x2  Code  Gb  py32f072_it.o [5]
RCC_GetHSIFreq           0x800'088d   0x12  Code  Lc  py32f072_hal_rcc.o [3]
RCC_IRQHandler           0x800'19af         Code  Wk  startup_py32f072xx.o [2]
RTC_IRQHandler           0x800'0edb         Code  Wk  startup_py32f072xx.o [2]
Region$$Table$$Base      0x800'1ac0          --   Gb  - Linker created -
Region$$Table$$Limit     0x800'1ae4          --   Gb  - Linker created -
Reset_Handler            0x800'1c49         Code  Wk  startup_py32f072xx.o [2]
RxData                  0x2000'00f0    0x8  Data  Gb  main.o [5]
SPI1_IRQHandler          0x800'1c95         Code  Wk  startup_py32f072xx.o [2]
SPI2_IRQHandler          0x800'1c97         Code  Wk  startup_py32f072xx.o [2]
SVC_Handler              0x800'1c2b    0x2  Code  Gb  py32f072_it.o [5]
SysTick_Config           0x800'0a9b   0x30  Code  Lc  py32f072_hal_cortex.o [3]
SysTick_Handler          0x800'1c2f    0x8  Code  Gb  py32f072_it.o [5]
SystemCoreClock         0x2000'001c    0x4  Data  Gb  system_py32f072.o [1]
SystemInit               0x800'19f1   0x2a  Code  Gb  system_py32f072.o [1]
TIM14_IRQHandler         0x800'1c89         Code  Wk  startup_py32f072xx.o [2]
TIM15_IRQHandler         0x800'1c8b         Code  Wk  startup_py32f072xx.o [2]
TIM16_IRQHandler         0x800'1c8d         Code  Wk  startup_py32f072xx.o [2]
TIM17_IRQHandler         0x800'1c8f         Code  Wk  startup_py32f072xx.o [2]
TIM1_BRK_UP_TRG_COM_IRQHandler
                         0x800'1c7d         Code  Wk  startup_py32f072xx.o [2]
TIM1_CC_IRQHandler       0x800'1c7f         Code  Wk  startup_py32f072xx.o [2]
TIM2_IRQHandler          0x800'1c81         Code  Wk  startup_py32f072xx.o [2]
TIM3_IRQHandler          0x800'1c83         Code  Wk  startup_py32f072xx.o [2]
TIM6_LPTIM1_DAC_IRQHandler
                         0x800'1c85         Code  Wk  startup_py32f072xx.o [2]
TIM7_IRQHandler          0x800'1c87         Code  Wk  startup_py32f072xx.o [2]
TxData                  0x2000'0000    0x8  Data  Gb  main.o [5]
UART_AdvFeatureConfig    0x800'0e89   0x36  Code  Lc  py32f072_hal_uart.o [3]
UART_SetConfig           0x800'0ced  0x19a  Code  Lc  py32f072_hal_uart.o [3]
UART_WaitOnFlagUntilTimeout
                         0x800'0c81   0x68  Code  Lc  py32f072_hal_uart.o [3]
USART1_IRQHandler        0x800'1c99         Code  Wk  startup_py32f072xx.o [2]
USART2_IRQHandler        0x800'1c9b         Code  Wk  startup_py32f072xx.o [2]
USART3_4_IRQHandler      0x800'1c9d         Code  Wk  startup_py32f072xx.o [2]
USB_IRQHandler           0x800'1ca1         Code  Wk  startup_py32f072xx.o [2]
WWDG_IRQHandler          0x800'0a0f         Code  Wk  startup_py32f072xx.o [2]
_PrintfTiny              0x800'183f  0x162  Code  Gb  xprintftiny.o [6]
_Prout                   0x800'1bf9   0x16  Code  Gb  xprout.o [6]
__ICFEDIT_region_RAM_end__ {Abs}
                        0x2000'3fff         Data  Gb  <internal module>
__ICFEDIT_region_RAM_start__ {Abs}
                        0x2000'0000         Data  Gb  <internal module>
__NVIC_EnableIRQ         0x800'0a11   0x18  Code  Lc  py32f072_hal_cortex.o [3]
__NVIC_SetPriority       0x800'0a29   0x72  Code  Lc  py32f072_hal_cortex.o [3]
__aeabi_idiv0            0x800'0b01         Code  Gb  IntDivZer.o [7]
__aeabi_memcpy4          0x800'092d         Code  Gb  ABImemcpy.o [7]
__aeabi_memcpy8          0x800'092d         Code  Gb  ABImemcpy.o [7]
__aeabi_memset           0x800'16c5         Code  Gb  ABImemset.o [7]
__aeabi_uidiv            0x800'0961         Code  Gb  I32DivModFast.o [7]
__aeabi_uidivmod         0x800'0961         Code  Gb  I32DivModFast.o [7]
__cmain                  0x800'1b45         Code  Gb  cmain.o [7]
__exit                   0x800'1b7d   0x14  Code  Gb  exit.o [8]
__iar_Memset4_word       0x800'16e5         Code  Gb  ABImemset.o [7]
__iar_Memset_word        0x800'16d1         Code  Gb  ABImemset.o [7]
__iar_copy_init3         0x800'1a69   0x30  Code  Gb  copy_init3.o [7]
__iar_data_init3         0x800'1a99   0x28  Code  Gb  data_init.o [7]
__iar_program_start      0x800'1bad         Code  Gb  cstartup_M.o [7]
__iar_zero_init3         0x800'1a2d   0x3c  Code  Gb  zero_init3.o [7]
__low_level_init         0x800'1b63    0x4  Code  Gb  low_level_init.o [6]
__vector_table           0x800'0000         Data  Gb  startup_py32f072xx.o [2]
_call_main               0x800'1b51         Code  Gb  cmain.o [7]
_exit                    0x800'1b71         Code  Gb  cexit.o [7]
exit                     0x800'1b67    0x8  Code  Gb  exit.o [6]
main                     0x800'1379   0xee  Code  Gb  main.o [5]
memset                   0x800'1365   0x14  Code  Gb  memset.o [7]
out                      0x800'1825   0x1a  Code  Lc  xprintftiny.o [6]
printf                   0x800'17fd   0x28  Code  Gb  printf.o [6]
putchar                  0x800'17d5   0x14  Code  Gb  py32f072xx_Start_Kit.o [4]
strlen                   0x800'19a1         Code  Gb  strlen.o [7]
uwTick                  0x2000'00f8    0x4  Data  Gb  py32f072_hal.o [3]
uwTickFreq              0x2000'0018    0x4  Data  Gb  py32f072_hal.o [3]
uwTickPrio              0x2000'0014    0x4  Data  Gb  py32f072_hal.o [3]


[1] = C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\CMSIS_6603591812247902717.dir
[2] = C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\EWARM_7214922893274846302.dir
[3] = C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir
[4] = C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\PY32F072xx_Start_Kit_1292202923306237531.dir
[5] = C:\Users\KING\Desktop\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\CAN\CAN_ExtendedID_LBME_polling\EWARM\Project\Obj\User_7280784329937237312.dir
[6] = dl6M_tln.a
[7] = rt6M_tl.a
[8] = shb_l.a

  7'018 bytes of readonly  code memory
    312 bytes of readonly  data memory
  1'276 bytes of readwrite data memory

Errors: none
Warnings: none
