###############################################################################
#
# IAR ELF Linker V9.40.1.364/W64 for ARM                  26/Feb/2025  14:57:31
# Copyright 2007-2023 IAR Systems AB.
#
#    Output file  =
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Exe\Project.out
#    Map file     =
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\List\Project.map
#    Command line =
#        -f
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Exe\Project.out.rsp
#        (D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\User_7280784329937237312.dir\main.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_cortex.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_dma.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_flash.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_gpio.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\User_7280784329937237312.dir\py32f072_hal_msp.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_pwr.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_rcc.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_rcc_ex.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_uart.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\User_7280784329937237312.dir\py32f072_it.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\PY32F072xx_Start_Kit_1292202923306237531.dir\py32f072xx_Start_Kit.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\EWARM_7214922893274846302.dir\startup_py32f072xx.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\CMSIS_6603591812247902717.dir\system_py32f072.o
#        --no_out_extension -o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Exe\Project.out
#        --map
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\List\Project.map
#        --config
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\py32f072xB_flash.icf
#        --semihosting --entry __iar_program_start --vfe --text_out locale
#        --cpu=Cortex-M0+ --fpu=None) --dependencies=n
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Exe\Project.out.iar_deps
#
###############################################################################

*******************************************************************************
*** RUNTIME MODEL ATTRIBUTES
***

CppFlavor       = *
__CPP_Runtime   = 1
__SystemLibrary = DLib
__dlib_version  = 6


*******************************************************************************
*** HEAP SELECTION
***

The basic heap was selected because --advanced_heap
was not specified and the application did not appear to
be primarily optimized for speed.


*******************************************************************************
*** PLACEMENT SUMMARY
***

"A0":  place at address 0x800'0000 { ro section .intvec };
"P1":  place in [from 0x800'0000 to 0x801'ffff] { ro };
define block CSTACK with size = 1K, alignment = 8 { };
define block HEAP with size = 512, alignment = 8 { };
"P2":  place in [from 0x2000'0000 to 0x2000'3fff] {
          rw, block CSTACK, block HEAP };
initialize by copy { rw };

  Section            Kind         Address   Size  Object
  -------            ----         -------   ----  ------
"A0":                                       0xc0
  .intvec            ro code   0x800'0000   0xc0  startup_py32f072xx.o [2]
                             - 0x800'00c0   0xc0

"P1":                                      0xb80
  .text              ro code   0x800'00c0  0x368  py32f072_hal_flash.o [3]
  .text              ro code   0x800'0428    0xc  py32f072_hal.o [3]
  .text              ro code   0x800'0434  0x1d8  py32f072_hal_gpio.o [3]
  .text              ro code   0x800'060c  0x148  py32f072xx_Start_Kit.o [4]
  .text              ro code   0x800'0754   0x14  memset.o [7]
  .text              ro code   0x800'0768   0xf0  py32f072_hal_cortex.o [3]
  .text              ro code   0x800'0858   0x4e  ABImemset.o [7]
  .text              ro code   0x800'08a6   0xae  I32DivModFast.o [7]
  .text              ro code   0x800'0954    0x2  IntDivZer.o [7]
  .text              ro code   0x800'0956   0x3e  packbits_init_single.o [7]
  .text              ro code   0x800'0994   0x74  main.o [5]
  .text              ro code   0x800'0a08   0x1c  py32f072_hal.o [3]
  .text              ro code   0x800'0a24   0x5c  py32f072_hal.o [3]
  .text              ro code   0x800'0a80   0x34  py32f072_hal_msp.o [5]
  .text              ro code   0x800'0ab4   0x3c  system_py32f072.o [1]
  .text              ro code   0x800'0af0   0x28  data_init.o [7]
  .iar.init_table    const     0x800'0b18   0x10  - Linker created -
  .rodata            const     0x800'0b28   0x20  py32f072_hal_flash.o [3]
  .text              ro code   0x800'0b48   0x1e  cmain.o [7]
  .text              ro code   0x800'0b66    0x4  low_level_init.o [6]
  .text              ro code   0x800'0b6a    0x8  exit.o [6]
  .rodata            const     0x800'0b72    0x2  py32f072xx_Start_Kit.o [4]
  .text              ro code   0x800'0b74    0xa  cexit.o [7]
  .rodata            const     0x800'0b7e    0x2  py32f072xx_Start_Kit.o [4]
  .text              ro code   0x800'0b80   0x14  exit.o [8]
  .text              ro code   0x800'0b94   0x1c  cstartup_M.o [7]
  .text              ro code   0x800'0bb0   0x18  py32f072_hal.o [3]
  .text              ro code   0x800'0bc8   0x12  py32f072_it.o [5]
  .text              ro code   0x800'0bda    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0bdc   0x10  startup_py32f072xx.o [2]
  .text              ro code   0x800'0bec    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0bee    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0bf0    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0bf2    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0bf4    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0bf6    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0bf8    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0bfa    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0bfc    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0bfe    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c00    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c02    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c04    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c06    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c08    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c0a    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c0c    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c0e    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c10    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c12    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c14    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c16    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c18    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c1a    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c1c    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c1e    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c20    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c22    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c24    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c26    0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'0c28    0x2  startup_py32f072xx.o [2]
  .rodata            const     0x800'0c2a    0x1  py32f072xx_Start_Kit.o [4]
  .rodata            const     0x800'0c2b    0x0  packbits_init_single.o [7]
  Initializer bytes  const     0x800'0c2b   0x15  <for P2-1>
                             - 0x800'0c40  0xb80

"P2", part 1 of 2:                          0x50
  P2-1                        0x2000'0000   0x50  <Init block>
    .data            inited   0x2000'0000    0x4  py32f072_hal.o [3]
    .data            inited   0x2000'0004    0x4  py32f072_hal.o [3]
    .data            inited   0x2000'0008    0x4  py32f072xx_Start_Kit.o [4]
    .data            inited   0x2000'000c    0x4  py32f072xx_Start_Kit.o [4]
    .data            inited   0x2000'0010    0x4  system_py32f072.o [1]
    .bss             inited   0x2000'0014   0x20  main.o [5]
    .bss             inited   0x2000'0034    0x4  py32f072_hal.o [3]
    .bss             inited   0x2000'0038   0x18  py32f072_hal_flash.o [3]
                            - 0x2000'0050   0x50

"P2", part 2 of 2:                         0x400
  CSTACK                      0x2000'0050  0x400  <Block>
    CSTACK           uninit   0x2000'0050  0x400  <Block tail>
                            - 0x2000'0450  0x400

Unused ranges:

         From           To      Size
         ----           --      ----
   0x800'0c40   0x801'ffff  0x1'f3c0
  0x2000'0450  0x2000'3fff    0x3bb0


*******************************************************************************
*** INIT TABLE
***

          Address      Size
          -------      ----
Copy/packbits (__iar_packbits_init_single3)
    1 source range, total size 0x15 (26% of destination):
           0x800'0c2b  0x15
    1 destination range, total size 0x50:
          0x2000'0000  0x50



*******************************************************************************
*** MODULE SUMMARY
***

    Module                  ro code  ro data  rw data
    ------                  -------  -------  -------
command line/config:
    -------------------------------------------------
    Total:

D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\CMSIS_6603591812247902717.dir: [1]
    system_py32f072.o            60        1        4
    -------------------------------------------------
    Total:                       60        1        4

D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\EWARM_7214922893274846302.dir: [2]
    startup_py32f072xx.o        272
    -------------------------------------------------
    Total:                      272

D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir: [3]
    py32f072_hal.o              156        3       12
    py32f072_hal_cortex.o       240
    py32f072_hal_flash.o        872       39       24
    py32f072_hal_gpio.o         472
    -------------------------------------------------
    Total:                    1'740       42       36

D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\PY32F072xx_Start_Kit_1292202923306237531.dir: [4]
    py32f072xx_Start_Kit.o      328        7        8
    -------------------------------------------------
    Total:                      328        7        8

D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\User_7280784329937237312.dir: [5]
    main.o                      116        8       32
    py32f072_hal_msp.o           52
    py32f072_it.o                18
    -------------------------------------------------
    Total:                      186        8       32

dl6M_tln.a: [6]
    exit.o                        8
    low_level_init.o              4
    -------------------------------------------------
    Total:                       12

rt6M_tl.a: [7]
    ABImemset.o                  78
    I32DivModFast.o             174
    IntDivZer.o                   2
    cexit.o                      10
    cmain.o                      30
    cstartup_M.o                 28
    data_init.o                  40
    memset.o                     20
    packbits_init_single.o       62
    -------------------------------------------------
    Total:                      444

shb_l.a: [8]
    exit.o                       20
    -------------------------------------------------
    Total:                       20

    Linker created                        16    1'024
-----------------------------------------------------
    Grand Total:              3'062       74    1'104


*******************************************************************************
*** ENTRY LIST
***

Entry                       Address   Size  Type      Object
-----                       -------   ----  ----      ------
.iar.init_table$$Base    0x800'0b18          --   Gb  - Linker created -
.iar.init_table$$Limit   0x800'0b28          --   Gb  - Linker created -
?main                    0x800'0b49         Code  Gb  cmain.o [7]
ADC_COMP_IRQHandler      0x800'0c03         Code  Wk  startup_py32f072xx.o [2]
APP_FlashOBProgram       0x800'09d5   0x2a  Code  Lc  main.o [5]
BSP_LED_Init             0x800'060d   0x60  Code  Gb  py32f072xx_Start_Kit.o [4]
BSP_LED_On               0x800'066d   0x1c  Code  Gb  py32f072xx_Start_Kit.o [4]
BSP_PB_GetState          0x800'071d   0x1a  Code  Gb  py32f072xx_Start_Kit.o [4]
BSP_PB_Init              0x800'0689   0x94  Code  Gb  py32f072xx_Start_Kit.o [4]
BUTTON_IRQn              0x800'0c2a    0x1  Data  Gb  py32f072xx_Start_Kit.o [4]
BUTTON_PIN               0x800'0b7e    0x2  Data  Gb  py32f072xx_Start_Kit.o [4]
BUTTON_PORT             0x2000'000c    0x4  Data  Gb  py32f072xx_Start_Kit.o [4]
CAN_IRQHandler           0x800'0c27         Code  Wk  startup_py32f072xx.o [2]
CSTACK$$Base            0x2000'0050          --   Gb  - Linker created -
CSTACK$$Limit           0x2000'0450          --   Gb  - Linker created -
DMA1_Channel1_IRQHandler
                         0x800'0bfd         Code  Wk  startup_py32f072xx.o [2]
DMA1_Channel2_3_IRQHandler
                         0x800'0bff         Code  Wk  startup_py32f072xx.o [2]
DMA1_Channel4_5_6_7_IRQHandler
                         0x800'0c01         Code  Wk  startup_py32f072xx.o [2]
EXTI0_1_IRQHandler       0x800'0bf5         Code  Wk  startup_py32f072xx.o [2]
EXTI2_3_IRQHandler       0x800'0bf7         Code  Wk  startup_py32f072xx.o [2]
EXTI4_15_IRQHandler      0x800'0bf9         Code  Wk  startup_py32f072xx.o [2]
FLASH_IRQHandler         0x800'0bf1         Code  Wk  startup_py32f072xx.o [2]
FLASH_OB_BOR_LevelConfig
                         0x800'01bf   0x12  Code  Lc  py32f072_hal_flash.o [3]
FLASH_OB_GetRDP          0x800'01ad   0x12  Code  Lc  py32f072_hal_flash.o [3]
FLASH_OB_GetUser         0x800'01a1    0xc  Code  Lc  py32f072_hal_flash.o [3]
FLASH_OB_OptrConfig      0x800'01d1   0x16  Code  Lc  py32f072_hal_flash.o [3]
FLASH_WaitForLastOperation
                         0x800'0157   0x26  Code  Gb  py32f072_hal_flash.o [3]
HAL_FLASH_Lock           0x800'00e3   0x1c  Code  Gb  py32f072_hal_flash.o [3]
HAL_FLASH_OBProgram      0x800'01e7  0x1f8  Code  Gb  py32f072_hal_flash.o [3]
HAL_FLASH_OB_Launch      0x800'0147   0x10  Code  Gb  py32f072_hal_flash.o [3]
HAL_FLASH_OB_Lock        0x800'0129   0x1e  Code  Gb  py32f072_hal_flash.o [3]
HAL_FLASH_OB_Unlock      0x800'00ff   0x2a  Code  Gb  py32f072_hal_flash.o [3]
HAL_FLASH_Unlock         0x800'00c1   0x22  Code  Gb  py32f072_hal_flash.o [3]
HAL_GPIO_Init            0x800'0435  0x190  Code  Gb  py32f072_hal_gpio.o [3]
HAL_GPIO_ReadPin         0x800'05d1   0x16  Code  Gb  py32f072_hal_gpio.o [3]
HAL_GPIO_WritePin        0x800'05e7   0x14  Code  Gb  py32f072_hal_gpio.o [3]
HAL_GetTick              0x800'0429    0xc  Code  Wk  py32f072_hal.o [3]
HAL_IncTick              0x800'0bb1   0x18  Code  Wk  py32f072_hal.o [3]
HAL_Init                 0x800'0a09   0x1c  Code  Gb  py32f072_hal.o [3]
HAL_InitTick             0x800'0a25   0x5c  Code  Wk  py32f072_hal.o [3]
HAL_MspInit              0x800'0a81   0x34  Code  Gb  py32f072_hal_msp.o [5]
HAL_NVIC_EnableIRQ       0x800'082d    0xa  Code  Gb  py32f072_hal_cortex.o [3]
HAL_NVIC_SetPriority     0x800'0823    0xa  Code  Gb  py32f072_hal_cortex.o [3]
HAL_SYSTICK_Config       0x800'0837    0x8  Code  Gb  py32f072_hal_cortex.o [3]
HardFault_Handler        0x800'0bcb    0x4  Code  Gb  py32f072_it.o [5]
I2C1_IRQHandler          0x800'0c19         Code  Wk  startup_py32f072xx.o [2]
I2C2_IRQHandler          0x800'0c1b         Code  Wk  startup_py32f072xx.o [2]
LCD_IRQHandler           0x800'0bfb         Code  Wk  startup_py32f072xx.o [2]
LED_PIN                  0x800'0b72    0x2  Data  Gb  py32f072xx_Start_Kit.o [4]
LED_PORT                0x2000'0008    0x4  Data  Gb  py32f072xx_Start_Kit.o [4]
NMI_Handler              0x800'0bc9    0x2  Code  Gb  py32f072_it.o [5]
OBInitCfg               0x2000'0014   0x20  Data  Gb  main.o [5]
PVD_IRQHandler           0x800'0bed         Code  Wk  startup_py32f072xx.o [2]
PendSV_Handler           0x800'0bd1    0x2  Code  Gb  py32f072_it.o [5]
RCC_IRQHandler           0x800'0bf3         Code  Wk  startup_py32f072xx.o [2]
RTC_IRQHandler           0x800'0bef         Code  Wk  startup_py32f072xx.o [2]
Region$$Table$$Base      0x800'0b18          --   Gb  - Linker created -
Region$$Table$$Limit     0x800'0b28          --   Gb  - Linker created -
Reset_Handler            0x800'0bdd         Code  Wk  startup_py32f072xx.o [2]
SPI1_IRQHandler          0x800'0c1d         Code  Wk  startup_py32f072xx.o [2]
SPI2_IRQHandler          0x800'0c1f         Code  Wk  startup_py32f072xx.o [2]
SVC_Handler              0x800'0bcf    0x2  Code  Gb  py32f072_it.o [5]
SysTick_Config           0x800'07f3   0x30  Code  Lc  py32f072_hal_cortex.o [3]
SysTick_Handler          0x800'0bd3    0x8  Code  Gb  py32f072_it.o [5]
SystemCoreClock         0x2000'0010    0x4  Data  Gb  system_py32f072.o [1]
SystemInit               0x800'0ab5   0x2a  Code  Gb  system_py32f072.o [1]
TIM14_IRQHandler         0x800'0c11         Code  Wk  startup_py32f072xx.o [2]
TIM15_IRQHandler         0x800'0c13         Code  Wk  startup_py32f072xx.o [2]
TIM16_IRQHandler         0x800'0c15         Code  Wk  startup_py32f072xx.o [2]
TIM17_IRQHandler         0x800'0c17         Code  Wk  startup_py32f072xx.o [2]
TIM1_BRK_UP_TRG_COM_IRQHandler
                         0x800'0c05         Code  Wk  startup_py32f072xx.o [2]
TIM1_CC_IRQHandler       0x800'0c07         Code  Wk  startup_py32f072xx.o [2]
TIM2_IRQHandler          0x800'0c09         Code  Wk  startup_py32f072xx.o [2]
TIM3_IRQHandler          0x800'0c0b         Code  Wk  startup_py32f072xx.o [2]
TIM6_LPTIM1_DAC_IRQHandler
                         0x800'0c0d         Code  Wk  startup_py32f072xx.o [2]
TIM7_IRQHandler          0x800'0c0f         Code  Wk  startup_py32f072xx.o [2]
USART1_IRQHandler        0x800'0c21         Code  Wk  startup_py32f072xx.o [2]
USART2_IRQHandler        0x800'0c23         Code  Wk  startup_py32f072xx.o [2]
USART3_4_IRQHandler      0x800'0c25         Code  Wk  startup_py32f072xx.o [2]
USB_IRQHandler           0x800'0c29         Code  Wk  startup_py32f072xx.o [2]
WWDG_IRQHandler          0x800'0bdb         Code  Wk  startup_py32f072xx.o [2]
_FlashTimmingParam       0x800'0b28   0x20  Data  Gb  py32f072_hal_flash.o [3]
__ICFEDIT_region_RAM_end__ {Abs}
                        0x2000'3fff         Data  Gb  <internal module>
__ICFEDIT_region_RAM_start__ {Abs}
                        0x2000'0000         Data  Gb  <internal module>
__NVIC_EnableIRQ         0x800'0769   0x18  Code  Lc  py32f072_hal_cortex.o [3]
__NVIC_SetPriority       0x800'0781   0x72  Code  Lc  py32f072_hal_cortex.o [3]
__aeabi_idiv0            0x800'0955         Code  Gb  IntDivZer.o [7]
__aeabi_memset           0x800'0859         Code  Gb  ABImemset.o [7]
__aeabi_uidiv            0x800'08a7         Code  Gb  I32DivModFast.o [7]
__aeabi_uidivmod         0x800'08a7         Code  Gb  I32DivModFast.o [7]
__cmain                  0x800'0b49         Code  Gb  cmain.o [7]
__exit                   0x800'0b81   0x14  Code  Gb  exit.o [8]
__iar_Memset4_word       0x800'0879         Code  Gb  ABImemset.o [7]
__iar_Memset_word        0x800'0865         Code  Gb  ABImemset.o [7]
__iar_data_init3         0x800'0af1   0x28  Code  Gb  data_init.o [7]
__iar_packbits_init_single3
                         0x800'0957   0x3e  Code  Gb  packbits_init_single.o [7]
__iar_program_start      0x800'0b95         Code  Gb  cstartup_M.o [7]
__low_level_init         0x800'0b67    0x4  Code  Gb  low_level_init.o [6]
__vector_table           0x800'0000         Data  Gb  startup_py32f072xx.o [2]
_call_main               0x800'0b55         Code  Gb  cmain.o [7]
_exit                    0x800'0b75         Code  Gb  cexit.o [7]
exit                     0x800'0b6b    0x8  Code  Gb  exit.o [6]
main                     0x800'0995   0x40  Code  Gb  main.o [5]
memset                   0x800'0755   0x14  Code  Gb  memset.o [7]
pFlash                  0x2000'0038   0x18  Data  Gb  py32f072_hal_flash.o [3]
uwTick                  0x2000'0034    0x4  Data  Gb  py32f072_hal.o [3]
uwTickFreq              0x2000'0004    0x4  Data  Gb  py32f072_hal.o [3]
uwTickPrio              0x2000'0000    0x4  Data  Gb  py32f072_hal.o [3]


[1] = D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\CMSIS_6603591812247902717.dir
[2] = D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\EWARM_7214922893274846302.dir
[3] = D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir
[4] = D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\PY32F072xx_Start_Kit_1292202923306237531.dir
[5] = D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_OptionByteWrite_RST\EWARM\Project\Obj\User_7280784329937237312.dir
[6] = dl6M_tln.a
[7] = rt6M_tl.a
[8] = shb_l.a

  3'062 bytes of readonly  code memory
     74 bytes of readonly  data memory
  1'104 bytes of readwrite data memory

Errors: none
Warnings: none
