<?xml version="1.0" encoding="utf-8" standalone="no"?>
<device schemaVersion="1.1" xmlns:xs="http://www.w3.org/2001/XMLSchema-instance" noNamespaceSchemaLocation="CMSIS-SVD.xsd">
  <vendor>Puya</vendor>
  <vendorID>Puya</vendorID>
  <name>PY32F002Xxx</name>
  <series>PY32F0</series>
  <version>1.0.0</version>
  <description>Arm 32-bit Cortex-M0+ Microcontroller based device, CPU clock up to 48 MHz.</description>
  <cpu>
    <name>CM0+</name>
    <revision>r0p1</revision>
    <endian>little</endian>
    <mpuPresent>false</mpuPresent>
    <fpuPresent>false</fpuPresent>
    <nvicPrioBits>4</nvicPrioBits>
    <vendorSystickConfig>false</vendorSystickConfig>
  </cpu>
  <addressUnitBits>8</addressUnitBits>
  <width>32</width>
  <size>32</size>
  <access>read-write</access>
  <resetValue>0x0</resetValue>
  <resetMask>0xFFFFFFFF</resetMask>
  <peripherals>
    <peripheral>
      <name>ADC</name>
      <description>Analog to Digital Converter</description>
      <groupName>ADC</groupName>
      <baseAddress>0x40012400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>ADC</name>
        <description>ADC Interrupt</description>
        <value>12</value>
      </interrupt>
      <registers>
        <register>
          <name>ISR</name>
          <displayName>ISR</displayName>
          <description>ADC interrupt and status register</description>
          <addressOffset>0x0</addressOffset>
          <fields>
            <field>
              <name>EOSMP</name>
              <description>ADC group regular end of sampling flag</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>EOC</name>
              <description>ADC group regular end of unitary conversion flag</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>EOSEQ</name>
              <description>ADC group regular end of sequence conversions flag</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>OVR</name>
              <description>ADC group regular overrun flag</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>AWD</name>
              <description>ADC analog watchdog flag</description>
              <bitRange>[7:7]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>IER</name>
          <displayName>IER</displayName>
          <description>ADC interrupt enable register</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>EOSMPIE</name>
              <description>ADC group regular end of sampling interrupt</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>EOCIE</name>
              <description>ADC group regular end of unitary conversion interrupt</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>EOSEQIE</name>
              <description>ADC group regular end of sequence conversions interrupt</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>OVRIE</name>
              <description>ADC group regular overrun interrupt</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>AWDIE</name>
              <description>ADC analog watchdog interrupt</description>
              <bitRange>[7:7]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>ADC control register</description>
          <addressOffset>0x8</addressOffset>
          <fields>
            <field>
              <name>ADEN</name>
              <description>ADC enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>ADDIS</name>
              <description>ADC enable</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>ADSTART</name>
              <description>ADC group regular conversion start</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>ADSTP</name>
              <description>ADC group regular conversion stop</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>VREF_BUFFERE</name>
              <description>desc VREF_BUFFERE</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>VERBUFF_SEL</name>
              <description>desc VERBUFF_SEL</description>
              <bitRange>[7:6]</bitRange>
            </field>
            <field>
              <name>ADCAL</name>
              <description>ADC group regular conversion calibration</description>
              <bitRange>[31:31]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR1</name>
          <displayName>CFGR1</displayName>
          <description>ADC configuration register 1</description>
          <addressOffset>0xC</addressOffset>
          <fields>
            <field>
              <name>SCANDIR</name>
              <description>Scan sequence direction</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>RESSEL</name>
              <description>ADC data resolution</description>
              <bitRange>[4:3]</bitRange>
            </field>
            <field>
              <name>ALIGN</name>
              <description>ADC data alignement</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>EXTSEL</name>
              <description>ADC group regular external trigger source</description>
              <bitRange>[8:6]</bitRange>
            </field>
            <field>
              <name>EXTEN</name>
              <description>ADC group regular external trigger polarity</description>
              <bitRange>[11:10]</bitRange>
            </field>
            <field>
              <name>OVRMOD</name>
              <description>ADC group regular overrun configuration</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>CONT</name>
              <description>ADC group regular continuous conversion mode</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>WAIT</name>
              <description>Wait conversion mode</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>DISCEN</name>
              <description>ADC group regular sequencer discontinuous mode</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>AWDSGL</name>
              <description>ADC analog watchdog monitoring a single channel or all channels</description>
              <bitRange>[22:22]</bitRange>
            </field>
            <field>
              <name>AWDEN</name>
              <description>ADC analog watchdog enable on scope ADC group regular</description>
              <bitRange>[23:23]</bitRange>
            </field>
            <field>
              <name>AWDCH</name>
              <description>ADC analog watchdog monitored channel selection</description>
              <bitRange>[29:26]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR2</name>
          <displayName>CFGR2</displayName>
          <description>ADC configuration register 2</description>
          <addressOffset>0x10</addressOffset>
          <fields>
            <field>
              <name>CKMODE</name>
              <description>ADC clock mode</description>
              <bitRange>[31:28]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SMPR</name>
          <displayName>SMPR</displayName>
          <description>ADC sampling time register</description>
          <addressOffset>0x14</addressOffset>
          <fields>
            <field>
              <name>SMP</name>
              <description>Sampling time selection</description>
              <bitRange>[2:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>TR</name>
          <displayName>TR</displayName>
          <description>ADC analog watchdog 1 threshold register</description>
          <addressOffset>0x20</addressOffset>
          <resetValue>0xFFF0000</resetValue>
          <fields>
            <field>
              <name>LT</name>
              <description>ADC analog watchdog threshold low</description>
              <bitRange>[11:0]</bitRange>
            </field>
            <field>
              <name>HT</name>
              <description>ADC analog watchdog threshold high</description>
              <bitRange>[27:16]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CHSELR</name>
          <displayName>CHSELR</displayName>
          <description>ADC group regular sequencer register</description>
          <addressOffset>0x28</addressOffset>
          <resetValue>0xFFF0000</resetValue>
          <fields>
            <field>
              <name>CHSEL0</name>
              <description>Channel-0 selection</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>CHSEL1</name>
              <description>Channel-1 selection</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>CHSEL2</name>
              <description>Channel-2 selection</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>CHSEL3</name>
              <description>Channel-3 selection</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>CHSEL4</name>
              <description>Channel-4 selection</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>CHSEL5</name>
              <description>Channel-5 selection</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>CHSEL6</name>
              <description>Channel-6 selection</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>CHSEL7</name>
              <description>Channel-7 selection</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>CHSEL8</name>
              <description>Channel-8 selection</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>CHSEL9</name>
              <description>Channel-9 selection</description>
              <bitRange>[9:9]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>ADC group regular data register</description>
          <addressOffset>0x40</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>DATA</name>
              <description>ADC group regular conversion data</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCSR</name>
          <displayName>CCSR</displayName>
          <description>ADC calibration configuration and status register</description>
          <addressOffset>0x44</addressOffset>
          <fields>
            <field>
              <name>CALSEL</name>
              <description>Calibration contents selection</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>CALSMP</name>
              <description>Calibration sample time selection</description>
              <bitRange>[13:12]</bitRange>
            </field>
            <field>
              <name>CALBYP</name>
              <description>desc CALBYP</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>CALSET</name>
              <description>Calibration factor selection</description>
              <bitRange>[15:15]</bitRange>
            </field>
            <field>
              <name>OFFSUC</name>
              <description>desc OFFSUC</description>
              <bitRange>[29:29]</bitRange>
            </field>
            <field>
              <name>CALSUC</name>
              <description>desc CALSUC</description>
              <bitRange>[30:30]</bitRange>
            </field>
            <field>
              <name>CALON</name>
              <description>Calibration flag</description>
              <bitRange>[31:31]</bitRange>
              <access>read-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR</name>
          <displayName>CCR</displayName>
          <description>ADC common configuration register</description>
          <addressOffset>0x308</addressOffset>
          <fields>
            <field>
              <name>VREFEN</name>
              <description>VREFINT enable</description>
              <bitRange>[22:22]</bitRange>
            </field>
            <field>
              <name>TSEN</name>
              <description>Temperature sensor enable</description>
              <bitRange>[23:23]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>CRC</name>
      <description>CRC calculation unit</description>
      <groupName>CRC</groupName>
      <baseAddress>0x40023000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>Data register</description>
          <addressOffset>0x0</addressOffset>
          <resetValue>0xFFFFFFFF</resetValue>
          <fields>
            <field>
              <name>DR</name>
              <description>Data Register</description>
              <bitRange>[31:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>IDR</name>
          <displayName>IDR</displayName>
          <description>Independent Data register</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>IDR</name>
              <description>Independent Data register</description>
              <bitRange>[7:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Control register</description>
          <addressOffset>0x8</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>RESET</name>
              <description>Reset bit</description>
              <bitRange>[0:0]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>DBGMCU</name>
      <description>Debug support</description>
      <groupName>DBGMCU</groupName>
      <baseAddress>0x40015800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>IDCODE</name>
          <displayName>IDCODE</displayName>
          <description>MCU Device ID Code Register</description>
          <addressOffset>0x0</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>REV_ID</name>
              <description>REV_ID</description>
              <bitRange>[31:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Debug MCU Configuration Register</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>DBG_STOP</name>
              <description>Debug Stop Mode</description>
              <bitRange>[1:1]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>APB_FZ1</name>
          <displayName>APB_FZ1</displayName>
          <description>APB Freeze Register1</description>
          <addressOffset>0x8</addressOffset>
          <fields>
            <field>
              <name>DBG_LPTIM_STOP</name>
              <description>Debug LPTIM stopped when Core ishalted</description>
              <bitRange>[31:31]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>APB_FZ2</name>
          <displayName>APB_FZ2</displayName>
          <description>APB Freeze Register2</description>
          <addressOffset>0xC</addressOffset>
          <fields>
            <field>
              <name>DBG_TIMER1_STOP</name>
              <description>Debug Timer 1 stopped when Core ishalted</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>DBG_TIM14_STOP</name>
              <description>Debug TIM 14 stopped whenCore is halted</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>EXTI</name>
      <description>External interrupt/event controller</description>
      <groupName>EXTI</groupName>
      <baseAddress>0x40021800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>EXTI0_1</name>
        <description>EXTI Line 0 and 1 Interrupt</description>
        <value>5</value>
      </interrupt>
      <interrupt>
        <name>EXTI2_3</name>
        <description>EXTI Line 2 and 3 Interrupt</description>
        <value>6</value>
      </interrupt>
      <interrupt>
        <name>EXTI4_15</name>
        <description>EXTI Line 4 to 15 Interrupt</description>
        <value>7</value>
      </interrupt>
      <registers>
        <register>
          <name>RTSR</name>
          <displayName>RTSR</displayName>
          <description>EXTI rising trigger selection register</description>
          <addressOffset>0x0</addressOffset>
          <fields>
            <field>
              <name>RT0</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>RT1</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>RT2</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>RT3</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>RT4</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>RT5</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>RT6</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>RT7</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>RT17</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>RT18</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[18:18]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>FTSR</name>
          <displayName>FTSR</displayName>
          <description>EXTI falling trigger selection register</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>FT0</name>
              <description>Falling trigger event configuration bit of Configurable Event input</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>FT1</name>
              <description>Falling trigger event configuration bit of Configurable Event input</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>FT2</name>
              <description>Falling trigger event configuration bit of Configurable Event input</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>FT3</name>
              <description>Falling trigger event configuration bit of Configurable Event input</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>FT4</name>
              <description>Falling trigger event configuration bit of Configurable Event input</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>FT5</name>
              <description>Falling trigger event configuration bit of Configurable Event input</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>FT6</name>
              <description>Falling trigger event configuration bit of Configurable Event input</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>FT7</name>
              <description>Falling trigger event configuration bit of Configurable Event input</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>FT17</name>
              <description>Falling trigger event configuration bit of Configurable Event input</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>FT18</name>
              <description>Falling trigger event configuration bit of Configurable Event input</description>
              <bitRange>[18:18]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SWIER</name>
          <displayName>SWIER</displayName>
          <description>EXTI software interrupt event register</description>
          <addressOffset>0x8</addressOffset>
          <fields>
            <field>
              <name>SWI0</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>SWI1</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>SWI2</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>SWI3</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>SWI4</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>SWI5</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>SWI6</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>SWI7</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>SWI17</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>SWI18</name>
              <description>Rising trigger event configuration bit of Configurable Event input</description>
              <bitRange>[18:18]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PR</name>
          <displayName>PR</displayName>
          <description>EXTI pending register</description>
          <addressOffset>0xC</addressOffset>
          <fields>
            <field>
              <name>PR0</name>
              <description>configurable event inputs x rising edge Pending bit.</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>PR1</name>
              <description>configurable event inputs x rising edge Pending bit.</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>PR2</name>
              <description>configurable event inputs x rising edge Pending bit.</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>PR3</name>
              <description>configurable event inputs x rising edge Pending bit.</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>PR4</name>
              <description>configurable event inputs x rising edge Pending bit.</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>PR5</name>
              <description>configurable event inputs x rising edge Pending bit.</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>PR6</name>
              <description>configurable event inputs x rising edge Pending bit.</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>PR7</name>
              <description>configurable event inputs x rising edge Pending bit.</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>PR17</name>
              <description>configurable event inputs x rising edge Pending bit.</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>PR18</name>
              <description>configurable event inputs x rising edge Pending bit.</description>
              <bitRange>[18:18]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>EXTICR1</name>
          <displayName>EXTICR1</displayName>
          <description>EXTI external interrupt selection register</description>
          <addressOffset>0x60</addressOffset>
          <fields>
            <field>
              <name>EXTI0</name>
              <description>GPIO port selection</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>EXTI1</name>
              <description>GPIO port selection</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>EXTI2</name>
              <description>GPIO port selection</description>
              <bitRange>[17:16]</bitRange>
            </field>
            <field>
              <name>EXTI3</name>
              <description>GPIO port selection</description>
              <bitRange>[25:24]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>EXTICR2</name>
          <displayName>EXTICR2</displayName>
          <description>EXTI external interrupt selection register</description>
          <addressOffset>0x64</addressOffset>
          <fields>
            <field>
              <name>EXTI4</name>
              <description>GPIO port selection</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>EXTI5</name>
              <description>GPIO port selection</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>EXTI6</name>
              <description>GPIO port selection</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>EXTI7</name>
              <description>GPIO port selection</description>
              <bitRange>[24:24]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>IMR</name>
          <displayName>IMR</displayName>
          <description>EXTI CPU wakeup with interrupt mask register</description>
          <addressOffset>0x80</addressOffset>
          <resetValue>0xFFF80000</resetValue>
          <fields>
            <field>
              <name>IM0</name>
              <description>CPU wakeup with interrupt mask on event input</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>IM1</name>
              <description>CPU wakeup with interrupt mask on event input</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>IM2</name>
              <description>CPU wakeup with interrupt mask on event input</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>IM3</name>
              <description>CPU wakeup with interrupt mask on event input</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>IM4</name>
              <description>CPU wakeup with interrupt mask on event input</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>IM5</name>
              <description>CPU wakeup with interrupt mask on event input</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>IM6</name>
              <description>CPU wakeup with interrupt mask on event input</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>IM7</name>
              <description>CPU wakeup with interrupt mask on event input</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>IM17</name>
              <description>CPU wakeup with interrupt mask on event input</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>IM18</name>
              <description>CPU wakeup with interrupt mask on event input</description>
              <bitRange>[18:18]</bitRange>
            </field>
            <field>
              <name>IM29</name>
              <description>CPU wakeup with interrupt mask on event input</description>
              <bitRange>[29:29]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>EMR</name>
          <displayName>EMR</displayName>
          <description>EXTI CPU wakeup with event mask register</description>
          <addressOffset>0x84</addressOffset>
          <fields>
            <field>
              <name>EM0</name>
              <description>CPU wakeup with event mask on event input</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>EM1</name>
              <description>CPU wakeup with event mask on event input</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>EM2</name>
              <description>CPU wakeup with event mask on event input</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>EM3</name>
              <description>CPU wakeup with event mask on event input</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>EM4</name>
              <description>CPU wakeup with event mask on event input</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>EM5</name>
              <description>CPU wakeup with event mask on event input</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>EM6</name>
              <description>CPU wakeup with event mask on event input</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>EM7</name>
              <description>CPU wakeup with event mask on event input</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>EM17</name>
              <description>CPU wakeup with event mask on event input</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>EM18</name>
              <description>CPU wakeup with event mask on event input</description>
              <bitRange>[18:18]</bitRange>
            </field>
            <field>
              <name>EM29</name>
              <description>CPU wakeup with event mask on event input</description>
              <bitRange>[29:29]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>FLASH</name>
      <description>Flash</description>
      <groupName>Flash</groupName>
      <baseAddress>0x40022000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>FLASH</name>
        <description>FLASH global Interrupt</description>
        <value>3</value>
      </interrupt>
      <registers>
        <register>
          <name>ACR</name>
          <displayName>ACR</displayName>
          <description>Access control register</description>
          <addressOffset>0x0</addressOffset>
          <resetValue>0x600</resetValue>
          <fields>
            <field>
              <name>LATENCY</name>
              <description>Latency</description>
              <bitRange>[0:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>KEYR</name>
          <displayName>KEYR</displayName>
          <description>Flash key register</description>
          <addressOffset>0x8</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>KEY</name>
              <description>Flash key</description>
              <bitRange>[31:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>OPTKEYR</name>
          <displayName>OPTKEYR</displayName>
          <description>Option byte key register</description>
          <addressOffset>0xC</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>OPTKEY</name>
              <description>Option byte key</description>
              <bitRange>[31:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>Status register</description>
          <addressOffset>0x10</addressOffset>
          <fields>
            <field>
              <name>EOP</name>
              <description>End of operation</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>WRPERR</name>
              <description>Write protected error</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>OPTVERR</name>
              <description>Option and Engineering bits loading validity error</description>
              <bitRange>[15:15]</bitRange>
            </field>
            <field>
              <name>BSY</name>
              <description>Busy</description>
              <bitRange>[16:16]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Flash control register</description>
          <addressOffset>0x14</addressOffset>
          <resetValue>0xC0000000</resetValue>
          <fields>
            <field>
              <name>PG</name>
              <description>Programming</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>PER</name>
              <description>Page erase</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>MER</name>
              <description>Mass erase</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>SER</name>
              <description>Sector erase</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>OPTSTRT</name>
              <description>Option byte program start</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>PGSTRT</name>
              <description>Flash main memory program start</description>
              <bitRange>[19:19]</bitRange>
            </field>
            <field>
              <name>EOPIE</name>
              <description>End of operation interrupt enable</description>
              <bitRange>[24:24]</bitRange>
            </field>
            <field>
              <name>ERRIE</name>
              <description>Error interrupt enable</description>
              <bitRange>[25:25]</bitRange>
            </field>
            <field>
              <name>OBL_LAUNCH</name>
              <description>Force the option byte loading</description>
              <bitRange>[27:27]</bitRange>
            </field>
            <field>
              <name>OPTLOCK</name>
              <description>Options Lock</description>
              <bitRange>[30:30]</bitRange>
            </field>
            <field>
              <name>LOCK</name>
              <description>FLASH_CR Lock</description>
              <bitRange>[31:31]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>OPTR</name>
          <displayName>OPTR</displayName>
          <description>Flash option register</description>
          <addressOffset>0x20</addressOffset>
          <resetValue>0x4F55B0AA</resetValue>
          <fields>
            <field>
              <name>BOREN</name>
              <description>BOR reset Level</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>BORF_LEV</name>
              <description>These bits contain the VDD supply level threshold that activates the reset</description>
              <bitRange>[11:9]</bitRange>
            </field>
            <field>
              <name>IWDG_SW</name>
              <description>Independent watchdog selection</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>SWD_MODE</name>
              <description>SWD_MODE</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>NRST_MODE</name>
              <description>NRST_MODE</description>
              <bitRange>[14:14]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SDKR</name>
          <displayName>SDKR</displayName>
          <description>Flash SDK address register</description>
          <addressOffset>0x24</addressOffset>
          <resetValue>0xFFE0001F</resetValue>
          <fields>
            <field>
              <name>SDK_STRT</name>
              <description>SDK area start address</description>
              <bitRange>[3:0]</bitRange>
            </field>
            <field>
              <name>SDK_END</name>
              <description>SDK area end address</description>
              <bitRange>[11:8]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>BTCR</name>
          <displayName>BTCR</displayName>
          <description>FLASH boot control register</description>
          <addressOffset>0x28</addressOffset>
          <fields>
            <field>
              <name>BOOT_SIZE</name>
              <description>desc BOOT_SIZE</description>
              <bitRange>[2:0]</bitRange>
            </field>
            <field>
              <name>BOOT0</name>
              <description>desc BOOT0</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>NBOOT1</name>
              <description>desc NBOOT1</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>WRPR</name>
          <displayName>WRPR</displayName>
          <description>Flash WRP address register</description>
          <addressOffset>0x2C</addressOffset>
          <resetValue>0xFFFF</resetValue>
          <fields>
            <field>
              <name>WRP</name>
              <description>WRP address</description>
              <bitRange>[5:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>STCR</name>
          <displayName>STCR</displayName>
          <description>Flash sleep time config register</description>
          <addressOffset>0x90</addressOffset>
          <resetValue>0x6400</resetValue>
          <fields>
            <field>
              <name>SLEEP_EN</name>
              <description>FLash sleep enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>SLEEP_TIME</name>
              <description>FLash sleep time configuration(counter based on HSI_10M)</description>
              <bitRange>[15:8]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>TS0</name>
          <displayName>TS0</displayName>
          <description>Flash TS0 register</description>
          <addressOffset>0x100</addressOffset>
          <resetValue>0xB4</resetValue>
          <fields>
            <field>
              <name>TS0</name>
              <description>FLash TS0 register</description>
              <bitRange>[8:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>TS1</name>
          <displayName>TS1</displayName>
          <description>Flash TS1 register</description>
          <addressOffset>0x104</addressOffset>
          <resetValue>0x1B0</resetValue>
          <fields>
            <field>
              <name>TS1</name>
              <description>FLash TS1 register</description>
              <bitRange>[9:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>TS2P</name>
          <displayName>TS2P</displayName>
          <description>Flash TS2P register</description>
          <addressOffset>0x108</addressOffset>
          <resetValue>0xB4</resetValue>
          <fields>
            <field>
              <name>TS2P</name>
              <description>FLash TS2P register</description>
              <bitRange>[8:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>TPS3</name>
          <displayName>TPS3</displayName>
          <description>Flash TPS3 register</description>
          <addressOffset>0x10C</addressOffset>
          <resetValue>0x6C0</resetValue>
          <fields>
            <field>
              <name>TPS3</name>
              <description>FLash TPS3 register</description>
              <bitRange>[11:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>TS3</name>
          <displayName>TS3</displayName>
          <description>Flash TS3 register</description>
          <addressOffset>0x110</addressOffset>
          <resetValue>0xB4</resetValue>
          <fields>
            <field>
              <name>TS3</name>
              <description>FLash TS3 register</description>
              <bitRange>[8:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PERTPE</name>
          <displayName>PERTPE</displayName>
          <description>Flash PERTPE register</description>
          <addressOffset>0x114</addressOffset>
          <resetValue>0x14820</resetValue>
          <fields>
            <field>
              <name>PERTPE</name>
              <description>FLash PERTPE register</description>
              <bitRange>[17:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SMERTPE</name>
          <displayName>SMERTPE</displayName>
          <description>Flash SMERTPE register</description>
          <addressOffset>0x118</addressOffset>
          <resetValue>0x14820</resetValue>
          <fields>
            <field>
              <name>SMERTPE</name>
              <description>FLash SMERTPE register</description>
              <bitRange>[17:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PRGTPE</name>
          <displayName>PRGTPE</displayName>
          <description>Flash PRGTPE register</description>
          <addressOffset>0x11C</addressOffset>
          <resetValue>0x5DC0</resetValue>
          <fields>
            <field>
              <name>PRGTPE</name>
              <description>FLash PRGTPE register</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PRETPE</name>
          <displayName>PRETPE</displayName>
          <description>Flash PRETPE register</description>
          <addressOffset>0x120</addressOffset>
          <resetValue>0x12C0</resetValue>
          <fields>
            <field>
              <name>PRETPE</name>
              <description>FLash PRETPE register</description>
              <bitRange>[13:0]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>GPIOA</name>
      <description>General-purpose I/Os</description>
      <groupName>GPIO</groupName>
      <baseAddress>0x50000000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>MODER</name>
          <displayName>MODER</displayName>
          <description>GPIO port mode register</description>
          <addressOffset>0x0</addressOffset>
          <resetValue>0xEBFFFFFF</resetValue>
          <fields>
            <field>
              <name>MODE0</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>MODE1</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[3:2]</bitRange>
            </field>
            <field>
              <name>MODE2</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[5:4]</bitRange>
            </field>
            <field>
              <name>MODE3</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[7:6]</bitRange>
            </field>
            <field>
              <name>MODE4</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>MODE5</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[11:10]</bitRange>
            </field>
            <field>
              <name>MODE6</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[13:12]</bitRange>
            </field>
            <field>
              <name>MODE7</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[15:14]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>OTYPER</name>
          <displayName>OTYPER</displayName>
          <description>GPIO port output type register</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>OT0</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>OT1</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>OT2</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>OT3</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>OT4</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>OT5</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>OT6</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>OT7</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[7:7]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>OSPEEDR</name>
          <displayName>OSPEEDR</displayName>
          <description>GPIO port output speed register</description>
          <addressOffset>0x8</addressOffset>
          <resetValue>0xC000000</resetValue>
          <fields>
            <field>
              <name>OSPEED0</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>OSPEED1</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[3:2]</bitRange>
            </field>
            <field>
              <name>OSPEED2</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[5:4]</bitRange>
            </field>
            <field>
              <name>OSPEED3</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[7:6]</bitRange>
            </field>
            <field>
              <name>OSPEED4</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>OSPEED5</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[11:10]</bitRange>
            </field>
            <field>
              <name>OSPEED6</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[13:12]</bitRange>
            </field>
            <field>
              <name>OSPEED7</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[15:14]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PUPDR</name>
          <displayName>PUPDR</displayName>
          <description>GPIO port pull-up/pull-down register</description>
          <addressOffset>0xC</addressOffset>
          <resetValue>0x24000000</resetValue>
          <fields>
            <field>
              <name>PUPD0</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>PUPD1</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[3:2]</bitRange>
            </field>
            <field>
              <name>PUPD2</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[5:4]</bitRange>
            </field>
            <field>
              <name>PUPD3</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[7:6]</bitRange>
            </field>
            <field>
              <name>PUPD4</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>PUPD5</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[11:10]</bitRange>
            </field>
            <field>
              <name>PUPD6</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[13:12]</bitRange>
            </field>
            <field>
              <name>PUPD7</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[15:14]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>IDR</name>
          <displayName>IDR</displayName>
          <description>GPIO port input data register</description>
          <addressOffset>0x10</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>ID0</name>
              <description>Port input data (y = 0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>ID1</name>
              <description>Port input data (y = 0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>ID2</name>
              <description>Port input data (y = 0..15)</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>ID3</name>
              <description>Port input data (y = 0..15)</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>ID4</name>
              <description>Port input data (y = 0..15)</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>ID5</name>
              <description>Port input data (y = 0..15)</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>ID6</name>
              <description>Port input data (y = 0..15)</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>ID7</name>
              <description>Port input data (y = 0..15)</description>
              <bitRange>[7:7]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>ODR</name>
          <displayName>ODR</displayName>
          <description>GPIO port output data register</description>
          <addressOffset>0x14</addressOffset>
          <fields>
            <field>
              <name>OD0</name>
              <description>Port output data (y = 0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>OD1</name>
              <description>Port output data (y = 0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>OD2</name>
              <description>Port output data (y = 0..15)</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>OD3</name>
              <description>Port output data (y = 0..15)</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>OD4</name>
              <description>Port output data (y = 0..15)</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>OD5</name>
              <description>Port output data (y = 0..15)</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>OD6</name>
              <description>Port output data (y = 0..15)</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>OD7</name>
              <description>Port output data (y = 0..15)</description>
              <bitRange>[7:7]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>BSRR</name>
          <displayName>BSRR</displayName>
          <description>GPIO port bit set/reset register</description>
          <addressOffset>0x18</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>BS0</name>
              <description>Port x set bit y (y= 0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>BS1</name>
              <description>Port x set bit y (y= 0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>BS2</name>
              <description>Port x set bit y (y= 0..15)</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>BS3</name>
              <description>Port x set bit y (y= 0..15)</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>BS4</name>
              <description>Port x set bit y (y= 0..15)</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>BS5</name>
              <description>Port x set bit y (y= 0..15)</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>BS6</name>
              <description>Port x set bit y (y= 0..15)</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>BS7</name>
              <description>Port x set bit y (y= 0..15)</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>BR0</name>
              <description>Port x set bit y (y= 0..15)</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>BR1</name>
              <description>Port x reset bit y (y = 0..15)</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>BR2</name>
              <description>Port x reset bit y (y = 0..15)</description>
              <bitRange>[18:18]</bitRange>
            </field>
            <field>
              <name>BR3</name>
              <description>Port x reset bit y (y = 0..15)</description>
              <bitRange>[19:19]</bitRange>
            </field>
            <field>
              <name>BR4</name>
              <description>Port x reset bit y (y = 0..15)</description>
              <bitRange>[20:20]</bitRange>
            </field>
            <field>
              <name>BR5</name>
              <description>Port x reset bit y (y = 0..15)</description>
              <bitRange>[21:21]</bitRange>
            </field>
            <field>
              <name>BR6</name>
              <description>Port x reset bit y (y = 0..15)</description>
              <bitRange>[22:22]</bitRange>
            </field>
            <field>
              <name>BR7</name>
              <description>Port x reset bit y (y = 0..15)</description>
              <bitRange>[23:23]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>LCKR</name>
          <displayName>LCKR</displayName>
          <description>GPIO port configuration lock register</description>
          <addressOffset>0x1C</addressOffset>
          <fields>
            <field>
              <name>LCK0</name>
              <description>Port x lock bit y (y= 0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>LCK1</name>
              <description>Port x lock bit y (y= 0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>LCK2</name>
              <description>Port x lock bit y (y= 0..15)</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>LCK3</name>
              <description>Port x lock bit y (y= 0..15)</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>LCK4</name>
              <description>Port x lock bit y (y= 0..15)</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>LCK5</name>
              <description>Port x lock bit y (y= 0..15)</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>LCK6</name>
              <description>Port x lock bit y (y= 0..15)</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>LCK7</name>
              <description>Port x lock bit y (y= 0..15)</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>LCKK</name>
              <description>Port x lock bit y (y= 0..15)</description>
              <bitRange>[16:16]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>AFRL</name>
          <displayName>AFRL</displayName>
          <description>GPIO alternate function low register</description>
          <addressOffset>0x20</addressOffset>
          <fields>
            <field>
              <name>AFSEL0</name>
              <description>Alternate function selection for port x bit y (y = 0..7)</description>
              <bitRange>[3:0]</bitRange>
            </field>
            <field>
              <name>AFSEL1</name>
              <description>Alternate function selection for port x bit y (y = 0..7)</description>
              <bitRange>[7:4]</bitRange>
            </field>
            <field>
              <name>AFSEL2</name>
              <description>Alternate function selection for port x bit y (y = 0..7)</description>
              <bitRange>[11:8]</bitRange>
            </field>
            <field>
              <name>AFSEL3</name>
              <description>Alternate function selection for port x bit y (y = 0..7)</description>
              <bitRange>[15:12]</bitRange>
            </field>
            <field>
              <name>AFSEL4</name>
              <description>Alternate function selection for port x bit y (y = 0..7)</description>
              <bitRange>[19:16]</bitRange>
            </field>
            <field>
              <name>AFSEL5</name>
              <description>Alternate function selection for port x bit y (y = 0..7)</description>
              <bitRange>[23:20]</bitRange>
            </field>
            <field>
              <name>AFSEL6</name>
              <description>Alternate function selection for port x bit y (y = 0..7)</description>
              <bitRange>[27:24]</bitRange>
            </field>
            <field>
              <name>AFSEL7</name>
              <description>Alternate function selection for port x bit y (y = 0..7)</description>
              <bitRange>[31:28]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>BRR</name>
          <displayName>BRR</displayName>
          <description>port bit reset register</description>
          <addressOffset>0x28</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>BR0</name>
              <description>Port Reset bit</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>BR1</name>
              <description>Port Reset bit</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>BR2</name>
              <description>Port Reset bit</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>BR3</name>
              <description>Port Reset bit</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>BR4</name>
              <description>Port Reset bit</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>BR5</name>
              <description>Port Reset bit</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>BR6</name>
              <description>Port Reset bit</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>BR7</name>
              <description>Port Reset bit</description>
              <bitRange>[7:7]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral derivedFrom="GPIOA">
      <name>GPIOB</name>
      <baseAddress>0x50000400</baseAddress>
    </peripheral>
    <peripheral>
      <name>GPIOC</name>
      <description>General-purpose I/Os</description>
      <groupName>GPIO</groupName>
      <baseAddress>0x50000800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>MODER</name>
          <displayName>MODER</displayName>
          <description>GPIO port mode register</description>
          <addressOffset>0x0</addressOffset>
          <resetValue>0xEBFFFFFF</resetValue>
          <fields>
            <field>
              <name>MODE0</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>MODE1</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[3:2]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>OTYPER</name>
          <displayName>OTYPER</displayName>
          <description>GPIO port output type register</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>OT0</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>OT1</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>OSPEEDR</name>
          <displayName>OSPEEDR</displayName>
          <description>GPIO port output speed register</description>
          <addressOffset>0x8</addressOffset>
          <resetValue>0xC000000</resetValue>
          <fields>
            <field>
              <name>OSPEED0</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>OSPEED1</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[3:2]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PUPDR</name>
          <displayName>PUPDR</displayName>
          <description>GPIO port pull-up/pull-down register</description>
          <addressOffset>0xC</addressOffset>
          <resetValue>0x24000000</resetValue>
          <fields>
            <field>
              <name>PUPD0</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>PUPD1</name>
              <description>Port x configuration bits (y = 0..15)</description>
              <bitRange>[3:2]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>IDR</name>
          <displayName>IDR</displayName>
          <description>GPIO port input data register</description>
          <addressOffset>0x10</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>ID0</name>
              <description>Port input data (y = 0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>ID1</name>
              <description>Port input data (y = 0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>ODR</name>
          <displayName>ODR</displayName>
          <description>GPIO port output data register</description>
          <addressOffset>0x14</addressOffset>
          <fields>
            <field>
              <name>OD0</name>
              <description>Port output data (y = 0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>OD1</name>
              <description>Port output data (y = 0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>BSRR</name>
          <displayName>BSRR</displayName>
          <description>GPIO port bit set/reset register</description>
          <addressOffset>0x18</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>BS0</name>
              <description>Port x set bit y (y= 0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>BS1</name>
              <description>Port x set bit y (y= 0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>BR0</name>
              <description>Port x set bit y (y= 0..15)</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>BR1</name>
              <description>Port x reset bit y (y = 0..15)</description>
              <bitRange>[17:17]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>LCKR</name>
          <displayName>LCKR</displayName>
          <description>GPIO port configuration lock register</description>
          <addressOffset>0x1C</addressOffset>
          <fields>
            <field>
              <name>LCK0</name>
              <description>Port x lock bit y (y= 0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>LCK1</name>
              <description>Port x lock bit y (y= 0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>LCKK</name>
              <description>Port x lock bit y (y= 0..15)</description>
              <bitRange>[16:16]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>AFRL</name>
          <displayName>AFRL</displayName>
          <description>GPIO alternate function low register</description>
          <addressOffset>0x20</addressOffset>
          <fields>
            <field>
              <name>AFSEL0</name>
              <description>Alternate function selection for port x bit y (y = 0..7)</description>
              <bitRange>[3:0]</bitRange>
            </field>
            <field>
              <name>AFSEL1</name>
              <description>Alternate function selection for port x bit y (y = 0..7)</description>
              <bitRange>[7:4]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>BRR</name>
          <displayName>BRR</displayName>
          <description>port bit reset register</description>
          <addressOffset>0x28</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>BR0</name>
              <description>Port Reset bit</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>BR1</name>
              <description>Port Reset bit</description>
              <bitRange>[1:1]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>I2C</name>
      <description>Inter integrated circuit</description>
      <groupName>I2C</groupName>
      <baseAddress>0x40005400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>I2C1</name>
        <description>I2C1 global Interrupt</description>
        <value>23</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>Control register 1</description>
          <addressOffset>0x0</addressOffset>
          <fields>
            <field>
              <name>PE</name>
              <description>Peripheral enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>ENGC</name>
              <description>General call enable</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>NOSTRETCH</name>
              <description>Clock stretching disable (Slavemode)</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>START</name>
              <description>Start generation</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>STOP</name>
              <description>Stop generation</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>ACK</name>
              <description>Acknowledge enable</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>POS</name>
              <description>Acknowledge/PEC Position (for datareception)</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>SWRST</name>
              <description>Software reset</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>Control register 2</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>FREQ</name>
              <description>Peripheral clock frequency</description>
              <bitRange>[5:0]</bitRange>
            </field>
            <field>
              <name>ITERREN</name>
              <description>Error interrupt enable</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>ITEVTEN</name>
              <description>Event interrupt enable</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>ITBUFEN</name>
              <description>Buffer interrupt enable</description>
              <bitRange>[10:10]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>OAR1</name>
          <displayName>OAR1</displayName>
          <description>Own address register 1</description>
          <addressOffset>0x8</addressOffset>
          <fields>
            <field>
              <name>ADD</name>
              <description>Interface address</description>
              <bitRange>[7:1]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>Data register</description>
          <addressOffset>0x10</addressOffset>
          <fields>
            <field>
              <name>DR</name>
              <description>8-bit data register</description>
              <bitRange>[7:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SR1</name>
          <displayName>SR1</displayName>
          <description>Status register 1</description>
          <addressOffset>0x14</addressOffset>
          <fields>
            <field>
              <name>SB</name>
              <description>Start bit (Master mode)</description>
              <bitRange>[0:0]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>ADDR</name>
              <description>Address sent (master mode)/matched(slave mode)</description>
              <bitRange>[1:1]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>BTF</name>
              <description>Byte transfer finished</description>
              <bitRange>[2:2]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>STOPF</name>
              <description>Stop detection (slavemode)</description>
              <bitRange>[4:4]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>RxNE</name>
              <description>Data register not empty(receivers)</description>
              <bitRange>[6:6]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>TxE</name>
              <description>Data register empty(transmitters)</description>
              <bitRange>[7:7]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>BERR</name>
              <description>Bus error</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>ARLO</name>
              <description>Arbitration lost (mastermode)</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>AF</name>
              <description>Acknowledge failure</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>OVR</name>
              <description>Overrun/Underrun</description>
              <bitRange>[11:11]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SR2</name>
          <displayName>SR2</displayName>
          <description>Status register 2</description>
          <addressOffset>0x18</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>MSL</name>
              <description>Master/slave</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>BUSY</name>
              <description>Bus busy</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>TRA</name>
              <description>Transmitter/receiver</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>GENCALL</name>
              <description>General call address (Slavemode)</description>
              <bitRange>[4:4]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR</name>
          <displayName>CCR</displayName>
          <description>Clock control register</description>
          <addressOffset>0x1C</addressOffset>
          <fields>
            <field>
              <name>CCR</name>
              <description>Clock control register in Fast/Standardmode (Master mode)</description>
              <bitRange>[11:0]</bitRange>
            </field>
            <field>
              <name>DUTY</name>
              <description>Fast mode duty cycle</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>F_S</name>
              <description>I2C master mode selection</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>TRISE</name>
          <displayName>TRISE</displayName>
          <description>TRISE register</description>
          <addressOffset>0x20</addressOffset>
          <resetValue>0x2</resetValue>
          <fields>
            <field>
              <name>TRISE</name>
              <description>Maximum rise time in Fast/Standard mode(Master mode)</description>
              <bitRange>[5:0]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>IWDG</name>
      <description>Independent watchdog</description>
      <groupName>IWDG</groupName>
      <baseAddress>0x40003000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>KR</name>
          <displayName>KR</displayName>
          <description>Key register (IWDG_KR)</description>
          <addressOffset>0x0</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>KEY</name>
              <description>Key value</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PR</name>
          <displayName>PR</displayName>
          <description>Prescaler register (IWDG_PR)</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>PR</name>
              <description>Prescaler divider</description>
              <bitRange>[2:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>RLR</name>
          <displayName>RLR</displayName>
          <description>Reload register (IWDG_RLR)</description>
          <addressOffset>0x8</addressOffset>
          <resetValue>0xFFF</resetValue>
          <fields>
            <field>
              <name>RL</name>
              <description>Watchdog counter reload value</description>
              <bitRange>[11:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>Status register (IWDG_SR)</description>
          <addressOffset>0xC</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>PVU</name>
              <description>Watchdog prescaler value update</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>RVU</name>
              <description>Watchdog counter reload value update</description>
              <bitRange>[1:1]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>LPTIM1</name>
      <description>Low power timer</description>
      <groupName>LPTIM1</groupName>
      <baseAddress>0x40007C00</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>LPTIM1_DAC</name>
        <description>LPTIM1, DAC global Interrupts</description>
        <value>17</value>
      </interrupt>
      <registers>
        <register>
          <name>ISR</name>
          <displayName>ISR</displayName>
          <description>Interrupt and Status Register</description>
          <addressOffset>0x0</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>ARRM</name>
              <description>Autoreload match</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>ARROK</name>
              <description>Autoreload match update OK</description>
              <bitRange>[4:4]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>ICR</name>
          <displayName>ICR</displayName>
          <description>Interrupt Clear Register</description>
          <addressOffset>0x4</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>ARRMCF</name>
              <description>Autoreload match Clear Flag</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>ARROKCF</name>
              <description>Autoreload match update OK Clear Flag</description>
              <bitRange>[4:4]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>IER</name>
          <displayName>IER</displayName>
          <description>Interrupt Enable Register</description>
          <addressOffset>0x8</addressOffset>
          <fields>
            <field>
              <name>ARRMIE</name>
              <description>Autoreload matchInterrupt Enable</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>ARROKIE</name>
              <description>Autoreload match update OK Interrupt Enable</description>
              <bitRange>[4:4]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR</name>
          <displayName>CFGR</displayName>
          <description>Configuration Register</description>
          <addressOffset>0xC</addressOffset>
          <fields>
            <field>
              <name>PRESC</name>
              <description>Clock prescaler</description>
              <bitRange>[11:9]</bitRange>
            </field>
            <field>
              <name>PRELOAD</name>
              <description>Registers update mode</description>
              <bitRange>[22:22]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Control Register</description>
          <addressOffset>0x10</addressOffset>
          <fields>
            <field>
              <name>ENABLE</name>
              <description>LPTIM Enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>SNGSTRT</name>
              <description>LPTIM start in single mode</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>CNTSTRT</name>
              <description>CNTSTRT</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>COUNTRST</name>
              <description>Reset counter</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>RSTARE</name>
              <description>Reset after read enable</description>
              <bitRange>[4:4]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <displayName>ARR</displayName>
          <description>Autoreload Register</description>
          <addressOffset>0x18</addressOffset>
          <resetValue>0x1</resetValue>
          <fields>
            <field>
              <name>ARR</name>
              <description>Auto reload value</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <displayName>CNT</displayName>
          <description>Counter Register</description>
          <addressOffset>0x1C</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>CNT</name>
              <description>Counter value</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>PWR</name>
      <description>Power control</description>
      <groupName>PWR</groupName>
      <baseAddress>0x40007000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>Power control register 1</description>
          <addressOffset>0x0</addressOffset>
          <resetValue>0x30000</resetValue>
          <fields>
            <field>
              <name>BIAS_CR</name>
              <description>MR Bias current</description>
              <bitRange>[3:0]</bitRange>
            </field>
            <field>
              <name>BIAS_CR_SEL</name>
              <description>MR Bias current selection</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>FLS_SLPTIME</name>
              <description>Flash wait time after wakeup from the stop mode</description>
              <bitRange>[13:12]</bitRange>
            </field>
            <field>
              <name>LPR</name>
              <description>Low-power run</description>
              <bitRange>[15:14]</bitRange>
            </field>
            <field>
              <name>SRAM_RETV</name>
              <description>SRAM retention voltage control</description>
              <bitRange>[18:16]</bitRange>
            </field>
            <field>
              <name>HSION_CTRL</name>
              <description>HSI open time control</description>
              <bitRange>[19:19]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>RCC</name>
      <description>Reset and clock control</description>
      <groupName>RCC</groupName>
      <baseAddress>0x40021000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>RCC</name>
        <description>RCC global Interrupt</description>
        <value>4</value>
      </interrupt>
      <registers>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Clock control register</description>
          <addressOffset>0x0</addressOffset>
          <resetValue>0x100</resetValue>
          <fields>
            <field>
              <name>HSION</name>
              <description>HSI16 clock enable</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>HSIRDY</name>
              <description>HSI16 clock ready flag</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>HSIDIV</name>
              <description>HSI16 clock division factor</description>
              <bitRange>[13:11]</bitRange>
            </field>
            <field>
              <name>HSEEN</name>
              <bitRange>[18:18]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>ICSCR</name>
          <displayName>ICSCR</displayName>
          <description>Internal clock sources calibration register</description>
          <addressOffset>0x4</addressOffset>
          <resetValue>0x10000000</resetValue>
          <fields>
            <field>
              <name>HSI_TRIM</name>
              <description>HSI clock trimming</description>
              <bitRange>[12:0]</bitRange>
            </field>
            <field>
              <name>HSI_FS</name>
              <description>HSI frequency selection</description>
              <bitRange>[15:13]</bitRange>
            </field>
            <field>
              <name>LSI_TRIM</name>
              <description>LSI clock trimming</description>
              <bitRange>[24:16]</bitRange>
            </field>
            <field>
              <name>LSI_STARTUP</name>
              <description>LSI startup time</description>
              <bitRange>[27:26]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR</name>
          <displayName>CFGR</displayName>
          <description>Clock configuration register</description>
          <addressOffset>0x8</addressOffset>
          <fields>
            <field>
              <name>SW</name>
              <description>System clock switch</description>
              <bitRange>[2:0]</bitRange>
            </field>
            <field>
              <name>SWS</name>
              <description>System clock switch status</description>
              <bitRange>[5:3]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>HPRE</name>
              <description>AHB prescaler</description>
              <bitRange>[11:8]</bitRange>
            </field>
            <field>
              <name>PPRE</name>
              <description>APB prescaler</description>
              <bitRange>[14:12]</bitRange>
            </field>
            <field>
              <name>MCOSEL</name>
              <description>Microcontroller clock output</description>
              <bitRange>[26:24]</bitRange>
            </field>
            <field>
              <name>MCOPRE</name>
              <description>Microcontroller clock output prescaler</description>
              <bitRange>[30:28]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>ECSCR</name>
          <displayName>ECSCR</displayName>
          <description>External clock source control register</description>
          <addressOffset>0x10</addressOffset>
          <fields>
            <field>
              <name>LSE_DRIVER</name>
              <description>desc LSE_DRIVER</description>
              <bitRange>[17:16]</bitRange>
            </field>
            <field>
              <name>LSE_STARTUP</name>
              <description>desc LSE_STARTUP</description>
              <bitRange>[21:20]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CIER</name>
          <displayName>CIER</displayName>
          <description>Clock interrupt enable register</description>
          <addressOffset>0x18</addressOffset>
          <fields>
            <field>
              <name>LSIRDYIE</name>
              <description>LSI ready interrupt enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>LSERDYIE</name>
              <description>LSE ready interrupt enable</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>HSIRDYIE</name>
              <description>HSI ready interrupt enable</description>
              <bitRange>[3:3]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CIFR</name>
          <displayName>CIFR</displayName>
          <description>Clock interrupt flag register</description>
          <addressOffset>0x1C</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>LSIRDYF</name>
              <description>LSI ready interrupt flag</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>LSERDYF</name>
              <description>LSE ready interrupt flag</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>HSIRDYF</name>
              <description>HSI ready interrupt flag</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>LSECSSF</name>
              <description>LSE clock secure system interrupt flag</description>
              <bitRange>[9:9]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CICR</name>
          <displayName>CICR</displayName>
          <description>Clock interrupt clear register</description>
          <addressOffset>0x20</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>LSIRDYC</name>
              <description>LSI ready interrupt clear</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>LSERDYC</name>
              <description>LSE ready interrupt clear</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>HSIRDYC</name>
              <description>HSI ready interrupt clear</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>LSECSSC</name>
              <description>LSE clock secure system interrupt flag clear</description>
              <bitRange>[9:9]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>IOPRSTR</name>
          <displayName>IOPRSTR</displayName>
          <description>GPIO reset register</description>
          <addressOffset>0x24</addressOffset>
          <fields>
            <field>
              <name>GPIOARST</name>
              <description>I/O port A reset</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>GPIOBRST</name>
              <description>I/O port B reset</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>GPIOCRST</name>
              <description>I/O port C reset</description>
              <bitRange>[2:2]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>AHBRSTR</name>
          <displayName>AHBRSTR</displayName>
          <description>AHB peripheral reset register</description>
          <addressOffset>0x28</addressOffset>
          <fields>
            <field>
              <name>FLASHRST</name>
              <description>FLASH reset</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>CRCRST</name>
              <description>CRC reset</description>
              <bitRange>[12:12]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>APBRSTR1</name>
          <displayName>APBRSTR1</displayName>
          <description>APB peripheral reset register 1</description>
          <addressOffset>0x2C</addressOffset>
          <fields>
            <field>
              <name>I2CRST</name>
              <description>I2C reset</description>
              <bitRange>[21:21]</bitRange>
            </field>
            <field>
              <name>DBGRST</name>
              <description>Debug support reset</description>
              <bitRange>[27:27]</bitRange>
            </field>
            <field>
              <name>PWRRST</name>
              <description>Power interface reset</description>
              <bitRange>[28:28]</bitRange>
            </field>
            <field>
              <name>LPTIMRST</name>
              <description>Low Power Timer reset</description>
              <bitRange>[31:31]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>APBRSTR2</name>
          <displayName>APBRSTR2</displayName>
          <description>APB peripheral reset register 2</description>
          <addressOffset>0x30</addressOffset>
          <fields>
            <field>
              <name>SYSCFGRST</name>
              <description>SYSCFG reset</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>TIM1RST</name>
              <description>TIM1 timer reset</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>SPI1RST</name>
              <description>SPI1 reset</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>USART1RST</name>
              <description>USART1 reset</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>TIM14RST</name>
              <description>TIM14 reset</description>
              <bitRange>[15:15]</bitRange>
            </field>
            <field>
              <name>ADCRST</name>
              <description>ADC reset</description>
              <bitRange>[20:20]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>IOPENR</name>
          <displayName>IOPENR</displayName>
          <description>GPIO clock enable register</description>
          <addressOffset>0x34</addressOffset>
          <fields>
            <field>
              <name>GPIOAEN</name>
              <description>I/O port A clock enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>GPIOBEN</name>
              <description>I/O port B clock enable</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>GPIOCEN</name>
              <description>I/O port C clock enable</description>
              <bitRange>[2:2]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>AHBENR</name>
          <displayName>AHBENR</displayName>
          <description>AHB peripheral clock enable register</description>
          <addressOffset>0x38</addressOffset>
          <fields>
            <field>
              <name>FLASHEN</name>
              <description>Flash memory interface clock enable</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>SRAMEN</name>
              <description>SRAM memory interface clock enable</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>CRCEN</name>
              <description>CRC clock enable</description>
              <bitRange>[12:12]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>APBENR1</name>
          <displayName>APBENR1</displayName>
          <description>APB peripheral clock enable register 1</description>
          <addressOffset>0x3C</addressOffset>
          <fields>
            <field>
              <name>I2CEN</name>
              <description>I2C clock enable</description>
              <bitRange>[21:21]</bitRange>
            </field>
            <field>
              <name>DBGEN</name>
              <description>Debug support clock enable</description>
              <bitRange>[27:27]</bitRange>
            </field>
            <field>
              <name>PWREN</name>
              <description>Power interface clock enable</description>
              <bitRange>[28:28]</bitRange>
            </field>
            <field>
              <name>LPTIMEN</name>
              <description>LPTIM clock enable</description>
              <bitRange>[31:31]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>APBENR2</name>
          <displayName>APBENR2</displayName>
          <description>APB peripheral clock enable register 2</description>
          <addressOffset>0x40</addressOffset>
          <fields>
            <field>
              <name>SYSCFGEN</name>
              <description>SYSCFG and VREFBUF clock enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>TIM1EN</name>
              <description>TIM1 timer clock enable</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>SPI1EN</name>
              <description>SPI1 clock enable</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>USART1EN</name>
              <description>USART1 clock enable</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>TIM14EN</name>
              <description>TIM14 clock enable</description>
              <bitRange>[15:15]</bitRange>
            </field>
            <field>
              <name>ADCEN</name>
              <description>ADC clock enable</description>
              <bitRange>[20:20]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCIPR</name>
          <displayName>CCIPR</displayName>
          <description>Peripherals independent clock configuration register</description>
          <addressOffset>0x54</addressOffset>
          <fields>
            <field>
              <name>LPTIM1SEL</name>
              <description>LPTIM1 clock source selection</description>
              <bitRange>[19:18]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>BDCR</name>
          <displayName>BDCR</displayName>
          <description>RTC domain control register</description>
          <addressOffset>0x5C</addressOffset>
          <fields>
            <field>
              <name>LSEON</name>
              <description>LSE oscillator enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>LSERDY</name>
              <description>LSE oscillator ready</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>LSEBYP</name>
              <description>LSE oscillator bypass</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>LSECSSON</name>
              <description>LSE CSS enable</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>LSECSSD</name>
              <description>LSE CSS detect</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>LSCOEN</name>
              <description>Low-speed clock output (LSCO) enable</description>
              <bitRange>[24:24]</bitRange>
            </field>
            <field>
              <name>LSCOSEL</name>
              <description>Low-speed clock output selection</description>
              <bitRange>[25:25]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CSR</name>
          <displayName>CSR</displayName>
          <description>Control/status register</description>
          <addressOffset>0x60</addressOffset>
          <fields>
            <field>
              <name>LSION</name>
              <description>LSI oscillator enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>LSIRDY</name>
              <description>LSI oscillator ready</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>PINRST_FLTDIS</name>
              <description>desc PINRST_FLTDIS</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>RMVF</name>
              <description>Remove reset flags</description>
              <bitRange>[23:23]</bitRange>
            </field>
            <field>
              <name>OBLRSTF</name>
              <description>Option byte loader reset flag</description>
              <bitRange>[25:25]</bitRange>
            </field>
            <field>
              <name>PINRSTF</name>
              <description>Pin reset flag</description>
              <bitRange>[26:26]</bitRange>
            </field>
            <field>
              <name>PWRRSTF</name>
              <description>BOR or POR/PDR flag</description>
              <bitRange>[27:27]</bitRange>
            </field>
            <field>
              <name>SFTRSTF</name>
              <description>Software reset flag</description>
              <bitRange>[28:28]</bitRange>
            </field>
            <field>
              <name>IWDGRSTF</name>
              <description>Independent window watchdog reset flag</description>
              <bitRange>[29:29]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>SPI1</name>
      <description>Serial peripheral interface</description>
      <groupName>SPI</groupName>
      <baseAddress>0x40013000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>SPI1</name>
        <description>SPI1 global Interrupt</description>
        <value>25</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <description>desc CR1</description>
          <addressOffset>0x0</addressOffset>
          <fields>
            <field>
              <name>CPHA</name>
              <description>desc CPHA</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>CPOL</name>
              <description>desc CPOL</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>MSTR</name>
              <description>desc MSTR</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>BR</name>
              <description>desc BR</description>
              <bitRange>[5:3]</bitRange>
            </field>
            <field>
              <name>SPE</name>
              <description>desc SPE</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>LSBFIRST</name>
              <description>desc LSBFIRST</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>SSI</name>
              <description>desc SSI</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>SSM</name>
              <description>desc SSM</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>RXONLY</name>
              <description>desc RXONLY</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>DDF</name>
              <description>desc DDF</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>BIDIOE</name>
              <description>desc BIDIOE</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>BIDIMODE</name>
              <description>desc BIDIMODE</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <description>desc CR2</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>SSOE</name>
              <description>desc SSOE</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>ERRIE</name>
              <description>desc ERRIE</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>RXNEIE</name>
              <description>desc RXNEIE</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>TXEIE</name>
              <description>desc TXEIE</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>DS</name>
              <description>desc DS</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>SLVFM</name>
              <description>desc SLVFM</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <description>desc SR</description>
          <addressOffset>0x8</addressOffset>
          <resetValue>0x2</resetValue>
          <fields>
            <field>
              <name>RXNE</name>
              <description>desc RXNE</description>
              <bitRange>[0:0]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>TXE</name>
              <description>desc TXE</description>
              <bitRange>[1:1]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>MODF</name>
              <description>desc MODF</description>
              <bitRange>[5:5]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>OVR</name>
              <description>desc OVR</description>
              <bitRange>[6:6]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>BSY</name>
              <description>desc BSY</description>
              <bitRange>[7:7]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>FRLVL</name>
              <description>desc FRLVL</description>
              <bitRange>[10:9]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>FTLVL</name>
              <description>desc FTLVL</description>
              <bitRange>[12:11]</bitRange>
              <access>read-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <description>desc DR</description>
          <addressOffset>0xC</addressOffset>
          <fields>
            <field>
              <name>DR</name>
              <description>desc DR</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>SYSCFG</name>
      <description>System configuration controller</description>
      <groupName>SYSCFG</groupName>
      <baseAddress>0x40010000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x30</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CFGR1</name>
          <displayName>CFGR1</displayName>
          <description>SYSCFG configuration register 1</description>
          <addressOffset>0x0</addressOffset>
          <fields>
            <field>
              <name>MEM_MODE</name>
              <description>Memory mapping selection bits</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>I2C_PA2_FMP</name>
              <description>desc I2C_PA2_FMP</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>I2C_PB3_FMP</name>
              <description>desc I2C_PB3_FMP</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>I2C_PB4_FMP</name>
              <description>desc I2C_PB4_FMP</description>
              <bitRange>[18:18]</bitRange>
            </field>
            <field>
              <name>I2C_PB6_FMP</name>
              <description>desc I2C_PB6_FMP</description>
              <bitRange>[19:19]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR2</name>
          <displayName>CFGR2</displayName>
          <description>SYSCFG configuration register 2</description>
          <addressOffset>0x18</addressOffset>
          <fields>
            <field>
              <name>LOCKUP_LOCK</name>
              <description>Cortex-M0+ LOCKUP bit enable bit</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>ETR_SRC_TIM1</name>
              <description>TIM1 ETR source selection</description>
              <bitRange>[10:9]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>GPIO_ENS</name>
          <description>desc GPIO_ENS</description>
          <addressOffset>0x1C</addressOffset>
          <fields>
            <field>
              <name>PA_ENS</name>
              <description>desc PA_ENS</description>
              <bitRange>[7:0]</bitRange>
            </field>
            <field>
              <name>PB_ENS</name>
              <description>desc PB_ENS</description>
              <bitRange>[15:8]</bitRange>
            </field>
            <field>
              <name>PC_ENS</name>
              <description>desc PC_ENS</description>
              <bitRange>[17:16]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>TIM1</name>
      <description>Advanced timer</description>
      <groupName>TIM</groupName>
      <baseAddress>0x40012C00</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>TIM1_BRK_UP_TRG_COM</name>
        <description>TIM1 Break, Update, Trigger and Commutation Interrupt</description>
        <value>13</value>
      </interrupt>
      <interrupt>
        <name>TIM1_CC</name>
        <description>TIM1 Capture Compare Interrupt</description>
        <value>14</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <description>desc CR1</description>
          <addressOffset>0x0</addressOffset>
          <resetMask>0x3FF</resetMask>
          <fields>
            <field>
              <name>CEN</name>
              <description>desc CEN</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>UDIS</name>
              <description>desc UDIS</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>URS</name>
              <description>desc URS</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>OPM</name>
              <description>desc OPM</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>DIR</name>
              <description>desc DIR</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>CMS</name>
              <description>desc CMS</description>
              <bitRange>[6:5]</bitRange>
            </field>
            <field>
              <name>ARPE</name>
              <description>desc ARPE</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>CKD</name>
              <description>desc CKD</description>
              <bitRange>[9:8]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <description>desc CR2</description>
          <addressOffset>0x4</addressOffset>
          <resetMask>0xF8</resetMask>
          <fields>
            <field>
              <name>CCPC</name>
              <description>desc CCPC</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>CCUS</name>
              <description>desc CCUS</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>MMS</name>
              <description>desc MMS</description>
              <bitRange>[6:4]</bitRange>
            </field>
            <field>
              <name>TI1S</name>
              <description>desc TI1S</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>OIS1</name>
              <description>desc OIS1</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>OIS1N</name>
              <description>desc OIS1N</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>OIS2</name>
              <description>desc OIS2</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>OIS2N</name>
              <description>desc OIS2N</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>OIS3</name>
              <description>desc OIS3</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>OIS3N</name>
              <description>desc OIS3N</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>OIS4</name>
              <description>desc OIS4</description>
              <bitRange>[14:14]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SMCR</name>
          <description>desc SMCR</description>
          <addressOffset>0x8</addressOffset>
          <resetMask>0xFFF7</resetMask>
          <fields>
            <field>
              <name>SMS</name>
              <description>desc SMS</description>
              <bitRange>[2:0]</bitRange>
            </field>
            <field>
              <name>OCCS</name>
              <description>desc OCCS</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>TS</name>
              <description>desc TS</description>
              <bitRange>[6:4]</bitRange>
            </field>
            <field>
              <name>MSM</name>
              <description>desc MSM</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>ETF</name>
              <description>desc ETF</description>
              <bitRange>[11:8]</bitRange>
            </field>
            <field>
              <name>ETPS</name>
              <description>desc ETPS</description>
              <bitRange>[13:12]</bitRange>
            </field>
            <field>
              <name>ECE</name>
              <description>desc ECE</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>ETP</name>
              <description>desc ETP</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>DIER</name>
          <description>desc DIER</description>
          <addressOffset>0xC</addressOffset>
          <resetMask>0x5F5F</resetMask>
          <fields>
            <field>
              <name>UIE</name>
              <description>desc UIE</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>CC1IE</name>
              <description>desc CC1IE</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>CC2IE</name>
              <description>desc CC2IE</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>CC3IE</name>
              <description>desc CC3IE</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>CC4IE</name>
              <description>desc CC4IE</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>COMIE</name>
              <description>desc COMIE</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>TIE</name>
              <description>desc TIE</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>BIE</name>
              <description>desc BIE</description>
              <bitRange>[7:7]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <description>desc SR</description>
          <addressOffset>0x10</addressOffset>
          <resetMask>0x1E5F</resetMask>
          <fields>
            <field>
              <name>UIF</name>
              <description>desc UIF</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>CC1IF</name>
              <description>desc CC1IF</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>CC2IF</name>
              <description>desc CC2IF</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>CC3IF</name>
              <description>desc CC3IF</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>CC4IF</name>
              <description>desc CC4IF</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>COMIF</name>
              <description>desc COMIF</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>TIF</name>
              <description>desc TIF</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>BIF</name>
              <description>desc BIF</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>CC1OF</name>
              <description>desc CC1OF</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>CC2OF</name>
              <description>desc CC2OF</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>CC3OF</name>
              <description>desc CC3OF</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>CC4OF</name>
              <description>desc CC4OF</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>IC1IR</name>
              <description>desc IC1IR</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>IC2IR</name>
              <description>desc IC2IR</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>IC3IR</name>
              <description>desc IC3IR</description>
              <bitRange>[18:18]</bitRange>
            </field>
            <field>
              <name>IC4IR</name>
              <description>desc IC3IR</description>
              <bitRange>[19:19]</bitRange>
            </field>
            <field>
              <name>IC1IF</name>
              <description>desc IC1IF</description>
              <bitRange>[20:20]</bitRange>
            </field>
            <field>
              <name>IC2IF</name>
              <description>desc IC2IF</description>
              <bitRange>[21:21]</bitRange>
            </field>
            <field>
              <name>IC3IF</name>
              <description>desc IC3IF</description>
              <bitRange>[22:22]</bitRange>
            </field>
            <field>
              <name>IC4IF</name>
              <description>desc IC3IF</description>
              <bitRange>[23:23]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>EGR</name>
          <description>desc EGR</description>
          <addressOffset>0x14</addressOffset>
          <access>write-only</access>
          <resetMask>0x5F</resetMask>
          <fields>
            <field>
              <name>UG</name>
              <description>desc UG</description>
              <bitRange>[0:0]</bitRange>
              <access>write-only</access>
            </field>
            <field>
              <name>CC1G</name>
              <description>Capture/Compare 1 Generation</description>
              <bitRange>[1:1]</bitRange>
              <access>write-only</access>
            </field>
            <field>
              <name>CC2G</name>
              <description>desc CC2G</description>
              <bitRange>[2:2]</bitRange>
              <access>write-only</access>
            </field>
            <field>
              <name>CC3G</name>
              <description>desc CC3G</description>
              <bitRange>[3:3]</bitRange>
              <access>write-only</access>
            </field>
            <field>
              <name>CC4G</name>
              <description>desc CC4G</description>
              <bitRange>[4:4]</bitRange>
              <access>write-only</access>
            </field>
            <field>
              <name>COMG</name>
              <description>desc COMG</description>
              <bitRange>[5:5]</bitRange>
              <access>write-only</access>
            </field>
            <field>
              <name>TG</name>
              <description>desc TG</description>
              <bitRange>[6:6]</bitRange>
              <access>write-only</access>
            </field>
            <field>
              <name>BG</name>
              <description>desc BG</description>
              <bitRange>[7:7]</bitRange>
              <access>write-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_OUTPUT</name>
          <description>desc CCMR1:OUTPUT</description>
          <addressOffset>0x18</addressOffset>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>CC1S</name>
              <description>desc CC1S</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>OC1FE</name>
              <description>desc OC1FE</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>OC1PE</name>
              <description>desc OC1PE</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>OC1M</name>
              <description>desc OC1M</description>
              <bitRange>[6:4]</bitRange>
            </field>
            <field>
              <name>OC1CE</name>
              <description>desc OC1CE</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>CC2S</name>
              <description>desc CC2S</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>OC2FE</name>
              <description>desc OC2FE</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>OC2PE</name>
              <description>desc OC2PE</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>OC2M</name>
              <description>desc OC2M</description>
              <bitRange>[14:12]</bitRange>
            </field>
            <field>
              <name>OC2CE</name>
              <description>desc OC2CE</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_INPUT</name>
          <description>desc CCMR1:INPUT</description>
          <alternateRegister>CCMR1_OUTPUT</alternateRegister>
          <addressOffset>0x18</addressOffset>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>CC1S</name>
              <description>desc CC1S</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>IC1PSC</name>
              <description>desc IC1PSC</description>
              <bitRange>[3:2]</bitRange>
            </field>
            <field>
              <name>IC1F</name>
              <description>desc IC1F</description>
              <bitRange>[7:4]</bitRange>
            </field>
            <field>
              <name>CC2S</name>
              <description>desc CC2S</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>IC2PSC</name>
              <description>desc IC2PSC</description>
              <bitRange>[11:10]</bitRange>
            </field>
            <field>
              <name>IC2F</name>
              <description>desc IC2F</description>
              <bitRange>[15:12]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR2_OUTPUT</name>
          <description>desc CCMR2:OUTPUT</description>
          <addressOffset>0x1C</addressOffset>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>CC3S</name>
              <description>desc CC3S</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>OC3FE</name>
              <description>desc OC3FE</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>OC3PE</name>
              <description>desc OC3PE</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>OC3M</name>
              <description>desc OC3M</description>
              <bitRange>[6:4]</bitRange>
            </field>
            <field>
              <name>OC3CE</name>
              <description>desc OC3CE</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>CC4S</name>
              <description>desc CC4S</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>OC4FE</name>
              <description>desc OC4FE</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>OC4PE</name>
              <description>desc OC4PE</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>OC4M</name>
              <description>desc OC4M</description>
              <bitRange>[14:12]</bitRange>
            </field>
            <field>
              <name>OC4CE</name>
              <description>desc OC4CE</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR2_INPUT</name>
          <description>desc CCMR2:INPUT</description>
          <alternateRegister>CCMR2_OUTPUT</alternateRegister>
          <addressOffset>0x1C</addressOffset>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>CC3S</name>
              <description>desc CC3S</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>IC3PSC</name>
              <description>desc IC3PSC</description>
              <bitRange>[3:2]</bitRange>
            </field>
            <field>
              <name>IC3F</name>
              <description>desc IC3F</description>
              <bitRange>[7:4]</bitRange>
            </field>
            <field>
              <name>CC4S</name>
              <description>desc CC4S</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>IC4PSC</name>
              <description>desc IC4PSC</description>
              <bitRange>[11:10]</bitRange>
            </field>
            <field>
              <name>IC4F</name>
              <description>desc IC4F</description>
              <bitRange>[15:12]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCER</name>
          <description>desc CCER</description>
          <addressOffset>0x20</addressOffset>
          <resetMask>0x3333</resetMask>
          <fields>
            <field>
              <name>CC1E</name>
              <description>desc CC1E</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>CC1P</name>
              <description>desc CC1P</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>CC1NE</name>
              <description>desc CC1NE</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>CC1NP</name>
              <description>desc CC1NP</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>CC2E</name>
              <description>desc CC2E</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>CC2P</name>
              <description>desc CC2P</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>CC2NE</name>
              <description>desc CC2NE</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>CC2NP</name>
              <description>desc CC2NP</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>CC3E</name>
              <description>desc CC3E</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>CC3P</name>
              <description>desc CC3P</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>CC3NE</name>
              <description>desc CC3NE</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>CC3NP</name>
              <description>desc CC3NP</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>CC4E</name>
              <description>desc CC4E</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>CC4P</name>
              <description>desc CC4P</description>
              <bitRange>[13:13]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <description>desc CNT</description>
          <addressOffset>0x24</addressOffset>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>CNT</name>
              <description>desc CNT</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PSC</name>
          <description>desc PSC</description>
          <addressOffset>0x28</addressOffset>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>PSC</name>
              <description>desc PSC</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <description>desc ARR</description>
          <addressOffset>0x2C</addressOffset>
          <resetValue>0xFFFF</resetValue>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>ARR</name>
              <description>desc ARR</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>RCR</name>
          <description>desc RCR</description>
          <addressOffset>0x30</addressOffset>
          <resetValue>0xFFFF</resetValue>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>REP</name>
              <description>desc REP</description>
              <bitRange>[7:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR1</name>
          <description>desc CCR1</description>
          <addressOffset>0x34</addressOffset>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>CCR1</name>
              <description>desc CCR1</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR2</name>
          <description>desc CCR2</description>
          <addressOffset>0x38</addressOffset>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>CCR2</name>
              <description>desc CCR2</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR3</name>
          <description>desc CCR3</description>
          <addressOffset>0x3C</addressOffset>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>CCR3</name>
              <description>desc CCR3</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR4</name>
          <description>desc CCR4</description>
          <addressOffset>0x40</addressOffset>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>CCR4</name>
              <description>desc CCR4</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>BDTR</name>
          <description>desc BDTR</description>
          <addressOffset>0x44</addressOffset>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>DTG</name>
              <description>desc DTG</description>
              <bitRange>[7:0]</bitRange>
            </field>
            <field>
              <name>LOCK</name>
              <description>desc LOCK</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>OSSI</name>
              <description>desc OSSI</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>OSSR</name>
              <description>desc OSSR</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>BKE</name>
              <description>desc BKE</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>BKP</name>
              <description>desc BKP</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>AOE</name>
              <description>desc AOE</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>MOE</name>
              <description>desc MOE</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>TIM14</name>
      <description>General purpose timer</description>
      <groupName>TIM</groupName>
      <baseAddress>0x40002000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>TIM14</name>
        <description>TIM14 global Interrupt</description>
        <value>19</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <description>desc CR1</description>
          <addressOffset>0x0</addressOffset>
          <resetMask>0x3FF</resetMask>
          <fields>
            <field>
              <name>CEN</name>
              <description>desc CEN</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>UDIS</name>
              <description>desc UDIS</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>URS</name>
              <description>desc URS</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>OPM</name>
              <description>desc OPM</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>ARPE</name>
              <description>desc ARPE</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>CKD</name>
              <description>desc CKD</description>
              <bitRange>[9:8]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>DIER</name>
          <description>desc DIER</description>
          <addressOffset>0xC</addressOffset>
          <resetMask>0x5F5F</resetMask>
          <fields>
            <field>
              <name>UIE</name>
              <description>desc UIE</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>CC1IE</name>
              <description>desc CC1IE</description>
              <bitRange>[1:1]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <description>desc SR</description>
          <addressOffset>0x10</addressOffset>
          <resetMask>0x1E5F</resetMask>
          <fields>
            <field>
              <name>UIF</name>
              <description>desc UIF</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>CC1IF</name>
              <description>desc CC1IF</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>CC1OF</name>
              <description>desc CC1OF</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>IC1IR</name>
              <description>desc IC1IR</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>IC1IF</name>
              <description>desc IC1IF</description>
              <bitRange>[20:20]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>EGR</name>
          <description>desc EGR</description>
          <addressOffset>0x14</addressOffset>
          <access>write-only</access>
          <resetMask>0x5F</resetMask>
          <fields>
            <field>
              <name>UG</name>
              <description>desc UG</description>
              <bitRange>[0:0]</bitRange>
              <access>write-only</access>
            </field>
            <field>
              <name>CC1G</name>
              <description>Capture/Compare 1 Generation</description>
              <bitRange>[1:1]</bitRange>
              <access>write-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_OUTPUT</name>
          <description>desc CCMR1:OUTPUT</description>
          <addressOffset>0x18</addressOffset>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>CC1S</name>
              <description>desc CC1S</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>OC1PE</name>
              <description>desc OC1PE</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>OC1M</name>
              <description>desc OC1M</description>
              <bitRange>[6:4]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_INPUT</name>
          <description>desc CCMR1:INPUT</description>
          <alternateRegister>CCMR1_OUTPUT</alternateRegister>
          <addressOffset>0x18</addressOffset>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>CC1S</name>
              <description>desc CC1S</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>IC1PSC</name>
              <description>desc IC1PSC</description>
              <bitRange>[3:2]</bitRange>
            </field>
            <field>
              <name>IC1F</name>
              <description>desc IC1F</description>
              <bitRange>[7:4]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCER</name>
          <description>desc CCER</description>
          <addressOffset>0x20</addressOffset>
          <resetMask>0x3333</resetMask>
          <fields>
            <field>
              <name>CC1E</name>
              <description>desc CC1E</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>CC1P</name>
              <description>desc CC1P</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>CC1NP</name>
              <description>desc CC1NP</description>
              <bitRange>[3:3]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <description>desc CNT</description>
          <addressOffset>0x24</addressOffset>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>CNT</name>
              <description>desc CNT</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PSC</name>
          <description>desc PSC</description>
          <addressOffset>0x28</addressOffset>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>PSC</name>
              <description>desc PSC</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <description>desc ARR</description>
          <addressOffset>0x2C</addressOffset>
          <resetValue>0xFFFF</resetValue>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>ARR</name>
              <description>desc ARR</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR1</name>
          <description>desc CCR1</description>
          <addressOffset>0x34</addressOffset>
          <resetMask>0xFFFF</resetMask>
          <fields>
            <field>
              <name>CCR1</name>
              <description>desc CCR1</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>OR</name>
          <description>desc OR</description>
          <addressOffset>0x50</addressOffset>
          <fields>
            <field>
              <name>TI1_RMP</name>
              <description>desc TI1_RMP</description>
              <bitRange>[1:0]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>USART1</name>
      <description>Universal synchronous asynchronous receiver transmitter</description>
      <groupName>USART</groupName>
      <baseAddress>0x40013800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>USART1</name>
        <description>USART1 global Interrupt</description>
        <value>27</value>
      </interrupt>
      <registers>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>Status register</description>
          <addressOffset>0x0</addressOffset>
          <resetValue>0xC0</resetValue>
          <fields>
            <field>
              <name>PE</name>
              <description>Parity error</description>
              <bitRange>[0:0]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>FE</name>
              <description>Framing error</description>
              <bitRange>[1:1]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>NE</name>
              <description>Noise error flag</description>
              <bitRange>[2:2]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>ORE</name>
              <description>Overrun error</description>
              <bitRange>[3:3]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>IDLE</name>
              <description>IDLE line detected</description>
              <bitRange>[4:4]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>RXNE</name>
              <description>Read data register not empty</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>TC</name>
              <description>Transmission complete</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>TXE</name>
              <description>Transmit data register empty</description>
              <bitRange>[7:7]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>CTS</name>
              <description>CTS flag</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>ABRF</name>
              <description>Automate baudrate detection flag</description>
              <bitRange>[10:10]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>ABRE</name>
              <description>Automate baudrate detection error flag</description>
              <bitRange>[11:11]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>ABRRQ</name>
              <description>Automate baudrate detection requeset</description>
              <bitRange>[12:12]</bitRange>
              <access>write-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>Data register</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>DR</name>
              <description>Data value</description>
              <bitRange>[8:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>BRR</name>
          <displayName>BRR</displayName>
          <description>Baud rate register</description>
          <addressOffset>0x8</addressOffset>
          <fields>
            <field>
              <name>DIV_Fraction</name>
              <description>fraction of USARTDIV</description>
              <bitRange>[3:0]</bitRange>
            </field>
            <field>
              <name>DIV_Mantissa</name>
              <description>mantissa of USARTDIV</description>
              <bitRange>[15:4]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>Control register 1</description>
          <addressOffset>0xC</addressOffset>
          <fields>
            <field>
              <name>RWU</name>
              <description>Receiver wakeup</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>RE</name>
              <description>Receiver enable</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>TE</name>
              <description>Transmitter enable</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>IDLEIE</name>
              <description>IDLE interrupt enable</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>RXNEIE</name>
              <description>RXNE interrupt enable</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transmission complete interrupt enable</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>TXEIE</name>
              <description>TXE interrupt enable</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>PEIE</name>
              <description>PE interrupt enable</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>PS</name>
              <description>Parity selection</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>PCE</name>
              <description>Parity control enable</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>WAKE</name>
              <description>Wakeup method</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>M</name>
              <description>Word length</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>UE</name>
              <description>USART enable</description>
              <bitRange>[13:13]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>Control register 2</description>
          <addressOffset>0x10</addressOffset>
          <fields>
            <field>
              <name>ADD</name>
              <description>Address of the USART node</description>
              <bitRange>[3:0]</bitRange>
            </field>
            <field>
              <name>LBCL</name>
              <description>Last bit clock pulse</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>CPHA</name>
              <description>Clock phase</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>CPOL</name>
              <description>Clock polarity</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>CLKEN</name>
              <description>Clock enable</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>STOP</name>
              <description>STOP bits</description>
              <bitRange>[13:12]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR3</name>
          <displayName>CR3</displayName>
          <description>Control register 3</description>
          <addressOffset>0x14</addressOffset>
          <fields>
            <field>
              <name>EIE</name>
              <description>Error interrupt enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>HDSEL</name>
              <description>Half-duplex selection</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>RTSE</name>
              <description>RTS enable</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>CTSE</name>
              <description>CTS enable</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>CTSIE</name>
              <description>CTS interrupt enable</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>OVER8</name>
              <description>Oversampling mode</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>ABREN</name>
              <description>Auto baudrate enable</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>ABRMOD</name>
              <description>Auto baudrate mode</description>
              <bitRange>[14:13]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
  </peripherals>
</device>