<?xml version="1.0" encoding="utf-8" standalone="no"?>
<device schemaVersion="1.1" xmlns:xs="http://www.w3.org/2001/XMLSchema-instance" noNamespaceSchemaLocation="CMSIS-SVD.xsd">
  <vendor>Puya</vendor>
  <vendorID>Puya</vendorID>
  <name>PY32F002Axx</name>
  <series>PY32F0</series>
  <version>1.0.0</version>
  <description>Arm 32-bit Cortex-M0+ Microcontroller based device, CPU clock up to 48 MHz.</description>
  <cpu>
    <name>CM0+</name>
    <revision>r0p1</revision>
    <endian>little</endian>
    <mpuPresent>false</mpuPresent>
    <fpuPresent>false</fpuPresent>
    <nvicPrioBits>4</nvicPrioBits>
    <vendorSystickConfig>false</vendorSystickConfig>
  </cpu>
  <addressUnitBits>8</addressUnitBits>
  <width>32</width>
  <size>32</size>
  <access>read-write</access>
  <resetValue>0x0</resetValue>
  <resetMask>0xFFFFFFFF</resetMask>
  <peripherals>
    <peripheral>
      <name>ADC</name>
      <description>Analog to Digital Converter</description>
      <groupName>ADC</groupName>
      <baseAddress>0x40012400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>ADC_COMP</name>
        <description>ADC and COMP Interrupt through EXTI Lines 17 and 18</description>
        <value>12</value>
      </interrupt>
      <registers>
        <register>
          <name>ISR</name>
          <displayName>ISR</displayName>
          <description>ADC interrupt and status register</description>
          <addressOffset>0x0</addressOffset>
          <fields>
            <field>
              <name>EOSMP</name>
              <description>ADC group regular end of samplingflag</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>EOC</name>
              <description>ADC group regular end of unitaryconversion flag</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>EOSEQ</name>
              <description>ADC group regular end of sequenceconversions flag</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>OVR</name>
              <description>ADC group regular overrunflag</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>AWD</name>
              <description>ADC analog watchdog flag</description>
              <bitRange>[7:7]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>IER</name>
          <displayName>IER</displayName>
          <description>ADC interrupt enable register</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>EOSMPIE</name>
              <description>ADC group regular end of samplinginterrupt</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>EOCIE</name>
              <description>ADC group regular end of unitaryconversion interrupt</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>EOSEQIE</name>
              <description>ADC group regular end of sequenceconversions interrupt</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>OVRIE</name>
              <description>ADC group regular overruninterrupt</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>AWDIE</name>
              <description>ADC analog watchdoginterrupt</description>
              <bitRange>[7:7]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>ADC control register</description>
          <addressOffset>0x8</addressOffset>
          <fields>
            <field>
              <name>ADEN</name>
              <description>ADC enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>ADSTART</name>
              <description>ADC group regular conversionstart</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>ADSTP</name>
              <description>ADC group regular conversionstop</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>ADCAL</name>
              <description>ADC group regular conversioncalibration</description>
              <bitRange>[31:31]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR1</name>
          <displayName>CFGR1</displayName>
          <description>ADC configuration register 1</description>
          <addressOffset>0xC</addressOffset>
          <fields>
            <field>
              <name>SCANDIR</name>
              <description>Scan sequence direction</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>RESSEL</name>
              <description>ADC data resolution</description>
              <bitRange>[4:3]</bitRange>
            </field>
            <field>
              <name>ALIGN</name>
              <description>ADC data alignement</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>EXTSEL</name>
              <description>ADC group regular external triggersource</description>
              <bitRange>[8:6]</bitRange>
            </field>
            <field>
              <name>EXTEN</name>
              <description>ADC group regular external triggerpolarity</description>
              <bitRange>[11:10]</bitRange>
            </field>
            <field>
              <name>OVRMOD</name>
              <description>ADC group regular overrunconfiguration</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>CONT</name>
              <description>ADC group regular continuous conversionmode</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>WAIT</name>
              <description>Wait conversion mode</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>DISCEN</name>
              <description>ADC group regular sequencerdiscontinuous mode</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>AWDSGL</name>
              <description>ADC analog watchdog monitoring asingle channel or all channels</description>
              <bitRange>[22:22]</bitRange>
            </field>
            <field>
              <name>AWDEN</name>
              <description>ADC analog watchdog enable on scopeADC group regular</description>
              <bitRange>[23:23]</bitRange>
            </field>
            <field>
              <name>AWDCH</name>
              <description>ADC analog watchdog monitored channelselection</description>
              <bitRange>[29:26]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR2</name>
          <displayName>CFGR2</displayName>
          <description>ADC configuration register 2</description>
          <addressOffset>0x10</addressOffset>
          <fields>
            <field>
              <name>CKMODE</name>
              <description>ADC clock mode</description>
              <bitRange>[31:28]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SMPR</name>
          <displayName>SMPR</displayName>
          <description>ADC sampling time register</description>
          <addressOffset>0x14</addressOffset>
          <fields>
            <field>
              <name>SMP</name>
              <description>Sampling time selection</description>
              <bitRange>[2:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>TR</name>
          <displayName>TR</displayName>
          <description>ADC analog watchdog 1 threshold register</description>
          <addressOffset>0x20</addressOffset>
          <resetValue>0xFFF0000</resetValue>
          <fields>
            <field>
              <name>LT</name>
              <description>ADC analog watchdog thresholdlow</description>
              <bitRange>[11:0]</bitRange>
            </field>
            <field>
              <name>HT</name>
              <description>ADC analog watchdog thresholdhigh</description>
              <bitRange>[27:16]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CHSELR</name>
          <displayName>CHSELR</displayName>
          <description>ADC group regular sequencer register</description>
          <addressOffset>0x28</addressOffset>
          <resetValue>0xFFF0000</resetValue>
          <fields>
            <field>
              <name>CHSEL0</name>
              <description>Channel-0 selection</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>CHSEL1</name>
              <description>Channel-1 selection</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>CHSEL2</name>
              <description>Channel-2 selection</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>CHSEL3</name>
              <description>Channel-3 selection</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>CHSEL4</name>
              <description>Channel-4 selection</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>CHSEL5</name>
              <description>Channel-5 selection</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>CHSEL6</name>
              <description>Channel-6 selection</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>CHSEL7</name>
              <description>Channel-7 selection</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>CHSEL8</name>
              <description>Channel-8 selection</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>CHSEL9</name>
              <description>Channel-9 selection</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>CHSEL11</name>
              <description>Channel-11 selection</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>CHSEL12</name>
              <description>Channel-12 selection</description>
              <bitRange>[12:12]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>ADC group regular data register</description>
          <addressOffset>0x40</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>DATA</name>
              <description>ADC group regular conversiondata</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCSR</name>
          <displayName>CCSR</displayName>
          <description>ADC calibration configuration and status register</description>
          <addressOffset>0x44</addressOffset>
          <fields>
            <field>
              <name>CALSEL</name>
              <description>Calibration contents selection</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>CALSMP</name>
              <description>Calibration sample time selection</description>
              <bitRange>[13:12]</bitRange>
            </field>
            <field>
              <name>CALSET</name>
              <description>Calibration factor selection</description>
              <bitRange>[15:15]</bitRange>
            </field>
            <field>
              <name>CALFAIL</name>
              <description>Calibration fail flag</description>
              <bitRange>[30:30]</bitRange>
            </field>
            <field>
              <name>CALON</name>
              <description>Calibration flag</description>
              <bitRange>[31:31]</bitRange>
              <access>read-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>CALRR1</name>
          <displayName>CALRR1</displayName>
          <description>ADC calibration result register 1</description>
          <addressOffset>0x48</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>CALC4OUT</name>
              <description>C4 result</description>
              <bitRange>[7:0]</bitRange>
            </field>
            <field>
              <name>CALC5OUT</name>
              <description>C5 result</description>
              <bitRange>[15:8]</bitRange>
            </field>
            <field>
              <name>CALBOUT</name>
              <description>offset result</description>
              <bitRange>[22:16]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CALRR2</name>
          <displayName>CALRR2</displayName>
          <description>ADC calibration result register 2</description>
          <addressOffset>0x4C</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>CALC0OUT</name>
              <description>C0 result</description>
              <bitRange>[7:0]</bitRange>
            </field>
            <field>
              <name>CALC1OUT</name>
              <description>C1 result</description>
              <bitRange>[15:8]</bitRange>
            </field>
            <field>
              <name>CALC2OUT</name>
              <description>C2 result</description>
              <bitRange>[23:16]</bitRange>
            </field>
            <field>
              <name>CALC3OUT</name>
              <description>C3 result</description>
              <bitRange>[31:24]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CALFIR1</name>
          <displayName>CALFIR1</displayName>
          <description>ADC calibration factor input register 1</description>
          <addressOffset>0x50</addressOffset>
          <fields>
            <field>
              <name>CALC4IO</name>
              <description>Calibration C4 factor input</description>
              <bitRange>[7:0]</bitRange>
            </field>
            <field>
              <name>CALC5IO</name>
              <description>Calibration C5 factor input</description>
              <bitRange>[15:8]</bitRange>
            </field>
            <field>
              <name>CALBIO</name>
              <description>Calibration offset factor input</description>
              <bitRange>[22:16]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CALFIR2</name>
          <displayName>CALFIR2</displayName>
          <description>ADC calibration factor input register 2</description>
          <addressOffset>0x54</addressOffset>
          <fields>
            <field>
              <name>CALC0IO</name>
              <description>Calibration C0 factor input</description>
              <bitRange>[7:0]</bitRange>
            </field>
            <field>
              <name>CALC1IO</name>
              <description>Calibration C1 factor input</description>
              <bitRange>[15:8]</bitRange>
            </field>
            <field>
              <name>CALC2IO</name>
              <description>Calibration C2 factor input</description>
              <bitRange>[23:16]</bitRange>
            </field>
            <field>
              <name>CALC3IO</name>
              <description>Calibration C3 factor input</description>
              <bitRange>[31:24]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR</name>
          <displayName>CCR</displayName>
          <description>ADC common configuration register</description>
          <addressOffset>0x308</addressOffset>
          <fields>
            <field>
              <name>VREFEN</name>
              <description>VREFINT enable</description>
              <bitRange>[22:22]</bitRange>
            </field>
            <field>
              <name>TSEN</name>
              <description>Temperature sensor enable</description>
              <bitRange>[23:23]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>COMP1</name>
      <description>Comparator</description>
      <groupName>COMP</groupName>
      <baseAddress>0x40010200</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x10</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CSR</name>
          <displayName>CSR</displayName>
          <description>COMP control and status register</description>
          <addressOffset>0x0</addressOffset>
          <fields>
            <field>
              <name>COMP_EN</name>
              <description>COMP enable bit</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>SCALER_EN</name>
              <description>SCALER enable bit</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>INMSEL</name>
              <description>Comparator signal selector forinverting input INM</description>
              <bitRange>[7:4]</bitRange>
            </field>
            <field>
              <name>INPSEL</name>
              <description>Comparator signal selector fornon-inverting input</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>WINMODE</name>
              <description>Comparator non-inverting inputselector for window mode</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>POLARITY</name>
              <description>Comparator polarityselector</description>
              <bitRange>[15:15]</bitRange>
            </field>
            <field>
              <name>HYST</name>
              <description>Comparator hysteresis enableselector</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>PWRMODE</name>
              <description>Comparator power modeselector</description>
              <bitRange>[19:18]</bitRange>
            </field>
            <field>
              <name>COMP_OUT</name>
              <description>Comparator output status</description>
              <bitRange>[30:30]</bitRange>
            </field>
            <field>
              <name>LOCK</name>
              <description>CSR register lock</description>
              <bitRange>[31:31]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>FR</name>
          <displayName>FR</displayName>
          <description>Comparator Filterregister</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>FLTEN</name>
              <description>Filter enable bit</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>FLTCNT</name>
              <description>Comparator filter and counter</description>
              <bitRange>[31:16]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>COMP2</name>
      <description>Comparator</description>
      <groupName>COMP</groupName>
      <baseAddress>0x40010210</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x10</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CSR</name>
          <displayName>CSR</displayName>
          <description>COMP control and status register</description>
          <addressOffset>0x0</addressOffset>
          <fields>
            <field>
              <name>COMP_EN</name>
              <description>COMP enable bit</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>INMSEL</name>
              <description>Comparator signal selector forinverting input INM</description>
              <bitRange>[7:4]</bitRange>
            </field>
            <field>
              <name>INPSEL</name>
              <description>Comparator signal selector fornon-inverting input</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>WINMODE</name>
              <description>Comparator non-inverting inputselector for window mode</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>POLARITY</name>
              <description>Comparator polarityselector</description>
              <bitRange>[15:15]</bitRange>
            </field>
            <field>
              <name>PWRMODE</name>
              <description>Comparator power modeselector</description>
              <bitRange>[19:18]</bitRange>
            </field>
            <field>
              <name>COMP_OUT</name>
              <description>Comparator output status</description>
              <bitRange>[30:30]</bitRange>
            </field>
            <field>
              <name>LOCK</name>
              <description>CSR register lock</description>
              <bitRange>[31:31]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>FR</name>
          <displayName>FR</displayName>
          <description>Comparator Filterregister</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>FLTEN</name>
              <description>Filter enable bit</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>FLTCNT</name>
              <description>Comparator filter and counter</description>
              <bitRange>[31:16]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>CRC</name>
      <description>CRC calculation unit</description>
      <groupName>CRC</groupName>
      <baseAddress>0x40023000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>Data register</description>
          <addressOffset>0x0</addressOffset>
          <resetValue>0xFFFFFFFF</resetValue>
          <fields>
            <field>
              <name>DR</name>
              <description>Data Register</description>
              <bitRange>[31:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>IDR</name>
          <displayName>IDR</displayName>
          <description>Independent Data register</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>IDR</name>
              <description>Independent Data register</description>
              <bitRange>[7:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Control register</description>
          <addressOffset>0x8</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>RESET</name>
              <description>Reset bit</description>
              <bitRange>[0:0]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>DBGMCU</name>
      <description>Debug support</description>
      <groupName>DBGMCU</groupName>
      <baseAddress>0x40015800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>IDCODE</name>
          <displayName>IDCODE</displayName>
          <description>MCU Device ID Code Register</description>
          <addressOffset>0x0</addressOffset>
          <access>read-only</access>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Debug MCU Configuration Register</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>DBG_STOP</name>
              <description>Debug Stop Mode</description>
              <bitRange>[1:1]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>APB_FZ1</name>
          <displayName>APB_FZ1</displayName>
          <description>APB Freeze Register1</description>
          <addressOffset>0x8</addressOffset>
          <fields>
            <field>
              <name>DBG_IWDG_STOP</name>
              <description>Debug Independent Wachdog stopped when Core is halted</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>DBG_LPTIM_STOP</name>
              <description>Debug LPTIM stopped when Core is halted</description>
              <bitRange>[31:31]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>APB_FZ2</name>
          <displayName>APB_FZ2</displayName>
          <description>APB Freeze Register2</description>
          <addressOffset>0xC</addressOffset>
          <fields>
            <field>
              <name>DBG_TIMER1_STOP</name>
              <description>Debug Timer 1 stopped when Core is halted</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>DBG_TIMER16_STOP</name>
              <description>Debug Timer 16 stopped when Core is halted</description>
              <bitRange>[17:17]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>EXTI</name>
      <description>External interrupt/eventcontroller</description>
      <groupName>EXTI</groupName>
      <baseAddress>0x40021800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>EXTI0_1</name>
        <description>EXTI Line 0 and 1 Interrupt</description>
        <value>5</value>
      </interrupt>
      <interrupt>
        <name>EXTI2_3</name>
        <description>EXTI Line 2 and 3 Interrupt</description>
        <value>6</value>
      </interrupt>
      <interrupt>
        <name>EXTI4_15</name>
        <description>EXTI Line 4 to 15 Interrupt</description>
        <value>7</value>
      </interrupt>
      <registers>
        <register>
          <name>RTSR</name>
          <displayName>RTSR</displayName>
          <description>EXTI rising trigger selectionregister</description>
          <addressOffset>0x0</addressOffset>
          <fields>
            <field>
              <name>RT0</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>RT1</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>RT2</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>RT3</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>RT4</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>RT5</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>RT6</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>RT7</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>RT8</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>RT9</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>RT10</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>RT11</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>RT12</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>RT13</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>RT14</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>RT15</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[15:15]</bitRange>
            </field>
            <field>
              <name>RT16</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>RT17</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>RT18</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[18:18]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>FTSR</name>
          <displayName>FTSR</displayName>
          <description>EXTI falling trigger selectionregister</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>FT0</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>FT1</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>FT2</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>FT3</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>FT4</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>FT5</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>FT6</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>FT7</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>FT8</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>FT9</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>FT10</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>FT11</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>FT12</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>FT13</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>FT14</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>FT15</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[15:15]</bitRange>
            </field>
            <field>
              <name>FT16</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>FT17</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>FT18</name>
              <description>Falling trigger event configuration bitof Configurable Event input</description>
              <bitRange>[18:18]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SWIER</name>
          <displayName>SWIER</displayName>
          <description>EXTI software interrupt eventregister</description>
          <addressOffset>0x8</addressOffset>
          <fields>
            <field>
              <name>SWI0</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>SWI1</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>SWI2</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>SWI3</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>SWI4</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>SWI5</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>SWI6</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>SWI7</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>SWI8</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>SWI9</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>SWI10</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>SWI11</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>SWI12</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>SWI13</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>SWI14</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>SWI15</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[15:15]</bitRange>
            </field>
            <field>
              <name>SWI16</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>SWI17</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>SWI18</name>
              <description>Rising trigger event configuration bitof Configurable Event input</description>
              <bitRange>[18:18]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PR</name>
          <displayName>PR</displayName>
          <description>EXTI pendingregister</description>
          <addressOffset>0xC</addressOffset>
          <fields>
            <field>
              <name>PR0</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>PR1</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>PR2</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>PR3</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>PR4</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>PR5</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>PR6</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>PR7</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>PR8</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>PR9</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>PR10</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>PR11</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>PR12</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>PR13</name>
              <description>configurable event inputs x rising edgePending bit</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>PR14</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>PR15</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[15:15]</bitRange>
            </field>
            <field>
              <name>PR16</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>PR17</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>PR18</name>
              <description>configurable event inputs x rising edgePending bit.</description>
              <bitRange>[18:18]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>EXTICR1</name>
          <displayName>EXTICR1</displayName>
          <description>EXTI external interrupt selectionregister</description>
          <addressOffset>0x60</addressOffset>
          <fields>
            <field>
              <name>EXTI0</name>
              <description>GPIO port selection</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>EXTI1</name>
              <description>GPIO port selection</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>EXTI2</name>
              <description>GPIO port selection</description>
              <bitRange>[17:16]</bitRange>
            </field>
            <field>
              <name>EXTI3</name>
              <description>GPIO port selection</description>
              <bitRange>[25:24]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>EXTICR2</name>
          <displayName>EXTICR2</displayName>
          <description>EXTI external interrupt selectionregister</description>
          <addressOffset>0x64</addressOffset>
          <fields>
            <field>
              <name>EXTI4</name>
              <description>GPIO port selection</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>EXTI5</name>
              <description>GPIO port selection</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>EXTI6</name>
              <description>GPIO port selection</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>EXTI7</name>
              <description>GPIO port selection</description>
              <bitRange>[24:24]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>EXTICR3</name>
          <displayName>EXTICR3</displayName>
          <description>EXTI external interrupt selectionregister</description>
          <addressOffset>0x68</addressOffset>
          <fields>
            <field>
              <name>EXTI8</name>
              <description>GPIO port selection</description>
              <bitRange>[0:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>IMR</name>
          <displayName>IMR</displayName>
          <description>EXTI CPU wakeup with interrupt maskregister</description>
          <addressOffset>0x80</addressOffset>
          <resetValue>0xFFF80000</resetValue>
          <fields>
            <field>
              <name>IM0</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>IM1</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>IM2</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>IM3</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>IM4</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>IM5</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>IM6</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>IM7</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>IM8</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>IM9</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>IM10</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>IM11</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>IM12</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>IM13</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>IM14</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>IM15</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[15:15]</bitRange>
            </field>
            <field>
              <name>IM16</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>IM17</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>IM18</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[18:18]</bitRange>
            </field>
            <field>
              <name>IM19</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[19:19]</bitRange>
            </field>
            <field>
              <name>IM29</name>
              <description>CPU wakeup with interrupt mask on eventinput</description>
              <bitRange>[29:29]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>EMR</name>
          <displayName>EMR</displayName>
          <description>EXTI CPU wakeup with event maskregister</description>
          <addressOffset>0x84</addressOffset>
          <fields>
            <field>
              <name>EM0</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>EM1</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>EM2</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>EM3</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>EM4</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>EM5</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>EM6</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>EM7</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>EM8</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>EM9</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>EM10</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>EM11</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>EM12</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>EM13</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>EM14</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>EM15</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[15:15]</bitRange>
            </field>
            <field>
              <name>EM16</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>EM17</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>EM18</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[18:18]</bitRange>
            </field>
            <field>
              <name>EM19</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[19:19]</bitRange>
            </field>
            <field>
              <name>EM29</name>
              <description>CPU wakeup with event mask on eventinput</description>
              <bitRange>[29:29]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>FLASH</name>
      <description>Flash</description>
      <groupName>Flash</groupName>
      <baseAddress>0x40022000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>FLASH</name>
        <description>FLASH global Interrupt</description>
        <value>3</value>
      </interrupt>
      <registers>
        <register>
          <name>ACR</name>
          <displayName>ACR</displayName>
          <description>Access control register</description>
          <addressOffset>0x0</addressOffset>
          <resetValue>0x600</resetValue>
          <fields>
            <field>
              <name>LATENCY</name>
              <description>Latency</description>
              <bitRange>[0:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>KEYR</name>
          <displayName>KEYR</displayName>
          <description>Flash key register</description>
          <addressOffset>0x8</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>KEY</name>
              <description>Flash key</description>
              <bitRange>[31:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>OPTKEYR</name>
          <displayName>OPTKEYR</displayName>
          <description>Option byte key register</description>
          <addressOffset>0xC</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>OPTKEY</name>
              <description>Option byte key</description>
              <bitRange>[31:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>Status register</description>
          <addressOffset>0x10</addressOffset>
          <fields>
            <field>
              <name>EOP</name>
              <description>End of operation</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>WRPERR</name>
              <description>Write protected error</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>OPTVERR</name>
              <description>Option and Engineering bits loadingvalidity error</description>
              <bitRange>[15:15]</bitRange>
            </field>
            <field>
              <name>BSY</name>
              <description>Busy</description>
              <bitRange>[16:16]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Flash control register</description>
          <addressOffset>0x14</addressOffset>
          <resetValue>0xC0000000</resetValue>
          <fields>
            <field>
              <name>PG</name>
              <description>Programming</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>PER</name>
              <description>Page erase</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>MER</name>
              <description>Mass erase</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>SER</name>
              <description>Sector erase</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>OPTSTRT</name>
              <description>Option byte program start</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>PGTSTRT</name>
              <description>Flash main memory program start</description>
              <bitRange>[19:19]</bitRange>
            </field>
            <field>
              <name>EOPIE</name>
              <description>End of operation interruptenable</description>
              <bitRange>[24:24]</bitRange>
            </field>
            <field>
              <name>ERRIE</name>
              <description>Error interrupt enable</description>
              <bitRange>[25:25]</bitRange>
            </field>
            <field>
              <name>OBL_LAUNCH</name>
              <description>Force the option byteloading</description>
              <bitRange>[27:27]</bitRange>
            </field>
            <field>
              <name>OPTLOCK</name>
              <description>Options Lock</description>
              <bitRange>[30:30]</bitRange>
            </field>
            <field>
              <name>LOCK</name>
              <description>FLASH_CR Lock</description>
              <bitRange>[31:31]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>OPTR</name>
          <displayName>OPTR</displayName>
          <description>Flash option register</description>
          <addressOffset>0x20</addressOffset>
          <resetValue>0x4F55B0AA</resetValue>
          <fields>
            <field>
              <name>RDP</name>
              <description>Read Protection</description>
              <bitRange>[7:0]</bitRange>
            </field>
            <field>
              <name>BOREN</name>
              <description>BOR reset Level</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>BORF_LEV</name>
              <description>These bits contain the VDD supply levelthreshold that activates the reset</description>
              <bitRange>[11:9]</bitRange>
            </field>
            <field>
              <name>IDWG_SW</name>
              <description>Independent watchdogselection</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>NRST_MODE</name>
              <description>NRST_MODE</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>nBOOT1</name>
              <description>Boot configuration</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SDKR</name>
          <displayName>SDKR</displayName>
          <description>Flash SDK address register</description>
          <addressOffset>0x24</addressOffset>
          <resetValue>0xFFE0001F</resetValue>
          <fields>
            <field>
              <name>SDK_STRT</name>
              <description>SDK area start address</description>
              <bitRange>[4:0]</bitRange>
            </field>
            <field>
              <name>SDK_END</name>
              <description>SDK area end address</description>
              <bitRange>[12:8]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>WRPR</name>
          <displayName>WRPR</displayName>
          <description>Flash WRP addressregister</description>
          <addressOffset>0x2C</addressOffset>
          <resetValue>0xFFFF</resetValue>
          <fields>
            <field>
              <name>WRP</name>
              <description>WRP address</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>STCR</name>
          <displayName>STCR</displayName>
          <description>Flash sleep time configregister</description>
          <addressOffset>0x90</addressOffset>
          <resetValue>0x6400</resetValue>
          <fields>
            <field>
              <name>SLEEP_EN</name>
              <description>FLash sleep enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>SLEEP_TIME</name>
              <description>FLash sleep time configuration(counter based on HSI_10M)</description>
              <bitRange>[15:8]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>TS0</name>
          <displayName>TS0</displayName>
          <description>Flash TS0 register</description>
          <addressOffset>0x100</addressOffset>
          <resetValue>0xB4</resetValue>
          <fields>
            <field>
              <name>TS0</name>
              <description>FLash TS0 register</description>
              <bitRange>[7:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>TS1</name>
          <displayName>TS1</displayName>
          <description>Flash TS1 register</description>
          <addressOffset>0x104</addressOffset>
          <resetValue>0x1B0</resetValue>
          <fields>
            <field>
              <name>TS1</name>
              <description>FLash TS1 register</description>
              <bitRange>[8:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>TS2P</name>
          <displayName>TS2P</displayName>
          <description>Flash TS2P register</description>
          <addressOffset>0x108</addressOffset>
          <resetValue>0xB4</resetValue>
          <fields>
            <field>
              <name>TS2P</name>
              <description>FLash TS2P register</description>
              <bitRange>[7:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>TPS3</name>
          <displayName>TPS3</displayName>
          <description>Flash TPS3 register</description>
          <addressOffset>0x10C</addressOffset>
          <resetValue>0x6C0</resetValue>
          <fields>
            <field>
              <name>TPS3</name>
              <description>FLash TPS3 register</description>
              <bitRange>[10:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>TS3</name>
          <displayName>TS3</displayName>
          <description>Flash TS3 register</description>
          <addressOffset>0x110</addressOffset>
          <resetValue>0xB4</resetValue>
          <fields>
            <field>
              <name>TS3</name>
              <description>FLash TS3 register</description>
              <bitRange>[7:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PERTPE</name>
          <displayName>PERTPE</displayName>
          <description>Flash PERTPE register</description>
          <addressOffset>0x114</addressOffset>
          <resetValue>0xEA60</resetValue>
          <fields>
            <field>
              <name>PERTPE</name>
              <description>FLash PERTPE register</description>
              <bitRange>[16:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SMERTPE</name>
          <displayName>SMERTPE</displayName>
          <description>Flash SMERTPE register</description>
          <addressOffset>0x118</addressOffset>
          <resetValue>0xFD20</resetValue>
          <fields>
            <field>
              <name>SMERTPE</name>
              <description>FLash SMERTPE register</description>
              <bitRange>[16:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PRGTPE</name>
          <displayName>PRGTPE</displayName>
          <description>Flash PRGTPE register</description>
          <addressOffset>0x11C</addressOffset>
          <resetValue>0x8CA0</resetValue>
          <fields>
            <field>
              <name>PRGTPE</name>
              <description>FLash PRGTPE register</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PRETPE</name>
          <displayName>PRETPE</displayName>
          <description>Flash PRETPE register</description>
          <addressOffset>0x120</addressOffset>
          <resetValue>0x12C0</resetValue>
          <fields>
            <field>
              <name>PRETPE</name>
              <description>FLash PRETPE register</description>
              <bitRange>[12:0]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>GPIOA</name>
      <description>General-purpose I/Os</description>
      <groupName>GPIO</groupName>
      <baseAddress>0x50000000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>MODER</name>
          <displayName>MODER</displayName>
          <description>GPIO port mode register</description>
          <addressOffset>0x0</addressOffset>
          <resetValue>0xEBFFFFFF</resetValue>
          <fields>
            <field>
              <name>MODE0</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>MODE1</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[3:2]</bitRange>
            </field>
            <field>
              <name>MODE2</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[5:4]</bitRange>
            </field>
            <field>
              <name>MODE3</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[7:6]</bitRange>
            </field>
            <field>
              <name>MODE4</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>MODE5</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[11:10]</bitRange>
            </field>
            <field>
              <name>MODE6</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[13:12]</bitRange>
            </field>
            <field>
              <name>MODE7</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[15:14]</bitRange>
            </field>
            <field>
              <name>MODE8</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[17:16]</bitRange>
            </field>
            <field>
              <name>MODE9</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[19:18]</bitRange>
            </field>
            <field>
              <name>MODE10</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[21:20]</bitRange>
            </field>
            <field>
              <name>MODE11</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[23:22]</bitRange>
            </field>
            <field>
              <name>MODE12</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[25:24]</bitRange>
            </field>
            <field>
              <name>MODE13</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[27:26]</bitRange>
            </field>
            <field>
              <name>MODE14</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[29:28]</bitRange>
            </field>
            <field>
              <name>MODE15</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[31:30]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>OTYPER</name>
          <displayName>OTYPER</displayName>
          <description>GPIO port output type register</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>OT0</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>OT1</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>OT2</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>OT3</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>OT4</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>OT5</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>OT6</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>OT7</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>OT8</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>OT9</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>OT10</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>OT11</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>OT12</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>OT13</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>OT14</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>OT15</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>OSPEEDR</name>
          <displayName>OSPEEDR</displayName>
          <description>GPIO port output speedregister</description>
          <addressOffset>0x8</addressOffset>
          <resetValue>0xC000000</resetValue>
          <fields>
            <field>
              <name>OSPEED0</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>OSPEED1</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[3:2]</bitRange>
            </field>
            <field>
              <name>OSPEED2</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[5:4]</bitRange>
            </field>
            <field>
              <name>OSPEED3</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[7:6]</bitRange>
            </field>
            <field>
              <name>OSPEED4</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>OSPEED5</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[11:10]</bitRange>
            </field>
            <field>
              <name>OSPEED6</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[13:12]</bitRange>
            </field>
            <field>
              <name>OSPEED7</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[15:14]</bitRange>
            </field>
            <field>
              <name>OSPEED8</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[17:16]</bitRange>
            </field>
            <field>
              <name>OSPEED9</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[19:18]</bitRange>
            </field>
            <field>
              <name>OSPEED10</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[21:20]</bitRange>
            </field>
            <field>
              <name>OSPEED11</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[23:22]</bitRange>
            </field>
            <field>
              <name>OSPEED12</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[25:24]</bitRange>
            </field>
            <field>
              <name>OSPEED13</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[27:26]</bitRange>
            </field>
            <field>
              <name>OSPEED14</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[29:28]</bitRange>
            </field>
            <field>
              <name>OSPEED15</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[31:30]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PUPDR</name>
          <displayName>PUPDR</displayName>
          <description>GPIO port pull-up/pull-downregister</description>
          <addressOffset>0xC</addressOffset>
          <resetValue>0x24000000</resetValue>
          <fields>
            <field>
              <name>PUPD0</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>PUPD1</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[3:2]</bitRange>
            </field>
            <field>
              <name>PUPD2</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[5:4]</bitRange>
            </field>
            <field>
              <name>PUPD3</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[7:6]</bitRange>
            </field>
            <field>
              <name>PUPD4</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>PUPD5</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[11:10]</bitRange>
            </field>
            <field>
              <name>PUPD6</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[13:12]</bitRange>
            </field>
            <field>
              <name>PUPD7</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[15:14]</bitRange>
            </field>
            <field>
              <name>PUPD8</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[17:16]</bitRange>
            </field>
            <field>
              <name>PUPD9</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[19:18]</bitRange>
            </field>
            <field>
              <name>PUPD10</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[21:20]</bitRange>
            </field>
            <field>
              <name>PUPD11</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[23:22]</bitRange>
            </field>
            <field>
              <name>PUPD12</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[25:24]</bitRange>
            </field>
            <field>
              <name>PUPD13</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[27:26]</bitRange>
            </field>
            <field>
              <name>PUPD14</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[29:28]</bitRange>
            </field>
            <field>
              <name>PUPD15</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[31:30]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>IDR</name>
          <displayName>IDR</displayName>
          <description>GPIO port input data register</description>
          <addressOffset>0x10</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>ID0</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>ID1</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>ID2</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>ID3</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>ID4</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>ID5</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>ID6</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>ID7</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>ID8</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>ID9</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>ID10</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>ID11</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>ID12</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>ID13</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>ID14</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>ID15</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>ODR</name>
          <displayName>ODR</displayName>
          <description>GPIO port output data register</description>
          <addressOffset>0x14</addressOffset>
          <fields>
            <field>
              <name>OD0</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>OD1</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>OD2</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>OD3</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>OD4</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>OD5</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>OD6</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>OD7</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>OD8</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>OD9</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>OD10</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>OD11</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>OD12</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>OD13</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>OD14</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>OD15</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>BSRR</name>
          <displayName>BSRR</displayName>
          <description>GPIO port bit set/resetregister</description>
          <addressOffset>0x18</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>BS0</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>BS1</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>BS2</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>BS3</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>BS4</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>BS5</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>BS6</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>BS7</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>BS8</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>BS9</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>BS10</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>BS11</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>BS12</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>BS13</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>BS14</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>BS15</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[15:15]</bitRange>
            </field>
            <field>
              <name>BR0</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>BR1</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>BR2</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[18:18]</bitRange>
            </field>
            <field>
              <name>BR3</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[19:19]</bitRange>
            </field>
            <field>
              <name>BR4</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[20:20]</bitRange>
            </field>
            <field>
              <name>BR5</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[21:21]</bitRange>
            </field>
            <field>
              <name>BR6</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[22:22]</bitRange>
            </field>
            <field>
              <name>BR7</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[23:23]</bitRange>
            </field>
            <field>
              <name>BR8</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[24:24]</bitRange>
            </field>
            <field>
              <name>BR9</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[25:25]</bitRange>
            </field>
            <field>
              <name>BR10</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[26:26]</bitRange>
            </field>
            <field>
              <name>BR11</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[27:27]</bitRange>
            </field>
            <field>
              <name>BR12</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[28:28]</bitRange>
            </field>
            <field>
              <name>BR13</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[29:29]</bitRange>
            </field>
            <field>
              <name>BR14</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[30:30]</bitRange>
            </field>
            <field>
              <name>BR15</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[31:31]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>LCKR</name>
          <displayName>LCKR</displayName>
          <description>GPIO port configuration lockregister</description>
          <addressOffset>0x1C</addressOffset>
          <fields>
            <field>
              <name>LCK0</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>LCK1</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>LCK2</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>LCK3</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>LCK4</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>LCK5</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>LCK6</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>LCK7</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>LCK8</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>LCK9</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>LCK10</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>LCK11</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>LCK12</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>LCK13</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>LCK14</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>LCK15</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[15:15]</bitRange>
            </field>
            <field>
              <name>LCKK</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[16:16]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>AFRL</name>
          <displayName>AFRL</displayName>
          <description>GPIO alternate function lowregister</description>
          <addressOffset>0x20</addressOffset>
          <fields>
            <field>
              <name>AFSEL0</name>
              <description>Alternate function selection for port xbit y (y = 0..7)</description>
              <bitRange>[3:0]</bitRange>
            </field>
            <field>
              <name>AFSEL1</name>
              <description>Alternate function selection for port xbit y (y = 0..7)</description>
              <bitRange>[7:4]</bitRange>
            </field>
            <field>
              <name>AFSEL2</name>
              <description>Alternate function selection for port xbit y (y = 0..7)</description>
              <bitRange>[11:8]</bitRange>
            </field>
            <field>
              <name>AFSEL3</name>
              <description>Alternate function selection for port xbit y (y = 0..7)</description>
              <bitRange>[15:12]</bitRange>
            </field>
            <field>
              <name>AFSEL4</name>
              <description>Alternate function selection for port xbit y (y = 0..7)</description>
              <bitRange>[19:16]</bitRange>
            </field>
            <field>
              <name>AFSEL5</name>
              <description>Alternate function selection for port xbit y (y = 0..7)</description>
              <bitRange>[23:20]</bitRange>
            </field>
            <field>
              <name>AFSEL6</name>
              <description>Alternate function selection for port xbit y (y = 0..7)</description>
              <bitRange>[27:24]</bitRange>
            </field>
            <field>
              <name>AFSEL7</name>
              <description>Alternate function selection for port xbit y (y = 0..7)</description>
              <bitRange>[31:28]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>AFRH</name>
          <displayName>AFRH</displayName>
          <description>GPIO alternate function highregister</description>
          <addressOffset>0x24</addressOffset>
          <fields>
            <field>
              <name>AFSEL8</name>
              <description>Alternate function selection for port xbit y (y = 8..15)</description>
              <bitRange>[3:0]</bitRange>
            </field>
            <field>
              <name>AFSEL9</name>
              <description>Alternate function selection for port xbit y (y = 8..15)</description>
              <bitRange>[7:4]</bitRange>
            </field>
            <field>
              <name>AFSEL10</name>
              <description>Alternate function selection for port xbit y (y = 8..15)</description>
              <bitRange>[11:8]</bitRange>
            </field>
            <field>
              <name>AFSEL11</name>
              <description>Alternate function selection for port xbit y (y = 8..15)</description>
              <bitRange>[15:12]</bitRange>
            </field>
            <field>
              <name>AFSEL12</name>
              <description>Alternate function selection for port xbit y (y = 8..15)</description>
              <bitRange>[19:16]</bitRange>
            </field>
            <field>
              <name>AFSEL13</name>
              <description>Alternate function selection for port xbit y (y = 8..15)</description>
              <bitRange>[23:20]</bitRange>
            </field>
            <field>
              <name>AFSEL14</name>
              <description>Alternate function selection for port xbit y (y = 8..15)</description>
              <bitRange>[27:24]</bitRange>
            </field>
            <field>
              <name>AFSEL15</name>
              <description>Alternate function selection for port xbit y (y = 8..15)</description>
              <bitRange>[31:28]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>BRR</name>
          <displayName>BRR</displayName>
          <description>port bit reset register</description>
          <addressOffset>0x28</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>BR0</name>
              <description>Port Reset bit</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>BR1</name>
              <description>Port Reset bit</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>BR2</name>
              <description>Port Reset bit</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>BR3</name>
              <description>Port Reset bit</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>BR4</name>
              <description>Port Reset bit</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>BR5</name>
              <description>Port Reset bit</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>BR6</name>
              <description>Port Reset bit</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>BR7</name>
              <description>Port Reset bit</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>BR8</name>
              <description>Port Reset bit</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>BR9</name>
              <description>Port Reset bit</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>BR10</name>
              <description>Port Reset bit</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>BR11</name>
              <description>Port Reset bit</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>BR12</name>
              <description>Port Reset bit</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>BR13</name>
              <description>Port Reset bit</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>BR14</name>
              <description>Port Reset bit</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>BR15</name>
              <description>Port Reset bit</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>GPIOB</name>
      <description>General-purpose I/Os</description>
      <groupName>GPIO</groupName>
      <baseAddress>0x50000400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>MODER</name>
          <displayName>MODER</displayName>
          <description>GPIO port mode register</description>
          <addressOffset>0x0</addressOffset>
          <resetValue>0xFFFFFFFF</resetValue>
          <fields>
            <field>
              <name>MODE0</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>MODE1</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[3:2]</bitRange>
            </field>
            <field>
              <name>MODE2</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[5:4]</bitRange>
            </field>
            <field>
              <name>MODE3</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[7:6]</bitRange>
            </field>
            <field>
              <name>MODE4</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>MODE5</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[11:10]</bitRange>
            </field>
            <field>
              <name>MODE6</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[13:12]</bitRange>
            </field>
            <field>
              <name>MODE7</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[15:14]</bitRange>
            </field>
            <field>
              <name>MODE8</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[17:16]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>OTYPER</name>
          <displayName>OTYPER</displayName>
          <description>GPIO port output type register</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>OT0</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>OT1</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>OT2</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>OT3</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>OT4</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>OT5</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>OT6</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>OT7</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>OT8</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[8:8]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>OSPEEDR</name>
          <displayName>OSPEEDR</displayName>
          <description>GPIO port output speedregister</description>
          <addressOffset>0x8</addressOffset>
          <fields>
            <field>
              <name>OSPEED0</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>OSPEED1</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[3:2]</bitRange>
            </field>
            <field>
              <name>OSPEED2</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[5:4]</bitRange>
            </field>
            <field>
              <name>OSPEED3</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[7:6]</bitRange>
            </field>
            <field>
              <name>OSPEED4</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>OSPEED5</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[11:10]</bitRange>
            </field>
            <field>
              <name>OSPEED6</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[13:12]</bitRange>
            </field>
            <field>
              <name>OSPEED7</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[15:14]</bitRange>
            </field>
            <field>
              <name>OSPEED8</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[17:16]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PUPDR</name>
          <displayName>PUPDR</displayName>
          <description>GPIO port pull-up/pull-downregister</description>
          <addressOffset>0xC</addressOffset>
          <fields>
            <field>
              <name>PUPD0</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>PUPD1</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[3:2]</bitRange>
            </field>
            <field>
              <name>PUPD2</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[5:4]</bitRange>
            </field>
            <field>
              <name>PUPD3</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[7:6]</bitRange>
            </field>
            <field>
              <name>PUPD4</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>PUPD5</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[11:10]</bitRange>
            </field>
            <field>
              <name>PUPD6</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[13:12]</bitRange>
            </field>
            <field>
              <name>PUPD7</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[15:14]</bitRange>
            </field>
            <field>
              <name>PUPD8</name>
              <description>Port x configuration bits (y =0..15)</description>
              <bitRange>[17:16]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>IDR</name>
          <displayName>IDR</displayName>
          <description>GPIO port input data register</description>
          <addressOffset>0x10</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>ID0</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>ID1</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>ID2</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>ID3</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>ID4</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>ID5</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>ID6</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>ID7</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>ID8</name>
              <description>Port input data (y =0..15)</description>
              <bitRange>[8:8]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>ODR</name>
          <displayName>ODR</displayName>
          <description>GPIO port output data register</description>
          <addressOffset>0x14</addressOffset>
          <fields>
            <field>
              <name>OD0</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>OD1</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>OD2</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>OD3</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>OD4</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>OD5</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>OD6</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>OD7</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>OD8</name>
              <description>Port output data (y =0..15)</description>
              <bitRange>[8:8]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>BSRR</name>
          <displayName>BSRR</displayName>
          <description>GPIO port bit set/resetregister</description>
          <addressOffset>0x18</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>BS0</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>BS1</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>BS2</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>BS3</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>BS4</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>BS5</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>BS6</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>BS7</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>BS8</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>BR0</name>
              <description>Port x set bit y (y=0..15)</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>BR1</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>BR2</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[18:18]</bitRange>
            </field>
            <field>
              <name>BR3</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[19:19]</bitRange>
            </field>
            <field>
              <name>BR4</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[20:20]</bitRange>
            </field>
            <field>
              <name>BR5</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[21:21]</bitRange>
            </field>
            <field>
              <name>BR6</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[22:22]</bitRange>
            </field>
            <field>
              <name>BR7</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[23:23]</bitRange>
            </field>
            <field>
              <name>BR8</name>
              <description>Port x reset bit y (y =0..15)</description>
              <bitRange>[24:24]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>LCKR</name>
          <displayName>LCKR</displayName>
          <description>GPIO port configuration lockregister</description>
          <addressOffset>0x1C</addressOffset>
          <fields>
            <field>
              <name>LCK0</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>LCK1</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>LCK2</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>LCK3</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>LCK4</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>LCK5</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>LCK6</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>LCK7</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>LCK8</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>LCKK</name>
              <description>Port x lock bit y (y=0..15)</description>
              <bitRange>[16:16]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>AFRL</name>
          <displayName>AFRL</displayName>
          <description>GPIO alternate function lowregister</description>
          <addressOffset>0x20</addressOffset>
          <fields>
            <field>
              <name>AFSEL0</name>
              <description>Alternate function selection for port xbit y (y = 0..7)</description>
              <bitRange>[3:0]</bitRange>
            </field>
            <field>
              <name>AFSEL1</name>
              <description>Alternate function selection for port xbit y (y = 0..7)</description>
              <bitRange>[7:4]</bitRange>
            </field>
            <field>
              <name>AFSEL2</name>
              <description>Alternate function selection for port xbit y (y = 0..7)</description>
              <bitRange>[11:8]</bitRange>
            </field>
            <field>
              <name>AFSEL3</name>
              <description>Alternate function selection for port xbit y (y = 0..7)</description>
              <bitRange>[15:12]</bitRange>
            </field>
            <field>
              <name>AFSEL4</name>
              <description>Alternate function selection for port xbit y (y = 0..7)</description>
              <bitRange>[19:16]</bitRange>
            </field>
            <field>
              <name>AFSEL5</name>
              <description>Alternate function selection for port xbit y (y = 0..7)</description>
              <bitRange>[23:20]</bitRange>
            </field>
            <field>
              <name>AFSEL6</name>
              <description>Alternate function selection for port xbit y (y = 0..7)</description>
              <bitRange>[27:24]</bitRange>
            </field>
            <field>
              <name>AFSEL7</name>
              <description>Alternate function selection for port xbit y (y = 0..7)</description>
              <bitRange>[31:28]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>AFRH</name>
          <displayName>AFRH</displayName>
          <description>GPIO alternate function highregister</description>
          <addressOffset>0x24</addressOffset>
          <fields>
            <field>
              <name>AFSEL8</name>
              <description>Alternate function selection for port xbit y (y = 8..15)</description>
              <bitRange>[3:0]</bitRange>
            </field>
            <field>
              <name>AFSEL9</name>
              <description>Alternate function selection for port xbit y (y = 8..15)</description>
              <bitRange>[7:4]</bitRange>
            </field>
            <field>
              <name>AFSEL10</name>
              <description>Alternate function selection for port xbit y (y = 8..15)</description>
              <bitRange>[11:8]</bitRange>
            </field>
            <field>
              <name>AFSEL11</name>
              <description>Alternate function selection for port xbit y (y = 8..15)</description>
              <bitRange>[15:12]</bitRange>
            </field>
            <field>
              <name>AFSEL12</name>
              <description>Alternate function selection for port xbit y (y = 8..15)</description>
              <bitRange>[19:16]</bitRange>
            </field>
            <field>
              <name>AFSEL13</name>
              <description>Alternate function selection for port xbit y (y = 8..15)</description>
              <bitRange>[23:20]</bitRange>
            </field>
            <field>
              <name>AFSEL14</name>
              <description>Alternate function selection for port xbit y (y = 8..15)</description>
              <bitRange>[27:24]</bitRange>
            </field>
            <field>
              <name>AFSEL15</name>
              <description>Alternate function selection for port xbit y (y = 8..15)</description>
              <bitRange>[31:28]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>BRR</name>
          <displayName>BRR</displayName>
          <description>port bit reset register</description>
          <addressOffset>0x28</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>BR0</name>
              <description>Port Reset bit</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>BR1</name>
              <description>Port Reset bit</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>BR2</name>
              <description>Port Reset bit</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>BR3</name>
              <description>Port Reset bit</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>BR4</name>
              <description>Port Reset bit</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>BR5</name>
              <description>Port Reset bit</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>BR6</name>
              <description>Port Reset bit</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>BR7</name>
              <description>Port Reset bit</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>BR8</name>
              <description>Port Reset bit</description>
              <bitRange>[8:8]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral derivedFrom="GPIOB">
      <name>GPIOF</name>
      <baseAddress>0x50001400</baseAddress>
    </peripheral>
    <peripheral>
      <name>I2C</name>
      <description>Inter integrated circuit</description>
      <groupName>I2C</groupName>
      <baseAddress>0x40005400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>I2C1</name>
        <description>I2C1 global Interrupt</description>
        <value>23</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>Control register 1</description>
          <addressOffset>0x0</addressOffset>
          <fields>
            <field>
              <name>PE</name>
              <description>Peripheral enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>ENPEC</name>
              <description>PEC enable</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>ENGC</name>
              <description>General call enable</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>NOSTRETCH</name>
              <description>Clock stretching disable (Slave mode)</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>START</name>
              <description>Start generation</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>STOP</name>
              <description>Stop generation</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>ACK</name>
              <description>Acknowledge enable</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>POS</name>
              <description>Acknowledge/PEC Position (for data reception)</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>PEC</name>
              <description>Packet error checking</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>SWRST</name>
              <description>Software reset</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>Control register 2</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>FREQ</name>
              <description>Peripheral clock frequency</description>
              <bitRange>[5:0]</bitRange>
            </field>
            <field>
              <name>ITERREN</name>
              <description>Error interrupt enable</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>ITEVTEN</name>
              <description>Event interrupt enable</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>ITBUFEN</name>
              <description>Buffer interrupt enable</description>
              <bitRange>[10:10]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>OAR1</name>
          <displayName>OAR1</displayName>
          <description>Own address register 1</description>
          <addressOffset>0x8</addressOffset>
          <fields>
            <field>
              <name>ADD</name>
              <description>Interface address</description>
              <bitRange>[7:1]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>Data register</description>
          <addressOffset>0x10</addressOffset>
          <fields>
            <field>
              <name>DR</name>
              <description>8-bit data register</description>
              <bitRange>[7:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SR1</name>
          <displayName>SR1</displayName>
          <description>Status register 1</description>
          <addressOffset>0x14</addressOffset>
          <fields>
            <field>
              <name>SB</name>
              <description>Start bit (Master mode)</description>
              <bitRange>[0:0]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>ADDR</name>
              <description>Address sent (master mode)/matched (slave mode)</description>
              <bitRange>[1:1]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>BTF</name>
              <description>Byte transfer finished</description>
              <bitRange>[2:2]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>STOPF</name>
              <description>Stop detection (slave mode)</description>
              <bitRange>[4:4]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>RxNE</name>
              <description>Data register not empty (receivers)</description>
              <bitRange>[6:6]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>TxE</name>
              <description>Data register empty (transmitters)</description>
              <bitRange>[7:7]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>BERR</name>
              <description>Bus error</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>ARLO</name>
              <description>Arbitration lost (master mode)</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>AF</name>
              <description>Acknowledge failure</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>OVR</name>
              <description>Overrun/Underrun</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>PECERR</name>
              <description>PEC Error in reception</description>
              <bitRange>[12:12]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SR2</name>
          <displayName>SR2</displayName>
          <description>Status register 2</description>
          <addressOffset>0x18</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>MSL</name>
              <description>Master/slave</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>BUSY</name>
              <description>Bus busy</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>TRA</name>
              <description>Transmitter/receiver</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>GENCALL</name>
              <description>General call address (Slave mode)</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>DUALF</name>
              <description>Dual flag (Slave mode)</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>PEC</name>
              <description>acket error checking register</description>
              <bitRange>[15:8]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR</name>
          <displayName>CCR</displayName>
          <description>Clock control register</description>
          <addressOffset>0x1C</addressOffset>
          <fields>
            <field>
              <name>CCR</name>
              <description>Clock control register in Fast/Standard mode (Master mode)</description>
              <bitRange>[11:0]</bitRange>
            </field>
            <field>
              <name>DUTY</name>
              <description>Fast mode duty cycle</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>F_S</name>
              <description>I2C master mode selection</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>TRISE</name>
          <displayName>TRISE</displayName>
          <description>TRISE register</description>
          <addressOffset>0x20</addressOffset>
          <resetValue>0x2</resetValue>
          <fields>
            <field>
              <name>TRISE</name>
              <description>Maximum rise time in Fast/Standard mode (Master mode)</description>
              <bitRange>[5:0]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>IWDG</name>
      <description>Independent watchdog</description>
      <groupName>IWDG</groupName>
      <baseAddress>0x40003000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>KR</name>
          <displayName>KR</displayName>
          <description>Key register (IWDG_KR)</description>
          <addressOffset>0x0</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>KEY</name>
              <description>Key value</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PR</name>
          <displayName>PR</displayName>
          <description>Prescaler register (IWDG_PR)</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>PR</name>
              <description>Prescaler divider</description>
              <bitRange>[2:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>RLR</name>
          <displayName>RLR</displayName>
          <description>Reload register (IWDG_RLR)</description>
          <addressOffset>0x8</addressOffset>
          <resetValue>0xFFF</resetValue>
          <fields>
            <field>
              <name>RL</name>
              <description>Watchdog counter reloadvalue</description>
              <bitRange>[11:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>Status register (IWDG_SR)</description>
          <addressOffset>0xC</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>PVU</name>
              <description>Watchdog prescaler valueupdate</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>RVU</name>
              <description>Watchdog counter reload valueupdate</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>WVU</name>
              <description>Watchdog counter window value update</description>
              <bitRange>[2:2]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>WINR</name>
          <displayName>WINR</displayName>
          <description>Window register (IWDG_SR)</description>
          <addressOffset>0x10</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>WIN</name>
              <description>window counter</description>
              <bitRange>[11:0]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>LPTIM</name>
      <description>Low power timer</description>
      <groupName>LPTIM</groupName>
      <baseAddress>0x40007C00</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>ISR</name>
          <displayName>ISR</displayName>
          <description>Interrupt and Status Register</description>
          <addressOffset>0x0</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>ARRM</name>
              <description>Autoreload match</description>
              <bitRange>[1:1]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>ICR</name>
          <displayName>ICR</displayName>
          <description>Interrupt Clear Register</description>
          <addressOffset>0x4</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>ARRMCF</name>
              <description>Autoreload match ClearFlag</description>
              <bitRange>[1:1]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>IER</name>
          <displayName>IER</displayName>
          <description>Interrupt Enable Register</description>
          <addressOffset>0x8</addressOffset>
          <fields>
            <field>
              <name>ARRMIE</name>
              <description>Autoreload match InterruptEnable</description>
              <bitRange>[1:1]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR</name>
          <displayName>CFGR</displayName>
          <description>Configuration Register</description>
          <addressOffset>0xC</addressOffset>
          <fields>
            <field>
              <name>PRESC</name>
              <description>Clock prescaler</description>
              <bitRange>[11:9]</bitRange>
            </field>
            <field>
              <name>PRELOAD</name>
              <description>Registers update mode</description>
              <bitRange>[22:22]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Control Register</description>
          <addressOffset>0x10</addressOffset>
          <fields>
            <field>
              <name>ENABLE</name>
              <description>LPTIM Enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>SNGSTRT</name>
              <description>LPTIM start in single mode</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>RSTARE</name>
              <description>Reset after read enable</description>
              <bitRange>[4:4]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <displayName>ARR</displayName>
          <description>Autoreload Register</description>
          <addressOffset>0x18</addressOffset>
          <resetValue>0x1</resetValue>
          <fields>
            <field>
              <name>ARR</name>
              <description>Auto reload value</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <displayName>CNT</displayName>
          <description>Counter Register</description>
          <addressOffset>0x1C</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>CNT</name>
              <description>Counter value</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>RCC</name>
      <description>Reset and clock control</description>
      <groupName>RCC</groupName>
      <baseAddress>0x40021000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>RCC</name>
        <description>RCC global Interrupt</description>
        <value>4</value>
      </interrupt>
      <registers>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Clock control register</description>
          <addressOffset>0x0</addressOffset>
          <resetValue>0x100</resetValue>
          <fields>
            <field>
              <name>HSION</name>
              <description>HSI16 clock enable</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>HSIKERON</name>
              <description>HSI16 always enable for peripheralkernels</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>HSIRDY</name>
              <description>HSI16 clock ready flag</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>HSIDIV</name>
              <description>HSI16 clock divisionfactor</description>
              <bitRange>[13:11]</bitRange>
            </field>
            <field>
              <name>HSEON</name>
              <description>HSE clock enable</description>
              <bitRange>[16:16]</bitRange>
            </field>
            <field>
              <name>HSERDY</name>
              <description>HSE clock ready flag</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>HSEBYP</name>
              <description>HSE crystal oscillatorbypass</description>
              <bitRange>[18:18]</bitRange>
            </field>
            <field>
              <name>CSSON</name>
              <description>Clock security systemenable</description>
              <bitRange>[19:19]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>ICSCR</name>
          <displayName>ICSCR</displayName>
          <description>Internal clock sources calibrationregister</description>
          <addressOffset>0x4</addressOffset>
          <resetValue>0x10000000</resetValue>
          <fields>
            <field>
              <name>HSI_TRIM</name>
              <description>HSI clock trimming</description>
              <bitRange>[12:0]</bitRange>
            </field>
            <field>
              <name>HSI_FS</name>
              <description>HSI frequency selection</description>
              <bitRange>[15:13]</bitRange>
            </field>
            <field>
              <name>LSI_TRIM</name>
              <description>LSI clock trimming</description>
              <bitRange>[24:16]</bitRange>
            </field>
            <field>
              <name>LSI_STARTUP</name>
              <description>LSI startup time</description>
              <bitRange>[27:26]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR</name>
          <displayName>CFGR</displayName>
          <description>Clock configuration register</description>
          <addressOffset>0x8</addressOffset>
          <fields>
            <field>
              <name>SW</name>
              <description>System clock switch</description>
              <bitRange>[2:0]</bitRange>
            </field>
            <field>
              <name>SWS</name>
              <description>System clock switch status</description>
              <bitRange>[5:3]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>HPRE</name>
              <description>AHB prescaler</description>
              <bitRange>[11:8]</bitRange>
            </field>
            <field>
              <name>PPRE</name>
              <description>APB prescaler</description>
              <bitRange>[14:12]</bitRange>
            </field>
            <field>
              <name>MCOSEL</name>
              <description>Microcontroller clockoutput</description>
              <bitRange>[26:24]</bitRange>
            </field>
            <field>
              <name>MCOPRE</name>
              <description>Microcontroller clock outputprescaler</description>
              <bitRange>[30:28]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>ECSCR</name>
          <displayName>ECSCR</displayName>
          <description>External clock source control register</description>
          <addressOffset>0x10</addressOffset>
          <fields>
            <field>
              <name>HSE_FREQ</name>
              <description>HSE clock freqency selection</description>
              <bitRange>[3:2]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CIER</name>
          <displayName>CIER</displayName>
          <description>Clock interrupt enableregister</description>
          <addressOffset>0x18</addressOffset>
          <fields>
            <field>
              <name>LSIRDYIE</name>
              <description>LSI ready interrupt enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>HSIRDYIE</name>
              <description>HSI ready interrupt enable</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>HSERDYIE</name>
              <description>HSE ready interrupt enable</description>
              <bitRange>[4:4]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CIFR</name>
          <displayName>CIFR</displayName>
          <description>Clock interrupt flag register</description>
          <addressOffset>0x1C</addressOffset>
          <access>read-only</access>
          <fields>
            <field>
              <name>LSIRDYF</name>
              <description>LSI ready interrupt flag</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>HSIRDYF</name>
              <description>HSI ready interrupt flag</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>HSERDYF</name>
              <description>HSE ready interrupt flag</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>CSSF</name>
              <description>HSE clock secure system interrupt flag</description>
              <bitRange>[8:8]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CICR</name>
          <displayName>CICR</displayName>
          <description>Clock interrupt clear register</description>
          <addressOffset>0x20</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>LSIRDYC</name>
              <description>LSI ready interrupt clear</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>HSIRDYC</name>
              <description>HSI ready interrupt clear</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>HSERDYC</name>
              <description>HSE ready interrupt clear</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>CSSC</name>
              <description>clock secure system interrupt flag clear</description>
              <bitRange>[8:8]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>IOPRSTR</name>
          <displayName>IOPRSTR</displayName>
          <description>GPIO reset register</description>
          <addressOffset>0x24</addressOffset>
          <fields>
            <field>
              <name>GPIOARST</name>
              <description>I/O port A reset</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>GPIOBRST</name>
              <description>I/O port B reset</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>GPIOFRST</name>
              <description>I/O port F reset</description>
              <bitRange>[5:5]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>AHBRSTR</name>
          <displayName>AHBRSTR</displayName>
          <description>AHB peripheral reset register</description>
          <addressOffset>0x28</addressOffset>
          <fields>
            <field>
              <name>CRCRST</name>
              <description>CRC reset</description>
              <bitRange>[12:12]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>APBRSTR1</name>
          <displayName>APBRSTR1</displayName>
          <description>APB peripheral reset register1</description>
          <addressOffset>0x2C</addressOffset>
          <fields>
            <field>
              <name>I2CRST</name>
              <description>I2C reset</description>
              <bitRange>[21:21]</bitRange>
            </field>
            <field>
              <name>DBGRST</name>
              <description>Debug support reset</description>
              <bitRange>[27:27]</bitRange>
            </field>
            <field>
              <name>PWRRST</name>
              <description>Power interface reset</description>
              <bitRange>[28:28]</bitRange>
            </field>
            <field>
              <name>LPTIMRST</name>
              <description>Low Power Timer reset</description>
              <bitRange>[31:31]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>APBRSTR2</name>
          <displayName>APBRSTR2</displayName>
          <description>APB peripheral reset register2</description>
          <addressOffset>0x30</addressOffset>
          <fields>
            <field>
              <name>SYSCFGRST</name>
              <description>SYSCFG and COMPreset</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>TIM1RST</name>
              <description>TIM1 timer reset</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>SPI1RST</name>
              <description>SPI1 reset</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>USART1RST</name>
              <description>USART1 reset</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>TIM16RST</name>
              <description>TIM16 timer reset</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>ADCRST</name>
              <description>ADC reset</description>
              <bitRange>[20:20]</bitRange>
            </field>
            <field>
              <name>COMP1RST</name>
              <description>COMP1 reset</description>
              <bitRange>[21:21]</bitRange>
            </field>
            <field>
              <name>COMP2RST</name>
              <description>COMP2 reset</description>
              <bitRange>[22:22]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>IOPENR</name>
          <displayName>IOPENR</displayName>
          <description>GPIO clock enable register</description>
          <addressOffset>0x34</addressOffset>
          <fields>
            <field>
              <name>GPIOAEN</name>
              <description>I/O port A clock enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>GPIOBEN</name>
              <description>I/O port B clock enable</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>GPIOFEN</name>
              <description>I/O port F clock enable</description>
              <bitRange>[5:5]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>AHBENR</name>
          <displayName>AHBENR</displayName>
          <description>AHB peripheral clock enableregister</description>
          <addressOffset>0x38</addressOffset>
          <fields>
            <field>
              <name>FLASHEN</name>
              <description>Flash memory interface clockenable</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>SRAMEN</name>
              <description>SRAM memory interface clockenable</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>CRCEN</name>
              <description>CRC clock enable</description>
              <bitRange>[12:12]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>APBENR1</name>
          <displayName>APBENR1</displayName>
          <description>APB peripheral clock enable register1</description>
          <addressOffset>0x3C</addressOffset>
          <fields>
            <field>
              <name>I2CEN</name>
              <description>I2C clock enable</description>
              <bitRange>[21:21]</bitRange>
            </field>
            <field>
              <name>DBGEN</name>
              <description>Debug support clock enable</description>
              <bitRange>[27:27]</bitRange>
            </field>
            <field>
              <name>PWREN</name>
              <description>Power interface clockenable</description>
              <bitRange>[28:28]</bitRange>
            </field>
            <field>
              <name>LPTIMEN</name>
              <description>LPTIM clock enable</description>
              <bitRange>[31:31]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>APBENR2</name>
          <displayName>APBENR2</displayName>
          <description>APB peripheral clock enable register2</description>
          <addressOffset>0x40</addressOffset>
          <fields>
            <field>
              <name>SYSCFGEN</name>
              <description>SYSCFG, COMP and VREFBUF clockenable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>TIM1EN</name>
              <description>TIM1 timer clock enable</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>SPI1EN</name>
              <description>SPI1 clock enable</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>USART1EN</name>
              <description>USART1 clock enable</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>TIM16EN</name>
              <description>TIM16 timer clock enable</description>
              <bitRange>[17:17]</bitRange>
            </field>
            <field>
              <name>ADCEN</name>
              <description>ADC clock enable</description>
              <bitRange>[20:20]</bitRange>
            </field>
            <field>
              <name>COMP1EN</name>
              <description>COMP1 clock enable</description>
              <bitRange>[21:21]</bitRange>
            </field>
            <field>
              <name>COMP2EN</name>
              <description>COMP2 clock enable</description>
              <bitRange>[22:22]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCIPR</name>
          <displayName>CCIPR</displayName>
          <description>Peripherals independent clock configurationregister</description>
          <addressOffset>0x54</addressOffset>
          <fields>
            <field>
              <name>COMP1SEL</name>
              <description>COMP1 clock sourceselection</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>COMP2SEL</name>
              <description>COMP2 clock sourceselection</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>LPTIM1SEL</name>
              <description>LPTIM1 clock sourceselection</description>
              <bitRange>[19:18]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>BDCR</name>
          <displayName>BDCR</displayName>
          <description>RTC domain control register</description>
          <addressOffset>0x5C</addressOffset>
          <fields>
            <field>
              <name>LSCOEN</name>
              <description>Low-speed clock output (LSCO)enable</description>
              <bitRange>[24:24]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CSR</name>
          <displayName>CSR</displayName>
          <description>Control/status register</description>
          <addressOffset>0x60</addressOffset>
          <fields>
            <field>
              <name>LSION</name>
              <description>LSI oscillator enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>LSIRDY</name>
              <description>LSI oscillator ready</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>RMVF</name>
              <description>Remove reset flags</description>
              <bitRange>[23:23]</bitRange>
            </field>
            <field>
              <name>OBLRSTF</name>
              <description>Option byte loader resetflag</description>
              <bitRange>[25:25]</bitRange>
            </field>
            <field>
              <name>PINRSTF</name>
              <description>Pin reset flag</description>
              <bitRange>[26:26]</bitRange>
            </field>
            <field>
              <name>PWRRSTF</name>
              <description>BOR or POR/PDR flag</description>
              <bitRange>[27:27]</bitRange>
            </field>
            <field>
              <name>SFTRSTF</name>
              <description>Software reset flag</description>
              <bitRange>[28:28]</bitRange>
            </field>
            <field>
              <name>IWDGRSTF</name>
              <description>Independent window watchdog resetflag</description>
              <bitRange>[29:29]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>SPI1</name>
      <description>Serial peripheral interface</description>
      <groupName>SPI</groupName>
      <baseAddress>0x40013000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>SPI1</name>
        <description>SPI1 global Interrupt</description>
        <value>25</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>control register 1</description>
          <addressOffset>0x0</addressOffset>
          <fields>
            <field>
              <name>CPHA</name>
              <description>Clock phase</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>CPOL</name>
              <description>Clock polarity</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>MSTR</name>
              <description>Master selection</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>BR</name>
              <description>Baud rate control</description>
              <bitRange>[5:3]</bitRange>
            </field>
            <field>
              <name>SPE</name>
              <description>SPI enable</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>LSBFIRST</name>
              <description>Frame format</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>SSI</name>
              <description>Internal slave selection</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>SSM</name>
              <description>Software slave management</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>RXONLY</name>
              <description>Receive only</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>BIDIOE</name>
              <description>Output enable in bidirectional mode</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>BIDIMODE</name>
              <description>Bidirectional data mode enable</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>control register 2</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>SSOE</name>
              <description>SS output enable</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>ERRIE</name>
              <description>Error interrupt enable</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>RXNEIE</name>
              <description>RX buffer not empty interrupt enable</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>TXEIE</name>
              <description>Tx buffer empty interrupt enable</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>DS</name>
              <description>Data length</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>FRXTH</name>
              <description>FIFO reception threshold</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>SLVFM</name>
              <description>Slave fast mode enable</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x8</addressOffset>
          <resetValue>0x2</resetValue>
          <fields>
            <field>
              <name>RXNE</name>
              <description>Receive buffer not empty</description>
              <bitRange>[0:0]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>TXE</name>
              <description>Transmit buffer empty</description>
              <bitRange>[1:1]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>MODF</name>
              <description>Mode fault</description>
              <bitRange>[5:5]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>OVR</name>
              <description>Overrun flag</description>
              <bitRange>[6:6]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>BSY</name>
              <description>Busy flag</description>
              <bitRange>[7:7]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>FRLVL</name>
              <description>FIFO reception level</description>
              <bitRange>[10:9]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>FTLVL</name>
              <description>FIFO transmission level</description>
              <bitRange>[12:11]</bitRange>
              <access>read-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>data register</description>
          <addressOffset>0xC</addressOffset>
          <fields>
            <field>
              <name>DR</name>
              <description>Data register</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>SYSCFG</name>
      <description>System configuration controller</description>
      <groupName>SYSCFG</groupName>
      <baseAddress>0x40010000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x30</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CFGR1</name>
          <displayName>CFGR1</displayName>
          <description>SYSCFG configuration register1</description>
          <addressOffset>0x0</addressOffset>
          <fields>
            <field>
              <name>MEM_MODE</name>
              <description>Memory mapping selectionbits</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>I2C_PA2_ANF</name>
              <description>Analog filter enable control driving capabilityactivation bits PA2</description>
              <bitRange>[18:18]</bitRange>
            </field>
            <field>
              <name>I2C_PA3_ANF</name>
              <description>Analog filter enable control driving capabilityactivation bits PA3</description>
              <bitRange>[19:19]</bitRange>
            </field>
            <field>
              <name>I2C_PA7_ANF</name>
              <description>Analog filter enable control driving capabilityactivation bits PA7</description>
              <bitRange>[20:20]</bitRange>
            </field>
            <field>
              <name>I2C_PA8_ANF</name>
              <description>Analog filter enable control driving capabilityactivation bits PA8</description>
              <bitRange>[21:21]</bitRange>
            </field>
            <field>
              <name>I2C_PA9_ANF</name>
              <description>Analog filter enable control driving capabilityactivation bits PA9</description>
              <bitRange>[22:22]</bitRange>
            </field>
            <field>
              <name>I2C_PA10_ANF</name>
              <description>Analog filter enable control driving capabilityactivation bits PA10</description>
              <bitRange>[23:23]</bitRange>
            </field>
            <field>
              <name>I2C_PA11_ANF</name>
              <description>Analog filter enable control driving capabilityactivation bits PA11</description>
              <bitRange>[24:24]</bitRange>
            </field>
            <field>
              <name>I2C_PA12_ANF</name>
              <description>Analog filter enable control driving capabilityactivation bits PA12</description>
              <bitRange>[25:25]</bitRange>
            </field>
            <field>
              <name>I2C_PB6_ANF</name>
              <description>Analog filter enable control driving capabilityactivation bits PB6</description>
              <bitRange>[26:26]</bitRange>
            </field>
            <field>
              <name>I2C_PB7_ANF</name>
              <description>Analog filter enable control driving capabilityactivation bits PB7</description>
              <bitRange>[27:27]</bitRange>
            </field>
            <field>
              <name>I2C_PB8_ANF</name>
              <description>Analog filter enable control driving capabilityactivation bits PB8</description>
              <bitRange>[28:28]</bitRange>
            </field>
            <field>
              <name>I2C_PF0_ANF</name>
              <description>Analog filter enable control driving capabilityactivation bits PF0</description>
              <bitRange>[29:29]</bitRange>
            </field>
            <field>
              <name>I2C_PF1_ANF</name>
              <description>Analog filter enable control driving capabilityactivation bits PF1</description>
              <bitRange>[30:30]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR2</name>
          <displayName>CFGR2</displayName>
          <description>SYSCFG configuration register2</description>
          <addressOffset>0x18</addressOffset>
          <fields>
            <field>
              <name>LOCKUP_LOCK</name>
              <description>Cortex-M0+ LOCKUP bit enablebit</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>ETR_SRC_TIM1</name>
              <description>TIM1 ETR source selection</description>
              <bitRange>[10:9]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>TIM1</name>
      <description>Advanced timer</description>
      <groupName>TIM</groupName>
      <baseAddress>0x40012C00</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>TIM1_BRK_UP_TRG_COM</name>
        <description>TIM1 Break, Update, Trigger and Commutation Interrupt</description>
        <value>13</value>
      </interrupt>
      <interrupt>
        <name>TIM1_CC</name>
        <description>TIM1 Capture Compare Interrupt</description>
        <value>14</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>control register 1</description>
          <addressOffset>0x0</addressOffset>
          <fields>
            <field>
              <name>CEN</name>
              <description>Counter enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>UDIS</name>
              <description>Update disable</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>URS</name>
              <description>Update request source</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>OPM</name>
              <description>One-pulse mode</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>DIR</name>
              <description>Direction</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>CMS</name>
              <description>Center-aligned modeselection</description>
              <bitRange>[6:5]</bitRange>
            </field>
            <field>
              <name>ARPE</name>
              <description>Auto-reload preload enable</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>CKD</name>
              <description>Clock division</description>
              <bitRange>[9:8]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>control register 2</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>CCPC</name>
              <description>Capture/compare preloadedcontrol</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>CCUS</name>
              <description>Capture/compare control updateselection</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>MMS</name>
              <description>Master mode selection</description>
              <bitRange>[6:4]</bitRange>
            </field>
            <field>
              <name>TI1S</name>
              <description>TI1 selection</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>OIS1</name>
              <description>Output Idle state 1</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>OIS1N</name>
              <description>Output Idle state 1</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>OIS2</name>
              <description>Output Idle state 2</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>OIS2N</name>
              <description>Output Idle state 2</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>OIS3</name>
              <description>Output Idle state 3</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>OIS3N</name>
              <description>Output Idle state 3</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>OIS4</name>
              <description>Output Idle state 4</description>
              <bitRange>[14:14]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SMCR</name>
          <displayName>SMCR</displayName>
          <description>slave mode control register</description>
          <addressOffset>0x8</addressOffset>
          <fields>
            <field>
              <name>SMS</name>
              <description>Slave mode selection</description>
              <bitRange>[2:0]</bitRange>
            </field>
            <field>
              <name>OCCS</name>
              <description>OCREF clear selection bit</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>TS</name>
              <description>Trigger selection</description>
              <bitRange>[6:4]</bitRange>
            </field>
            <field>
              <name>MSM</name>
              <description>Master/Slave mode</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>ETF</name>
              <description>External trigger filter</description>
              <bitRange>[11:8]</bitRange>
            </field>
            <field>
              <name>ETPS</name>
              <description>External trigger prescaler</description>
              <bitRange>[13:12]</bitRange>
            </field>
            <field>
              <name>ECE</name>
              <description>External clock enable</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>ETP</name>
              <description>External trigger polarity</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>DIER</name>
          <displayName>DIER</displayName>
          <description>DMA/Interrupt enable register</description>
          <addressOffset>0xC</addressOffset>
          <fields>
            <field>
              <name>UIE</name>
              <description>Update interrupt enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>CC1IE</name>
              <description>Capture/Compare 1 interruptenable</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>CC2IE</name>
              <description>Capture/Compare 2 interruptenable</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>CC3IE</name>
              <description>Capture/Compare 3 interruptenable</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>CC4IE</name>
              <description>Capture/Compare 4 interruptenable</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>COMIE</name>
              <description>COM interrupt enable</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>TIE</name>
              <description>Trigger interrupt enable</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>BIE</name>
              <description>Break interrupt enable</description>
              <bitRange>[7:7]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x10</addressOffset>
          <fields>
            <field>
              <name>UIF</name>
              <description>Update interrupt flag</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>CC1IF</name>
              <description>Capture/compare 1 interruptflag</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>CC2IF</name>
              <description>Capture/Compare 2 interruptflag</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>CC3IF</name>
              <description>Capture/Compare 3 interruptflag</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>CC4IF</name>
              <description>Capture/Compare 4 interruptflag</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>COMIF</name>
              <description>COM interrupt flag</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>TIF</name>
              <description>Trigger interrupt flag</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>BIF</name>
              <description>Break interrupt flag</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>CC1OF</name>
              <description>Capture/Compare 1 overcaptureflag</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>CC2OF</name>
              <description>Capture/compare 2 overcaptureflag</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>CC3OF</name>
              <description>Capture/Compare 3 overcaptureflag</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>CC4OF</name>
              <description>Capture/Compare 4 overcaptureflag</description>
              <bitRange>[12:12]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>EGR</name>
          <displayName>EGR</displayName>
          <description>event generation register</description>
          <addressOffset>0x14</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>UG</name>
              <description>Update generation</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>CC1G</name>
              <description>Capture/compare 1generation</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>CC2G</name>
              <description>Capture/compare 2generation</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>CC3G</name>
              <description>Capture/compare 3generation</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>CC4G</name>
              <description>Capture/compare 4generation</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>COMG</name>
              <description>Capture/Compare control updategeneration</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>TG</name>
              <description>Trigger generation</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>BG</name>
              <description>Break generation</description>
              <bitRange>[7:7]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_Output</name>
          <displayName>CCMR1_Output</displayName>
          <description>capture/compare mode register (outputmode)</description>
          <addressOffset>0x18</addressOffset>
          <fields>
            <field>
              <name>CC1S</name>
              <description>Capture/Compare 1selection</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>OC1FE</name>
              <description>Output Compare 1 fastenable</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>OC1PE</name>
              <description>Output Compare 1 preloadenable</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>OC1M</name>
              <description>Output Compare 1 mode</description>
              <bitRange>[6:4]</bitRange>
            </field>
            <field>
              <name>OC1CE</name>
              <description>Output Compare 1 clearenable</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>CC2S</name>
              <description>Capture/Compare 2selection</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>OC2FE</name>
              <description>Output Compare 2 fastenable</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>OC2PE</name>
              <description>Output Compare 2 preloadenable</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>OC2M</name>
              <description>Output Compare 2 mode</description>
              <bitRange>[14:12]</bitRange>
            </field>
            <field>
              <name>OC2CE</name>
              <description>Output Compare 2 clearenable</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_Input</name>
          <displayName>CCMR1_Input</displayName>
          <description>capture/compare mode register 1 (inputmode)</description>
          <alternateRegister>CCMR1_Output</alternateRegister>
          <addressOffset>0x18</addressOffset>
          <fields>
            <field>
              <name>CC1S</name>
              <description>Capture/Compare 1selection</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>ICPSC</name>
              <description>Input capture 1 prescaler</description>
              <bitRange>[3:2]</bitRange>
            </field>
            <field>
              <name>IC1F</name>
              <description>Input capture 1 filter</description>
              <bitRange>[7:4]</bitRange>
            </field>
            <field>
              <name>CC2S</name>
              <description>Capture/Compare 2selection</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>IC2PSC</name>
              <description>Input capture 2 prescaler</description>
              <bitRange>[11:10]</bitRange>
            </field>
            <field>
              <name>IC2F</name>
              <description>Input capture 2 filter</description>
              <bitRange>[15:12]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR2_Output</name>
          <displayName>CCMR2_Output</displayName>
          <description>capture/compare mode register (outputmode)</description>
          <addressOffset>0x1C</addressOffset>
          <fields>
            <field>
              <name>CC3S</name>
              <description>Capture/Compare 3selection</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>OC3FE</name>
              <description>Output compare 3 fastenable</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>OC3PE</name>
              <description>Output compare 3 preloadenable</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>OC3M</name>
              <description>Output compare 3 mode</description>
              <bitRange>[6:4]</bitRange>
            </field>
            <field>
              <name>OC3CE</name>
              <description>Output compare 3 clearenable</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>CC4S</name>
              <description>Capture/Compare 4selection</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>OC4FE</name>
              <description>Output compare 4 fastenable</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>OC4PE</name>
              <description>Output compare 4 preloadenable</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>OC4M</name>
              <description>Output compare 4 mode</description>
              <bitRange>[14:12]</bitRange>
            </field>
            <field>
              <name>OC4CE</name>
              <description>Output compare 4 clearenable</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR2_Input</name>
          <displayName>CCMR2_Input</displayName>
          <description>capture/compare mode register 2 (inputmode)</description>
          <alternateRegister>CCMR2_Output</alternateRegister>
          <addressOffset>0x1C</addressOffset>
          <fields>
            <field>
              <name>CC3S</name>
              <description>Capture/compare 3selection</description>
              <bitRange>[1:0]</bitRange>
            </field>
            <field>
              <name>IC3PSC</name>
              <description>Input capture 3 prescaler</description>
              <bitRange>[3:2]</bitRange>
            </field>
            <field>
              <name>IC3F</name>
              <description>Input capture 3 filter</description>
              <bitRange>[7:4]</bitRange>
            </field>
            <field>
              <name>CC4S</name>
              <description>Capture/Compare 4selection</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>IC4PSC</name>
              <description>Input capture 4 prescaler</description>
              <bitRange>[11:10]</bitRange>
            </field>
            <field>
              <name>IC4F</name>
              <description>Input capture 4 filter</description>
              <bitRange>[15:12]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCER</name>
          <displayName>CCER</displayName>
          <description>capture/compare enableregister</description>
          <addressOffset>0x20</addressOffset>
          <fields>
            <field>
              <name>CC1E</name>
              <description>Capture/Compare 1 outputenable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>CC1P</name>
              <description>Capture/Compare 1 outputPolarity</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>CC1NE</name>
              <description>Capture/Compare 1 complementary outputenable</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>CC1NP</name>
              <description>Capture/Compare 1 outputPolarity</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>CC2E</name>
              <description>Capture/Compare 2 outputenable</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>CC2P</name>
              <description>Capture/Compare 2 outputPolarity</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>CC2NE</name>
              <description>Capture/Compare 2 complementary outputenable</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>CC2NP</name>
              <description>Capture/Compare 2 outputPolarity</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>CC3E</name>
              <description>Capture/Compare 3 outputenable</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>CC3P</name>
              <description>Capture/Compare 3 outputPolarity</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>CC3NE</name>
              <description>Capture/Compare 3 complementary outputenable</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>CC3NP</name>
              <description>Capture/Compare 3 outputPolarity</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>CC4E</name>
              <description>Capture/Compare 4 outputenable</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>CC4P</name>
              <description>Capture/Compare 3 outputPolarity</description>
              <bitRange>[13:13]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <displayName>CNT</displayName>
          <description>counter</description>
          <addressOffset>0x24</addressOffset>
          <fields>
            <field>
              <name>CNT</name>
              <description>counter value</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PSC</name>
          <displayName>PSC</displayName>
          <description>prescaler</description>
          <addressOffset>0x28</addressOffset>
          <fields>
            <field>
              <name>PSC</name>
              <description>Prescaler value</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <displayName>ARR</displayName>
          <description>auto-reload register</description>
          <addressOffset>0x2C</addressOffset>
          <fields>
            <field>
              <name>ARR</name>
              <description>Auto-reload value</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>RCR</name>
          <displayName>RCR</displayName>
          <description>repetition counter register</description>
          <addressOffset>0x30</addressOffset>
          <fields>
            <field>
              <name>REP</name>
              <description>Repetition counter value</description>
              <bitRange>[7:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR1</name>
          <displayName>CCR1</displayName>
          <description>capture/compare register 1</description>
          <addressOffset>0x34</addressOffset>
          <fields>
            <field>
              <name>CCR1</name>
              <description>Capture/Compare 1 value</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR2</name>
          <displayName>CCR2</displayName>
          <description>capture/compare register 2</description>
          <addressOffset>0x38</addressOffset>
          <fields>
            <field>
              <name>CCR2</name>
              <description>Capture/Compare 2 value</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR3</name>
          <displayName>CCR3</displayName>
          <description>capture/compare register 3</description>
          <addressOffset>0x3C</addressOffset>
          <fields>
            <field>
              <name>CCR3</name>
              <description>Capture/Compare value</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR4</name>
          <displayName>CCR4</displayName>
          <description>capture/compare register 4</description>
          <addressOffset>0x40</addressOffset>
          <fields>
            <field>
              <name>CCR4</name>
              <description>Capture/Compare value</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>BDTR</name>
          <displayName>BDTR</displayName>
          <description>break and dead-time register</description>
          <addressOffset>0x44</addressOffset>
          <fields>
            <field>
              <name>DTG</name>
              <description>Dead-time generator setup</description>
              <bitRange>[7:0]</bitRange>
            </field>
            <field>
              <name>LOCK</name>
              <description>Lock configuration</description>
              <bitRange>[9:8]</bitRange>
            </field>
            <field>
              <name>OSSI</name>
              <description>Off-state selection for Idlemode</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>OSSR</name>
              <description>Off-state selection for Runmode</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>BKE</name>
              <description>Break enable</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>BKP</name>
              <description>Break polarity</description>
              <bitRange>[13:13]</bitRange>
            </field>
            <field>
              <name>AOE</name>
              <description>Automatic output enable</description>
              <bitRange>[14:14]</bitRange>
            </field>
            <field>
              <name>MOE</name>
              <description>Main output enable</description>
              <bitRange>[15:15]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>TIM16</name>
      <description>General purpose timer</description>
      <groupName>TIM</groupName>
      <baseAddress>0x40014400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>TIM16</name>
        <description>TIM16 global Interrupt</description>
        <value>21</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>TIM16 control register1</description>
          <addressOffset>0x0</addressOffset>
          <fields>
            <field>
              <name>CEN</name>
              <description>Counter enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>UDIS</name>
              <description>Update disable</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>URS</name>
              <description>Update request source</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>OPM</name>
              <description>One pulse mode</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>ARPE</name>
              <description>Auto-reload preload enable</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>CKD</name>
              <description>Prescaler factor</description>
              <bitRange>[9:8]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>DIER</name>
          <displayName>DIER</displayName>
          <description>DMA/Interrupt enable register</description>
          <addressOffset>0xC</addressOffset>
          <fields>
            <field>
              <name>UIE</name>
              <description>Update interrupt enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x10</addressOffset>
          <fields>
            <field>
              <name>UIF</name>
              <description>Update interrupt flag</description>
              <bitRange>[0:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>EGR</name>
          <displayName>EGR</displayName>
          <description>event generation register</description>
          <addressOffset>0x14</addressOffset>
          <access>write-only</access>
          <fields>
            <field>
              <name>UG</name>
              <description>Update generation</description>
              <bitRange>[0:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <displayName>CNT</displayName>
          <description>counter</description>
          <addressOffset>0x24</addressOffset>
          <fields>
            <field>
              <name>CNT</name>
              <description>counter value</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>PSC</name>
          <displayName>PSC</displayName>
          <description>prescaler</description>
          <addressOffset>0x28</addressOffset>
          <fields>
            <field>
              <name>PSC</name>
              <description>Prescaler value</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <displayName>ARR</displayName>
          <description>auto-reload register</description>
          <addressOffset>0x2C</addressOffset>
          <fields>
            <field>
              <name>ARR</name>
              <description>Auto-reload value</description>
              <bitRange>[15:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>RCR</name>
          <displayName>RCR</displayName>
          <description>repetition counter register</description>
          <addressOffset>0x30</addressOffset>
          <fields>
            <field>
              <name>REP</name>
              <description>Repetition counter value</description>
              <bitRange>[7:0]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>USART1</name>
      <description>Universal synchronous asynchronous receivertransmitter</description>
      <groupName>USART</groupName>
      <baseAddress>0x40013800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>USART1</name>
        <description>USART1 global Interrupt</description>
        <value>27</value>
      </interrupt>
      <registers>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>Status register</description>
          <addressOffset>0x0</addressOffset>
          <resetValue>0xC0</resetValue>
          <fields>
            <field>
              <name>PE</name>
              <description>Parity error</description>
              <bitRange>[0:0]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>FE</name>
              <description>Framing error</description>
              <bitRange>[1:1]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>NE</name>
              <description>Noise error flag</description>
              <bitRange>[2:2]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>ORE</name>
              <description>Overrun error</description>
              <bitRange>[3:3]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>IDLE</name>
              <description>IDLE line detected</description>
              <bitRange>[4:4]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>RXNE</name>
              <description>Read data register notempty</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>TC</name>
              <description>Transmission complete</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>TXE</name>
              <description>Transmit data registerempty</description>
              <bitRange>[7:7]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>CTS</name>
              <description>CTS flag</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>ABRF</name>
              <description>Automate baudrate detection flag</description>
              <bitRange>[10:10]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>ABRE</name>
              <description>Automate baudrate detection error flag</description>
              <bitRange>[11:11]</bitRange>
              <access>read-only</access>
            </field>
            <field>
              <name>ABRRQ</name>
              <description>Automate baudrate detection requeset</description>
              <bitRange>[12:12]</bitRange>
              <access>write-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>Data register</description>
          <addressOffset>0x4</addressOffset>
          <fields>
            <field>
              <name>DR</name>
              <description>Data value</description>
              <bitRange>[8:0]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>BRR</name>
          <displayName>BRR</displayName>
          <description>Baud rate register</description>
          <addressOffset>0x8</addressOffset>
          <fields>
            <field>
              <name>DIV_Fraction</name>
              <description>fraction of USARTDIV</description>
              <bitRange>[3:0]</bitRange>
            </field>
            <field>
              <name>DIV_Mantissa</name>
              <description>mantissa of USARTDIV</description>
              <bitRange>[15:4]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>Control register 1</description>
          <addressOffset>0xC</addressOffset>
          <fields>
            <field>
              <name>SBK</name>
              <description>Send break</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>RWU</name>
              <description>Receiver wakeup</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>RE</name>
              <description>Receiver enable</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>TE</name>
              <description>Transmitter enable</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>IDLEIE</name>
              <description>IDLE interrupt enable</description>
              <bitRange>[4:4]</bitRange>
            </field>
            <field>
              <name>RXNEIE</name>
              <description>RXNE interrupt enable</description>
              <bitRange>[5:5]</bitRange>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transmission complete interruptenable</description>
              <bitRange>[6:6]</bitRange>
            </field>
            <field>
              <name>TXEIE</name>
              <description>TXE interrupt enable</description>
              <bitRange>[7:7]</bitRange>
            </field>
            <field>
              <name>PEIE</name>
              <description>PE interrupt enable</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>PS</name>
              <description>Parity selection</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>PCE</name>
              <description>Parity control enable</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>WAKE</name>
              <description>Wakeup method</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>M</name>
              <description>Word length</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>UE</name>
              <description>USART enable</description>
              <bitRange>[13:13]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>Control register 2</description>
          <addressOffset>0x10</addressOffset>
          <fields>
            <field>
              <name>ADD</name>
              <description>Address of the USART node</description>
              <bitRange>[3:0]</bitRange>
            </field>
            <field>
              <name>LBCL</name>
              <description>Last bit clock pulse</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>CPHA</name>
              <description>Clock phase</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>CPOL</name>
              <description>Clock polarity</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>CLKEN</name>
              <description>Clock enable</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>STOP</name>
              <description>STOP bits</description>
              <bitRange>[13:12]</bitRange>
            </field>
          </fields>
        </register>
        <register>
          <name>CR3</name>
          <displayName>CR3</displayName>
          <description>Control register 3</description>
          <addressOffset>0x14</addressOffset>
          <fields>
            <field>
              <name>EIE</name>
              <description>Error interrupt enable</description>
              <bitRange>[0:0]</bitRange>
            </field>
            <field>
              <name>IREN</name>
              <description>IrDA mode enable</description>
              <bitRange>[1:1]</bitRange>
            </field>
            <field>
              <name>IRLP</name>
              <description>IrDA low-power</description>
              <bitRange>[2:2]</bitRange>
            </field>
            <field>
              <name>HDSEL</name>
              <description>Half-duplex selection</description>
              <bitRange>[3:3]</bitRange>
            </field>
            <field>
              <name>RTSE</name>
              <description>RTS enable</description>
              <bitRange>[8:8]</bitRange>
            </field>
            <field>
              <name>CTSE</name>
              <description>CTS enable</description>
              <bitRange>[9:9]</bitRange>
            </field>
            <field>
              <name>CTSIE</name>
              <description>CTS interrupt enable</description>
              <bitRange>[10:10]</bitRange>
            </field>
            <field>
              <name>OVER8</name>
              <description>Oversampling mode</description>
              <bitRange>[11:11]</bitRange>
            </field>
            <field>
              <name>ABREN</name>
              <description>Auto baudrate enable</description>
              <bitRange>[12:12]</bitRange>
            </field>
            <field>
              <name>ABRMOD</name>
              <description>Auto baudrate mode</description>
              <bitRange>[14:13]</bitRange>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
  </peripherals>
</device>