###############################################################################
#
# IAR ELF Linker V9.40.1.364/W64 for ARM                  28/Mar/2025  14:13:20
# Copyright 2007-2023 IAR Systems AB.
#
#    Output file  =
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Exe\Project.out
#    Map file     =
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\List\Project.map
#    Command line =
#        -f
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Exe\Project.out.rsp
#        (D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir\Can_User.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir\Emulated_EEPROM.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir\Emulated_EEPROM_Access.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir\Flash_test.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir\Flash_User.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir\main.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir\NVS_Test.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_adc.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_adc_ex.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_can.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_comp.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_cortex.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_crc.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_ctc.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_dac.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_dac_ex.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_div.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_dma.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_exti.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_flash.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_gpio.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_i2c.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_i2s.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_irda.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_iwdg.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_lcd.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_lptim.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir\py32f072c_hal_msp.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_opa.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_opa_ex.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir\py32f072c_hal_opt.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_pwr.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_rcc.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_rcc_ex.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_rtc.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_rtc_ex.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_smartcard.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_spi.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_tim.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_tim_ex.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_uart.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_usart.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_hal_wwdg.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir\py32f072c_it.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_adc.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_comp.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_crc.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_ctc.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_dac.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_dma.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_exti.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_gpio.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_i2c.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_lcd.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_lptim.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_pwr.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_rcc.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_rtc.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_spi.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_tim.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_usart.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir\py32f072c_ll_utils.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072Cxx_Start_Kit_5388743466937382780.dir\py32f072cxx_Start_Kit.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\EWARM_7214922893274846302.dir\startup_py32f072cxx.o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\CMSIS_6603591812247902717.dir\system_py32f072c.o
#        --no_out_extension -o
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Exe\Project.out
#        --map
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\List\Project.map
#        --config
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\py32f072cxB_flash.icf
#        --semihosting --entry __iar_program_start --vfe --text_out locale
#        --cpu=Cortex-M0+ --fpu=None) --dependencies=n
#        D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Exe\Project.out.iar_deps
#
###############################################################################

*******************************************************************************
*** RUNTIME MODEL ATTRIBUTES
***

CppFlavor       = *
__CPP_Runtime   = 1
__SystemLibrary = DLib
__dlib_version  = 6


*******************************************************************************
*** HEAP SELECTION
***

The basic heap was selected because --advanced_heap
was not specified and the application did not appear to
be primarily optimized for speed.


*******************************************************************************
*** PLACEMENT SUMMARY
***

"A0":  place at address 0x800'0000 { ro section .intvec };
"P1":  place in [from 0x800'0000 to 0x801'ffff] { ro };
define block CSTACK with size = 1K, alignment = 8 { };
define block HEAP with size = 512, alignment = 8 { };
"P2":  place in [from 0x2000'0000 to 0x2000'3fff] {
          rw, block CSTACK, block HEAP };
initialize by copy { rw };

  Section            Kind         Address    Size  Object
  -------            ----         -------    ----  ------
"A0":                                        0xc0
  .intvec            ro code   0x800'0000    0xc0  startup_py32f072cxx.o [2]
                             - 0x800'00c0    0xc0

"P1":                                      0x2d6c
  .text              ro code   0x800'00c0   0xa9c  Emulated_EEPROM_Access.o [5]
  .text              ro code   0x800'0b5c    0xe0  I32DivModFast.o [7]
  .text              ro code   0x800'0c3c     0x2  IntDivZer.o [7]
  .text              ro code   0x800'0c3e    0x3e  packbits_init_single.o [7]
  .text              ro code   0x800'0c7c   0x804  py32f072c_hal_rcc.o [3]
  .text              ro code   0x800'1480     0xc  py32f072c_hal.o [3]
  .text              ro code   0x800'148c    0x5c  py32f072c_hal.o [3]
  .text              ro code   0x800'14e8    0x34  ABImemcpy.o [7]
  .text              ro code   0x800'151c    0xf0  py32f072c_hal_cortex.o [3]
  .text              ro code   0x800'160c   0x560  py32f072c_hal_flash.o [3]
  .text              ro code   0x800'1b6c   0x3d4  py32f072c_hal_uart.o [3]
  .text              ro code   0x800'1f40     0x2  py32f072c_hal_uart.o [3]
  .rodata            const     0x800'1f42     0x2  py32f072cxx_Start_Kit.o [4]
  .text              ro code   0x800'1f44   0x1d4  py32f072cxx_Start_Kit.o [4]
  .text              ro code   0x800'2118   0x1c0  py32f072c_hal_gpio.o [3]
  .text              ro code   0x800'22d8   0x17c  xprintftiny.o [6]
  .text              ro code   0x800'2454     0xe  strlen.o [7]
  .rodata            const     0x800'2462     0x2  py32f072cxx_Start_Kit.o [4]
  .text              ro code   0x800'2464   0x170  Flash_User.o [5]
  .text              ro code   0x800'25d4    0x4e  ABImemset.o [7]
  .text              ro code   0x800'2622     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2624    0x28  printf.o [6]
  .text              ro code   0x800'264c   0x13c  main.o [5]
  .text              ro code   0x800'2788    0x1c  py32f072c_hal.o [3]
  .text              ro code   0x800'27a4    0x74  NVS_Test.o [5]
  .text              ro code   0x800'2818    0x7c  Emulated_EEPROM.o [5]
  .text              ro code   0x800'2894    0x14  memset.o [7]
  .text              ro code   0x800'28a8    0x34  py32f072c_hal_msp.o [5]
  .rodata            const     0x800'28dc   0x100  Emulated_EEPROM_Access.o [5]
  .rodata            const     0x800'29dc   0x100  Emulated_EEPROM_Access.o [5]
  .rodata            const     0x800'2adc    0x40  system_py32f072c.o [1]
  .text              ro code   0x800'2b1c    0x3c  system_py32f072c.o [1]
  .text              ro code   0x800'2b58    0x3c  zero_init3.o [7]
  .rodata            const     0x800'2b94    0x34  main.o [5]
  .rodata            const     0x800'2bc8    0x30  Flash_User.o [5]
  .text              ro code   0x800'2bf8    0x28  data_init.o [7]
  .rodata            const     0x800'2c20    0x24  main.o [5]
  .iar.init_table    const     0x800'2c44    0x20  - Linker created -
  .rodata            const     0x800'2c64    0x20  py32f072c_hal_flash.o [3]
  .rodata            const     0x800'2c84    0x20  system_py32f072c.o [1]
  .rodata            const     0x800'2ca4    0x20  system_py32f072c.o [1]
  .text              ro code   0x800'2cc4    0x1e  cmain.o [7]
  .text              ro code   0x800'2ce2     0x4  low_level_init.o [6]
  .text              ro code   0x800'2ce6     0x8  exit.o [6]
  .text              ro code   0x800'2cee     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2cf0     0xa  cexit.o [7]
  .text              ro code   0x800'2cfa     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2cfc    0x14  exit.o [8]
  .text              ro code   0x800'2d10    0x1c  cstartup_M.o [7]
  .text              ro code   0x800'2d2c    0x18  py32f072c_hal.o [3]
  .text              ro code   0x800'2d44    0x16  xprout.o [6]
  .text              ro code   0x800'2d5a     0x2  startup_py32f072cxx.o [2]
  .rodata            const     0x800'2d5c    0x14  Emulated_EEPROM.o [5]
  .rodata            const     0x800'2d70    0x14  py32f072c_hal_rcc.o [3]
  .text              ro code   0x800'2d84    0x12  py32f072c_it.o [5]
  .text              ro code   0x800'2d96     0x2  startup_py32f072cxx.o [2]
  .rodata            const     0x800'2d98    0x10  py32f072c_hal_rcc.o [3]
  .text              ro code   0x800'2da8    0x10  startup_py32f072cxx.o [2]
  .rodata            const     0x800'2db8     0x8  main.o [5]
  .rodata            const     0x800'2dc0     0x8  py32f072c_hal_rcc.o [3]
  .rodata            const     0x800'2dc8     0x8  py32f072c_hal_rcc.o [3]
  .text              ro code   0x800'2dd0     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2dd2     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2dd4     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2dd6     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2dd8     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2dda     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2ddc     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2dde     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2de0     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2de2     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2de4     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2de6     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2de8     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2dea     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2dec     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2dee     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2df0     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2df2     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2df4     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2df6     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2df8     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2dfa     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2dfc     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2dfe     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2e00     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2e02     0x2  startup_py32f072cxx.o [2]
  .text              ro code   0x800'2e04     0x2  startup_py32f072cxx.o [2]
  .rodata            const     0x800'2e06     0x1  py32f072cxx_Start_Kit.o [4]
  .rodata            const     0x800'2e07     0x0  zero_init3.o [7]
  .rodata            const     0x800'2e07     0x0  packbits_init_single.o [7]
  Initializer bytes  const     0x800'2e07    0x25  <for P2-1>
                             - 0x800'2e2c  0x2d6c

"P2", part 1 of 3:                           0x35
  P2-1                        0x2000'0000    0x35  <Init block>
    .data            inited   0x2000'0000    0x20  Flash_test.o [5]
    .data            inited   0x2000'0020     0x4  py32f072c_hal.o [3]
    .data            inited   0x2000'0024     0x4  py32f072c_hal.o [3]
    .data            inited   0x2000'0028     0x4  py32f072cxx_Start_Kit.o [4]
    .data            inited   0x2000'002c     0x4  py32f072cxx_Start_Kit.o [4]
    .data            inited   0x2000'0030     0x4  system_py32f072c.o [1]
    .data            inited   0x2000'0034     0x1  NVS_Test.o [5]
                            - 0x2000'0035    0x35

"P2", part 2 of 3:                          0x2e8
  .bss               zero     0x2000'0038   0x100  Emulated_EEPROM.o [5]
  .bss               zero     0x2000'0138   0x100  Flash_User.o [5]
  .bss               zero     0x2000'0238    0x4c  py32f072cxx_Start_Kit.o [4]
  .bss               zero     0x2000'0284    0x20  main.o [5]
  .bss               zero     0x2000'02a4    0x18  Emulated_EEPROM.o [5]
  .bss               zero     0x2000'02bc    0x18  py32f072c_hal_flash.o [3]
  .bss               zero     0x2000'02d4    0x10  Emulated_EEPROM_Access.o [5]
  .bss               zero     0x2000'02e4     0x4  Emulated_EEPROM_Access.o [5]
  .bss               zero     0x2000'02e8     0x4  Emulated_EEPROM_Access.o [5]
  .bss               zero     0x2000'02ec     0x4  Emulated_EEPROM_Access.o [5]
  .bss               zero     0x2000'02f0     0x4  Emulated_EEPROM_Access.o [5]
  .bss               zero     0x2000'02f4     0x4  Emulated_EEPROM_Access.o [5]
  .bss               zero     0x2000'02f8     0x4  NVS_Test.o [5]
  .bss               zero     0x2000'02fc     0x4  NVS_Test.o [5]
  .bss               zero     0x2000'0300     0x4  NVS_Test.o [5]
  .bss               zero     0x2000'0304     0x4  NVS_Test.o [5]
  .bss               zero     0x2000'0308     0x4  NVS_Test.o [5]
  .bss               zero     0x2000'030c     0x4  NVS_Test.o [5]
  .bss               zero     0x2000'0310     0x4  NVS_Test.o [5]
  .bss               zero     0x2000'0314     0x4  NVS_Test.o [5]
  .bss               zero     0x2000'0318     0x4  py32f072c_hal.o [3]
  .bss               zero     0x2000'031c     0x1  NVS_Test.o [5]
  .bss               zero     0x2000'031d     0x1  NVS_Test.o [5]
  .bss               zero     0x2000'031e     0x1  NVS_Test.o [5]
  .bss               zero     0x2000'031f     0x1  NVS_Test.o [5]
                            - 0x2000'0320   0x2e8

"P2", part 3 of 3:                          0x400
  CSTACK                      0x2000'0320   0x400  <Block>
    CSTACK           uninit   0x2000'0320   0x400  <Block tail>
                            - 0x2000'0720   0x400

Unused ranges:

         From           To      Size
         ----           --      ----
   0x800'2e2c   0x801'ffff  0x1'd1d4
  0x2000'0035  0x2000'0037       0x3
  0x2000'0720  0x2000'3fff    0x38e0


*******************************************************************************
*** INIT TABLE
***

          Address      Size
          -------      ----
Zero (__iar_zero_init3)
    1 destination range, total size 0x2e8:
          0x2000'0038  0x2e8

Copy/packbits (__iar_packbits_init_single3)
    1 source range, total size 0x25 (69% of destination):
           0x800'2e07   0x25
    1 destination range, total size 0x35:
          0x2000'0000   0x35



*******************************************************************************
*** MODULE SUMMARY
***

    Module                    ro code  ro data  rw data
    ------                    -------  -------  -------
command line/config:
    ---------------------------------------------------
    Total:

D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\CMSIS_6603591812247902717.dir: [1]
    system_py32f072c.o             60      131        4
    ---------------------------------------------------
    Total:                         60      131        4

D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\EWARM_7214922893274846302.dir: [2]
    startup_py32f072cxx.o         272
    ---------------------------------------------------
    Total:                        272

D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir: [3]
    py32f072c_hal.o               156        5       12
    py32f072c_hal_cortex.o        240
    py32f072c_hal_flash.o       1'376       32       24
    py32f072c_hal_gpio.o          448
    py32f072c_hal_rcc.o         2'052       52
    py32f072c_hal_uart.o          982
    ---------------------------------------------------
    Total:                      5'254       89       36

D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072Cxx_Start_Kit_5388743466937382780.dir: [4]
    py32f072cxx_Start_Kit.o       468       11       84
    ---------------------------------------------------
    Total:                        468       11       84

D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir: [5]
    Emulated_EEPROM.o             124       20      280
    Emulated_EEPROM_Access.o    2'716      512       36
    Flash_User.o                  368       48      256
    Flash_test.o                            22       32
    NVS_Test.o                    116        1       37
    main.o                        316       96       32
    py32f072c_hal_msp.o            52
    py32f072c_it.o                 18
    ---------------------------------------------------
    Total:                      3'710      699      673

dl6M_tln.a: [6]
    exit.o                          8
    low_level_init.o                4
    printf.o                       40
    xprintftiny.o                 380
    xprout.o                       22
    ---------------------------------------------------
    Total:                        454

rt6M_tl.a: [7]
    ABImemcpy.o                    52
    ABImemset.o                    78
    I32DivModFast.o               224
    IntDivZer.o                     2
    cexit.o                        10
    cmain.o                        30
    cstartup_M.o                   28
    data_init.o                    40
    memset.o                       20
    packbits_init_single.o         62
    strlen.o                       14
    zero_init3.o                   60
    ---------------------------------------------------
    Total:                        620

shb_l.a: [8]
    exit.o                         20
    ---------------------------------------------------
    Total:                         20

    Linker created                          32    1'024
-------------------------------------------------------
    Grand Total:               10'858      962    1'821


*******************************************************************************
*** ENTRY LIST
***

Entry                       Address   Size  Type      Object
-----                       -------   ----  ----      ------
.iar.init_table$$Base    0x800'2c44          --   Gb  - Linker created -
.iar.init_table$$Limit   0x800'2c64          --   Gb  - Linker created -
?main                    0x800'2cc5         Code  Gb  cmain.o [7]
ADC_COMP_IRQHandler      0x800'2ddf         Code  Wk  startup_py32f072cxx.o [2]
AHBPrescTable            0x800'2adc   0x40  Data  Gb  system_py32f072c.o [1]
APBPrescTable            0x800'2c84   0x20  Data  Gb  system_py32f072c.o [1]
APP_ErrorHandler         0x800'2785    0x4  Code  Gb  main.o [5]
APP_SystemClockConfig    0x800'26f9   0x6c  Code  Lc  main.o [5]
BSP_LED_Init             0x800'1f45   0x56  Code  Gb  py32f072cxx_Start_Kit.o [4]
BSP_LED_On               0x800'1f9b   0x1c  Code  Gb  py32f072cxx_Start_Kit.o [4]
BSP_PB_Init              0x800'1fb7   0x8a  Code  Gb  py32f072cxx_Start_Kit.o [4]
BSP_USART_Config         0x800'2041   0x9a  Code  Gb  py32f072cxx_Start_Kit.o [4]
BUTTON_IRQn              0x800'2e06    0x1  Data  Gb  py32f072cxx_Start_Kit.o [4]
BUTTON_PIN               0x800'2462    0x2  Data  Gb  py32f072cxx_Start_Kit.o [4]
BUTTON_PORT             0x2000'002c    0x4  Data  Gb  py32f072cxx_Start_Kit.o [4]
BenCiXieRu              0x2000'030c    0x4  Data  Gb  NVS_Test.o [5]
BenCiXieRuNum           0x2000'0310    0x4  Data  Gb  NVS_Test.o [5]
CAN_IRQHandler           0x800'2e03         Code  Wk  startup_py32f072cxx.o [2]
CAN_Received            0x2000'031c    0x1  Data  Gb  NVS_Test.o [5]
CSTACK$$Base            0x2000'0320          --   Gb  - Linker created -
CSTACK$$Limit           0x2000'0720          --   Gb  - Linker created -
DMA1_Channel1_IRQHandler
                         0x800'2dd9         Code  Wk  startup_py32f072cxx.o [2]
DMA1_Channel2_3_IRQHandler
                         0x800'2ddb         Code  Wk  startup_py32f072cxx.o [2]
DMA1_Channel4_5_6_7_IRQHandler
                         0x800'2ddd         Code  Wk  startup_py32f072cxx.o [2]
DebugUartHandle         0x2000'0238   0x4c  Data  Gb  py32f072cxx_Start_Kit.o [4]
EEPROM_Access_Init       0x800'00c1  0x68e  Code  Gb  Emulated_EEPROM_Access.o [5]
EEPROM_CRC_Calc          0x800'0af9   0x46  Code  Lc  Emulated_EEPROM_Access.o [5]
EEPROM_Init              0x800'2819   0x30  Code  Gb  Emulated_EEPROM.o [5]
EEPROM_Read_Block_Data   0x800'0755   0xac  Code  Gb  Emulated_EEPROM_Access.o [5]
EEPROM_Read_Data         0x800'2861   0x1a  Code  Gb  Emulated_EEPROM.o [5]
EEPROM_Write_Block_Data
                         0x800'080d  0x2ec  Code  Gb  Emulated_EEPROM_Access.o [5]
EEPROM_Write_Data        0x800'287b   0x1a  Code  Gb  Emulated_EEPROM.o [5]
EXTI0_1_IRQHandler       0x800'2dd1         Code  Wk  startup_py32f072cxx.o [2]
EXTI2_3_IRQHandler       0x800'2dd3         Code  Wk  startup_py32f072cxx.o [2]
EXTI4_15_IRQHandler      0x800'2dd5         Code  Wk  startup_py32f072cxx.o [2]
ErrNum                  0x2000'0034    0x1  Data  Gb  NVS_Test.o [5]
ErrNumDisplay           0x2000'031e    0x1  Data  Gb  NVS_Test.o [5]
FLASH_IRQHandler         0x800'2d5b         Code  Wk  startup_py32f072cxx.o [2]
FLASH_MassErase          0x800'1671   0x1a  Code  Lc  py32f072c_hal_flash.o [3]
FLASH_PageErase          0x800'168b   0x16  Code  Lc  py32f072c_hal_flash.o [3]
FLASH_Program_Page       0x800'16b3   0x40  Code  Lc  py32f072c_hal_flash.o [3]
FLASH_SectorErase        0x800'16a1   0x12  Code  Lc  py32f072c_hal_flash.o [3]
FLASH_WaitForLastOperation
                         0x800'164b   0x26  Code  Gb  py32f072c_hal_flash.o [3]
Flash_Data_CheckBlank    0x800'2545   0x88  Code  Gb  Flash_User.o [5]
Flash_Data_PageErase     0x800'24ff   0x46  Code  Gb  Flash_User.o [5]
Flash_Data_Read          0x800'2465   0x1c  Code  Gb  Flash_User.o [5]
Flash_Data_Write         0x800'2481   0x7e  Code  Gb  Flash_User.o [5]
Flash_Data_Write::copyData
                        0x2000'0138  0x100  Data  Lc  Flash_User.o [5]
HAL_FLASH_Erase          0x800'170d  0x246  Code  Gb  py32f072c_hal_flash.o [3]
HAL_FLASH_Lock           0x800'162f   0x1c  Code  Gb  py32f072c_hal_flash.o [3]
HAL_FLASH_Program        0x800'1995  0x1a2  Code  Gb  py32f072c_hal_flash.o [3]
HAL_FLASH_Unlock         0x800'160d   0x22  Code  Gb  py32f072c_hal_flash.o [3]
HAL_GPIO_Init            0x800'2119  0x190  Code  Gb  py32f072c_hal_gpio.o [3]
HAL_GPIO_WritePin        0x800'22b5   0x14  Code  Gb  py32f072c_hal_gpio.o [3]
HAL_GetTick              0x800'1481    0xc  Code  Wk  py32f072c_hal.o [3]
HAL_IncTick              0x800'2d2d   0x18  Code  Wk  py32f072c_hal.o [3]
HAL_Init                 0x800'2789   0x1c  Code  Gb  py32f072c_hal.o [3]
HAL_InitTick             0x800'148d   0x5c  Code  Wk  py32f072c_hal.o [3]
HAL_MspInit              0x800'28a9   0x2c  Code  Gb  py32f072c_hal_msp.o [5]
HAL_NVIC_EnableIRQ       0x800'15e1    0xa  Code  Gb  py32f072c_hal_cortex.o [3]
HAL_NVIC_SetPriority     0x800'15d7    0xa  Code  Gb  py32f072c_hal_cortex.o [3]
HAL_RCC_ClockConfig      0x800'11a5  0x176  Code  Gb  py32f072c_hal_rcc.o [3]
HAL_RCC_GetHCLKFreq      0x800'1405    0x6  Code  Gb  py32f072c_hal_rcc.o [3]
HAL_RCC_GetPCLK1Freq     0x800'1411   0x1e  Code  Gb  py32f072c_hal_rcc.o [3]
HAL_RCC_GetSysClockFreq
                         0x800'133d   0xc8  Code  Gb  py32f072c_hal_rcc.o [3]
HAL_RCC_OscConfig        0x800'0c7d  0x508  Code  Gb  py32f072c_hal_rcc.o [3]
HAL_SYSTICK_Config       0x800'15eb    0x8  Code  Gb  py32f072c_hal_cortex.o [3]
HAL_UART_Init            0x800'1b6d   0x84  Code  Gb  py32f072c_hal_uart.o [3]
HAL_UART_MspInit         0x800'1f41    0x2  Code  Wk  py32f072c_hal_uart.o [3]
HAL_UART_Transmit        0x800'1bf9   0xf0  Code  Gb  py32f072c_hal_uart.o [3]
HSIFreqTable             0x800'2ca4   0x20  Data  Gb  system_py32f072c.o [1]
HardFault_Handler        0x800'2d87    0x4  Code  Gb  py32f072c_it.o [5]
I2C1_IRQHandler          0x800'2df5         Code  Wk  startup_py32f072cxx.o [2]
I2C2_IRQHandler          0x800'2df7         Code  Wk  startup_py32f072cxx.o [2]
LCD_IRQHandler           0x800'2dd7         Code  Wk  startup_py32f072cxx.o [2]
LED_PIN                  0x800'1f42    0x2  Data  Gb  py32f072cxx_Start_Kit.o [4]
LED_PORT                0x2000'0028    0x4  Data  Gb  py32f072cxx_Start_Kit.o [4]
LastLastNum             0x2000'0300    0x4  Data  Gb  NVS_Test.o [5]
LastNum                 0x2000'02fc    0x4  Data  Gb  NVS_Test.o [5]
NMI_Handler              0x800'2d85    0x2  Code  Gb  py32f072c_it.o [5]
NVSReadInit             0x2000'031f    0x1  Data  Gb  NVS_Test.o [5]
NVSTestCountRead        0x2000'0308    0x4  Data  Gb  NVS_Test.o [5]
NVS_Init                 0x800'27a5   0x40  Code  Gb  NVS_Test.o [5]
PVD_IRQHandler           0x800'2cef         Code  Wk  startup_py32f072cxx.o [2]
PendSV_Handler           0x800'2d8d    0x2  Code  Gb  py32f072c_it.o [5]
RCC_GetHSIFreq           0x800'1449   0x12  Code  Lc  py32f072c_hal_rcc.o [3]
RCC_IRQHandler           0x800'2d97         Code  Wk  startup_py32f072cxx.o [2]
RTC_IRQHandler           0x800'2cfb         Code  Wk  startup_py32f072cxx.o [2]
Region$$Table$$Base      0x800'2c44          --   Gb  - Linker created -
Region$$Table$$Limit     0x800'2c64          --   Gb  - Linker created -
Reset_Handler            0x800'2da9         Code  Wk  startup_py32f072cxx.o [2]
SPI1_IRQHandler          0x800'2df9         Code  Wk  startup_py32f072cxx.o [2]
SPI2_IRQHandler          0x800'2dfb         Code  Wk  startup_py32f072cxx.o [2]
SVC_Handler              0x800'2d8b    0x2  Code  Gb  py32f072c_it.o [5]
SysTick_Config           0x800'15a7   0x30  Code  Lc  py32f072c_hal_cortex.o [3]
SysTick_Handler          0x800'2d8f    0x8  Code  Gb  py32f072c_it.o [5]
SystemCoreClock         0x2000'0030    0x4  Data  Gb  system_py32f072c.o [1]
SystemInit               0x800'2b1d   0x2a  Code  Gb  system_py32f072c.o [1]
TIM14_IRQHandler         0x800'2ded         Code  Wk  startup_py32f072cxx.o [2]
TIM15_IRQHandler         0x800'2def         Code  Wk  startup_py32f072cxx.o [2]
TIM16_IRQHandler         0x800'2df1         Code  Wk  startup_py32f072cxx.o [2]
TIM17_IRQHandler         0x800'2df3         Code  Wk  startup_py32f072cxx.o [2]
TIM1_BRK_UP_TRG_COM_IRQHandler
                         0x800'2de1         Code  Wk  startup_py32f072cxx.o [2]
TIM1_CC_IRQHandler       0x800'2de3         Code  Wk  startup_py32f072cxx.o [2]
TIM2_IRQHandler          0x800'2de5         Code  Wk  startup_py32f072cxx.o [2]
TIM3_IRQHandler          0x800'2de7         Code  Wk  startup_py32f072cxx.o [2]
TIM6_LPTIM1_DAC_IRQHandler
                         0x800'2de9         Code  Wk  startup_py32f072cxx.o [2]
TIM7_IRQHandler          0x800'2deb         Code  Wk  startup_py32f072cxx.o [2]
TestData2               0x2000'0000   0x20  Data  Gb  Flash_test.o [5]
UART_AdvFeatureConfig    0x800'1ef1   0x36  Code  Lc  py32f072c_hal_uart.o [3]
UART_SetConfig           0x800'1d55  0x19a  Code  Lc  py32f072c_hal_uart.o [3]
UART_WaitOnFlagUntilTimeout
                         0x800'1ce9   0x68  Code  Lc  py32f072c_hal_uart.o [3]
USART1_IRQHandler        0x800'2dfd         Code  Wk  startup_py32f072cxx.o [2]
USART2_IRQHandler        0x800'2dff         Code  Wk  startup_py32f072cxx.o [2]
USART3_4_IRQHandler      0x800'2e01         Code  Wk  startup_py32f072cxx.o [2]
USB_IRQHandler           0x800'2e05         Code  Wk  startup_py32f072cxx.o [2]
WWDG_IRQHandler          0x800'2623         Code  Wk  startup_py32f072cxx.o [2]
ZhiXingCiShu            0x2000'0304    0x4  Data  Gb  NVS_Test.o [5]
ZhiXingCiShuDisplay     0x2000'0314    0x4  Data  Gb  NVS_Test.o [5]
_FlashTimmingParam       0x800'2c64   0x20  Data  Gb  py32f072c_hal_flash.o [3]
_PrintfTiny              0x800'22f3  0x162  Code  Gb  xprintftiny.o [6]
_Prout                   0x800'2d45   0x16  Code  Gb  xprout.o [6]
__ICFEDIT_region_RAM_end__ {Abs}
                        0x2000'3fff         Data  Gb  <internal module>
__ICFEDIT_region_RAM_start__ {Abs}
                        0x2000'0000         Data  Gb  <internal module>
__NVIC_EnableIRQ         0x800'151d   0x18  Code  Lc  py32f072c_hal_cortex.o [3]
__NVIC_SetPriority       0x800'1535   0x72  Code  Lc  py32f072c_hal_cortex.o [3]
__aeabi_idiv             0x800'0b89         Code  Gb  I32DivModFast.o [7]
__aeabi_idiv0            0x800'0c3d         Code  Gb  IntDivZer.o [7]
__aeabi_idivmod          0x800'0b89         Code  Gb  I32DivModFast.o [7]
__aeabi_memcpy4          0x800'14e9         Code  Gb  ABImemcpy.o [7]
__aeabi_memcpy8          0x800'14e9         Code  Gb  ABImemcpy.o [7]
__aeabi_memset           0x800'25d5         Code  Gb  ABImemset.o [7]
__aeabi_uidiv            0x800'0b8f         Code  Gb  I32DivModFast.o [7]
__aeabi_uidivmod         0x800'0b8f         Code  Gb  I32DivModFast.o [7]
__cmain                  0x800'2cc5         Code  Gb  cmain.o [7]
__exit                   0x800'2cfd   0x14  Code  Gb  exit.o [8]
__iar_Memset4_word       0x800'25f5         Code  Gb  ABImemset.o [7]
__iar_Memset_word        0x800'25e1         Code  Gb  ABImemset.o [7]
__iar_data_init3         0x800'2bf9   0x28  Code  Gb  data_init.o [7]
__iar_packbits_init_single3
                         0x800'0c3f   0x3e  Code  Gb  packbits_init_single.o [7]
__iar_program_start      0x800'2d11         Code  Gb  cstartup_M.o [7]
__iar_zero_init3         0x800'2b59   0x3c  Code  Gb  zero_init3.o [7]
__low_level_init         0x800'2ce3    0x4  Code  Gb  low_level_init.o [6]
__vector_table           0x800'0000         Data  Gb  startup_py32f072cxx.o [2]
_call_main               0x800'2cd1         Code  Gb  cmain.o [7]
_exit                    0x800'2cf1         Code  Gb  cexit.o [7]
exit                     0x800'2ce7    0x8  Code  Gb  exit.o [6]
g_NVSTestStatus         0x2000'031d    0x1  Data  Gb  NVS_Test.o [5]
g_pfnEEPROMMemBlankCheck
                        0x2000'02ec    0x4  Data  Gb  Emulated_EEPROM_Access.o [5]
g_pfnEEPROMMemErase     0x2000'02e8    0x4  Data  Gb  Emulated_EEPROM_Access.o [5]
g_pfnEEPROMMemRead      0x2000'02f0    0x4  Data  Gb  Emulated_EEPROM_Access.o [5]
g_pfnEEPROMMemWrite     0x2000'02f4    0x4  Data  Gb  Emulated_EEPROM_Access.o [5]
g_pstEEPROMBlock        0x2000'02e4    0x4  Data  Gb  Emulated_EEPROM_Access.o [5]
g_stEEPROMAccess        0x2000'02d4   0x10  Data  Gb  Emulated_EEPROM_Access.o [5]
g_stEEPROMBlockAccess   0x2000'02a4   0x18  Data  Gb  Emulated_EEPROM.o [5]
g_stEEPROMBlockTable     0x800'2d5c   0x14  Data  Lc  Emulated_EEPROM.o [5]
g_u32EEPROMBlock0Buffer
                        0x2000'0038  0x100  Data  Gb  Emulated_EEPROM.o [5]
g_u8EEPROMCRCTableH      0x800'28dc  0x100  Data  Lc  Emulated_EEPROM_Access.o [5]
g_u8EEPROMCRCTableL      0x800'29dc  0x100  Data  Lc  Emulated_EEPROM_Access.o [5]
main                     0x800'264d   0xac  Code  Gb  main.o [5]
main::laji              0x2000'0284   0x20  Data  Lc  main.o [5]
memset                   0x800'2895   0x14  Code  Gb  memset.o [7]
out                      0x800'22d9   0x1a  Code  Lc  xprintftiny.o [6]
pFlash                  0x2000'02bc   0x18  Data  Gb  py32f072c_hal_flash.o [3]
printf                   0x800'2625   0x28  Code  Gb  printf.o [6]
putchar                  0x800'20db   0x14  Code  Gb  py32f072cxx_Start_Kit.o [4]
strlen                   0x800'2455         Code  Gb  strlen.o [7]
testnumhaha             0x2000'02f8    0x4  Data  Gb  NVS_Test.o [5]
uwTick                  0x2000'0318    0x4  Data  Gb  py32f072c_hal.o [3]
uwTickFreq              0x2000'0024    0x4  Data  Gb  py32f072c_hal.o [3]
uwTickPrio              0x2000'0020    0x4  Data  Gb  py32f072c_hal.o [3]


[1] = D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\CMSIS_6603591812247902717.dir
[2] = D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\EWARM_7214922893274846302.dir
[3] = D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072C_HAL_Driver_2501715651630984704.dir
[4] = D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072Cxx_Start_Kit_5388743466937382780.dir
[5] = D:\code\py32f072\PY32F072E_Firmware_V1.0.5\Projects\PY32F072C-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir
[6] = dl6M_tln.a
[7] = rt6M_tl.a
[8] = shb_l.a

  10'858 bytes of readonly  code memory
     962 bytes of readonly  data memory
   1'821 bytes of readwrite data memory

Errors: none
Warnings: none
