================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例演示了COMP比较器唤醒功能，PA0作为比较器正端输入，VREFINT作为比较器负端输
入，进入stop模式后，通过调整PA0上的输入电压，产生中断唤醒stop模式。

Function descriptions:
This example demonstrates the COMP comparator wake-up function, with PA0 as the
positive input and VREFINT as the negative input of the comparator. After
entering stop mode, the interrupt wake-up stop mode is generated by adjusting
the input voltage on PA0.
================================================================================
测试环境：
测试用板：PY32F072C_STK
MDK版本： 5.28
IAR版本： 9.20
GCC 版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32F072C_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤：
1. 编译下载程序到MCU，并运行；
2. LED亮起后按下按键，进入stop模式，LED熄灭；
3. 在PA0上输入从小于1.1V到的大于1.3V电压时，产生中断，LED点亮1s；
4. 接下来LED每隔200ms进行翻转，程序正常运行。

Example execution steps:
1.Compile and download the program to MCU and run it;
2.After the LED lights up, press the button to enter the stop mode, and the
LED goes out;
3.When inputting a voltage from less than 1.1V to greater than 1.3V on PA0, an
interrupt is generated and the LED lights up for 1 second;
4. Next, the LED flips every 200ms and the program runs normally
================================================================================
注意事项：


Notes:

================================================================================