###############################################################################
#
# IAR ELF Linker V9.40.1.364/W64 for ARM                  26/Feb/2025  15:57:02
# Copyright 2007-2023 IAR Systems AB.
#
#    Output file  =
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Exe\Project.out
#    Map file     =
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\List\Project.map
#    Command line =
#        -f
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Exe\Project.out.rsp
#        (D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir\main.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_cortex.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_dma.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_flash.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_gpio.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir\py32f072_hal_msp.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_pwr.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_rcc.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_rcc_ex.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir\py32f072_hal_uart.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir\py32f072_it.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072xx_Start_Kit_1292202923306237531.dir\py32f072xx_Start_Kit.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\EWARM_7214922893274846302.dir\startup_py32f072xx.o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\CMSIS_6603591812247902717.dir\system_py32f072.o
#        --no_out_extension -o
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Exe\Project.out
#        --map
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\List\Project.map
#        --config
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\py32f072xB_flash.icf
#        --semihosting --entry __iar_program_start --vfe --text_out locale
#        --cpu=Cortex-M0+ --fpu=None) --dependencies=n
#        D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Exe\Project.out.iar_deps
#
###############################################################################

*******************************************************************************
*** RUNTIME MODEL ATTRIBUTES
***

CppFlavor       = *
__CPP_Runtime   = 1
__SystemLibrary = DLib
__dlib_version  = 6


*******************************************************************************
*** HEAP SELECTION
***

The basic heap was selected because --advanced_heap
was not specified and the application did not appear to
be primarily optimized for speed.


*******************************************************************************
*** PLACEMENT SUMMARY
***

"A0":  place at address 0x800'0000 { ro section .intvec };
"P1":  place in [from 0x800'0000 to 0x801'ffff] { ro };
define block CSTACK with size = 1K, alignment = 8 { };
define block HEAP with size = 512, alignment = 8 { };
"P2":  place in [from 0x2000'0000 to 0x2000'3fff] {
          rw, block CSTACK, block HEAP };
initialize by copy { rw };

  Section            Kind         Address    Size  Object
  -------            ----         -------    ----  ------
"A0":                                        0xc0
  .intvec            ro code   0x800'0000    0xc0  startup_py32f072xx.o [2]
                             - 0x800'00c0    0xc0

"P1":                                      0x203b
  .text              ro code   0x800'00c0   0x804  py32f072_hal_rcc.o [3]
  .text              ro code   0x800'08c4     0xc  py32f072_hal.o [3]
  .text              ro code   0x800'08d0    0x5c  py32f072_hal.o [3]
  .text              ro code   0x800'092c    0x34  ABImemcpy.o [7]
  .text              ro code   0x800'0960    0xae  I32DivModFast.o [7]
  .rodata            const     0x800'0a0e     0x2  py32f072xx_Start_Kit.o [4]
  .text              ro code   0x800'0a10    0xf0  py32f072_hal_cortex.o [3]
  .text              ro code   0x800'0b00     0x2  IntDivZer.o [7]
  .rodata            const     0x800'0b02     0x2  py32f072xx_Start_Kit.o [4]
  .text              ro code   0x800'0b04   0x560  py32f072_hal_flash.o [3]
  .text              ro code   0x800'1064   0x3d4  py32f072_hal_uart.o [3]
  .text              ro code   0x800'1438     0x2  py32f072_hal_uart.o [3]
  .text              ro code   0x800'143a     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'143c   0x20c  py32f072xx_Start_Kit.o [4]
  .text              ro code   0x800'1648    0x14  memset.o [7]
  .text              ro code   0x800'165c   0x1d8  py32f072_hal_gpio.o [3]
  .text              ro code   0x800'1834    0x4e  ABImemset.o [7]
  .text              ro code   0x800'1882     0x2  startup_py32f072xx.o [2]
  .rodata            const     0x800'1884   0x200  main.o [5]
  .text              ro code   0x800'1a84   0x1a0  main.o [5]
  .text              ro code   0x800'1c24    0x1c  py32f072_hal.o [3]
  .text              ro code   0x800'1c40    0x28  printf.o [6]
  .text              ro code   0x800'1c68    0x34  py32f072_hal_msp.o [5]
  .text              ro code   0x800'1c9c   0x17c  xprintftiny.o [6]
  .text              ro code   0x800'1e18     0xe  strlen.o [7]
  .text              ro code   0x800'1e26     0x2  startup_py32f072xx.o [2]
  .rodata            const     0x800'1e28    0x40  system_py32f072.o [1]
  .text              ro code   0x800'1e68    0x3c  system_py32f072.o [1]
  .text              ro code   0x800'1ea4    0x3c  zero_init3.o [7]
  .text              ro code   0x800'1ee0    0x30  copy_init3.o [7]
  .text              ro code   0x800'1f10    0x28  data_init.o [7]
  .iar.init_table    const     0x800'1f38    0x24  - Linker created -
  .rodata            const     0x800'1f5c    0x20  py32f072_hal_flash.o [3]
  .rodata            const     0x800'1f7c    0x20  system_py32f072.o [1]
  .rodata            const     0x800'1f9c    0x20  system_py32f072.o [1]
  .text              ro code   0x800'1fbc    0x1e  cmain.o [7]
  .text              ro code   0x800'1fda     0x4  low_level_init.o [6]
  .text              ro code   0x800'1fde     0x8  exit.o [6]
  .text              ro code   0x800'1fe6     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1fe8     0xa  cexit.o [7]
  .text              ro code   0x800'1ff2     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'1ff4    0x14  exit.o [8]
  .text              ro code   0x800'2008    0x1c  cstartup_M.o [7]
  .text              ro code   0x800'2024    0x18  py32f072_hal.o [3]
  .text              ro code   0x800'203c    0x16  xprout.o [6]
  .text              ro code   0x800'2052     0x2  startup_py32f072xx.o [2]
  .rodata            const     0x800'2054    0x14  py32f072_hal_rcc.o [3]
  Initializer bytes  const     0x800'2068    0x14  <for P2-1>
  .text              ro code   0x800'207c    0x12  py32f072_it.o [5]
  .text              ro code   0x800'208e     0x2  startup_py32f072xx.o [2]
  .rodata            const     0x800'2090    0x10  py32f072_hal_rcc.o [3]
  .text              ro code   0x800'20a0    0x10  startup_py32f072xx.o [2]
  .rodata            const     0x800'20b0     0x8  main.o [5]
  .rodata            const     0x800'20b8     0x8  py32f072_hal_rcc.o [3]
  .rodata            const     0x800'20c0     0x8  py32f072_hal_rcc.o [3]
  .text              ro code   0x800'20c8     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20ca     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20cc     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20ce     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20d0     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20d2     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20d4     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20d6     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20d8     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20da     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20dc     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20de     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20e0     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20e2     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20e4     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20e6     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20e8     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20ea     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20ec     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20ee     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20f0     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20f2     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20f4     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20f6     0x2  startup_py32f072xx.o [2]
  .text              ro code   0x800'20f8     0x2  startup_py32f072xx.o [2]
  .rodata            const     0x800'20fa     0x1  py32f072xx_Start_Kit.o [4]
  .rodata            const     0x800'20fb     0x0  zero_init3.o [7]
  .rodata            const     0x800'20fb     0x0  copy_init3.o [7]
                             - 0x800'20fb  0x203b

"P2", part 1 of 3:                           0x14
  P2-1                        0x2000'0000    0x14  <Init block>
    .data            inited   0x2000'0000     0x4  py32f072_hal.o [3]
    .data            inited   0x2000'0004     0x4  py32f072_hal.o [3]
    .data            inited   0x2000'0008     0x4  py32f072xx_Start_Kit.o [4]
    .data            inited   0x2000'000c     0x4  py32f072xx_Start_Kit.o [4]
    .data            inited   0x2000'0010     0x4  system_py32f072.o [1]
                            - 0x2000'0014    0x14

"P2", part 2 of 3:                           0x68
  .bss               zero     0x2000'0014    0x4c  py32f072xx_Start_Kit.o [4]
  .bss               zero     0x2000'0060    0x18  py32f072_hal_flash.o [3]
  .bss               zero     0x2000'0078     0x4  py32f072_hal.o [3]
                            - 0x2000'007c    0x68

"P2", part 3 of 3:                          0x400
  CSTACK                      0x2000'0080   0x400  <Block>
    CSTACK           uninit   0x2000'0080   0x400  <Block tail>
                            - 0x2000'0480   0x400

Unused ranges:

         From           To      Size
         ----           --      ----
   0x800'20fb   0x801'ffff  0x1'df05
  0x2000'007c  0x2000'007f       0x4
  0x2000'0480  0x2000'3fff    0x3b80


*******************************************************************************
*** INIT TABLE
***

          Address      Size
          -------      ----
Zero (__iar_zero_init3)
    1 destination range, total size 0x68:
          0x2000'0014  0x68

Copy (__iar_copy_init3)
    1 source range, total size 0x14:
           0x800'2068  0x14
    1 destination range, total size 0x14:
          0x2000'0000  0x14



*******************************************************************************
*** MODULE SUMMARY
***

    Module                  ro code  ro data  rw data
    ------                  -------  -------  -------
command line/config:
    -------------------------------------------------
    Total:

D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\CMSIS_6603591812247902717.dir: [1]
    system_py32f072.o            60      132        4
    -------------------------------------------------
    Total:                       60      132        4

D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\EWARM_7214922893274846302.dir: [2]
    startup_py32f072xx.o        272
    -------------------------------------------------
    Total:                      272

D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir: [3]
    py32f072_hal.o              156        8       12
    py32f072_hal_cortex.o       240
    py32f072_hal_flash.o      1'376       32       24
    py32f072_hal_gpio.o         472
    py32f072_hal_rcc.o        2'052       52
    py32f072_hal_uart.o         982
    -------------------------------------------------
    Total:                    5'278       92       36

D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072xx_Start_Kit_1292202923306237531.dir: [4]
    py32f072xx_Start_Kit.o      524       13       84
    -------------------------------------------------
    Total:                      524       13       84

D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir: [5]
    main.o                      416      520
    py32f072_hal_msp.o           52
    py32f072_it.o                18
    -------------------------------------------------
    Total:                      486      520

dl6M_tln.a: [6]
    exit.o                        8
    low_level_init.o              4
    printf.o                     40
    xprintftiny.o               380
    xprout.o                     22
    -------------------------------------------------
    Total:                      454

rt6M_tl.a: [7]
    ABImemcpy.o                  52
    ABImemset.o                  78
    I32DivModFast.o             174
    IntDivZer.o                   2
    cexit.o                      10
    cmain.o                      30
    copy_init3.o                 48
    cstartup_M.o                 28
    data_init.o                  40
    memset.o                     20
    strlen.o                     14
    zero_init3.o                 60
    -------------------------------------------------
    Total:                      556

shb_l.a: [8]
    exit.o                       20
    -------------------------------------------------
    Total:                       20

    Linker created                        36    1'024
-----------------------------------------------------
    Grand Total:              7'650      793    1'148


*******************************************************************************
*** ENTRY LIST
***

Entry                       Address   Size  Type      Object
-----                       -------   ----  ----      ------
.iar.init_table$$Base    0x800'1f38          --   Gb  - Linker created -
.iar.init_table$$Limit   0x800'1f5c          --   Gb  - Linker created -
?main                    0x800'1fbd         Code  Gb  cmain.o [7]
ADC_COMP_IRQHandler      0x800'20d3         Code  Wk  startup_py32f072xx.o [2]
AHBPrescTable            0x800'1e28   0x40  Data  Gb  system_py32f072.o [1]
APBPrescTable            0x800'1f7c   0x20  Data  Gb  system_py32f072.o [1]
APP_ErrorHandler         0x800'1c21    0x4  Code  Gb  main.o [5]
APP_FlashBlank           0x800'1bbb   0x24  Code  Lc  main.o [5]
APP_FlashErase           0x800'1b61   0x30  Code  Lc  main.o [5]
APP_FlashProgram         0x800'1b91   0x2a  Code  Lc  main.o [5]
APP_FlashVerify          0x800'1bdf   0x28  Code  Lc  main.o [5]
APP_SystemClockConfig    0x800'1af5   0x6c  Code  Lc  main.o [5]
BSP_LED_Init             0x800'143d   0x60  Code  Gb  py32f072xx_Start_Kit.o [4]
BSP_LED_On               0x800'149d   0x1c  Code  Gb  py32f072xx_Start_Kit.o [4]
BSP_PB_GetState          0x800'154d   0x1a  Code  Gb  py32f072xx_Start_Kit.o [4]
BSP_PB_Init              0x800'14b9   0x94  Code  Gb  py32f072xx_Start_Kit.o [4]
BSP_USART_Config         0x800'1567   0xa4  Code  Gb  py32f072xx_Start_Kit.o [4]
BUTTON_IRQn              0x800'20fa    0x1  Data  Gb  py32f072xx_Start_Kit.o [4]
BUTTON_PIN               0x800'0b02    0x2  Data  Gb  py32f072xx_Start_Kit.o [4]
BUTTON_PORT             0x2000'000c    0x4  Data  Gb  py32f072xx_Start_Kit.o [4]
CAN_IRQHandler           0x800'20f7         Code  Wk  startup_py32f072xx.o [2]
CSTACK$$Base            0x2000'0080          --   Gb  - Linker created -
CSTACK$$Limit           0x2000'0480          --   Gb  - Linker created -
DATA                     0x800'1884  0x200  Data  Gb  main.o [5]
DMA1_Channel1_IRQHandler
                         0x800'20cd         Code  Wk  startup_py32f072xx.o [2]
DMA1_Channel2_3_IRQHandler
                         0x800'20cf         Code  Wk  startup_py32f072xx.o [2]
DMA1_Channel4_5_6_7_IRQHandler
                         0x800'20d1         Code  Wk  startup_py32f072xx.o [2]
DebugUartHandle         0x2000'0014   0x4c  Data  Gb  py32f072xx_Start_Kit.o [4]
EXTI0_1_IRQHandler       0x800'2053         Code  Wk  startup_py32f072xx.o [2]
EXTI2_3_IRQHandler       0x800'208f         Code  Wk  startup_py32f072xx.o [2]
EXTI4_15_IRQHandler      0x800'20c9         Code  Wk  startup_py32f072xx.o [2]
FLASH_IRQHandler         0x800'1fe7         Code  Wk  startup_py32f072xx.o [2]
FLASH_MassErase          0x800'0b69   0x1a  Code  Lc  py32f072_hal_flash.o [3]
FLASH_PageErase          0x800'0b83   0x16  Code  Lc  py32f072_hal_flash.o [3]
FLASH_Program_Page       0x800'0bab   0x40  Code  Lc  py32f072_hal_flash.o [3]
FLASH_SectorErase        0x800'0b99   0x12  Code  Lc  py32f072_hal_flash.o [3]
FLASH_WaitForLastOperation
                         0x800'0b43   0x26  Code  Gb  py32f072_hal_flash.o [3]
HAL_FLASH_Erase          0x800'0c05  0x246  Code  Gb  py32f072_hal_flash.o [3]
HAL_FLASH_Lock           0x800'0b27   0x1c  Code  Gb  py32f072_hal_flash.o [3]
HAL_FLASH_Program        0x800'0e8d  0x1a2  Code  Gb  py32f072_hal_flash.o [3]
HAL_FLASH_Unlock         0x800'0b05   0x22  Code  Gb  py32f072_hal_flash.o [3]
HAL_GPIO_Init            0x800'165d  0x190  Code  Gb  py32f072_hal_gpio.o [3]
HAL_GPIO_ReadPin         0x800'17f9   0x16  Code  Gb  py32f072_hal_gpio.o [3]
HAL_GPIO_WritePin        0x800'180f   0x14  Code  Gb  py32f072_hal_gpio.o [3]
HAL_GetTick              0x800'08c5    0xc  Code  Wk  py32f072_hal.o [3]
HAL_IncTick              0x800'2025   0x18  Code  Wk  py32f072_hal.o [3]
HAL_Init                 0x800'1c25   0x1c  Code  Gb  py32f072_hal.o [3]
HAL_InitTick             0x800'08d1   0x5c  Code  Wk  py32f072_hal.o [3]
HAL_MspInit              0x800'1c69   0x34  Code  Gb  py32f072_hal_msp.o [5]
HAL_NVIC_EnableIRQ       0x800'0ad5    0xa  Code  Gb  py32f072_hal_cortex.o [3]
HAL_NVIC_SetPriority     0x800'0acb    0xa  Code  Gb  py32f072_hal_cortex.o [3]
HAL_RCC_ClockConfig      0x800'05e9  0x176  Code  Gb  py32f072_hal_rcc.o [3]
HAL_RCC_GetHCLKFreq      0x800'0849    0x6  Code  Gb  py32f072_hal_rcc.o [3]
HAL_RCC_GetPCLK1Freq     0x800'0855   0x1e  Code  Gb  py32f072_hal_rcc.o [3]
HAL_RCC_GetSysClockFreq
                         0x800'0781   0xc8  Code  Gb  py32f072_hal_rcc.o [3]
HAL_RCC_OscConfig        0x800'00c1  0x508  Code  Gb  py32f072_hal_rcc.o [3]
HAL_SYSTICK_Config       0x800'0adf    0x8  Code  Gb  py32f072_hal_cortex.o [3]
HAL_UART_Init            0x800'1065   0x84  Code  Gb  py32f072_hal_uart.o [3]
HAL_UART_MspInit         0x800'1439    0x2  Code  Wk  py32f072_hal_uart.o [3]
HAL_UART_Transmit        0x800'10f1   0xf0  Code  Gb  py32f072_hal_uart.o [3]
HSIFreqTable             0x800'1f9c   0x20  Data  Gb  system_py32f072.o [1]
HardFault_Handler        0x800'207f    0x4  Code  Gb  py32f072_it.o [5]
I2C1_IRQHandler          0x800'20e9         Code  Wk  startup_py32f072xx.o [2]
I2C2_IRQHandler          0x800'20eb         Code  Wk  startup_py32f072xx.o [2]
LCD_IRQHandler           0x800'20cb         Code  Wk  startup_py32f072xx.o [2]
LED_PIN                  0x800'0a0e    0x2  Data  Gb  py32f072xx_Start_Kit.o [4]
LED_PORT                0x2000'0008    0x4  Data  Gb  py32f072xx_Start_Kit.o [4]
NMI_Handler              0x800'207d    0x2  Code  Gb  py32f072_it.o [5]
PVD_IRQHandler           0x800'1883         Code  Wk  startup_py32f072xx.o [2]
PendSV_Handler           0x800'2085    0x2  Code  Gb  py32f072_it.o [5]
RCC_GetHSIFreq           0x800'088d   0x12  Code  Lc  py32f072_hal_rcc.o [3]
RCC_IRQHandler           0x800'1ff3         Code  Wk  startup_py32f072xx.o [2]
RTC_IRQHandler           0x800'1e27         Code  Wk  startup_py32f072xx.o [2]
Region$$Table$$Base      0x800'1f38          --   Gb  - Linker created -
Region$$Table$$Limit     0x800'1f5c          --   Gb  - Linker created -
Reset_Handler            0x800'20a1         Code  Wk  startup_py32f072xx.o [2]
SPI1_IRQHandler          0x800'20ed         Code  Wk  startup_py32f072xx.o [2]
SPI2_IRQHandler          0x800'20ef         Code  Wk  startup_py32f072xx.o [2]
SVC_Handler              0x800'2083    0x2  Code  Gb  py32f072_it.o [5]
SysTick_Config           0x800'0a9b   0x30  Code  Lc  py32f072_hal_cortex.o [3]
SysTick_Handler          0x800'2087    0x8  Code  Gb  py32f072_it.o [5]
SystemCoreClock         0x2000'0010    0x4  Data  Gb  system_py32f072.o [1]
SystemInit               0x800'1e69   0x2a  Code  Gb  system_py32f072.o [1]
TIM14_IRQHandler         0x800'20e1         Code  Wk  startup_py32f072xx.o [2]
TIM15_IRQHandler         0x800'20e3         Code  Wk  startup_py32f072xx.o [2]
TIM16_IRQHandler         0x800'20e5         Code  Wk  startup_py32f072xx.o [2]
TIM17_IRQHandler         0x800'20e7         Code  Wk  startup_py32f072xx.o [2]
TIM1_BRK_UP_TRG_COM_IRQHandler
                         0x800'20d5         Code  Wk  startup_py32f072xx.o [2]
TIM1_CC_IRQHandler       0x800'20d7         Code  Wk  startup_py32f072xx.o [2]
TIM2_IRQHandler          0x800'20d9         Code  Wk  startup_py32f072xx.o [2]
TIM3_IRQHandler          0x800'20db         Code  Wk  startup_py32f072xx.o [2]
TIM6_LPTIM1_DAC_IRQHandler
                         0x800'20dd         Code  Wk  startup_py32f072xx.o [2]
TIM7_IRQHandler          0x800'20df         Code  Wk  startup_py32f072xx.o [2]
UART_AdvFeatureConfig    0x800'13e9   0x36  Code  Lc  py32f072_hal_uart.o [3]
UART_SetConfig           0x800'124d  0x19a  Code  Lc  py32f072_hal_uart.o [3]
UART_WaitOnFlagUntilTimeout
                         0x800'11e1   0x68  Code  Lc  py32f072_hal_uart.o [3]
USART1_IRQHandler        0x800'20f1         Code  Wk  startup_py32f072xx.o [2]
USART2_IRQHandler        0x800'20f3         Code  Wk  startup_py32f072xx.o [2]
USART3_4_IRQHandler      0x800'20f5         Code  Wk  startup_py32f072xx.o [2]
USB_IRQHandler           0x800'20f9         Code  Wk  startup_py32f072xx.o [2]
WWDG_IRQHandler          0x800'143b         Code  Wk  startup_py32f072xx.o [2]
_FlashTimmingParam       0x800'1f5c   0x20  Data  Gb  py32f072_hal_flash.o [3]
_PrintfTiny              0x800'1cb7  0x162  Code  Gb  xprintftiny.o [6]
_Prout                   0x800'203d   0x16  Code  Gb  xprout.o [6]
__ICFEDIT_region_RAM_end__ {Abs}
                        0x2000'3fff         Data  Gb  <internal module>
__ICFEDIT_region_RAM_start__ {Abs}
                        0x2000'0000         Data  Gb  <internal module>
__NVIC_EnableIRQ         0x800'0a11   0x18  Code  Lc  py32f072_hal_cortex.o [3]
__NVIC_SetPriority       0x800'0a29   0x72  Code  Lc  py32f072_hal_cortex.o [3]
__aeabi_idiv0            0x800'0b01         Code  Gb  IntDivZer.o [7]
__aeabi_memcpy4          0x800'092d         Code  Gb  ABImemcpy.o [7]
__aeabi_memcpy8          0x800'092d         Code  Gb  ABImemcpy.o [7]
__aeabi_memset           0x800'1835         Code  Gb  ABImemset.o [7]
__aeabi_uidiv            0x800'0961         Code  Gb  I32DivModFast.o [7]
__aeabi_uidivmod         0x800'0961         Code  Gb  I32DivModFast.o [7]
__cmain                  0x800'1fbd         Code  Gb  cmain.o [7]
__exit                   0x800'1ff5   0x14  Code  Gb  exit.o [8]
__iar_Memset4_word       0x800'1855         Code  Gb  ABImemset.o [7]
__iar_Memset_word        0x800'1841         Code  Gb  ABImemset.o [7]
__iar_copy_init3         0x800'1ee1   0x30  Code  Gb  copy_init3.o [7]
__iar_data_init3         0x800'1f11   0x28  Code  Gb  data_init.o [7]
__iar_program_start      0x800'2009         Code  Gb  cstartup_M.o [7]
__iar_zero_init3         0x800'1ea5   0x3c  Code  Gb  zero_init3.o [7]
__low_level_init         0x800'1fdb    0x4  Code  Gb  low_level_init.o [6]
__vector_table           0x800'0000         Data  Gb  startup_py32f072xx.o [2]
_call_main               0x800'1fc9         Code  Gb  cmain.o [7]
_exit                    0x800'1fe9         Code  Gb  cexit.o [7]
exit                     0x800'1fdf    0x8  Code  Gb  exit.o [6]
main                     0x800'1a85   0x70  Code  Gb  main.o [5]
memset                   0x800'1649   0x14  Code  Gb  memset.o [7]
out                      0x800'1c9d   0x1a  Code  Lc  xprintftiny.o [6]
pFlash                  0x2000'0060   0x18  Data  Gb  py32f072_hal_flash.o [3]
printf                   0x800'1c41   0x28  Code  Gb  printf.o [6]
putchar                  0x800'160b   0x14  Code  Gb  py32f072xx_Start_Kit.o [4]
strlen                   0x800'1e19         Code  Gb  strlen.o [7]
uwTick                  0x2000'0078    0x4  Data  Gb  py32f072_hal.o [3]
uwTickFreq              0x2000'0004    0x4  Data  Gb  py32f072_hal.o [3]
uwTickPrio              0x2000'0000    0x4  Data  Gb  py32f072_hal.o [3]


[1] = D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\CMSIS_6603591812247902717.dir
[2] = D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\EWARM_7214922893274846302.dir
[3] = D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072_HAL_Driver_13276881132468293653.dir
[4] = D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\PY32F072xx_Start_Kit_1292202923306237531.dir
[5] = D:\软件工作资料\DFlash测试\PY32F072\PY32F072_Firmware_V1.0.5\Projects\PY32F072-STK\Example\FLASH\FLASH_PageEraseAndWrite\EWARM\Project\Obj\User_7280784329937237312.dir
[6] = dl6M_tln.a
[7] = rt6M_tl.a
[8] = shb_l.a

  7'650 bytes of readonly  code memory
    793 bytes of readonly  data memory
  1'148 bytes of readwrite data memory

Errors: none
Warnings: none
