Component: ARM Compiler 5.06 update 7 (build 960) Tool: armlink [4d3601]

==============================================================================

Section Cross References

    gpio.o(i.GPIO_Init) refers to gpio.o(i.PORT_Init) for PORT_Init
    gpio.o(i.GPIO_Init) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    gpio.o(i.GPIO_Init) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    gpio.o(i.PORT_Init) refers to gpio.o(i.__ARM_common_switch8) for __ARM_common_switch8
    sys_tick.o(i.SysTick_Handler) refers to tasks.o(i.Sys_Exact_50us_Tasks) for Sys_Exact_50us_Tasks
    sys_tick.o(i.SysTick_Handler) refers to eeprommanage.o(.text.eeprom_1ms_timeCount) for eeprom_1ms_timeCount
    sys_tick.o(i.SysTick_Handler) refers to tasks.o(i.Sys_Exact_100ms_Tasks) for Sys_Exact_100ms_Tasks
    sys_tick.o(i.SysTick_Handler) refers to sys_scheduler.o(i.Sys_Scheduling_Tmr) for Sys_Scheduling_Tmr
    sys_tick.o(i.SysTick_Handler) refers to common_interface.o(i.Common_Input_Para) for Common_Input_Para
    sys_tick.o(i.SysTick_Handler) refers to sys_tick.o(.bss) for g_stSysTickTimer
    sys_tick.o(i.SysTick_Handler) refers to sys_tick.o(.data) for g_u16SysRollingCounter1ms
    sys_tick.o(i.Sys_Tick_Timer_Call_Back_Reg) refers to sys_tick.o(.bss) for pfnSysTickCallBack
    sys_tick.o(i.Sys_Tick_Timer_Start) refers to system_bat32a239.o(i.SystemCoreClockUpdate) for SystemCoreClockUpdate
    sys_tick.o(i.Sys_Tick_Timer_Start) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    sys_tick.o(i.Sys_Tick_Timer_Start) refers to sys_tick.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    sys_tick.o(i.Sys_Tick_Timer_Start) refers to sys_tick.o(.bss) for g_stSysTickTimer
    sys_tick.o(i.Sys_Tick_Timer_Start) refers to sys_tick.o(.data) for g_u16SysRollingCounter50us
    sys_tick.o(i.Sys_Tick_Timer_Start) refers to system_bat32a239.o(.data) for SystemCoreClock
    adc.o(i.ADC_Converse) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    adc.o(i.ADC_Get_Conversion_Result) refers to adc.o(.data) for u8ADCSequenceRunningFlag
    adc.o(i.ADC_Get_Conversion_Status) refers to adc.o(.data) for u8ADCSequenceRunningFlag
    adc.o(i.ADC_Init) refers to adc.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    adc.o(i.ADC_MidAvg_Filter) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    adc.o(i.ADC_SelfTest) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    adc.o(i.ADC_Start) refers to adc.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    adc.o(i.ADC_Start_Conversion) refers to adc.o(i.ADC_Start) for ADC_Start
    adc.o(i.ADC_Start_Conversion) refers to adc.o(.data) for u8ADCChannelCount
    adc.o(i.ADC_Start_Conversion) refers to analog_signals.o(.constdata) for u8ADCChList
    adc.o(i.ADC_Stop) refers to adc.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    adc.o(i.ADC_Stop_Conversion) refers to adc.o(i.ADC_Stop) for ADC_Stop
    adc.o(i.Analog_Signal_Conv_Real_Time_Run) refers to adc.o(i.ADC_Start) for ADC_Start
    adc.o(i.Analog_Signal_Conv_Real_Time_Run) refers to adc.o(.data) for u8ADCChannelCount
    adc.o(i.Analog_Signal_Conv_Real_Time_Run) refers to analog_signals.o(.constdata) for u8ADCChList
    analog_circuits.o(i.ADC_Input_Voltage_Calc) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    analog_circuits.o(i.ADC_Res_Calc_Circuit101) refers to llmul.o(.text) for __aeabi_lmul
    analog_circuits.o(i.ADC_Res_Calc_Circuit101) refers to lludiv.o(.text) for __aeabi_uldivmod
    analog_circuits.o(i.ADC_Res_Calc_Circuit101) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    analog_circuits.o(i.ADC_Res_Calc_Circuit102) refers to llmul.o(.text) for __aeabi_lmul
    analog_circuits.o(i.ADC_Res_Calc_Circuit102) refers to lludiv.o(.text) for __aeabi_uldivmod
    analog_circuits.o(i.ADC_Res_Calc_Circuit102) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    analog_circuits.o(i.ADC_Res_Calc_Circuit103) refers to llmul.o(.text) for __aeabi_lmul
    analog_circuits.o(i.ADC_Res_Calc_Circuit103) refers to lludiv.o(.text) for __aeabi_uldivmod
    analog_circuits.o(i.ADC_Res_Calc_Circuit103) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    analog_circuits.o(i.ADC_Res_Calc_Circuit201) refers to llmul.o(.text) for __aeabi_lmul
    analog_circuits.o(i.ADC_Res_Calc_Circuit201) refers to lludiv.o(.text) for __aeabi_uldivmod
    analog_circuits.o(i.ADC_Res_Calc_Circuit201) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    analog_circuits.o(i.ADC_Res_Calc_Circuit202) refers to llmul.o(.text) for __aeabi_lmul
    analog_circuits.o(i.ADC_Res_Calc_Circuit202) refers to lludiv.o(.text) for __aeabi_uldivmod
    analog_circuits.o(i.ADC_Res_Calc_Circuit202) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    analog_circuits.o(i.ADC_Res_Calc_Circuit203) refers to llmul.o(.text) for __aeabi_lmul
    analog_circuits.o(i.ADC_Res_Calc_Circuit203) refers to lludiv.o(.text) for __aeabi_uldivmod
    analog_circuits.o(i.ADC_Res_Calc_Circuit203) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    analog_circuits.o(i.ADC_Res_Calc_Circuit301) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    analog_circuits.o(i.ADC_Res_Calc_Circuit302) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    analog_circuits.o(i.ADC_Res_Calc_Circuit303) refers to llmul.o(.text) for __aeabi_lmul
    analog_circuits.o(i.ADC_Res_Calc_Circuit303) refers to lludiv.o(.text) for __aeabi_uldivmod
    analog_circuits.o(i.ADC_Res_Calc_Circuit303) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    analog_circuits.o(i.ADC_VRef_Calibrate) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    analog_circuits.o(i.ADC_Voltage_Calc_Circuit101) refers to aeabi_sdivfast.o(.text) for __aeabi_idivmod
    analog_circuits.o(i.ADC_Voltage_Calc_Circuit102) refers to llmul.o(.text) for __aeabi_lmul
    analog_circuits.o(i.ADC_Voltage_Calc_Circuit102) refers to lludiv.o(.text) for __aeabi_uldivmod
    analog_signals.o(i.ADC_Conv_Single_Channel) refers to adc.o(i.ADC_Get_Conversion_Status) for ADC_Get_Conversion_Status
    analog_signals.o(i.ADC_Conv_Single_Channel) refers to adc.o(i.ADC_Start_Conversion) for ADC_Start_Conversion
    analog_signals.o(i.ADC_Conv_Single_Channel) refers to adc.o(i.Analog_Signal_Conv_Real_Time_Run) for Analog_Signal_Conv_Real_Time_Run
    analog_signals.o(i.ADC_Conv_Single_Channel) refers to adc.o(i.ADC_Get_Conversion_Result) for ADC_Get_Conversion_Result
    analog_signals.o(i.ADC_Conv_Single_Channel) refers to analog_circuits.o(i.ADC_Input_Voltage_Calc) for ADC_Input_Voltage_Calc
    analog_signals.o(i.ADC_Conv_Single_Channel) refers to analog_circuits.o(i.ADC_Data_Calibrate) for ADC_Data_Calibrate
    analog_signals.o(i.ADC_Conv_Single_Channel) refers to analog_signals.o(.data) for u16ADCSample
    analog_signals.o(i.ADC_Conv_Single_Channel) refers to analog_signals.o(.constdata) for stADCChCfg
    analog_signals.o(i.ADC_Read_Signal) refers to analog_signals.o(.bss) for stADCData
    analog_signals.o(i.ADC_Read_Signal_Valid) refers to analog_signals.o(.bss) for stADCData
    analog_signals.o(i.Analog_Signal_Conv_Init) refers to adc.o(i.ADC_Stop_Conversion) for ADC_Stop_Conversion
    analog_signals.o(i.Analog_Signal_Conv_Init) refers to adc.o(i.ADC_Init) for ADC_Init
    analog_signals.o(i.Analog_Signal_Conv_Init) refers to analog_signals.o(.bss) for stADCData
    analog_signals.o(i.Analog_Signal_Conv_Init) refers to analog_signals.o(.data) for stADCCtrl
    analog_signals.o(i.Analog_Signal_Conv_Init) refers to adc.o(.data) for u8ADCSequenceRunningFlag
    analog_signals.o(i.Analog_Signal_Conv_Service) refers to gpio.o(i.__ARM_common_switch8) for __ARM_common_switch8
    analog_signals.o(i.Analog_Signal_Conv_Service) refers to adc.o(i.ADC_Start_Conversion) for ADC_Start_Conversion
    analog_signals.o(i.Analog_Signal_Conv_Service) refers to adc.o(i.ADC_Get_Conversion_Status) for ADC_Get_Conversion_Status
    analog_signals.o(i.Analog_Signal_Conv_Service) refers to adc.o(i.ADC_Stop_Conversion) for ADC_Stop_Conversion
    analog_signals.o(i.Analog_Signal_Conv_Service) refers to adc.o(i.ADC_Get_Conversion_Result) for ADC_Get_Conversion_Result
    analog_signals.o(i.Analog_Signal_Conv_Service) refers to analog_circuits.o(i.ADC_Input_Voltage_Calc) for ADC_Input_Voltage_Calc
    analog_signals.o(i.Analog_Signal_Conv_Service) refers to analog_signals.o(i.ADC_Read_Signal) for ADC_Read_Signal
    analog_signals.o(i.Analog_Signal_Conv_Service) refers to analog_signals.o(i.ADC_Read_Signal_Valid) for ADC_Read_Signal_Valid
    analog_signals.o(i.Analog_Signal_Conv_Service) refers to analog_circuits.o(i.ADC_Data_Calibrate) for ADC_Data_Calibrate
    analog_signals.o(i.Analog_Signal_Conv_Service) refers to analog_signals.o(i.Analog_Signal_Conv_Init) for Analog_Signal_Conv_Init
    analog_signals.o(i.Analog_Signal_Conv_Service) refers to analog_signals.o(.data) for stADCCtrl
    analog_signals.o(i.Analog_Signal_Conv_Service) refers to analog_signals.o(.constdata) for stADCChCfg
    analog_signals.o(i.Analog_Signal_Conv_Service) refers to analog_signals.o(.bss) for stADCData
    analog_signals.o(i.Analog_Signal_Conv_Stop) refers to adc.o(i.ADC_Stop) for ADC_Stop
    analog_signals.o(i.Analog_Signal_Conv_Stop) refers to analog_signals.o(.bss) for stADCData
    analog_signals.o(i.Analog_Signal_Conv_Stop) refers to analog_signals.o(.data) for stADCCtrl
    analog_signals.o(.constdata) refers to analog_circuits.o(i.ADC_Voltage_Calc_Circuit102) for ADC_Voltage_Calc_Circuit102
    analog_signals.o(.constdata) refers to analog_circuits.o(i.ADC_Voltage_Calc_Circuit101) for ADC_Voltage_Calc_Circuit101
    analog_signals.o(.constdata) refers to analog_circuits.o(i.ADC_Res_Calc_Circuit101) for ADC_Res_Calc_Circuit101
    sci.o(i.IIC00_MasterReceive) refers to sci.o(i.IIC00_StartCondition) for IIC00_StartCondition
    sci.o(i.IIC00_MasterReceive) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.IIC00_MasterReceive) refers to sci.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    sci.o(i.IIC00_MasterReceive) refers to sci.o(.data) for g_iic00_master_status_flag
    sci.o(i.IIC00_MasterSend) refers to sci.o(i.IIC00_StartCondition) for IIC00_StartCondition
    sci.o(i.IIC00_MasterSend) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.IIC00_MasterSend) refers to sci.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    sci.o(i.IIC00_MasterSend) refers to sci.o(.data) for g_iic00_master_status_flag
    sci.o(i.IIC00_StopCondition) refers to sci.o(.data) for g_iic00_master_status_flag
    sci.o(i.IIC01_MasterReceive) refers to sci.o(i.IIC01_StartCondition) for IIC01_StartCondition
    sci.o(i.IIC01_MasterReceive) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.IIC01_MasterReceive) refers to sci.o(.data) for g_iic01_master_status_flag
    sci.o(i.IIC01_MasterSend) refers to sci.o(i.IIC01_StartCondition) for IIC01_StartCondition
    sci.o(i.IIC01_MasterSend) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.IIC01_MasterSend) refers to sci.o(.data) for g_iic01_master_status_flag
    sci.o(i.IIC10_MasterReceive) refers to sci.o(i.IIC10_StartCondition) for IIC10_StartCondition
    sci.o(i.IIC10_MasterReceive) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.IIC10_MasterReceive) refers to sci.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    sci.o(i.IIC10_MasterReceive) refers to sci.o(.data) for g_iic10_master_status_flag
    sci.o(i.IIC10_MasterSend) refers to sci.o(i.IIC10_StartCondition) for IIC10_StartCondition
    sci.o(i.IIC10_MasterSend) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.IIC10_MasterSend) refers to sci.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    sci.o(i.IIC10_MasterSend) refers to sci.o(.data) for g_iic10_master_status_flag
    sci.o(i.IIC10_StopCondition) refers to sci.o(.data) for g_iic10_master_status_flag
    sci.o(i.IIC11_MasterReceive) refers to sci.o(i.IIC11_StartCondition) for IIC11_StartCondition
    sci.o(i.IIC11_MasterReceive) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.IIC11_MasterReceive) refers to sci.o(.data) for g_iic11_master_status_flag
    sci.o(i.IIC11_MasterSend) refers to sci.o(i.IIC11_StartCondition) for IIC11_StartCondition
    sci.o(i.IIC11_MasterSend) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.IIC11_MasterSend) refers to sci.o(.data) for g_iic11_master_status_flag
    sci.o(i.IIC20_MasterReceive) refers to sci.o(i.IIC20_StartCondition) for IIC20_StartCondition
    sci.o(i.IIC20_MasterReceive) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.IIC20_MasterReceive) refers to sci.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    sci.o(i.IIC20_MasterReceive) refers to sci.o(.data) for g_iic20_master_status_flag
    sci.o(i.IIC20_MasterSend) refers to sci.o(i.IIC20_StartCondition) for IIC20_StartCondition
    sci.o(i.IIC20_MasterSend) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.IIC20_MasterSend) refers to sci.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    sci.o(i.IIC20_MasterSend) refers to sci.o(.data) for g_iic20_master_status_flag
    sci.o(i.IIC20_StopCondition) refers to sci.o(.data) for g_iic20_master_status_flag
    sci.o(i.IIC21_MasterReceive) refers to sci.o(i.IIC21_StartCondition) for IIC21_StartCondition
    sci.o(i.IIC21_MasterReceive) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.IIC21_MasterReceive) refers to sci.o(.data) for g_iic21_master_status_flag
    sci.o(i.IIC21_MasterSend) refers to sci.o(i.IIC21_StartCondition) for IIC21_StartCondition
    sci.o(i.IIC21_MasterSend) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.IIC21_MasterSend) refers to sci.o(.data) for g_iic21_master_status_flag
    sci.o(i.IIC30_MasterReceive) refers to sci.o(i.IIC30_StartCondition) for IIC30_StartCondition
    sci.o(i.IIC30_MasterReceive) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.IIC30_MasterReceive) refers to sci.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    sci.o(i.IIC30_MasterReceive) refers to sci.o(.data) for g_iic30_master_status_flag
    sci.o(i.IIC30_MasterSend) refers to sci.o(i.IIC30_StartCondition) for IIC30_StartCondition
    sci.o(i.IIC30_MasterSend) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.IIC30_MasterSend) refers to sci.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    sci.o(i.IIC30_MasterSend) refers to sci.o(.data) for g_iic30_master_status_flag
    sci.o(i.IIC30_StopCondition) refers to sci.o(.data) for g_iic30_master_status_flag
    sci.o(i.IIC31_MasterReceive) refers to sci.o(i.IIC31_StartCondition) for IIC31_StartCondition
    sci.o(i.IIC31_MasterReceive) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.IIC31_MasterReceive) refers to sci.o(.data) for g_iic31_master_status_flag
    sci.o(i.IIC31_MasterSend) refers to sci.o(i.IIC31_StartCondition) for IIC31_StartCondition
    sci.o(i.IIC31_MasterSend) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.IIC31_MasterSend) refers to sci.o(.data) for g_iic31_master_status_flag
    sci.o(i.SPI00_MasterReceive) refers to sci.o(i.SPI00_Start) for SPI00_Start
    sci.o(i.SPI00_MasterReceive) refers to sci.o(.data) for dummy_sio00
    sci.o(i.SPI00_MasterSend) refers to sci.o(i.SPI00_Start) for SPI00_Start
    sci.o(i.SPI00_MasterSend) refers to sci.o(.data) for g_spi00_tx_count
    sci.o(i.SPI00_MasterSendReceive) refers to sci.o(i.SPI00_Start) for SPI00_Start
    sci.o(i.SPI00_MasterSendReceive) refers to sci.o(.data) for g_spi00_rx_count
    sci.o(i.SPI00_SlaveReceive) refers to sci.o(i.SPI00_Start) for SPI00_Start
    sci.o(i.SPI00_SlaveReceive) refers to sci.o(.data) for g_spi00_rx_count
    sci.o(i.SPI00_SlaveSend) refers to sci.o(i.SPI00_Start) for SPI00_Start
    sci.o(i.SPI00_SlaveSend) refers to sci.o(.data) for g_spi00_tx_count
    sci.o(i.SPI00_Start) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.SPI01_MasterReceive) refers to sci.o(i.SPI01_Start) for SPI01_Start
    sci.o(i.SPI01_MasterReceive) refers to sci.o(.data) for g_spi01_rx_count
    sci.o(i.SPI01_MasterSend) refers to sci.o(i.SPI01_Start) for SPI01_Start
    sci.o(i.SPI01_MasterSend) refers to sci.o(.data) for g_spi01_tx_count
    sci.o(i.SPI01_SlaveInit) refers to sci.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    sci.o(i.SPI01_SlaveReceive) refers to sci.o(i.SPI01_Start) for SPI01_Start
    sci.o(i.SPI01_SlaveReceive) refers to sci.o(.data) for g_spi01_rx_count
    sci.o(i.SPI01_SlaveSend) refers to sci.o(i.SPI01_Start) for SPI01_Start
    sci.o(i.SPI01_SlaveSend) refers to sci.o(.data) for g_spi01_tx_count
    sci.o(i.SPI01_SlaveSendReceive) refers to sci.o(i.SPI01_Start) for SPI01_Start
    sci.o(i.SPI01_SlaveSendReceive) refers to sci.o(.data) for g_spi01_rx_count
    sci.o(i.SPI01_Start) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.SPI01_Stop) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.SPI10_MasterReceive) refers to sci.o(i.SPI10_Start) for SPI10_Start
    sci.o(i.SPI10_MasterReceive) refers to sci.o(.data) for dummy_sio10
    sci.o(i.SPI10_MasterSend) refers to sci.o(i.SPI10_Start) for SPI10_Start
    sci.o(i.SPI10_MasterSend) refers to sci.o(.data) for g_spi10_tx_count
    sci.o(i.SPI10_MasterSendReceive) refers to sci.o(i.SPI10_Start) for SPI10_Start
    sci.o(i.SPI10_MasterSendReceive) refers to sci.o(.data) for g_spi10_rx_count
    sci.o(i.SPI10_SlaveInit) refers to sci.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    sci.o(i.SPI10_SlaveReceive) refers to sci.o(i.SPI10_Start) for SPI10_Start
    sci.o(i.SPI10_SlaveReceive) refers to sci.o(.data) for g_spi10_rx_count
    sci.o(i.SPI10_SlaveSend) refers to sci.o(i.SPI10_Start) for SPI10_Start
    sci.o(i.SPI10_SlaveSend) refers to sci.o(.data) for g_spi10_tx_count
    sci.o(i.SPI10_Start) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.SPI10_Stop) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.SPI11_MasterReceive) refers to sci.o(i.SPI11_Start) for SPI11_Start
    sci.o(i.SPI11_MasterReceive) refers to sci.o(.data) for dummy_sio11
    sci.o(i.SPI11_MasterSend) refers to sci.o(i.SPI11_Start) for SPI11_Start
    sci.o(i.SPI11_MasterSend) refers to sci.o(.data) for g_spi11_tx_count
    sci.o(i.SPI11_SlaveInit) refers to sci.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    sci.o(i.SPI11_SlaveReceive) refers to sci.o(i.SPI11_Start) for SPI11_Start
    sci.o(i.SPI11_SlaveReceive) refers to sci.o(.data) for g_spi11_rx_count
    sci.o(i.SPI11_SlaveSend) refers to sci.o(i.SPI11_Start) for SPI11_Start
    sci.o(i.SPI11_SlaveSend) refers to sci.o(.data) for g_spi11_tx_count
    sci.o(i.SPI11_SlaveSendReceive) refers to sci.o(i.SPI11_Start) for SPI11_Start
    sci.o(i.SPI11_SlaveSendReceive) refers to sci.o(.data) for g_spi11_rx_count
    sci.o(i.SPI11_Start) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.SPI11_Stop) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.SPI20_MasterReceive) refers to sci.o(i.SPI20_Start) for SPI20_Start
    sci.o(i.SPI20_MasterReceive) refers to sci.o(i.SPI20_Stop) for SPI20_Stop
    sci.o(i.SPI20_MasterReceive) refers to sci.o(.data) for dummy_sio20
    sci.o(i.SPI20_MasterSend) refers to sci.o(i.SPI20_Start) for SPI20_Start
    sci.o(i.SPI20_MasterSend) refers to sci.o(i.SPI20_Stop) for SPI20_Stop
    sci.o(i.SPI20_SlaveInit) refers to sci.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    sci.o(i.SPI20_SlaveReceive) refers to sci.o(i.SPI20_Start) for SPI20_Start
    sci.o(i.SPI20_SlaveReceive) refers to sci.o(.data) for g_spi20_rx_count
    sci.o(i.SPI20_SlaveSend) refers to sci.o(i.SPI20_Start) for SPI20_Start
    sci.o(i.SPI20_SlaveSend) refers to sci.o(.data) for g_spi20_tx_count
    sci.o(i.SPI20_Start) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.SPI21_MasterReceive) refers to sci.o(i.SPI21_Start) for SPI21_Start
    sci.o(i.SPI21_MasterReceive) refers to sci.o(.data) for g_spi21_rx_count
    sci.o(i.SPI21_MasterSend) refers to sci.o(i.SPI21_Start) for SPI21_Start
    sci.o(i.SPI21_MasterSend) refers to sci.o(.data) for g_spi21_tx_count
    sci.o(i.SPI21_MasterSendReceive) refers to sci.o(i.SPI21_Start) for SPI21_Start
    sci.o(i.SPI21_MasterSendReceive) refers to sci.o(.data) for g_spi21_rx_count
    sci.o(i.SPI21_SlaveInit) refers to sci.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    sci.o(i.SPI21_SlaveReceive) refers to sci.o(i.SPI21_Start) for SPI21_Start
    sci.o(i.SPI21_SlaveReceive) refers to sci.o(.data) for g_spi21_rx_count
    sci.o(i.SPI21_SlaveSend) refers to sci.o(i.SPI21_Start) for SPI21_Start
    sci.o(i.SPI21_SlaveSend) refers to sci.o(.data) for g_spi21_tx_count
    sci.o(i.SPI21_Start) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.SPI30_MasterReceive) refers to sci.o(i.SPI30_Start) for SPI30_Start
    sci.o(i.SPI30_MasterReceive) refers to sci.o(i.SPI30_Stop) for SPI30_Stop
    sci.o(i.SPI30_MasterReceive) refers to sci.o(.data) for dummy_sio30
    sci.o(i.SPI30_MasterSend) refers to sci.o(i.SPI30_Start) for SPI30_Start
    sci.o(i.SPI30_MasterSend) refers to sci.o(i.SPI30_Stop) for SPI30_Stop
    sci.o(i.SPI30_SlaveInit) refers to sci.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    sci.o(i.SPI30_SlaveReceive) refers to sci.o(i.SPI30_Start) for SPI30_Start
    sci.o(i.SPI30_SlaveReceive) refers to sci.o(.data) for g_spi30_rx_count
    sci.o(i.SPI30_SlaveSend) refers to sci.o(i.SPI30_Start) for SPI30_Start
    sci.o(i.SPI30_SlaveSend) refers to sci.o(.data) for g_spi30_tx_count
    sci.o(i.SPI30_Start) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.SPI31_MasterReceive) refers to sci.o(i.SPI31_Start) for SPI31_Start
    sci.o(i.SPI31_MasterReceive) refers to sci.o(.data) for g_spi31_rx_count
    sci.o(i.SPI31_MasterSend) refers to sci.o(i.SPI31_Start) for SPI31_Start
    sci.o(i.SPI31_MasterSend) refers to sci.o(.data) for g_spi31_tx_count
    sci.o(i.SPI31_MasterSendReceive) refers to sci.o(i.SPI31_Start) for SPI31_Start
    sci.o(i.SPI31_MasterSendReceive) refers to sci.o(.data) for g_spi31_rx_count
    sci.o(i.SPI31_SlaveInit) refers to sci.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    sci.o(i.SPI31_SlaveReceive) refers to sci.o(i.SPI31_Start) for SPI31_Start
    sci.o(i.SPI31_SlaveReceive) refers to sci.o(.data) for g_spi31_rx_count
    sci.o(i.SPI31_SlaveSend) refers to sci.o(i.SPI31_Start) for SPI31_Start
    sci.o(i.SPI31_SlaveSend) refers to sci.o(.data) for g_spi31_tx_count
    sci.o(i.SPI31_Start) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.UART0_BaudRate) refers to sci.o(i.UART_BaudRateCal) for UART_BaudRateCal
    sci.o(i.UART0_Init) refers to sci.o(i.UART0_BaudRate) for UART0_BaudRate
    sci.o(i.UART0_Receive_Int) refers to sci.o(.data) for g_uart0_rx_count
    sci.o(i.UART1_BaudRate) refers to sci.o(i.UART_BaudRateCal) for UART_BaudRateCal
    sci.o(i.UART1_Init) refers to sci.o(i.UART1_BaudRate) for UART1_BaudRate
    sci.o(i.UART1_Init) refers to sci.o(i.UART1_Start) for UART1_Start
    sci.o(i.UART1_Receive) refers to sci.o(.data) for g_uart1_rx_count
    sci.o(i.UART1_Send) refers to sci.o(.data) for gp_uart1_tx_address
    sci.o(i.UART1_Start) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.UART2_BaudRate) refers to sci.o(i.UART_BaudRateCal) for UART_BaudRateCal
    sci.o(i.UART2_Init) refers to sci.o(i.UART2_BaudRate) for UART2_BaudRate
    sci.o(i.UART2_Init) refers to sci.o(i.UART2_Start) for UART2_Start
    sci.o(i.UART2_Init) refers to sci_user.o(.data) for g_uart2_tx_state
    sci.o(i.UART2_Receive) refers to sci.o(.data) for g_uart2_rx_count
    sci.o(i.UART2_Send) refers to sci.o(.data) for gp_uart2_tx_address
    sci.o(i.UART2_Start) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.UART3_BaudRate) refers to sci.o(i.UART_BaudRateCal) for UART_BaudRateCal
    sci.o(i.UART3_Init) refers to sci.o(i.UART3_BaudRate) for UART3_BaudRate
    sci.o(i.UART3_Init) refers to sci.o(i.UART3_Start) for UART3_Start
    sci.o(i.UART3_Receive) refers to sci.o(.data) for g_uart3_rx_count
    sci.o(i.UART3_Send) refers to sci.o(.data) for gp_uart3_tx_address
    sci.o(i.UART3_Start) refers to sci.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    sci.o(i.UART_BaudRateCal) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    sci.o(i.UART_BaudRateCal) refers to sci.o(.constdata) for sps_tbl
    sci_user.o(i.Get_Uart2_State) refers to sci_user.o(.data) for g_uart2_tx_state
    sci_user.o(i.UART_Ch2_Send_Multiple_Byte) refers to mcu_core_protocol.o(.bss) for Uart2_tx_buf
    sci_user.o(i.UART_Ch2_Send_Multiple_Byte) refers to sci.o(.data) for gp_uart2_tx_address
    sci_user.o(i.UART_Ch2_Send_Multiple_Byte) refers to sci_user.o(.data) for g_uart2_tx_state
    sci_user.o(i.iic00_callback_master_receiveend) refers to sci.o(i.IIC00_Stop) for IIC00_Stop
    sci_user.o(i.iic00_callback_master_receiveend) refers to sci_user.o(.data) for g_iic00_rx_end
    sci_user.o(i.iic00_callback_master_sendend) refers to sci.o(i.IIC00_Stop) for IIC00_Stop
    sci_user.o(i.iic00_callback_master_sendend) refers to sci_user.o(.data) for g_iic00_tx_end
    sci_user.o(i.iic00_interrupt) refers to sci_user.o(i.iic00_callback_master_error) for iic00_callback_master_error
    sci_user.o(i.iic00_interrupt) refers to sci.o(i.IIC00_StopCondition) for IIC00_StopCondition
    sci_user.o(i.iic00_interrupt) refers to sci_user.o(i.iic00_callback_master_sendend) for iic00_callback_master_sendend
    sci_user.o(i.iic00_interrupt) refers to sci_user.o(i.iic00_callback_master_receiveend) for iic00_callback_master_receiveend
    sci_user.o(i.iic00_interrupt) refers to sci.o(.data) for g_iic00_tx_count
    sci_user.o(i.iic01_callback_master_receiveend) refers to sci.o(i.IIC01_Stop) for IIC01_Stop
    sci_user.o(i.iic01_callback_master_receiveend) refers to sci_user.o(.data) for g_iic01_rx_end
    sci_user.o(i.iic01_callback_master_sendend) refers to sci.o(i.IIC01_Stop) for IIC01_Stop
    sci_user.o(i.iic01_callback_master_sendend) refers to sci_user.o(.data) for g_iic01_tx_end
    sci_user.o(i.iic01_interrupt) refers to sci_user.o(i.iic01_callback_master_error) for iic01_callback_master_error
    sci_user.o(i.iic01_interrupt) refers to sci.o(i.IIC01_StopCondition) for IIC01_StopCondition
    sci_user.o(i.iic01_interrupt) refers to sci_user.o(i.iic01_callback_master_sendend) for iic01_callback_master_sendend
    sci_user.o(i.iic01_interrupt) refers to sci_user.o(i.iic01_callback_master_receiveend) for iic01_callback_master_receiveend
    sci_user.o(i.iic01_interrupt) refers to sci.o(.data) for g_iic01_tx_count
    sci_user.o(i.iic20_callback_master_receiveend) refers to sci.o(i.IIC20_Stop) for IIC20_Stop
    sci_user.o(i.iic20_callback_master_receiveend) refers to sci_user.o(.data) for g_iic20_rx_end
    sci_user.o(i.iic20_callback_master_sendend) refers to sci.o(i.IIC20_Stop) for IIC20_Stop
    sci_user.o(i.iic20_callback_master_sendend) refers to sci_user.o(.data) for g_iic20_tx_end
    sci_user.o(i.iic20_interrupt) refers to sci_user.o(i.iic20_callback_master_error) for iic20_callback_master_error
    sci_user.o(i.iic20_interrupt) refers to sci.o(i.IIC20_StopCondition) for IIC20_StopCondition
    sci_user.o(i.iic20_interrupt) refers to sci_user.o(i.iic20_callback_master_sendend) for iic20_callback_master_sendend
    sci_user.o(i.iic20_interrupt) refers to sci_user.o(i.iic20_callback_master_receiveend) for iic20_callback_master_receiveend
    sci_user.o(i.iic20_interrupt) refers to sci.o(.data) for g_iic20_tx_count
    sci_user.o(i.iic21_callback_master_receiveend) refers to sci.o(i.IIC21_Stop) for IIC21_Stop
    sci_user.o(i.iic21_callback_master_receiveend) refers to sci_user.o(.data) for g_iic21_rx_end
    sci_user.o(i.iic21_callback_master_sendend) refers to sci.o(i.IIC21_Stop) for IIC21_Stop
    sci_user.o(i.iic21_callback_master_sendend) refers to sci_user.o(.data) for g_iic21_tx_end
    sci_user.o(i.iic21_interrupt) refers to sci_user.o(i.iic21_callback_master_error) for iic21_callback_master_error
    sci_user.o(i.iic21_interrupt) refers to sci.o(i.IIC21_StopCondition) for IIC21_StopCondition
    sci_user.o(i.iic21_interrupt) refers to sci_user.o(i.iic21_callback_master_sendend) for iic21_callback_master_sendend
    sci_user.o(i.iic21_interrupt) refers to sci_user.o(i.iic21_callback_master_receiveend) for iic21_callback_master_receiveend
    sci_user.o(i.iic21_interrupt) refers to sci.o(.data) for g_iic21_tx_count
    sci_user.o(i.iic30_callback_master_receiveend) refers to sci.o(i.IIC30_Stop) for IIC30_Stop
    sci_user.o(i.iic30_callback_master_receiveend) refers to sci_user.o(.data) for g_iic30_rx_end
    sci_user.o(i.iic30_callback_master_sendend) refers to sci.o(i.IIC30_Stop) for IIC30_Stop
    sci_user.o(i.iic30_callback_master_sendend) refers to sci_user.o(.data) for g_iic30_tx_end
    sci_user.o(i.iic30_interrupt) refers to sci_user.o(i.iic30_callback_master_error) for iic30_callback_master_error
    sci_user.o(i.iic30_interrupt) refers to sci.o(i.IIC30_StopCondition) for IIC30_StopCondition
    sci_user.o(i.iic30_interrupt) refers to sci_user.o(i.iic30_callback_master_sendend) for iic30_callback_master_sendend
    sci_user.o(i.iic30_interrupt) refers to sci_user.o(i.iic30_callback_master_receiveend) for iic30_callback_master_receiveend
    sci_user.o(i.iic30_interrupt) refers to sci.o(.data) for g_iic30_tx_count
    sci_user.o(i.iic31_callback_master_receiveend) refers to sci.o(i.IIC31_Stop) for IIC31_Stop
    sci_user.o(i.iic31_callback_master_receiveend) refers to sci_user.o(.data) for g_iic31_rx_end
    sci_user.o(i.iic31_callback_master_sendend) refers to sci.o(i.IIC31_Stop) for IIC31_Stop
    sci_user.o(i.iic31_callback_master_sendend) refers to sci_user.o(.data) for g_iic31_tx_end
    sci_user.o(i.iic31_interrupt) refers to sci_user.o(i.iic31_callback_master_error) for iic31_callback_master_error
    sci_user.o(i.iic31_interrupt) refers to sci.o(i.IIC31_StopCondition) for IIC31_StopCondition
    sci_user.o(i.iic31_interrupt) refers to sci_user.o(i.iic31_callback_master_sendend) for iic31_callback_master_sendend
    sci_user.o(i.iic31_interrupt) refers to sci_user.o(i.iic31_callback_master_receiveend) for iic31_callback_master_receiveend
    sci_user.o(i.iic31_interrupt) refers to sci.o(.data) for g_iic31_tx_count
    sci_user.o(i.spi00_callback_receiveend) refers to sci.o(.data) for gp_spi00_rx_address
    sci_user.o(i.spi00_callback_sendend) refers to sci.o(.data) for gp_spi00_tx_address
    sci_user.o(i.spi00_interrupt) refers to sci_user.o(i.spi00_callback_error) for spi00_callback_error
    sci_user.o(i.spi00_interrupt) refers to sci_user.o(i.spi00_callback_receiveend) for spi00_callback_receiveend
    sci_user.o(i.spi00_interrupt) refers to sci_user.o(i.spi00_callback_sendend) for spi00_callback_sendend
    sci_user.o(i.spi00_interrupt) refers to sci.o(.data) for g_spi00_tx_count
    sci_user.o(i.spi01_callback_receiveend) refers to sci.o(i.SPI01_Stop) for SPI01_Stop
    sci_user.o(i.spi01_callback_receiveend) refers to sci.o(.data) for gp_spi01_rx_address
    sci_user.o(i.spi01_callback_sendend) refers to sci.o(i.SPI01_Stop) for SPI01_Stop
    sci_user.o(i.spi01_callback_sendend) refers to sci.o(.data) for gp_spi01_tx_address
    sci_user.o(i.spi01_interrupt) refers to sci_user.o(i.spi01_callback_error) for spi01_callback_error
    sci_user.o(i.spi01_interrupt) refers to sci_user.o(i.spi01_callback_receiveend) for spi01_callback_receiveend
    sci_user.o(i.spi01_interrupt) refers to sci_user.o(i.spi01_callback_sendend) for spi01_callback_sendend
    sci_user.o(i.spi01_interrupt) refers to sci.o(.data) for g_spi01_tx_count
    sci_user.o(i.spi10_callback_receiveend) refers to sci.o(.data) for gp_spi10_rx_address
    sci_user.o(i.spi10_callback_sendend) refers to sci.o(.data) for gp_spi10_tx_address
    sci_user.o(i.spi10_interrupt) refers to sci_user.o(i.spi10_callback_error) for spi10_callback_error
    sci_user.o(i.spi10_interrupt) refers to sci_user.o(i.spi10_callback_receiveend) for spi10_callback_receiveend
    sci_user.o(i.spi10_interrupt) refers to sci_user.o(i.spi10_callback_sendend) for spi10_callback_sendend
    sci_user.o(i.spi10_interrupt) refers to sci.o(.data) for g_spi10_tx_count
    sci_user.o(i.spi11_callback_receiveend) refers to sci.o(i.SPI11_Stop) for SPI11_Stop
    sci_user.o(i.spi11_callback_receiveend) refers to sci.o(.data) for gp_spi11_rx_address
    sci_user.o(i.spi11_callback_sendend) refers to sci.o(i.SPI11_Stop) for SPI11_Stop
    sci_user.o(i.spi11_callback_sendend) refers to sci.o(.data) for gp_spi11_tx_address
    sci_user.o(i.spi11_interrupt) refers to sci_user.o(i.spi11_callback_error) for spi11_callback_error
    sci_user.o(i.spi11_interrupt) refers to sci_user.o(i.spi11_callback_receiveend) for spi11_callback_receiveend
    sci_user.o(i.spi11_interrupt) refers to sci_user.o(i.spi11_callback_sendend) for spi11_callback_sendend
    sci_user.o(i.spi11_interrupt) refers to sci.o(.data) for g_spi11_tx_count
    sci_user.o(i.spi20_callback_receiveend) refers to sci.o(.data) for gp_spi20_rx_address
    sci_user.o(i.spi20_callback_sendend) refers to sci.o(.data) for gp_spi20_tx_address
    sci_user.o(i.spi20_interrupt) refers to sci_user.o(i.spi20_callback_error) for spi20_callback_error
    sci_user.o(i.spi20_interrupt) refers to sci_user.o(i.spi20_callback_receiveend) for spi20_callback_receiveend
    sci_user.o(i.spi20_interrupt) refers to sci_user.o(i.spi20_callback_sendend) for spi20_callback_sendend
    sci_user.o(i.spi20_interrupt) refers to sci.o(.data) for g_spi20_tx_count
    sci_user.o(i.spi21_callback_receiveend) refers to sci.o(.data) for gp_spi21_rx_address
    sci_user.o(i.spi21_callback_sendend) refers to sci.o(.data) for gp_spi21_tx_address
    sci_user.o(i.spi21_interrupt) refers to sci_user.o(i.spi21_callback_error) for spi21_callback_error
    sci_user.o(i.spi21_interrupt) refers to sci_user.o(i.spi21_callback_receiveend) for spi21_callback_receiveend
    sci_user.o(i.spi21_interrupt) refers to sci_user.o(i.spi21_callback_sendend) for spi21_callback_sendend
    sci_user.o(i.spi21_interrupt) refers to sci.o(.data) for g_spi21_tx_count
    sci_user.o(i.spi30_callback_receiveend) refers to sci.o(.data) for gp_spi30_rx_address
    sci_user.o(i.spi30_callback_sendend) refers to sci.o(.data) for gp_spi30_tx_address
    sci_user.o(i.spi30_interrupt) refers to sci_user.o(i.spi30_callback_error) for spi30_callback_error
    sci_user.o(i.spi30_interrupt) refers to sci_user.o(i.spi30_callback_receiveend) for spi30_callback_receiveend
    sci_user.o(i.spi30_interrupt) refers to sci_user.o(i.spi30_callback_sendend) for spi30_callback_sendend
    sci_user.o(i.spi30_interrupt) refers to sci.o(.data) for g_spi30_tx_count
    sci_user.o(i.spi31_callback_receiveend) refers to sci.o(.data) for gp_spi31_rx_address
    sci_user.o(i.spi31_callback_sendend) refers to sci.o(.data) for gp_spi31_tx_address
    sci_user.o(i.spi31_interrupt) refers to sci_user.o(i.spi31_callback_error) for spi31_callback_error
    sci_user.o(i.spi31_interrupt) refers to sci_user.o(i.spi31_callback_receiveend) for spi31_callback_receiveend
    sci_user.o(i.spi31_interrupt) refers to sci_user.o(i.spi31_callback_sendend) for spi31_callback_sendend
    sci_user.o(i.spi31_interrupt) refers to sci.o(.data) for g_spi31_tx_count
    sci_user.o(i.uart0_interrupt_send) refers to sci_user.o(i.uart0_callback_sendend) for uart0_callback_sendend
    sci_user.o(i.uart0_interrupt_send) refers to sci.o(.data) for g_uart0_tx_count
    sci_user.o(i.uart1_interrupt_receive) refers to sci_user.o(i.uart1_callback_error) for uart1_callback_error
    sci_user.o(i.uart1_interrupt_receive) refers to sci_user.o(i.uart1_callback_receiveend) for uart1_callback_receiveend
    sci_user.o(i.uart1_interrupt_receive) refers to sci_user.o(i.uart1_callback_softwareoverrun) for uart1_callback_softwareoverrun
    sci_user.o(i.uart1_interrupt_receive) refers to sci.o(.data) for g_uart1_rx_length
    sci_user.o(i.uart1_interrupt_send) refers to sci_user.o(i.uart1_callback_sendend) for uart1_callback_sendend
    sci_user.o(i.uart1_interrupt_send) refers to sci.o(.data) for g_uart1_tx_count
    sci_user.o(i.uart2_Get_0x10_Rev_Flag) refers to sci_user.o(.data) for uart_0x10_Rev_Flag
    sci_user.o(i.uart2_User_KL15_Init) refers to sci_user.o(.data) for uart_0x10_Rev_Flag
    sci_user.o(i.uart2_User_KL30_Init) refers to sci.o(.data) for g_uart2_rx_count
    sci_user.o(i.uart2_callback_error) refers to sci.o(.data) for g_uart2_rx_count
    sci_user.o(i.uart2_callback_sendend) refers to sci_user.o(.data) for g_uart2_tx_state
    sci_user.o(i.uart2_interrupt_send) refers to sci_user.o(i.uart2_callback_sendend) for uart2_callback_sendend
    sci_user.o(i.uart2_interrupt_send) refers to sci.o(.data) for g_uart2_tx_count
    sci_user.o(i.uart3_interrupt_receive) refers to sci_user.o(i.uart3_callback_error) for uart3_callback_error
    sci_user.o(i.uart3_interrupt_receive) refers to sci_user.o(i.uart3_callback_receiveend) for uart3_callback_receiveend
    sci_user.o(i.uart3_interrupt_receive) refers to sci_user.o(i.uart3_callback_softwareoverrun) for uart3_callback_softwareoverrun
    sci_user.o(i.uart3_interrupt_receive) refers to sci.o(.data) for g_uart3_rx_length
    sci_user.o(i.uart3_interrupt_send) refers to sci_user.o(i.uart3_callback_sendend) for uart3_callback_sendend
    sci_user.o(i.uart3_interrupt_send) refers to sci.o(.data) for g_uart3_tx_count
    clk.o(i.Clock_Init) refers to clk.o(i.CLK_Osc_Setting) for CLK_Osc_Setting
    clk.o(i.Clock_Init) refers to clk.o(i.CLK_PLL_Setting) for CLK_PLL_Setting
    clk.o(i.Clock_Init) refers to clk.o(i.CLK_PLL_Start) for CLK_PLL_Start
    clk.o(i.Clock_Init) refers to clk.o(sram_code) for CLK_Fclk_Select
    clk.o(i.Clock_Init) refers to system_bat32a239.o(.data) for SystemCoreClock
    clk.o(i.Sys_Enter_Sleep_Mode) refers to intp.o(i.INTP_Init) for INTP_Init
    clk.o(i.Sys_Enter_Sleep_Mode) refers to intp.o(i.INTP_Start) for INTP_Start
    clk.o(i.Sys_Enter_Sleep_Mode) refers to system_monitor_user.o(i.System_LINE_KL15) for System_LINE_KL15
    intp_user.o(i.intp0_callback) refers to intp_user.o(.data) for g_intp0Taken
    intp_user.o(i.intp0_interrupt) refers to intp_user.o(i.intp0_callback) for intp0_callback
    intp_user.o(i.intp10_callback) refers to intp_user.o(.data) for g_intp10Taken
    intp_user.o(i.intp10_interrupt) refers to intp_user.o(i.intp10_callback) for intp10_callback
    intp_user.o(i.intp11_callback) refers to intp_user.o(.data) for g_intp11Taken
    intp_user.o(i.intp11_interrupt) refers to intp_user.o(i.intp11_callback) for intp11_callback
    intp_user.o(i.intp1_callback) refers to intp_user.o(.data) for g_intp1Taken
    intp_user.o(i.intp1_interrupt) refers to intp_user.o(i.intp1_callback) for intp1_callback
    intp_user.o(i.intp2_callback) refers to intp_user.o(.data) for g_intp2Taken
    intp_user.o(i.intp2_interrupt) refers to intp_user.o(i.intp2_callback) for intp2_callback
    intp_user.o(i.intp3_callback) refers to intp_user.o(.data) for g_intp3Taken
    intp_user.o(i.intp3_interrupt) refers to intp_user.o(i.intp3_callback) for intp3_callback
    intp_user.o(i.intp4_callback) refers to intp_user.o(.data) for g_intp4Taken
    intp_user.o(i.intp4_interrupt) refers to intp_user.o(i.intp4_callback) for intp4_callback
    intp_user.o(i.intp5_callback) refers to intp_user.o(.data) for g_intp5Taken
    intp_user.o(i.intp5_interrupt) refers to intp_user.o(i.intp5_callback) for intp5_callback
    intp_user.o(i.intp6_callback) refers to intp_user.o(.data) for g_intp6Taken
    intp_user.o(i.intp6_interrupt) refers to intp_user.o(i.intp6_callback) for intp6_callback
    intp_user.o(i.intp7_callback) refers to intp_user.o(.data) for g_intp7Taken
    intp_user.o(i.intp7_interrupt) refers to intp_user.o(i.intp7_callback) for intp7_callback
    intp_user.o(i.intp8_callback) refers to intp_user.o(.data) for g_intp8Taken
    intp_user.o(i.intp8_interrupt) refers to intp_user.o(i.intp8_callback) for intp8_callback
    intp_user.o(i.intp9_callback) refers to intp_user.o(.data) for g_intp9Taken
    intp_user.o(i.intp9_interrupt) refers to intp_user.o(i.intp9_callback) for intp9_callback
    tim4.o(i.Capture_Init) refers to tim4.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    tim4.o(i.Capture_Stop) refers to tim4.o(i.__NVIC_ClearPendingIRQ) for __NVIC_ClearPendingIRQ
    rtc.o(i.Get_RTC_Time) refers to rtc.o(.data) for calendar
    rtc.o(i.RTC_Init) refers to rtc.o(i.RTC_Start) for RTC_Start
    rtc.o(i.RTC_Init) refers to rtc.o(i.RTC_Set_CounterValue) for RTC_Set_CounterValue
    rtc.o(i.RTC_Service) refers to rtc.o(i.RTC_Get_CounterValue) for RTC_Get_CounterValue
    rtc.o(i.RTC_Service) refers to rtc.o(.data) for calendar
    timera_b_c.o(i.TMB0_PWM_Pin33_Freq_Duty) refers to aeabi_sdivfast.o(.text) for __aeabi_idivmod
    timera_b_c.o(i.TMB0_PWM_Pin33_Init) refers to aeabi_sdivfast.o(.text) for __aeabi_idivmod
    timera_b_c.o(i.TMB0_PWM_Pin33_Init) refers to timera_b_c.o(i.TMB0_Start) for TMB0_Start
    timera_b_c.o(i.TMB0_Stop) refers to gpio.o(i.PORT_Init) for PORT_Init
    timera_b_c.o(i.TMB0_Stop) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    timera_b_c.o(i.bsp_TMA0_IntervalTimer) refers to timera_b_c.o(i.TMA0_Start) for TMA0_Start
    can.o(i.SetBaudRadio) refers to can.o(.data) for C0BTR_Reg
    can.o(i.bsp_CAN0_Rev_isr) refers to can.o(i.memcpy1) for memcpy1
    can.o(i.bsp_CAN0_Rev_isr) refers to app_service.o(i.App_SetSessionTimer) for App_SetSessionTimer
    can.o(i.bsp_CAN0_Rev_isr) refers to link_layer.o(i.LK_Link_main) for LK_Link_main
    can.o(i.bsp_CAN0_Rev_isr) refers to u2_link_layer.o(i.U2_LK_Link_main) for U2_LK_Link_main
    can.o(i.bsp_CAN0_Rev_isr) refers to can_user.o(i.Can_Receive_Msg) for Can_Receive_Msg
    can.o(i.bsp_CAN0_Rev_isr) refers to can_user.o(i.Set_CanSleepDelayTime) for Set_CanSleepDelayTime
    can.o(i.bsp_CAN0_Rev_isr) refers to app_service.o(.bss) for DiagnoCtl
    can.o(i.bsp_CAN0_Tx_isr) refers to can.o(.data) for CanSendLock
    can.o(i.bsp_CANSendFrame) refers to can_user.o(i.Set_CanSleepDelayTime) for Set_CanSleepDelayTime
    can.o(i.bsp_CAN_BusOff_Recover) refers to can.o(i.SetBaudRadio) for SetBaudRadio
    can.o(i.bsp_CAN_BusOff_Recover) refers to can.o(.data) for C0IE_Reg
    can.o(i.bsp_CAN_Init) refers to can.o(i.SetBaudRadio) for SetBaudRadio
    can.o(i.bsp_CAN_Init) refers to can.o(i.bsp_CanBuf_Clear) for bsp_CanBuf_Clear
    can.o(i.bsp_CAN_Init) refers to can.o(i.bsp_CanBuf_Init) for bsp_CanBuf_Init
    can.o(i.bsp_CAN_Init) refers to can.o(i.bsp_tx_msgbuf_init) for bsp_tx_msgbuf_init
    can.o(i.bsp_CAN_Init) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    can.o(i.bsp_CAN_Init) refers to can.o(.data) for C0IE_Reg
    can.o(i.bsp_CanBuf_Init) refers to can.o(i.bsp_rx_mask_init) for bsp_rx_mask_init
    can.o(i.bsp_CanBuf_Init) refers to can.o(i.bsp_rx_msgbuf_init) for bsp_rx_msgbuf_init
    can.o(i.bsp_Is_CAN_Sleep) refers to can_user.o(i.Get_RSCAN0Busoff_Status) for Get_RSCAN0Busoff_Status
    can.o(i.bsp_Is_CAN_Sleep) refers to can.o(i.bsp_CAN_BusOff_Recover) for bsp_CAN_BusOff_Recover
    can.o(i.bsp_Is_CAN_Sleep) refers to can.o(i.bsp_tx_msgbuf_abort) for bsp_tx_msgbuf_abort
    can.o(i.bsp_Is_CAN_Sleep) refers to can.o(i.bsp_CAN_Sleep) for bsp_CAN_Sleep
    can.o(i.bsp_rx_msgbuf_init) refers to gpio.o(i.__ARM_common_switch8) for __ARM_common_switch8
    bu98r10.o(i.BU98R10_All_ReadRam) refers to bu98r10.o(i.BU98R10_All_Command_Write) for BU98R10_All_Command_Write
    bu98r10.o(i.BU98R10_All_ReadRam) refers to bu98r10.o(i.BU98R10_All_Data_Write) for BU98R10_All_Data_Write
    bu98r10.o(i.BU98R10_Init) refers to bu98r10.o(i.BU98R10_All_Command_Write) for BU98R10_All_Command_Write
    bu98r10.o(i.BU98R10_Init) refers to bu98r10.o(i.BU98R10_All_Data_Write) for BU98R10_All_Data_Write
    bu98r10.o(i.BU98R10_Init) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    bu98r10.o(i.BU98R10_Init) refers to bu98r10.o(.data) for BU98R10Update
    bu98r10.o(i.BU98R10_Shutdown) refers to bu98r10.o(i.BU98R10_All_Command_Write) for BU98R10_All_Command_Write
    bu98r10.o(i.BU98R10_Update_Request) refers to bu98r10.o(.data) for u8BU98R10CheckCount
    bu98r10.o(i.BU98R10_Update_Service) refers to gpio.o(i.__ARM_common_switch8) for __ARM_common_switch8
    bu98r10.o(i.BU98R10_Update_Service) refers to bu98r10.o(i.BU98R10_All_Command_Write) for BU98R10_All_Command_Write
    bu98r10.o(i.BU98R10_Update_Service) refers to bu98r10.o(i.BU98R10_All_Data_Write) for BU98R10_All_Data_Write
    bu98r10.o(i.BU98R10_Update_Service) refers to bu98r10.o(.data) for BU98R10Update
    bu98r10.o(i.BU98R10_Update_Service) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.Conv_Single_DECHEX) refers to rt_memclr.o(.text) for __aeabi_memclr
    seg_lcd.o(i.SEG_Coolant_Temp_Display) refers to gpio.o(i.__ARM_common_switch8) for __ARM_common_switch8
    seg_lcd.o(i.SEG_Coolant_Temp_Display) refers to seg_lcd.o(.bss) for SEGLCDBackup
    seg_lcd.o(i.SEG_Coolant_Temp_Display) refers to bu98r10.o(.bss) for BU98R10Chip1DDRAM
    seg_lcd.o(i.SEG_Fuel_Level_Display) refers to gpio.o(i.__ARM_common_switch8) for __ARM_common_switch8
    seg_lcd.o(i.SEG_Fuel_Level_Display) refers to seg_lcd.o(.bss) for SEGLCDBackup
    seg_lcd.o(i.SEG_Fuel_Level_Display) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.SEG_LCD_ABS) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.SEG_LCD_AutoStarStop) refers to bu98r10.o(.bss) for BU98R10Chip1DDRAM
    seg_lcd.o(i.SEG_LCD_BatteryErr_Display) refers to mcu_core_protocol.o(.data) for BatteryErrFlg
    seg_lcd.o(i.SEG_LCD_BatteryErr_Display) refers to seg_lcd.o(.bss) for SEGLCDBackup
    seg_lcd.o(i.SEG_LCD_BatteryErr_Display) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.SEG_LCD_Battery_Voltage_Display) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    seg_lcd.o(i.SEG_LCD_Battery_Voltage_Display) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    seg_lcd.o(i.SEG_LCD_Battery_Voltage_Display) refers to seg_lcd.o(.bss) for SEGLCDBackup
    seg_lcd.o(i.SEG_LCD_Battery_Voltage_Display) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.SEG_LCD_Battery_Voltage_Display) refers to seg_lcd.o(.constdata) for SEG_DISPLAY_NUMBER0
    seg_lcd.o(i.SEG_LCD_Battery_Voltage_Display) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    seg_lcd.o(i.SEG_LCD_Battery_Voltage_Selftest) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    seg_lcd.o(i.SEG_LCD_Battery_Voltage_Selftest) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    seg_lcd.o(i.SEG_LCD_Battery_Voltage_Selftest) refers to seg_lcd.o(.bss) for SEGLCDBackup
    seg_lcd.o(i.SEG_LCD_Battery_Voltage_Selftest) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.SEG_LCD_Battery_Voltage_Selftest) refers to seg_lcd.o(.constdata) for SEG_DISPLAY_NUMBER0
    seg_lcd.o(i.SEG_LCD_Batterylow) refers to bu98r10.o(.bss) for BU98R10Chip1DDRAM
    seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Display) refers to aeabi_sdivfast.o(.text) for __aeabi_idivmod
    seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Display) refers to gpio.o(i.__ARM_common_switch8) for __ARM_common_switch8
    seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Display) refers to seg_lcd.o(.data) for OldSpeedStand
    seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Display) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Display) refers to seg_lcd.o(.bss) for SEGLCDBackup
    seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Selftest) refers to aeabi_sdivfast.o(.text) for __aeabi_idivmod
    seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Selftest) refers to gpio.o(i.__ARM_common_switch8) for __ARM_common_switch8
    seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Selftest) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Selftest) refers to seg_lcd.o(.bss) for SEGLCDBackup
    seg_lcd.o(i.SEG_LCD_FaultCode_Display) refers to seg_lcd.o(i.Conv_Single_DECHEX) for Conv_Single_DECHEX
    seg_lcd.o(i.SEG_LCD_FaultCode_Display) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.SEG_LCD_FaultCode_Display) refers to seg_lcd.o(.bss) for SEGLCDBackup
    seg_lcd.o(i.SEG_LCD_FaultCode_Display) refers to seg_lcd.o(.constdata) for SEG_HEX_DISPLAY_NUMBER0
    seg_lcd.o(i.SEG_LCD_Fuel) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.SEG_LCD_Gear_Display) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    seg_lcd.o(i.SEG_LCD_Gear_Display) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    seg_lcd.o(i.SEG_LCD_Gear_Display) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    seg_lcd.o(i.SEG_LCD_Gear_Display) refers to seg_lcd.o(.data) for Gear
    seg_lcd.o(i.SEG_LCD_Gear_Display) refers to seg_lcd.o(.bss) for SEGLCDBackup
    seg_lcd.o(i.SEG_LCD_Gear_Display) refers to bu98r10.o(.bss) for BU98R10Chip1DDRAM
    seg_lcd.o(i.SEG_LCD_Gear_Display) refers to seg_lcd.o(.constdata) for SEG_DISPLAY_NUMBER0
    seg_lcd.o(i.SEG_LCD_Gear_Selftest) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    seg_lcd.o(i.SEG_LCD_Gear_Selftest) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    seg_lcd.o(i.SEG_LCD_Gear_Selftest) refers to seg_lcd.o(.bss) for SEGLCDBackup
    seg_lcd.o(i.SEG_LCD_Gear_Selftest) refers to bu98r10.o(.bss) for BU98R10Chip1DDRAM
    seg_lcd.o(i.SEG_LCD_Gear_Selftest) refers to seg_lcd.o(.constdata) for SEG_DISPLAY_NUMBER0
    seg_lcd.o(i.SEG_LCD_HI_BEAM) refers to bu98r10.o(.bss) for BU98R10Chip1DDRAM
    seg_lcd.o(i.SEG_LCD_HighBeam) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.SEG_LCD_Init) refers to seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Display) for SEG_LCD_Vehicle_Speed_Num_Display
    seg_lcd.o(i.SEG_LCD_Init) refers to seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Display) for SEG_LCD_Engine_Speed_Seg_Display
    seg_lcd.o(i.SEG_LCD_Init) refers to seg_lcd.o(i.SEG_LCD_ODO_Trip_Display) for SEG_LCD_ODO_Trip_Display
    seg_lcd.o(i.SEG_LCD_Init) refers to seg_lcd.o(i.SEG_Fuel_Level_Display) for SEG_Fuel_Level_Display
    seg_lcd.o(i.SEG_LCD_Init) refers to seg_lcd.o(i.SEG_LCD_Battery_Voltage_Display) for SEG_LCD_Battery_Voltage_Display
    seg_lcd.o(i.SEG_LCD_Init) refers to seg_lcd.o(i.SEG_Coolant_Temp_Display) for SEG_Coolant_Temp_Display
    seg_lcd.o(i.SEG_LCD_Init) refers to seg_lcd.o(i.SEG_LCD_Gear_Display) for SEG_LCD_Gear_Display
    seg_lcd.o(i.SEG_LCD_Init) refers to bu98r10.o(i.BU98R10_Init) for BU98R10_Init
    seg_lcd.o(i.SEG_LCD_LeftTurn) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.SEG_LCD_OBD) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.SEG_LCD_ODO_Trip_Display) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    seg_lcd.o(i.SEG_LCD_ODO_Trip_Display) refers to seg_lcd.o(.bss) for SEGLCDBackup
    seg_lcd.o(i.SEG_LCD_ODO_Trip_Display) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.SEG_LCD_ODO_Trip_Display) refers to seg_lcd.o(.constdata) for SEG_UNDISPLAY_NUMBER0
    seg_lcd.o(i.SEG_LCD_ODO_Trip_FaultCode_Selftest) refers to aeabi_sdivfast.o(.text) for __aeabi_idivmod
    seg_lcd.o(i.SEG_LCD_ODO_Trip_FaultCode_Selftest) refers to seg_lcd.o(.bss) for SEGLCDBackup
    seg_lcd.o(i.SEG_LCD_ODO_Trip_FaultCode_Selftest) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.SEG_LCD_ODO_Trip_FaultCode_Selftest) refers to seg_lcd.o(.constdata) for SEG_DISPLAY_NUMBER0
    seg_lcd.o(i.SEG_LCD_OilPressure) refers to bu98r10.o(.bss) for BU98R10Chip1DDRAM
    seg_lcd.o(i.SEG_LCD_READY) refers to bu98r10.o(.bss) for BU98R10Chip1DDRAM
    seg_lcd.o(i.SEG_LCD_RightTurn) refers to bu98r10.o(.bss) for BU98R10Chip1DDRAM
    seg_lcd.o(i.SEG_LCD_Shore) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.SEG_LCD_Shutdown) refers to bu98r10.o(i.BU98R10_Shutdown) for BU98R10_Shutdown
    seg_lcd.o(i.SEG_LCD_Shutdown) refers to app_telltales.o(i.App_Telltales_AllOFF) for App_Telltales_AllOFF
    seg_lcd.o(i.SEG_LCD_Shutdown) refers to seg_lcd.o(.bss) for SEGLCDBackup
    seg_lcd.o(i.SEG_LCD_TSC) refers to bu98r10.o(.bss) for BU98R10Chip1DDRAM
    seg_lcd.o(i.SEG_LCD_Temp) refers to bu98r10.o(.bss) for BU98R10Chip1DDRAM
    seg_lcd.o(i.SEG_LCD_TirePressure) refers to bu98r10.o(.bss) for BU98R10Chip0DDRAM
    seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Display) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Display) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Display) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Display) refers to seg_lcd.o(.bss) for SEGLCDBackup
    seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Display) refers to bu98r10.o(.bss) for BU98R10Chip1DDRAM
    seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Display) refers to seg_lcd.o(.constdata) for SEG_DISPLAY_NUMBER0
    seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Selftest) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Selftest) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Selftest) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Selftest) refers to seg_lcd.o(.bss) for SEGLCDBackup
    seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Selftest) refers to bu98r10.o(.bss) for BU98R10Chip1DDRAM
    seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Selftest) refers to seg_lcd.o(.constdata) for SEG_DISPLAY_NUMBER0
    is31fl3236.o(i.IS31FL3236_Clear) refers to is31fl3236.o(.bss) for u8IS31Data
    is31fl3236.o(i.IS31FL3236_Init) refers to is31fl3236.o(i.IS31_Set_SDB_Pin) for IS31_Set_SDB_Pin
    is31fl3236.o(i.IS31FL3236_Init) refers to is31_iic_master.o(i.IS31_IIC_delay) for IS31_IIC_delay
    is31fl3236.o(i.IS31FL3236_Init) refers to is31_iic_master.o(i.IS31_IIC_Start) for IS31_IIC_Start
    is31fl3236.o(i.IS31FL3236_Init) refers to is31_iic_master.o(i.IS31_IIC_SendByte) for IS31_IIC_SendByte
    is31fl3236.o(i.IS31FL3236_Init) refers to is31_iic_master.o(i.IS31_IIC_WaitAck) for IS31_IIC_WaitAck
    is31fl3236.o(i.IS31FL3236_Init) refers to is31_iic_master.o(i.IS31_IIC_Stop) for IS31_IIC_Stop
    is31fl3236.o(i.IS31FL3236_Init) refers to is31_iic_master.o(i.IS31_IIC_ReadByte) for IS31_IIC_ReadByte
    is31fl3236.o(i.IS31FL3236_Init) refers to is31_iic_master.o(i.IS31_IIC_ACK) for IS31_IIC_ACK
    is31fl3236.o(i.IS31FL3236_Init) refers to is31fl3236.o(i.extend_i2c_write_one_byte) for extend_i2c_write_one_byte
    is31fl3236.o(i.IS31FL3236_Init) refers to wdt.o(i.WDT_Restart) for WDT_Restart
    is31fl3236.o(i.IS31FL3236_Init) refers to is31fl3236.o(.bss) for u8IS31Data
    is31fl3236.o(i.IS31FL3236_Init) refers to is31fl3236.o(.data) for chipType
    is31fl3236.o(i.IS31FL3236_Init) refers to is31_iic_master.o(.data) for IIC_addr
    is31fl3236.o(i.IS31FL3236_Update) refers to is31fl3236.o(i.IS31_Set_SDB_Pin) for IS31_Set_SDB_Pin
    is31fl3236.o(i.IS31FL3236_Update) refers to wdt.o(i.WDT_Restart) for WDT_Restart
    is31fl3236.o(i.IS31FL3236_Update) refers to is31fl3236.o(i.IS31FL3236_Init) for IS31FL3236_Init
    is31fl3236.o(i.IS31FL3236_Update) refers to is31_iic_master.o(i.IS31_IIC_Start) for IS31_IIC_Start
    is31fl3236.o(i.IS31FL3236_Update) refers to is31_iic_master.o(i.IS31_IIC_SendByte) for IS31_IIC_SendByte
    is31fl3236.o(i.IS31FL3236_Update) refers to is31_iic_master.o(i.IS31_IIC_WaitAck) for IS31_IIC_WaitAck
    is31fl3236.o(i.IS31FL3236_Update) refers to is31_iic_master.o(i.IS31_IIC_Stop) for IS31_IIC_Stop
    is31fl3236.o(i.IS31FL3236_Update) refers to is31fl3236.o(i.extend_i2c_write_one_byte) for extend_i2c_write_one_byte
    is31fl3236.o(i.IS31FL3236_Update) refers to is31fl3236.o(.data) for IS31FLxxxx_Device_Addr
    is31fl3236.o(i.IS31FL3236_Update) refers to is31_iic_master.o(.data) for IIC_addr
    is31fl3236.o(i.IS31FL3236_Update) refers to is31fl3236.o(.bss) for u8IS31Data
    is31fl3236.o(i.IS31_OFF_Wakeup) refers to is31fl3236.o(i.IS31_Set_SDB_Pin) for IS31_Set_SDB_Pin
    is31fl3236.o(i.IS31_Set_SDB_Pin) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    is31fl3236.o(i.IS31_Set_SDB_Pin) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    is31fl3236.o(i.IS31_Shutdown) refers to is31fl3236.o(i.IS31_Set_SDB_Pin) for IS31_Set_SDB_Pin
    is31fl3236.o(i.extend_i2c_write_one_byte) refers to is31_iic_master.o(i.IS31_IIC_Start) for IS31_IIC_Start
    is31fl3236.o(i.extend_i2c_write_one_byte) refers to is31_iic_master.o(i.IS31_IIC_SendByte) for IS31_IIC_SendByte
    is31fl3236.o(i.extend_i2c_write_one_byte) refers to is31_iic_master.o(i.IS31_IIC_WaitAck) for IS31_IIC_WaitAck
    is31fl3236.o(i.extend_i2c_write_one_byte) refers to is31_iic_master.o(i.IS31_IIC_Stop) for IS31_IIC_Stop
    aw93015.o(i.GET_Key_Prosess) refers to gpio.o(i.PORT_GetBit) for PORT_GetBit
    aw93015.o(i.GET_Key_Prosess) refers to aw93015.o(i.PD_IIC_ReadReg) for PD_IIC_ReadReg
    aw93015.o(i.GET_Key_Prosess) refers to aw93015.o(.data) for IntKey
    aw93015.o(i.IIC2_SDA_OUT) refers to gpio.o(i.PORT_Init) for PORT_Init
    aw93015.o(i.IIC2_SDA_OUT) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    aw93015.o(i.IIC_SDA2_IN) refers to gpio.o(i.PORT_Init) for PORT_Init
    aw93015.o(i.Init93015_IIC) refers to gpio.o(i.PORT_Init) for PORT_Init
    aw93015.o(i.Init93015_IIC) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    aw93015.o(i.Init93015_IIC) refers to aw93015.o(i.PD_IIC_ReadReg) for PD_IIC_ReadReg
    aw93015.o(i.Init93015_IIC) refers to aw93015.o(i.PD_IIC_WriteReg) for PD_IIC_WriteReg
    aw93015.o(i.Init93015_IIC) refers to wdt.o(i.WDT_Restart) for WDT_Restart
    aw93015.o(i.Init93015_IIC) refers to aw93015.o(.data) for IntKey
    aw93015.o(i.Init93015_IIC) refers to aw93015.o(.constdata) for PD_IIC_DAC_Int
    aw93015.o(i.PD_IIC_ReadPage) refers to aw93015.o(i.bsp_IIC2_Start) for bsp_IIC2_Start
    aw93015.o(i.PD_IIC_ReadPage) refers to aw93015.o(i.bsp_IIC2_SendByte) for bsp_IIC2_SendByte
    aw93015.o(i.PD_IIC_ReadPage) refers to aw93015.o(i.bsp_IIC2_WaitAck) for bsp_IIC2_WaitAck
    aw93015.o(i.PD_IIC_ReadPage) refers to aw93015.o(i.bsp_IIC2_ReadByte) for bsp_IIC2_ReadByte
    aw93015.o(i.PD_IIC_ReadPage) refers to aw93015.o(i.bsp_IIC2_ACK) for bsp_IIC2_ACK
    aw93015.o(i.PD_IIC_ReadPage) refers to aw93015.o(i.bsp_IIC2_Stop) for bsp_IIC2_Stop
    aw93015.o(i.PD_IIC_ReadPage) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    aw93015.o(i.PD_IIC_ReadPage) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    aw93015.o(i.PD_IIC_ReadReg) refers to aw93015.o(i.PD_IIC_ReadPage) for PD_IIC_ReadPage
    aw93015.o(i.PD_IIC_WritePage) refers to aw93015.o(i.bsp_IIC2_Start) for bsp_IIC2_Start
    aw93015.o(i.PD_IIC_WritePage) refers to aw93015.o(i.bsp_IIC2_SendByte) for bsp_IIC2_SendByte
    aw93015.o(i.PD_IIC_WritePage) refers to aw93015.o(i.bsp_IIC2_WaitAck) for bsp_IIC2_WaitAck
    aw93015.o(i.PD_IIC_WritePage) refers to aw93015.o(i.bsp_IIC2_Stop) for bsp_IIC2_Stop
    aw93015.o(i.PD_IIC_WritePage) refers to aw93015.o(.data) for WR_CN
    aw93015.o(i.PD_IIC_WritePage) refers to aw93015.o(.bss) for WR_REG
    aw93015.o(i.PD_IIC_WriteReg) refers to aw93015.o(i.PD_IIC_WritePage) for PD_IIC_WritePage
    aw93015.o(i.bsp_IIC2_ACK) refers to aw93015.o(i.IIC2_SDA_OUT) for IIC2_SDA_OUT
    aw93015.o(i.bsp_IIC2_ACK) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    aw93015.o(i.bsp_IIC2_ACK) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    aw93015.o(i.bsp_IIC2_NACK) refers to aw93015.o(i.IIC2_SDA_OUT) for IIC2_SDA_OUT
    aw93015.o(i.bsp_IIC2_NACK) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    aw93015.o(i.bsp_IIC2_NACK) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    aw93015.o(i.bsp_IIC2_ReadByte) refers to aw93015.o(i.IIC_SDA2_IN) for IIC_SDA2_IN
    aw93015.o(i.bsp_IIC2_ReadByte) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    aw93015.o(i.bsp_IIC2_ReadByte) refers to gpio.o(i.PORT_GetBit) for PORT_GetBit
    aw93015.o(i.bsp_IIC2_ReadByte) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    aw93015.o(i.bsp_IIC2_SendByte) refers to aw93015.o(i.IIC2_SDA_OUT) for IIC2_SDA_OUT
    aw93015.o(i.bsp_IIC2_SendByte) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    aw93015.o(i.bsp_IIC2_SendByte) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    aw93015.o(i.bsp_IIC2_Start) refers to aw93015.o(i.IIC2_SDA_OUT) for IIC2_SDA_OUT
    aw93015.o(i.bsp_IIC2_Start) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    aw93015.o(i.bsp_IIC2_Start) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    aw93015.o(i.bsp_IIC2_Stop) refers to aw93015.o(i.IIC2_SDA_OUT) for IIC2_SDA_OUT
    aw93015.o(i.bsp_IIC2_Stop) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    aw93015.o(i.bsp_IIC2_Stop) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    aw93015.o(i.bsp_IIC2_WaitAck) refers to aw93015.o(i.IIC_SDA2_IN) for IIC_SDA2_IN
    aw93015.o(i.bsp_IIC2_WaitAck) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    aw93015.o(i.bsp_IIC2_WaitAck) refers to gpio.o(i.PORT_GetBit) for PORT_GetBit
    aw93015.o(i.bsp_IIC2_WaitAck) refers to wdt.o(i.WDT_Restart) for WDT_Restart
    aw93015.o(i.bsp_IIC2_WaitAck) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    aw93015.o(i.bsp_IIC_delay) refers to wdt.o(i.WDT_Restart) for WDT_Restart
    is31_iic_master.o(i.IIC_SDAGet) refers to gpio.o(i.PORT_GetBit) for PORT_GetBit
    is31_iic_master.o(i.IS31_IIC_ACK) refers to is31_iic_master.o(i.IS31_IIC_SDA_Dir_Out) for IS31_IIC_SDA_Dir_Out
    is31_iic_master.o(i.IS31_IIC_ACK) refers to is31_iic_master.o(i.bsp_IIC_SDA_out) for bsp_IIC_SDA_out
    is31_iic_master.o(i.IS31_IIC_ACK) refers to is31_iic_master.o(i.bsp_IIC_SCL_out) for bsp_IIC_SCL_out
    is31_iic_master.o(i.IS31_IIC_NACK) refers to is31_iic_master.o(i.IS31_IIC_SDA_Dir_Out) for IS31_IIC_SDA_Dir_Out
    is31_iic_master.o(i.IS31_IIC_NACK) refers to is31_iic_master.o(i.bsp_IIC_SDA_out) for bsp_IIC_SDA_out
    is31_iic_master.o(i.IS31_IIC_NACK) refers to is31_iic_master.o(i.bsp_IIC_SCL_out) for bsp_IIC_SCL_out
    is31_iic_master.o(i.IS31_IIC_ReadByte) refers to is31_iic_master.o(i.IS31_IIC_SDA_Dir_In) for IS31_IIC_SDA_Dir_In
    is31_iic_master.o(i.IS31_IIC_ReadByte) refers to is31_iic_master.o(i.bsp_IIC_SCL_out) for bsp_IIC_SCL_out
    is31_iic_master.o(i.IS31_IIC_ReadByte) refers to gpio.o(i.PORT_GetBit) for PORT_GetBit
    is31_iic_master.o(i.IS31_IIC_SDA_Dir_In) refers to gpio.o(i.PORT_Init) for PORT_Init
    is31_iic_master.o(i.IS31_IIC_SDA_Dir_Out) refers to gpio.o(i.PORT_Init) for PORT_Init
    is31_iic_master.o(i.IS31_IIC_SendByte) refers to is31_iic_master.o(i.IS31_IIC_SDA_Dir_Out) for IS31_IIC_SDA_Dir_Out
    is31_iic_master.o(i.IS31_IIC_SendByte) refers to is31_iic_master.o(i.bsp_IIC_SDA_out) for bsp_IIC_SDA_out
    is31_iic_master.o(i.IS31_IIC_SendByte) refers to is31_iic_master.o(i.bsp_IIC_SCL_out) for bsp_IIC_SCL_out
    is31_iic_master.o(i.IS31_IIC_Start) refers to is31_iic_master.o(i.IS31_IIC_SDA_Dir_Out) for IS31_IIC_SDA_Dir_Out
    is31_iic_master.o(i.IS31_IIC_Start) refers to is31_iic_master.o(i.bsp_IIC_SDA_out) for bsp_IIC_SDA_out
    is31_iic_master.o(i.IS31_IIC_Start) refers to is31_iic_master.o(i.bsp_IIC_SCL_out) for bsp_IIC_SCL_out
    is31_iic_master.o(i.IS31_IIC_Stop) refers to is31_iic_master.o(i.IS31_IIC_SDA_Dir_Out) for IS31_IIC_SDA_Dir_Out
    is31_iic_master.o(i.IS31_IIC_Stop) refers to is31_iic_master.o(i.bsp_IIC_SCL_out) for bsp_IIC_SCL_out
    is31_iic_master.o(i.IS31_IIC_Stop) refers to is31_iic_master.o(i.bsp_IIC_SDA_out) for bsp_IIC_SDA_out
    is31_iic_master.o(i.IS31_IIC_WaitAck) refers to is31_iic_master.o(i.IS31_IIC_SDA_Dir_In) for IS31_IIC_SDA_Dir_In
    is31_iic_master.o(i.IS31_IIC_WaitAck) refers to is31_iic_master.o(i.bsp_IIC_SCL_out) for bsp_IIC_SCL_out
    is31_iic_master.o(i.IS31_IIC_WaitAck) refers to is31_iic_master.o(i.IIC_SDAGet) for IIC_SDAGet
    is31_iic_master.o(i.IS31_IIC_WaitAck) refers to wdt.o(i.WDT_Restart) for WDT_Restart
    is31_iic_master.o(i.IS31_IIC_WaitAck) refers to is31_iic_master.o(.data) for IIC_addr
    is31_iic_master.o(i.IS31_IIC_WaitAck) refers to is31fl3236.o(.data) for IIC_3236_NACK_Time
    is31_iic_master.o(i.IS31_IIC_delay) refers to wdt.o(i.WDT_Restart) for WDT_Restart
    is31_iic_master.o(i.Simulated_IIC_2_Init) refers to is31_iic_master.o(i.IS31_IIC_SCL_Dir_Out) for IS31_IIC_SCL_Dir_Out
    is31_iic_master.o(i.Simulated_IIC_2_Init) refers to is31_iic_master.o(i.IS31_IIC_SDA_Dir_Out) for IS31_IIC_SDA_Dir_Out
    is31_iic_master.o(i.Simulated_IIC_2_Init) refers to is31_iic_master.o(i.IS31_IIC_Stop) for IS31_IIC_Stop
    is31_iic_master.o(i.Simulated_Release_SCL) refers to is31_iic_master.o(i.bsp_IIC_SCL_out) for bsp_IIC_SCL_out
    is31_iic_master.o(i.Simulated_Release_SCL) refers to is31_iic_master.o(i.IS31_IIC_delay) for IS31_IIC_delay
    main.o(i.main) refers to sys_scheduler.o(i.Sys_Init) for Sys_Init
    main.o(i.main) refers to sys_scheduler.o(i.Sys_Scheduling_Service) for Sys_Scheduling_Service
    main.o(i.main) refers to wdt.o(i.WDT_Restart) for WDT_Restart
    tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group1) refers to powermanagement_user.o(i.Power_Management_Service_user) for Power_Management_Service_user
    tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group2) refers to fuel.o(i.Fuel_Cal_Sevice) for Fuel_Cal_Sevice
    tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group4) refers to rtc.o(i.RTC_Service) for RTC_Service
    tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group4) refers to services_mileage_user.o(i.CalcODO_100ms_Services) for CalcODO_100ms_Services
    tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group6) refers to mcu_core_protocol.o(i.Drive_Info_Display_Update_Service) for Drive_Info_Display_Update_Service
    tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group7) refers to can_user.o(i.ReqSilentTimer100mSService) for ReqSilentTimer100mSService
    tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group7) refers to can_user.o(i.Can_User_Time_Service) for Can_User_Time_Service
    tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group8) refers to can.o(i.bsp_CAN_MaskCheck) for bsp_CAN_MaskCheck
    tasks.o(i.Sys_Run_Mode_10ms_Tasks) refers to common_interface.o(i.Common_SetSelfcheckStart) for Common_SetSelfcheckStart
    tasks.o(i.Sys_Run_Mode_10ms_Tasks) refers to analog_signals.o(i.Analog_Signal_Conv_Service) for Analog_Signal_Conv_Service
    tasks.o(i.Sys_Run_Mode_10ms_Tasks) refers to backgroundlight.o(i.BackLightDamp) for BackLightDamp
    tasks.o(i.Sys_Run_Mode_10ms_Tasks) refers to line_in.o(i.Line_In_Debounce_Service) for Line_In_Debounce_Service
    tasks.o(i.Sys_Run_Mode_10ms_Tasks) refers to telltales_lib.o(i.Telltales_Management) for Telltales_Management
    tasks.o(i.Sys_Run_Mode_10ms_Tasks) refers to can_user.o(i.Can_BusOff_Fun) for Can_BusOff_Fun
    tasks.o(i.Sys_Run_Mode_10ms_Tasks) refers to mcu_core_protocol.o(i.Selfcheck_Display_Update_Service) for Selfcheck_Display_Update_Service
    tasks.o(i.Sys_Run_Mode_10ms_Tasks) refers to key.o(i.Key_Status_Detect_Service) for Key_Status_Detect_Service
    tasks.o(i.Sys_Run_Mode_20ms_Tasks) refers to bu98r10.o(i.BU98R10_Update_Request) for BU98R10_Update_Request
    tasks.o(i.Sys_Run_Mode_20ms_Tasks) refers to can_user.o(i.Diag_Req_Send) for Diag_Req_Send
    tasks.o(i.Sys_Run_Mode_20ms_Tasks) refers to is31fl3236.o(i.IS31FL3236_Update) for IS31FL3236_Update
    tasks.o(i.Sys_Run_Mode_2ms_Tasks) refers to adc.o(i.Analog_Signal_Conv_Real_Time_Run) for Analog_Signal_Conv_Real_Time_Run
    tasks.o(i.Sys_Run_Mode_2ms_Tasks) refers to powermanagement.o(i.Power_Management_Service) for Power_Management_Service
    tasks.o(i.Sys_Run_Mode_2ms_Tasks) refers to system_monitor.o(i.Sys_Status_Update_Service) for Sys_Status_Update_Service
    tasks.o(i.Sys_Run_Mode_2ms_Tasks) refers to bu98r10.o(i.BU98R10_Update_Service) for BU98R10_Update_Service
    tasks.o(i.Sys_Run_Mode_50ms_Tasks) refers to flash_synchronizer.o(i.Flash_Sync_Signal_Generation_Service) for Flash_Sync_Signal_Generation_Service
    tasks.o(i.Sys_Run_Mode_50ms_Tasks) refers to bglinterface.o(i.BGTask) for BGTask
    tasks.o(i.Sys_Run_Mode_50ms_Tasks) refers to can_user.o(i.CAN_LED_Check_50msTask) for CAN_LED_Check_50msTask
    tasks.o(i.Sys_Run_Mode_50ms_Tasks) refers to can_user.o(i.SetDtcFault) for SetDtcFault
    tasks.o(i.Sys_Run_Mode_5ms_Tasks) refers to can_user.o(i.CAN_RX_Tick) for CAN_RX_Tick
    tasks.o(i.Sys_Run_Mode_Pseudo_Real_Time_Tasks) refers to app_service.o(i.Diagnosis_main) for Diagnosis_main
    tasks.o(i.Sys_Run_Mode_Pseudo_Real_Time_Tasks) refers to u2_app_service.o(i.U2_Diagnosis_main) for U2_Diagnosis_main
    tasks.o(i.Sys_Run_Mode_Pseudo_Real_Time_Tasks) refers to can_user.o(.data) for CAN_Initflag
    tasks.o(.constdata) refers to key.o(i.Get_Key1_Line_In_Sts) for Get_Key1_Line_In_Sts
    tasks.o(.constdata) refers to key.o(i.Get_Key2_Line_In_Sts) for Get_Key2_Line_In_Sts
    sys_scheduler.o(i.Sys_Init) refers to init.o(i.Sys_Startup_Init) for Sys_Startup_Init
    sys_scheduler.o(i.Sys_Init) refers to sys_scheduler.o(.bss) for SysScheduling
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to bu98r10.o(i.BU98R10_Update_Service) for BU98R10_Update_Service
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to tasks.o(i.Sys_Run_Mode_2ms_Tasks) for Sys_Run_Mode_2ms_Tasks
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to tasks.o(i.Sys_Run_Mode_5ms_Tasks) for Sys_Run_Mode_5ms_Tasks
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to tasks.o(i.Sys_Run_Mode_10ms_Tasks) for Sys_Run_Mode_10ms_Tasks
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to tasks.o(i.Sys_Run_Mode_20ms_Tasks) for Sys_Run_Mode_20ms_Tasks
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to tasks.o(i.Sys_Run_Mode_50ms_Tasks) for Sys_Run_Mode_50ms_Tasks
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group1) for Sys_Run_Mode_100ms_Tasks_Group1
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group2) for Sys_Run_Mode_100ms_Tasks_Group2
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group3) for Sys_Run_Mode_100ms_Tasks_Group3
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group4) for Sys_Run_Mode_100ms_Tasks_Group4
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group5) for Sys_Run_Mode_100ms_Tasks_Group5
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group6) for Sys_Run_Mode_100ms_Tasks_Group6
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group7) for Sys_Run_Mode_100ms_Tasks_Group7
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group8) for Sys_Run_Mode_100ms_Tasks_Group8
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group9) for Sys_Run_Mode_100ms_Tasks_Group9
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group10) for Sys_Run_Mode_100ms_Tasks_Group10
    sys_scheduler.o(i.Sys_Scheduling_Service) refers to sys_scheduler.o(.bss) for SysScheduling
    sys_scheduler.o(i.Sys_Scheduling_Tmr) refers to tasks.o(i.Sys_Run_Mode_Pseudo_Real_Time_Tasks) for Sys_Run_Mode_Pseudo_Real_Time_Tasks
    sys_scheduler.o(i.Sys_Scheduling_Tmr) refers to app_serviceproc.o(i.Diagno_Tick) for Diagno_Tick
    sys_scheduler.o(i.Sys_Scheduling_Tmr) refers to u2_app_serviceproc.o(i.U2_Diagno_Tick) for U2_Diagno_Tick
    sys_scheduler.o(i.Sys_Scheduling_Tmr) refers to can_user.o(i.CAN_TX_Tick) for CAN_TX_Tick
    sys_scheduler.o(i.Sys_Scheduling_Tmr) refers to sys_tick.o(.data) for g_u16SysRollingCounter1ms
    sys_scheduler.o(i.Sys_Scheduling_Tmr) refers to sys_scheduler.o(.bss) for SysScheduling
    sys_scheduler.o(i.Sys_Scheduling_Tmr) refers to can_user.o(.data) for CAN_Initflag
    init.o(i.Sys_Startup_Init) refers to clk.o(i.Clock_Init) for Clock_Init
    init.o(i.Sys_Startup_Init) refers to gpio.o(i.GPIO_Init) for GPIO_Init
    init.o(i.Sys_Startup_Init) refers to is31_iic_master.o(i.Simulated_IIC_2_Init) for Simulated_IIC_2_Init
    init.o(i.Sys_Startup_Init) refers to is31fl3236.o(i.IS31FL3236_Init) for IS31FL3236_Init
    init.o(i.Sys_Startup_Init) refers to seg_lcd.o(i.SEG_LCD_Init) for SEG_LCD_Init
    init.o(i.Sys_Startup_Init) refers to seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Display) for SEG_LCD_Vehicle_Speed_Num_Display
    init.o(i.Sys_Startup_Init) refers to seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Display) for SEG_LCD_Engine_Speed_Seg_Display
    init.o(i.Sys_Startup_Init) refers to seg_lcd.o(i.SEG_LCD_ODO_Trip_Display) for SEG_LCD_ODO_Trip_Display
    init.o(i.Sys_Startup_Init) refers to seg_lcd.o(i.SEG_Fuel_Level_Display) for SEG_Fuel_Level_Display
    init.o(i.Sys_Startup_Init) refers to seg_lcd.o(i.SEG_LCD_Battery_Voltage_Display) for SEG_LCD_Battery_Voltage_Display
    init.o(i.Sys_Startup_Init) refers to seg_lcd.o(i.SEG_LCD_Gear_Display) for SEG_LCD_Gear_Display
    init.o(i.Sys_Startup_Init) refers to sys_tick.o(i.Sys_Tick_Timer_Start) for Sys_Tick_Timer_Start
    init.o(i.Sys_Startup_Init) refers to analog_signals.o(i.Analog_Signal_Conv_Init) for Analog_Signal_Conv_Init
    init.o(i.Sys_Startup_Init) refers to rtc.o(i.RTC_Init) for RTC_Init
    init.o(i.Sys_Startup_Init) refers to powermanagement_user.o(i.Power_Management_Lib_Init) for Power_Management_Lib_Init
    init.o(i.Sys_Startup_Init) refers to powermanagement.o(i.Power_Management_Init) for Power_Management_Init
    init.o(i.Sys_Startup_Init) refers to can.o(i.bsp_CAN_Init) for bsp_CAN_Init
    init.o(i.Sys_Startup_Init) refers to eemanager_interface.o(i.eeprom_StoreInfo_Init) for eeprom_StoreInfo_Init
    init.o(i.Sys_Startup_Init) refers to services_mileage_user.o(i.CalcODOKL30Init) for CalcODOKL30Init
    line_in.o(i.LINE_IN_Get_ABS) refers to gpio.o(i.PORT_GetBit) for PORT_GetBit
    line_in.o(i.LINE_IN_Get_AutoStarStop) refers to gpio.o(i.PORT_GetBit) for PORT_GetBit
    line_in.o(i.LINE_IN_Get_HighBeam) refers to gpio.o(i.PORT_GetBit) for PORT_GetBit
    line_in.o(i.LINE_IN_Get_LeftTurn) refers to gpio.o(i.PORT_GetBit) for PORT_GetBit
    line_in.o(i.LINE_IN_Get_OBD) refers to gpio.o(i.PORT_GetBit) for PORT_GetBit
    line_in.o(i.LINE_IN_Get_OilPressure) refers to gpio.o(i.PORT_GetBit) for PORT_GetBit
    line_in.o(i.LINE_IN_Get_RightTurn) refers to gpio.o(i.PORT_GetBit) for PORT_GetBit
    line_in.o(i.LINE_IN_Get_TirePressure) refers to gpio.o(i.PORT_GetBit) for PORT_GetBit
    line_in.o(i.Line_In_Debounce_Handle) refers to line_in.o(.constdata) for g_stLineInAttribute
    line_in.o(i.Line_In_Debounce_Handle) refers to line_in.o(.bss) for g_stLineInControl
    line_in.o(i.Line_In_Debounce_Service) refers to line_in.o(i.Line_In_Debounce_Handle) for Line_In_Debounce_Handle
    line_in.o(i.Line_In_Debounce_Service) refers to line_in.o(.constdata) for g_stLineInAttribute
    line_in.o(i.Line_In_Debounce_Service) refers to line_in.o(.data) for g_enLineInPowerStatus
    line_in.o(i.Line_In_Get_Status) refers to line_in.o(.bss) for g_stLineInControl
    line_in.o(i.Line_In_KL15_OFF_Init) refers to line_in.o(.data) for g_enLineInPowerStatus
    line_in.o(i.Line_In_KL15_OFF_Init) refers to line_in.o(.constdata) for g_stLineInAttribute
    line_in.o(i.Line_In_KL15_OFF_Init) refers to line_in.o(.bss) for g_stLineInControl
    line_in.o(i.Line_In_KL15_ON_Init) refers to line_in.o(.data) for g_enLineInPowerStatus
    line_in.o(i.Line_In_KL15_ON_Init) refers to line_in.o(.constdata) for g_stLineInAttribute
    line_in.o(i.Line_In_KL15_ON_Init) refers to line_in.o(.bss) for g_stLineInControl
    line_in.o(i.Line_In_KL30_Init) refers to line_in.o(.data) for g_enLineInPowerStatus
    line_in.o(i.Line_In_KL30_Init) refers to line_in.o(.bss) for g_stLineInControl
    line_in.o(i.Line_In_SetPowerSt) refers to line_in.o(.data) for g_enLineInPowerStatus
    line_in.o(.constdata) refers to line_in.o(i.LINE_IN_Get_RightTurn) for LINE_IN_Get_RightTurn
    line_in.o(.constdata) refers to line_in.o(i.LINE_IN_Get_LeftTurn) for LINE_IN_Get_LeftTurn
    line_in.o(.constdata) refers to line_in.o(i.LINE_IN_Get_HighBeam) for LINE_IN_Get_HighBeam
    line_in.o(.constdata) refers to line_in.o(i.LINE_IN_Get_ABS) for LINE_IN_Get_ABS
    line_in.o(.constdata) refers to line_in.o(i.LINE_IN_Get_AutoStarStop) for LINE_IN_Get_AutoStarStop
    line_in.o(.constdata) refers to line_in.o(i.LINE_IN_Get_TirePressure) for LINE_IN_Get_TirePressure
    line_in.o(.constdata) refers to line_in.o(i.LINE_IN_Get_OilPressure) for LINE_IN_Get_OilPressure
    line_in.o(.constdata) refers to line_in.o(i.LINE_IN_Get_OBD) for LINE_IN_Get_OBD
    powermanagement.o(i.PowerMemInit) refers to powermanagement.o(.bss) for pFuncPower
    powermanagement.o(i.PowerMemInit) refers to powermanagement.o(.data) for g_Power_St
    powermanagement.o(i.Power_Management_Init) refers to powermanagement.o(.bss) for pFuncPower
    powermanagement.o(i.Power_Management_Init) refers to powermanagement.o(.data) for g_Power_St
    powermanagement.o(i.Power_Management_Service) refers to gpio.o(i.__ARM_common_switch8) for __ARM_common_switch8
    powermanagement.o(i.Power_Management_Service) refers to powermanagement.o(.data) for g_Power_St
    powermanagement.o(i.Power_Management_Service) refers to powermanagement.o(.bss) for pFuncPower
    powermanagement_user.o(i.Power_IG_OFF_Init) refers to seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Display) for SEG_LCD_Vehicle_Speed_Num_Display
    powermanagement_user.o(i.Power_IG_OFF_Init) refers to seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Display) for SEG_LCD_Engine_Speed_Seg_Display
    powermanagement_user.o(i.Power_IG_OFF_Init) refers to seg_lcd.o(i.SEG_LCD_ODO_Trip_Display) for SEG_LCD_ODO_Trip_Display
    powermanagement_user.o(i.Power_IG_OFF_Init) refers to seg_lcd.o(i.SEG_Fuel_Level_Display) for SEG_Fuel_Level_Display
    powermanagement_user.o(i.Power_IG_OFF_Init) refers to seg_lcd.o(i.SEG_LCD_Battery_Voltage_Display) for SEG_LCD_Battery_Voltage_Display
    powermanagement_user.o(i.Power_IG_OFF_Init) refers to seg_lcd.o(i.SEG_LCD_Gear_Display) for SEG_LCD_Gear_Display
    powermanagement_user.o(i.Power_IG_OFF_Init) refers to seg_lcd.o(i.SEG_Coolant_Temp_Display) for SEG_Coolant_Temp_Display
    powermanagement_user.o(i.Power_IG_OFF_Init) refers to line_in.o(i.Line_In_KL15_OFF_Init) for Line_In_KL15_OFF_Init
    powermanagement_user.o(i.Power_IG_OFF_Init) refers to common_interface.o(i.Common_Set_IG_Sts) for Common_Set_IG_Sts
    powermanagement_user.o(i.Power_IG_OFF_Init) refers to can_user.o(i.Set_CanSleepDelayTime) for Set_CanSleepDelayTime
    powermanagement_user.o(i.Power_IG_OFF_Init) refers to powermanagement_user.o(.data) for g_sleepDelay
    powermanagement_user.o(i.Power_IG_ON_Init) refers to line_in.o(i.Line_In_KL15_ON_Init) for Line_In_KL15_ON_Init
    powermanagement_user.o(i.Power_IG_ON_Init) refers to telltales_lib.o(i.Telltales_KL15_Init) for Telltales_KL15_Init
    powermanagement_user.o(i.Power_IG_ON_Init) refers to can.o(i.bsp_CAN_SleepRelease) for bsp_CAN_SleepRelease
    powermanagement_user.o(i.Power_IG_ON_Init) refers to can.o(i.bsp_CAN_Init) for bsp_CAN_Init
    powermanagement_user.o(i.Power_IG_ON_Init) refers to mcu_core_protocol.o(i.Enable_Cyc_Msg) for Enable_Cyc_Msg
    powermanagement_user.o(i.Power_IG_ON_Init) refers to common_interface.o(i.Common_DataInit) for Common_DataInit
    powermanagement_user.o(i.Power_IG_ON_Init) refers to fuel.o(i.Fuel_KL15_Init) for Fuel_KL15_Init
    powermanagement_user.o(i.Power_IG_ON_Init) refers to data_gear.o(i.Data_Gear_KL15_Init) for Data_Gear_KL15_Init
    powermanagement_user.o(i.Power_IG_ON_Init) refers to timera_b_c.o(i.TMB0_PWM_Pin33_Init) for TMB0_PWM_Pin33_Init
    powermanagement_user.o(i.Power_IG_ON_Init) refers to app_service.o(i.DiagnosisInit_main) for DiagnosisInit_main
    powermanagement_user.o(i.Power_IG_ON_Init) refers to u2_app_service.o(i.U2_DiagnosisInit_main) for U2_DiagnosisInit_main
    powermanagement_user.o(i.Power_IG_ON_Init) refers to key.o(i.Key_Status_Init) for Key_Status_Init
    powermanagement_user.o(i.Power_IG_ON_Init) refers to mcu_core_protocol.o(i.Protocol_KL15_ON_Init) for Protocol_KL15_ON_Init
    powermanagement_user.o(i.Power_IG_ON_Init) refers to sci_user.o(i.uart2_User_KL15_Init) for uart2_User_KL15_Init
    powermanagement_user.o(i.Power_IG_ON_Init) refers to can_user.o(i.APP_CAN_Init) for APP_CAN_Init
    powermanagement_user.o(i.Power_IG_ON_Init) refers to services_mileage_user.o(i.CalcODOKL15Init) for CalcODOKL15Init
    powermanagement_user.o(i.Power_IG_ON_Init) refers to common_interface.o(i.Common_Set_IG_Sts) for Common_Set_IG_Sts
    powermanagement_user.o(i.Power_IG_ON_Init) refers to seg_lcd.o(i.SEG_LCD_Init) for SEG_LCD_Init
    powermanagement_user.o(i.Power_IG_ON_Init) refers to aw93015.o(i.Init93015_IIC) for Init93015_IIC
    powermanagement_user.o(i.Power_IG_ON_Init) refers to can_user.o(i.DtcFaultInit) for DtcFaultInit
    powermanagement_user.o(i.Power_IG_ON_Init) refers to can_user.o(i.BatteryVoltageDelayInit) for BatteryVoltageDelayInit
    powermanagement_user.o(i.Power_KL30_Init) refers to system_monitor_user.o(i.Sys_KL30_Init) for Sys_KL30_Init
    powermanagement_user.o(i.Power_KL30_Init) refers to line_in.o(i.Line_In_KL30_Init) for Line_In_KL30_Init
    powermanagement_user.o(i.Power_KL30_Init) refers to telltales_user.o(i.Telltales_Init) for Telltales_Init
    powermanagement_user.o(i.Power_KL30_Init) refers to fuel.o(i.Fuel_KL30_Init) for Fuel_KL30_Init
    powermanagement_user.o(i.Power_KL30_Init) refers to data_gear.o(i.Data_Gear_KL30_Init) for Data_Gear_KL30_Init
    powermanagement_user.o(i.Power_Management_Lib_Init) refers to powermanagement.o(i.PowerMemInit) for PowerMemInit
    powermanagement_user.o(i.Power_Management_Lib_Init) refers to powermanagement_user.o(i.Power_IG_OFF_Init) for Power_IG_OFF_Init
    powermanagement_user.o(i.Power_Management_Lib_Init) refers to powermanagement_user.o(i.Power_IG_ON_Init) for Power_IG_ON_Init
    powermanagement_user.o(i.Power_Management_Lib_Init) refers to powermanagement_user.o(i.Power_Sleep_Init) for Power_Sleep_Init
    powermanagement_user.o(i.Power_Management_Lib_Init) refers to powermanagement_user.o(i.Power_IG_OVP_Init) for Power_IG_OVP_Init
    powermanagement_user.o(i.Power_Management_Lib_Init) refers to powermanagement_user.o(i.Power_IG_LVP_Init) for Power_IG_LVP_Init
    powermanagement_user.o(i.Power_Management_Lib_Init) refers to powermanagement_user.o(i.Power_KL30_Init) for Power_KL30_Init
    powermanagement_user.o(i.Power_Management_Lib_Init) refers to powermanagement_user.o(i.Power_Wakeup_Init) for Power_Wakeup_Init
    powermanagement_user.o(i.Power_Management_Lib_Init) refers to powermanagement_user.o(i.Power_Stay_OFF) for Power_Stay_OFF
    powermanagement_user.o(i.Power_Management_Lib_Init) refers to powermanagement_user.o(i.Power_Stay_ON) for Power_Stay_ON
    powermanagement_user.o(i.Power_Management_Lib_Init) refers to powermanagement_user.o(i.Power_Stay_Sleep) for Power_Stay_Sleep
    powermanagement_user.o(i.Power_Management_Lib_Init) refers to powermanagement_user.o(i.Power_Stay_Protect) for Power_Stay_Protect
    powermanagement_user.o(i.Power_Management_Service_user) refers to powermanagement_user.o(.data) for g_sleepDelay
    powermanagement_user.o(i.Power_Sleep_Init) refers to sys_tick.o(i.Sys_Tick_Timer_Stop) for Sys_Tick_Timer_Stop
    powermanagement_user.o(i.Power_Sleep_Init) refers to tim4.o(i.Capture_Stop) for Capture_Stop
    powermanagement_user.o(i.Power_Sleep_Init) refers to analog_signals.o(i.Analog_Signal_Conv_Stop) for Analog_Signal_Conv_Stop
    powermanagement_user.o(i.Power_Sleep_Init) refers to seg_lcd.o(i.SEG_LCD_Shutdown) for SEG_LCD_Shutdown
    powermanagement_user.o(i.Power_Sleep_Init) refers to is31fl3236.o(i.IS31_Shutdown) for IS31_Shutdown
    powermanagement_user.o(i.Power_Sleep_Init) refers to gpio.o(i.GPIO_Init) for GPIO_Init
    powermanagement_user.o(i.Power_Sleep_Init) refers to can_user.o(.data) for CAN_Initflag
    powermanagement_user.o(i.Power_Stay_OFF) refers to system_monitor.o(i.System_FUN_KL30_Status_Get) for System_FUN_KL30_Status_Get
    powermanagement_user.o(i.Power_Stay_OFF) refers to system_monitor.o(i.System_FUN_KL15_Status_Get) for System_FUN_KL15_Status_Get
    powermanagement_user.o(i.Power_Stay_OFF) refers to rte_adc.o(i.RTE_Read_KL15_Voltage) for RTE_Read_KL15_Voltage
    powermanagement_user.o(i.Power_Stay_OFF) refers to can.o(i.bsp_Is_CAN_Sleep) for bsp_Is_CAN_Sleep
    powermanagement_user.o(i.Power_Stay_OFF) refers to powermanagement_user.o(.data) for g_sleepDelay
    powermanagement_user.o(i.Power_Stay_ON) refers to system_monitor.o(i.System_FUN_KL30_Status_Get) for System_FUN_KL30_Status_Get
    powermanagement_user.o(i.Power_Stay_ON) refers to system_monitor.o(i.System_FUN_KL15_Status_Get) for System_FUN_KL15_Status_Get
    powermanagement_user.o(i.Power_Stay_Sleep) refers to clk.o(i.Sys_Enter_Sleep_Mode) for Sys_Enter_Sleep_Mode
    powermanagement_user.o(i.Power_Wakeup_Init) refers to gpio.o(i.GPIO_Init) for GPIO_Init
    powermanagement_user.o(i.Power_Wakeup_Init) refers to sys_tick.o(i.Sys_Tick_Timer_Start) for Sys_Tick_Timer_Start
    powermanagement_user.o(i.Power_Wakeup_Init) refers to analog_signals.o(i.Analog_Signal_Conv_Init) for Analog_Signal_Conv_Init
    powermanagement_user.o(i.Power_Wakeup_Init) refers to system_monitor_user.o(i.Sys_WakeUp_Init) for Sys_WakeUp_Init
    powermanagement_user.o(i.Power_Wakeup_Init) refers to line_in.o(i.Line_In_KL30_Init) for Line_In_KL30_Init
    powermanagement_user.o(i.Power_Wakeup_Init) refers to telltales_user.o(i.Telltales_Init) for Telltales_Init
    powermanagement_user.o(i.Power_Wakeup_Init) refers to common_interface.o(i.Common_DataInit) for Common_DataInit
    powermanagement_user.o(i.Power_Wakeup_Init) refers to key.o(i.Key_Status_Init) for Key_Status_Init
    powermanagement_user.o(i.Power_Wakeup_Init) refers to is31fl3236.o(i.IS31_OFF_Wakeup) for IS31_OFF_Wakeup
    powermanagement_user.o(i.Power_Wakeup_Init) refers to is31fl3236.o(i.IS31FL3236_Update) for IS31FL3236_Update
    powermanagement_user.o(i.Power_Wakeup_Init) refers to aw93015.o(i.Init93015_IIC) for Init93015_IIC
    powermanagement_user.o(i.Power_Wakeup_Init) refers to can_user.o(i.APP_CAN_Init) for APP_CAN_Init
    powermanagement_user.o(i.Power_Wakeup_Init) refers to is31fl3236.o(i.IS31FL3236_Init) for IS31FL3236_Init
    powermanagement_user.o(.constdata) refers to key.o(i.Get_Key1_Line_In_Sts) for Get_Key1_Line_In_Sts
    powermanagement_user.o(.constdata) refers to key.o(i.Get_Key2_Line_In_Sts) for Get_Key2_Line_In_Sts
    system_monitor.o(i.Read_KL30_ConvertFinish) refers to system_monitor.o(.data) for SysWakeUpMode
    system_monitor.o(i.Sys_Set_DebounceTimer) refers to system_monitor.o(.data) for t_NM_KL30_Debounce
    system_monitor.o(i.Sys_Set_VolRange) refers to system_monitor.o(.data) for FUNSysVol_Range
    system_monitor.o(i.Sys_Status_Update_Service) refers to system_monitor.o(i.System_Fun_Process) for System_Fun_Process
    system_monitor.o(i.Sys_Status_Update_Service) refers to system_monitor.o(i.System_NM_Process) for System_NM_Process
    system_monitor.o(i.Sys_Status_Update_Service) refers to system_monitor_user.o(i.Sys_LogicProcess) for Sys_LogicProcess
    system_monitor.o(i.System_Calc_FunRange) refers to system_monitor.o(.data) for FUNSysVol_Range
    system_monitor.o(i.System_Calc_NMRange) refers to system_monitor.o(.data) for NMSysVol_Range
    system_monitor.o(i.System_FUN_KL15_Status_Get) refers to system_monitor.o(.bss) for SysFun_KL15Monitor
    system_monitor.o(i.System_FUN_KL30_Status_Get) refers to system_monitor.o(.bss) for SysFun_KL30Monitor
    system_monitor.o(i.System_Fast_WakeUp) refers to system_monitor_user.o(i.Sys_Force_Read_KL30_Voltage) for Sys_Force_Read_KL30_Voltage
    system_monitor.o(i.System_Fast_WakeUp) refers to system_monitor_user.o(i.Sys_BlockDelay) for Sys_BlockDelay
    system_monitor.o(i.System_Fast_WakeUp) refers to system_monitor_user.o(i.System_LINE_KL15) for System_LINE_KL15
    system_monitor.o(i.System_Fast_WakeUp) refers to system_monitor_user.o(i.Sys_LogicProcess) for Sys_LogicProcess
    system_monitor.o(i.System_Fast_WakeUp) refers to system_monitor.o(.data) for FUNSysVol_Range
    system_monitor.o(i.System_Fast_WakeUp) refers to system_monitor.o(.bss) for SysNM_KL30Monitor
    system_monitor.o(i.System_Fun_Process) refers to system_monitor_user.o(i.System_LINE_KL15) for System_LINE_KL15
    system_monitor.o(i.System_Fun_Process) refers to system_monitor_user.o(i.Sys_Read_KL30_Valid) for Sys_Read_KL30_Valid
    system_monitor.o(i.System_Fun_Process) refers to system_monitor_user.o(i.Sys_Read_KL30_Voltage) for Sys_Read_KL30_Voltage
    system_monitor.o(i.System_Fun_Process) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    system_monitor.o(i.System_Fun_Process) refers to system_monitor.o(i.System_Calc_FunRange) for System_Calc_FunRange
    system_monitor.o(i.System_Fun_Process) refers to system_monitor.o(.bss) for SysFun_KL15Monitor
    system_monitor.o(i.System_Fun_Process) refers to system_monitor.o(.data) for t_FUN_KL15_Debounce
    system_monitor.o(i.System_Monitor_KL30Init) refers to wdt.o(i.WDT_Restart) for WDT_Restart
    system_monitor.o(i.System_Monitor_KL30Init) refers to system_monitor.o(.data) for SysWakeUpMode
    system_monitor.o(i.System_Monitor_KL30Init) refers to system_monitor.o(.bss) for SysFun_KL30Monitor
    system_monitor.o(i.System_Monitor_KL30Init) refers to sys_tick.o(.data) for g_u16SysRollingCounter1ms
    system_monitor.o(i.System_Monitor_WakeupInit) refers to system_monitor.o(.data) for SysWakeUpMode
    system_monitor.o(i.System_Monitor_WakeupInit) refers to system_monitor.o(.bss) for SysFun_KL30Monitor
    system_monitor.o(i.System_NM_KL15_Status_Get) refers to system_monitor.o(.bss) for SysNM_KL15Monitor
    system_monitor.o(i.System_NM_KL30_Status_Get) refers to system_monitor.o(.bss) for SysNM_KL30Monitor
    system_monitor.o(i.System_NM_Process) refers to system_monitor_user.o(i.System_LINE_KL15) for System_LINE_KL15
    system_monitor.o(i.System_NM_Process) refers to system_monitor_user.o(i.Sys_Read_KL30_Valid) for Sys_Read_KL30_Valid
    system_monitor.o(i.System_NM_Process) refers to system_monitor_user.o(i.Sys_Read_KL30_Voltage) for Sys_Read_KL30_Voltage
    system_monitor.o(i.System_NM_Process) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    system_monitor.o(i.System_NM_Process) refers to system_monitor.o(i.System_Calc_NMRange) for System_Calc_NMRange
    system_monitor.o(i.System_NM_Process) refers to system_monitor.o(.bss) for SysNM_KL15Monitor
    system_monitor.o(i.System_NM_Process) refers to system_monitor.o(.data) for t_NM_KL15_Debounce
    system_monitor_user.o(i.Sys_Force_Read_KL30_Voltage) refers to rte_adc.o(i.RTE_ForceRead_KL30_Voltage) for RTE_ForceRead_KL30_Voltage
    system_monitor_user.o(i.Sys_KL30_Init) refers to system_monitor.o(i.Sys_Set_DebounceTimer) for Sys_Set_DebounceTimer
    system_monitor_user.o(i.Sys_KL30_Init) refers to system_monitor.o(i.Sys_Set_VolRange) for Sys_Set_VolRange
    system_monitor_user.o(i.Sys_KL30_Init) refers to system_monitor.o(i.System_Monitor_KL30Init) for System_Monitor_KL30Init
    system_monitor_user.o(i.Sys_KL30_Init) refers to system_monitor_user.o(.constdata) for SysNM_Range
    system_monitor_user.o(i.Sys_Read_KL30_Valid) refers to rte_adc.o(i.RTE_Read_KL30_Valid) for RTE_Read_KL30_Valid
    system_monitor_user.o(i.Sys_Read_KL30_Voltage) refers to rte_adc.o(i.RTE_Read_KL15_Voltage) for RTE_Read_KL15_Voltage
    system_monitor_user.o(i.Sys_Read_KL30_Voltage) refers to rte_adc.o(i.RTE_Read_KL30_Voltage) for RTE_Read_KL30_Voltage
    system_monitor_user.o(i.Sys_WakeUp_Init) refers to system_monitor.o(i.Sys_Set_DebounceTimer) for Sys_Set_DebounceTimer
    system_monitor_user.o(i.Sys_WakeUp_Init) refers to system_monitor.o(i.Sys_Set_VolRange) for Sys_Set_VolRange
    system_monitor_user.o(i.Sys_WakeUp_Init) refers to system_monitor.o(i.System_Monitor_WakeupInit) for System_Monitor_WakeupInit
    system_monitor_user.o(i.Sys_WakeUp_Init) refers to system_monitor.o(i.System_Fast_WakeUp) for System_Fast_WakeUp
    system_monitor_user.o(i.Sys_WakeUp_Init) refers to system_monitor_user.o(.constdata) for SysNM_Range
    system_monitor_user.o(i.System_LINE_KL15) refers to gpio.o(i.PORT_GetBit) for PORT_GetBit
    rte_adc.o(i.RTE_ADC_Init) refers to analog_signals.o(i.Analog_Signal_Conv_Init) for Analog_Signal_Conv_Init
    rte_adc.o(i.RTE_ForceRead_FUEL1_Voltage) refers to analog_signals.o(i.ADC_Conv_Single_Channel) for ADC_Conv_Single_Channel
    rte_adc.o(i.RTE_ForceRead_FUEL_VREF_Voltage) refers to analog_signals.o(i.ADC_Conv_Single_Channel) for ADC_Conv_Single_Channel
    rte_adc.o(i.RTE_ForceRead_KL30_Voltage) refers to analog_signals.o(i.ADC_Conv_Single_Channel) for ADC_Conv_Single_Channel
    rte_adc.o(i.RTE_Read_FUEL1_Valid) refers to analog_signals.o(i.ADC_Read_Signal_Valid) for ADC_Read_Signal_Valid
    rte_adc.o(i.RTE_Read_FUEL1_Voltage) refers to analog_signals.o(i.ADC_Read_Signal) for ADC_Read_Signal
    rte_adc.o(i.RTE_Read_FUEL_VREF_Valid) refers to analog_signals.o(i.ADC_Read_Signal_Valid) for ADC_Read_Signal_Valid
    rte_adc.o(i.RTE_Read_FUEL_VREF_Voltage) refers to analog_signals.o(i.ADC_Read_Signal) for ADC_Read_Signal
    rte_adc.o(i.RTE_Read_KL15_Voltage) refers to analog_signals.o(i.ADC_Read_Signal) for ADC_Read_Signal
    rte_adc.o(i.RTE_Read_KL30_Valid) refers to analog_signals.o(i.ADC_Read_Signal_Valid) for ADC_Read_Signal_Valid
    rte_adc.o(i.RTE_Read_KL30_Voltage) refers to analog_signals.o(i.ADC_Read_Signal) for ADC_Read_Signal
    common_interface.o(i.Common_BlockDelay) refers to common_interface.o(i.Common_RollingCounterClear) for Common_RollingCounterClear
    common_interface.o(i.Common_BlockDelay) refers to common_interface.o(i.Common_ReadRollingCounter) for Common_ReadRollingCounter
    common_interface.o(i.Common_DataInit) refers to common_interface.o(.data) for PowerSts
    common_interface.o(i.Common_GetIgnOffTime) refers to common_interface.o(.data) for PowerIgnOffTimeLine
    common_interface.o(i.Common_GetIgnOnTime) refers to common_interface.o(.data) for PowerIgnOnTimeLine
    common_interface.o(i.Common_Get_Act_E_Speed) refers to common_interface.o(.data) for Act_E_Speed
    common_interface.o(i.Common_Get_Act_E_Speed_Valid) refers to common_interface.o(.data) for Act_E_Speed_Valid
    common_interface.o(i.Common_Get_Act_RV_Speed) refers to common_interface.o(.data) for Act_RV_Speed
    common_interface.o(i.Common_Get_Act_V_Speed) refers to common_interface.o(.data) for Act_V_Speed
    common_interface.o(i.Common_Get_Act_V_Speed_Valid) refers to common_interface.o(.data) for Act_V_Speed_Valid
    common_interface.o(i.Common_Get_DispMode) refers to common_interface.o(.data) for g_Disp_Mode
    common_interface.o(i.Common_Get_Disp_E_Speed) refers to common_interface.o(.data) for Disp_E_Speed
    common_interface.o(i.Common_Get_Disp_E_Speed_Valid) refers to common_interface.o(.data) for Disp_E_Speed_Valid
    common_interface.o(i.Common_Get_Disp_RV_Speed) refers to common_interface.o(.data) for Disp_RV_Speed
    common_interface.o(i.Common_Get_Disp_V_Speed) refers to common_interface.o(.data) for Disp_V_Speed
    common_interface.o(i.Common_Get_Disp_V_Speed_Valid) refers to common_interface.o(.data) for Disp_V_Speed_Valid
    common_interface.o(i.Common_Get_E_Speed_TEST) refers to common_interface.o(.data) for Disp_E_Speed_Test
    common_interface.o(i.Common_Get_Fuel_TEST) refers to common_interface.o(.data) for Disp_Fuel_Test
    common_interface.o(i.Common_Get_Gauges_Disp_E_Speed) refers to common_interface.o(.data) for Disp_Gauges_E_Speed
    common_interface.o(i.Common_Get_IG_Sts) refers to common_interface.o(.data) for PowerSts
    common_interface.o(i.Common_Get_Language) refers to common_interface.o(.data) for g_Language
    common_interface.o(i.Common_Get_Temp_TEST) refers to common_interface.o(.data) for Disp_Temp_Test
    common_interface.o(i.Common_Get_V_Speed_TEST) refers to common_interface.o(.data) for Disp_V_Speed_Test
    common_interface.o(i.Common_Input_Para) refers to common_interface.o(i.Common_Get_IG_Sts) for Common_Get_IG_Sts
    common_interface.o(i.Common_Input_Para) refers to common_interface.o(.data) for PowerIgnOffTimeLine
    common_interface.o(i.Common_ReadRollingCounter) refers to common_interface.o(.data) for SysRollingCounter
    common_interface.o(i.Common_RollingCounterAdd) refers to common_interface.o(.data) for SysRollingCounter
    common_interface.o(i.Common_RollingCounterClear) refers to common_interface.o(.data) for SysRollingCounter
    common_interface.o(i.Common_SetSelfcheckStart) refers to common_interface.o(.data) for SelfcheckStart
    common_interface.o(i.Common_Set_Act_E_Speed) refers to common_interface.o(.data) for Act_E_Speed
    common_interface.o(i.Common_Set_Act_E_Speed_Valid) refers to common_interface.o(.data) for Act_E_Speed_Valid
    common_interface.o(i.Common_Set_Act_V_Speed) refers to common_interface.o(.data) for Act_V_Speed
    common_interface.o(i.Common_Set_Act_V_Speed_Valid) refers to common_interface.o(.data) for Act_V_Speed_Valid
    common_interface.o(i.Common_Set_DispMode) refers to common_interface.o(.data) for g_Disp_Mode
    common_interface.o(i.Common_Set_Disp_E_Speed) refers to common_interface.o(.data) for Disp_E_Speed
    common_interface.o(i.Common_Set_Disp_E_Speed_Valid) refers to common_interface.o(.data) for Disp_E_Speed_Valid
    common_interface.o(i.Common_Set_Disp_V_Speed) refers to common_interface.o(.data) for Disp_V_Speed
    common_interface.o(i.Common_Set_Disp_V_Speed_Valid) refers to common_interface.o(.data) for Disp_V_Speed_Valid
    common_interface.o(i.Common_Set_Gauges_E_Speed) refers to common_interface.o(.data) for Disp_Gauges_E_Speed
    common_interface.o(i.Common_Set_IG_Sts) refers to common_interface.o(.data) for PowerSts
    mcu_core_protocol.o(i.Check_Event_Msg) refers to sci_user.o(i.Get_Uart2_State) for Get_Uart2_State
    mcu_core_protocol.o(i.Check_Event_Msg) refers to mcu_core_protocol.o(i.Send_To_Core) for Send_To_Core
    mcu_core_protocol.o(i.Check_Event_Msg) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    mcu_core_protocol.o(i.Check_Event_Msg) refers to mcu_core_protocol.o(.data) for Event_Msg_Count
    mcu_core_protocol.o(i.Check_Event_Msg) refers to mcu_core_protocol.o(.bss) for Event_Send_Queue
    mcu_core_protocol.o(i.Disable_Cyc_Msg) refers to mcu_core_protocol.o(.data) for SendCtrl_Tbl
    mcu_core_protocol.o(i.Drive_Info_Display_Update_Service) refers to common_interface.o(i.Common_Get_Disp_V_Speed) for Common_Get_Disp_V_Speed
    mcu_core_protocol.o(i.Drive_Info_Display_Update_Service) refers to can_user.o(i.GetDtcAmnt) for GetDtcAmnt
    mcu_core_protocol.o(i.Drive_Info_Display_Update_Service) refers to common_interface.o(i.Common_GetIgnOnTime) for Common_GetIgnOnTime
    mcu_core_protocol.o(i.Drive_Info_Display_Update_Service) refers to can_user.o(i.GetDtcDispNum) for GetDtcDispNum
    mcu_core_protocol.o(i.Drive_Info_Display_Update_Service) refers to common_interface.o(i.Common_Get_Disp_E_Speed) for Common_Get_Disp_E_Speed
    mcu_core_protocol.o(i.Drive_Info_Display_Update_Service) refers to common_interface.o(i.Common_Get_IG_Sts) for Common_Get_IG_Sts
    mcu_core_protocol.o(i.Drive_Info_Display_Update_Service) refers to mcu_core_protocol.o(.data) for Checktime
    mcu_core_protocol.o(i.Enable_Cyc_Msg) refers to mcu_core_protocol.o(.data) for SendCtrl_Tbl
    mcu_core_protocol.o(i.GetSocDispSts) refers to mcu_core_protocol.o(.data) for Receive_ID_12
    mcu_core_protocol.o(i.Get_Event_Msg_Queue_Length) refers to mcu_core_protocol.o(.data) for Event_Msg_Count
    mcu_core_protocol.o(i.Get_ID_01_Data) refers to common_interface.o(i.Common_Get_DispMode) for Common_Get_DispMode
    mcu_core_protocol.o(i.Get_ID_01_Data) refers to common_interface.o(i.Common_Get_IG_Sts) for Common_Get_IG_Sts
    mcu_core_protocol.o(i.Get_ID_01_Data) refers to common_interface.o(i.Common_Get_Language) for Common_Get_Language
    mcu_core_protocol.o(i.Get_ID_01_Data) refers to bglinterface.o(i.Get_Day_Or_Night) for Get_Day_Or_Night
    mcu_core_protocol.o(i.Get_ID_01_Data) refers to common_interface.o(i.Common_Get_Disp_E_Speed) for Common_Get_Disp_E_Speed
    mcu_core_protocol.o(i.Get_ID_01_Data) refers to aeabi_sdivfast.o(.text) for __aeabi_idivmod
    mcu_core_protocol.o(i.Get_ID_01_Data) refers to common_interface.o(i.Common_Get_Disp_V_Speed) for Common_Get_Disp_V_Speed
    mcu_core_protocol.o(i.Get_ID_01_Data) refers to rtc.o(i.Get_RTC_Time) for Get_RTC_Time
    mcu_core_protocol.o(i.Get_ID_01_Data) refers to services_mileage_user.o(i.Data_ODO_Read) for Data_ODO_Read
    mcu_core_protocol.o(i.Get_ID_01_Data) refers to services_mileage_user.o(i.Data_Read_Trip) for Data_Read_Trip
    mcu_core_protocol.o(i.Get_ID_01_Data) refers to mcu_core_protocol.o(.data) for Send_ID_01_00
    mcu_core_protocol.o(i.Get_ID_01_Data) refers to mcu_core_protocol.o(.bss) for Send_ID_01_02
    mcu_core_protocol.o(i.Get_ID_01_Data) refers to flash_synchronizer.o(.data) for FlashSync05Hz
    mcu_core_protocol.o(i.Get_ID_02_Data) refers to common_interface.o(i.Common_Get_IG_Sts) for Common_Get_IG_Sts
    mcu_core_protocol.o(i.Get_ID_02_Data) refers to mcu_core_protocol.o(.bss) for Send_ID_02
    mcu_core_protocol.o(i.MCU_Send_Service) refers to sci_user.o(i.uart2_Get_0x10_Rev_Flag) for uart2_Get_0x10_Rev_Flag
    mcu_core_protocol.o(i.MCU_Send_Service) refers to sci_user.o(i.Get_Uart2_State) for Get_Uart2_State
    mcu_core_protocol.o(i.MCU_Send_Service) refers to mcu_core_protocol.o(i.Send_To_Core) for Send_To_Core
    mcu_core_protocol.o(i.MCU_Send_Service) refers to mcu_core_protocol.o(i.Check_Event_Msg) for Check_Event_Msg
    mcu_core_protocol.o(i.MCU_Send_Service) refers to mcu_core_protocol.o(.data) for SendCtrl_Tbl
    mcu_core_protocol.o(i.Protocol_KL15_ON_Init) refers to mcu_core_protocol.o(.data) for Event_Msg_QueueFront
    mcu_core_protocol.o(i.Selfcheck_Display_Update_Service) refers to common_interface.o(i.Common_Get_IG_Sts) for Common_Get_IG_Sts
    mcu_core_protocol.o(i.Selfcheck_Display_Update_Service) refers to common_interface.o(i.Common_GetIgnOnTime) for Common_GetIgnOnTime
    mcu_core_protocol.o(i.Selfcheck_Display_Update_Service) refers to seg_lcd.o(i.SEG_LCD_Gear_Display) for SEG_LCD_Gear_Display
    mcu_core_protocol.o(i.Selfcheck_Display_Update_Service) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    mcu_core_protocol.o(i.Selfcheck_Display_Update_Service) refers to seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Display) for SEG_LCD_Vehicle_Speed_Num_Display
    mcu_core_protocol.o(i.Selfcheck_Display_Update_Service) refers to seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Selftest) for SEG_LCD_Engine_Speed_Seg_Selftest
    mcu_core_protocol.o(i.Selfcheck_Display_Update_Service) refers to seg_lcd.o(i.SEG_Coolant_Temp_Display) for SEG_Coolant_Temp_Display
    mcu_core_protocol.o(i.Selfcheck_Display_Update_Service) refers to seg_lcd.o(i.SEG_Fuel_Level_Display) for SEG_Fuel_Level_Display
    mcu_core_protocol.o(i.Selfcheck_Display_Update_Service) refers to seg_lcd.o(i.SEG_LCD_Battery_Voltage_Selftest) for SEG_LCD_Battery_Voltage_Selftest
    mcu_core_protocol.o(i.Selfcheck_Display_Update_Service) refers to seg_lcd.o(i.SEG_LCD_Gear_Selftest) for SEG_LCD_Gear_Selftest
    mcu_core_protocol.o(i.Selfcheck_Display_Update_Service) refers to seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Selftest) for SEG_LCD_Vehicle_Speed_Num_Selftest
    mcu_core_protocol.o(i.Selfcheck_Display_Update_Service) refers to seg_lcd.o(i.SEG_LCD_ODO_Trip_FaultCode_Selftest) for SEG_LCD_ODO_Trip_FaultCode_Selftest
    mcu_core_protocol.o(i.Selfcheck_Display_Update_Service) refers to mcu_core_protocol.o(.data) for Animat_GEAR
    mcu_core_protocol.o(i.Send_Event_Msg) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    mcu_core_protocol.o(i.Send_Event_Msg) refers to mcu_core_protocol.o(.data) for Event_Msg_Count
    mcu_core_protocol.o(i.Send_Event_Msg) refers to mcu_core_protocol.o(.bss) for Event_Send_Queue
    mcu_core_protocol.o(i.Send_To_Core) refers to mcu_core_protocol.o(i.TFT_CreateCRCCheckSum) for TFT_CreateCRCCheckSum
    mcu_core_protocol.o(i.Send_To_Core) refers to sci_user.o(i.UART_Ch2_Send_Multiple_Byte) for UART_Ch2_Send_Multiple_Byte
    mcu_core_protocol.o(i.Send_To_Core) refers to mcu_core_protocol.o(.bss) for Uart2_tx_buf
    mcu_core_protocol.o(i.Send_To_Core) refers to mcu_core_protocol.o(.data) for PackageCnt
    mcu_core_protocol.o(i.Send_To_Core) refers to sci_user.o(.data) for g_uart2_tx_state
    mcu_core_protocol.o(i.SetUartRxMsg_0x12) refers to mcu_core_protocol.o(.data) for Receive_ID_12
    mcu_core_protocol.o(i.TFT_CreateCRCCheckSum) refers to mcu_core_protocol.o(.constdata) for CRC16_TAB_H
    mcu_core_protocol.o(.data) refers to mcu_core_protocol.o(i.Get_ID_01_Data) for Get_ID_01_Data
    mcu_core_protocol.o(.data) refers to mcu_core_protocol.o(i.Get_ID_02_Data) for Get_ID_02_Data
    telltales_user.o(i.LED_ABS_Execution) refers to seg_lcd.o(i.SEG_LCD_ABS) for SEG_LCD_ABS
    telltales_user.o(i.LED_ABS_Execution) refers to app_telltales.o(i.App_Telltales_Ctrl) for App_Telltales_Ctrl
    telltales_user.o(i.LED_ABS_Judgement) refers to line_in.o(i.Line_In_Get_Status) for Line_In_Get_Status
    telltales_user.o(i.LED_AutoStarStop_Execution) refers to seg_lcd.o(i.SEG_LCD_AutoStarStop) for SEG_LCD_AutoStarStop
    telltales_user.o(i.LED_AutoStarStop_Execution) refers to app_telltales.o(i.App_Telltales_Ctrl) for App_Telltales_Ctrl
    telltales_user.o(i.LED_AutoStarStop_Judgement) refers to line_in.o(i.Line_In_Get_Status) for Line_In_Get_Status
    telltales_user.o(i.LED_Auto_HI_BEAM_Execution) refers to seg_lcd.o(i.SEG_LCD_HI_BEAM) for SEG_LCD_HI_BEAM
    telltales_user.o(i.LED_Auto_HI_BEAM_Execution) refers to app_telltales.o(i.App_Telltales_Ctrl) for App_Telltales_Ctrl
    telltales_user.o(i.LED_Batterylow_Execution) refers to seg_lcd.o(i.SEG_LCD_Batterylow) for SEG_LCD_Batterylow
    telltales_user.o(i.LED_Batterylow_Execution) refers to app_telltales.o(i.App_Telltales_Ctrl) for App_Telltales_Ctrl
    telltales_user.o(i.LED_Batterylow_Judgement) refers to can_user.o(i.Get_LED_ECU_Battery_VoltageFlag) for Get_LED_ECU_Battery_VoltageFlag
    telltales_user.o(i.LED_Batterylow_Judgement) refers to can_signal_rx.o(i.CAN_MSG_Status) for CAN_MSG_Status
    telltales_user.o(i.LED_ENGINE_OIL_LOW_Execution) refers to seg_lcd.o(i.SEG_LCD_OilPressure) for SEG_LCD_OilPressure
    telltales_user.o(i.LED_ENGINE_OIL_LOW_Execution) refers to app_telltales.o(i.App_Telltales_Ctrl) for App_Telltales_Ctrl
    telltales_user.o(i.LED_Fuel_Execution) refers to seg_lcd.o(i.SEG_LCD_Fuel) for SEG_LCD_Fuel
    telltales_user.o(i.LED_Fuel_Execution) refers to app_telltales.o(i.App_Telltales_Ctrl) for App_Telltales_Ctrl
    telltales_user.o(i.LED_Fuel_Judgement) refers to fuel.o(i.Get_CurFuelSetp) for Get_CurFuelSetp
    telltales_user.o(i.LED_Fuel_Judgement) refers to fuel.o(i.Get_Fuel_Sensor_State) for Get_Fuel_Sensor_State
    telltales_user.o(i.LED_Fuel_Judgement) refers to flash_synchronizer.o(.data) for FlashSync1Hz
    telltales_user.o(i.LED_HI_BEAM_Execution) refers to seg_lcd.o(i.SEG_LCD_HighBeam) for SEG_LCD_HighBeam
    telltales_user.o(i.LED_HI_BEAM_Execution) refers to app_telltales.o(i.App_Telltales_Ctrl) for App_Telltales_Ctrl
    telltales_user.o(i.LED_HI_BEAM_Judgement) refers to line_in.o(i.Line_In_Get_Status) for Line_In_Get_Status
    telltales_user.o(i.LED_LEFT_Execution) refers to seg_lcd.o(i.SEG_LCD_LeftTurn) for SEG_LCD_LeftTurn
    telltales_user.o(i.LED_LEFT_Execution) refers to app_telltales.o(i.App_Telltales_Ctrl) for App_Telltales_Ctrl
    telltales_user.o(i.LED_LEFT_Judgement) refers to line_in.o(i.Line_In_Get_Status) for Line_In_Get_Status
    telltales_user.o(i.LED_MIL_Execution) refers to seg_lcd.o(i.SEG_LCD_OBD) for SEG_LCD_OBD
    telltales_user.o(i.LED_MIL_Execution) refers to app_telltales.o(i.App_Telltales_Ctrl) for App_Telltales_Ctrl
    telltales_user.o(i.LED_MIL_Judgement) refers to line_in.o(i.Line_In_Get_Status) for Line_In_Get_Status
    telltales_user.o(i.LED_READY_Execution) refers to seg_lcd.o(i.SEG_LCD_READY) for SEG_LCD_READY
    telltales_user.o(i.LED_READY_Execution) refers to app_telltales.o(i.App_Telltales_Ctrl) for App_Telltales_Ctrl
    telltales_user.o(i.LED_READY_Judgement) refers to can_communication_matrix.o(i.Get_ID_111_ISG_Ready) for Get_ID_111_ISG_Ready
    telltales_user.o(i.LED_RIGHT_Execution) refers to seg_lcd.o(i.SEG_LCD_RightTurn) for SEG_LCD_RightTurn
    telltales_user.o(i.LED_RIGHT_Execution) refers to app_telltales.o(i.App_Telltales_Ctrl) for App_Telltales_Ctrl
    telltales_user.o(i.LED_RIGHT_Judgement) refers to line_in.o(i.Line_In_Get_Status) for Line_In_Get_Status
    telltales_user.o(i.LED_Shore_Execution) refers to seg_lcd.o(i.SEG_LCD_Shore) for SEG_LCD_Shore
    telltales_user.o(i.LED_Shore_Execution) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    telltales_user.o(i.LED_Shore_Execution) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    telltales_user.o(i.LED_Shore_Judgement) refers to can_communication_matrix.o(i.Get_ID_111_Sig_ISG_SideStand) for Get_ID_111_Sig_ISG_SideStand
    telltales_user.o(i.LED_TPMS_Execution) refers to seg_lcd.o(i.SEG_LCD_TirePressure) for SEG_LCD_TirePressure
    telltales_user.o(i.LED_TPMS_Execution) refers to app_telltales.o(i.App_Telltales_Ctrl) for App_Telltales_Ctrl
    telltales_user.o(i.LED_Temp_Execution) refers to seg_lcd.o(i.SEG_LCD_Temp) for SEG_LCD_Temp
    telltales_user.o(i.LED_Temp_Execution) refers to app_telltales.o(i.App_Telltales_Ctrl) for App_Telltales_Ctrl
    telltales_user.o(i.Telltales_Init) refers to telltales_lib.o(i.Telltales_KL30_Wakeup_Init) for Telltales_KL30_Wakeup_Init
    telltales_user.o(i.Telltales_Init) refers to common_interface.o(i.Common_GetIgnOffTime) for Common_GetIgnOffTime
    telltales_user.o(i.Telltales_Init) refers to common_interface.o(i.Common_GetIgnOnTime) for Common_GetIgnOnTime
    telltales_user.o(i.Telltales_Init) refers to common_interface.o(i.Common_Get_IG_Sts) for Common_Get_IG_Sts
    telltales_user.o(i.Telltales_Init) refers to telltales_user.o(.constdata) for LED_Attribute
    telltales_user.o(i.Telltales_Init) refers to telltales_user.o(.bss) for Tel_Mem
    telltales_user.o(.constdata) refers to key.o(i.Get_Key1_Line_In_Sts) for Get_Key1_Line_In_Sts
    telltales_user.o(.constdata) refers to key.o(i.Get_Key2_Line_In_Sts) for Get_Key2_Line_In_Sts
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_RIGHT_Judgement) for LED_RIGHT_Judgement
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_RIGHT_Execution) for LED_RIGHT_Execution
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_LEFT_Judgement) for LED_LEFT_Judgement
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_LEFT_Execution) for LED_LEFT_Execution
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_HI_BEAM_Judgement) for LED_HI_BEAM_Judgement
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_HI_BEAM_Execution) for LED_HI_BEAM_Execution
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_MIL_Judgement) for LED_MIL_Judgement
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_MIL_Execution) for LED_MIL_Execution
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_ABS_Judgement) for LED_ABS_Judgement
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_ABS_Execution) for LED_ABS_Execution
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_TSC_Judgement) for LED_TSC_Judgement
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_TSC_Execution) for LED_TSC_Execution
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_AutoStarStop_Judgement) for LED_AutoStarStop_Judgement
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_AutoStarStop_Execution) for LED_AutoStarStop_Execution
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_Batterylow_Judgement) for LED_Batterylow_Judgement
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_Batterylow_Execution) for LED_Batterylow_Execution
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_Auto_HI_BEAM_Judgement) for LED_Auto_HI_BEAM_Judgement
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_Auto_HI_BEAM_Execution) for LED_Auto_HI_BEAM_Execution
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_Shore_Judgement) for LED_Shore_Judgement
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_Shore_Execution) for LED_Shore_Execution
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_ENGINE_OIL_LOW_Judgement) for LED_ENGINE_OIL_LOW_Judgement
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_ENGINE_OIL_LOW_Execution) for LED_ENGINE_OIL_LOW_Execution
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_TPMS_Judgement) for LED_TPMS_Judgement
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_TPMS_Execution) for LED_TPMS_Execution
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_READY_Judgement) for LED_READY_Judgement
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_READY_Execution) for LED_READY_Execution
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_Fuel_Judgement) for LED_Fuel_Judgement
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_Fuel_Execution) for LED_Fuel_Execution
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_Temp_Judgement) for LED_Temp_Judgement
    telltales_user.o(.constdata) refers to telltales_user.o(i.LED_Temp_Execution) for LED_Temp_Execution
    flash_synchronizer.o(i.Common_Get_Sync_Signal_Num) refers to flash_synchronizer.o(.data) for FlashTimer
    flash_synchronizer.o(i.Flash_Sync_Signal_Generation_Service) refers to flash_synchronizer.o(.data) for FlashTimer
    flash_synchronizer.o(i.Flash_Sync_Signal_Generation_Service) refers to flash_synchronizer.o(.constdata) for FlashSync1HzTable
    fuel.o(i.Fuel_Cal_Sevice) refers to fuel.o(i.Fuel_R_Cal) for Fuel_R_Cal
    fuel.o(i.Fuel_Cal_Sevice) refers to fuel.o(i.Fuel_State_Check) for Fuel_State_Check
    fuel.o(i.Fuel_Cal_Sevice) refers to fuel.o(i.Fuel_Gauges_Cal) for Fuel_Gauges_Cal
    fuel.o(i.Fuel_Gauges_Cal) refers to common_interface.o(i.Common_GetIgnOnTime) for Common_GetIgnOnTime
    fuel.o(i.Fuel_Gauges_Cal) refers to fuel.o(.data) for FuelSensorState
    fuel.o(i.Fuel_KL15_Init) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    fuel.o(i.Fuel_KL15_Init) refers to fuel.o(.data) for DesFuelSetp
    fuel.o(i.Fuel_KL30_Init) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    fuel.o(i.Fuel_R_Cal) refers to analog_signals.o(i.ADC_Read_Signal) for ADC_Read_Signal
    fuel.o(i.Fuel_R_Cal) refers to aeabi_sdivfast.o(.text) for __aeabi_idivmod
    fuel.o(i.Fuel_R_Cal) refers to fuel.o(.data) for timeCount
    fuel.o(i.Fuel_R_Cal) refers to fuel.o(.bss) for FuelData
    fuel.o(i.Fuel_State_Check) refers to fuel.o(.data) for FuelR
    fuel.o(i.Get_CurFuelSetp) refers to fuel.o(.data) for CurFuelSetp
    fuel.o(i.Get_Fuel_Disp_Byte) refers to fuel.o(.data) for CurFuelSetp
    fuel.o(i.Get_Fuel_Disp_Byte) refers to flash_synchronizer.o(.data) for FlashSync1Hz
    fuel.o(i.Get_Fuel_Sensor_State) refers to fuel.o(.data) for FuelSensorState
    eemanager_interface.o(i.EE_FeedDog) refers to wdt.o(i.WDT_Restart) for WDT_Restart
    eemanager_interface.o(i.EE_SCL_OUT) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    eemanager_interface.o(i.EE_SCL_OUT) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    eemanager_interface.o(i.EE_SCL_OutConfig) refers to gpio.o(i.PORT_Init) for PORT_Init
    eemanager_interface.o(i.EE_SDA_GetValue) refers to gpio.o(i.PORT_GetBit) for PORT_GetBit
    eemanager_interface.o(i.EE_SDA_InConfig) refers to gpio.o(i.PORT_Init) for PORT_Init
    eemanager_interface.o(i.EE_SDA_OUT) refers to gpio.o(i.PORT_SetBit) for PORT_SetBit
    eemanager_interface.o(i.EE_SDA_OUT) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    eemanager_interface.o(i.EE_SDA_OutConfig) refers to gpio.o(i.PORT_Init) for PORT_Init
    eemanager_interface.o(i.eeprom_StoreInfo_Init) refers to eeprommanage.o(.text.eeprom_SetParameter) for eeprom_SetParameter
    eemanager_interface.o(i.eeprom_StoreInfo_Init) refers to eemanager_interface.o(i.EE_SCL_OutConfig) for EE_SCL_OutConfig
    eemanager_interface.o(i.eeprom_StoreInfo_Init) refers to eemanager_interface.o(i.EE_SDA_OutConfig) for EE_SDA_OutConfig
    eemanager_interface.o(i.eeprom_comm_DelayUs) refers to eemanager_interface.o(i.EE_FeedDog) for EE_FeedDog
    eemanager_interface.o(i.eeprom_comm_DelayUs) refers to eemanager_interface.o(i.EE_NOP) for EE_NOP
    services_mileage_user.o(i.CalcODOIgnOffInit) refers to services_mileage_user.o(.data) for SaveODOValid
    services_mileage_user.o(i.CalcODOKL15Init) refers to services_mileage_user.o(.data) for SaveODOValid
    services_mileage_user.o(i.CalcODOKL30Init) refers to eeprommanage.o(.text.eeprom_ReadODO) for eeprom_ReadODO
    services_mileage_user.o(i.CalcODOKL30Init) refers to eeprommanage.o(.text.eeprom_ReadRecord) for eeprom_ReadRecord
    services_mileage_user.o(i.CalcODOKL30Init) refers to services_mileage_user.o(.bss) for g_ReadMileage
    services_mileage_user.o(i.CalcODOKL30Init) refers to services_mileage_user.o(.data) for odoVaild
    services_mileage_user.o(i.CalcODO_100ms_Services) refers to eeprommanage.o(.text.eeprom_ReadODO) for eeprom_ReadODO
    services_mileage_user.o(i.CalcODO_100ms_Services) refers to common_interface.o(i.Common_Get_IG_Sts) for Common_Get_IG_Sts
    services_mileage_user.o(i.CalcODO_100ms_Services) refers to eeprommanage.o(.text.eeprom_WriteODO) for eeprom_WriteODO
    services_mileage_user.o(i.CalcODO_100ms_Services) refers to can_communication_matrix.o(i.Get_ID_55C_Sig_ModifyODOSts) for Get_ID_55C_Sig_ModifyODOSts
    services_mileage_user.o(i.CalcODO_100ms_Services) refers to eeprommanage.o(.text.eeprom_ClearOdoSection) for eeprom_ClearOdoSection
    services_mileage_user.o(i.CalcODO_100ms_Services) refers to services_mileage_user.o(i.Mileage_Delay_ms) for Mileage_Delay_ms
    services_mileage_user.o(i.CalcODO_100ms_Services) refers to eeprommanage.o(.text.eeprom_WriteRecord) for eeprom_WriteRecord
    services_mileage_user.o(i.CalcODO_100ms_Services) refers to can_communication_matrix.o(i.Get_ID_55C_Sig_ModifyODOValue) for Get_ID_55C_Sig_ModifyODOValue
    services_mileage_user.o(i.CalcODO_100ms_Services) refers to can_communication_matrix.o(i.Get_ID_55C_Sig_ClearTrip) for Get_ID_55C_Sig_ClearTrip
    services_mileage_user.o(i.CalcODO_100ms_Services) refers to services_mileage_user.o(i.Data_Clear_Trip) for Data_Clear_Trip
    services_mileage_user.o(i.CalcODO_100ms_Services) refers to services_mileage_user.o(.data) for odoVaild
    services_mileage_user.o(i.CalcODO_100ms_Services) refers to services_mileage_user.o(.bss) for g_ReadMileage
    services_mileage_user.o(i.CalcODO_50ms_Services) refers to common_interface.o(i.Common_Get_IG_Sts) for Common_Get_IG_Sts
    services_mileage_user.o(i.CalcODO_50ms_Services) refers to common_interface.o(i.Common_Get_Act_V_Speed) for Common_Get_Act_V_Speed
    services_mileage_user.o(i.CalcODO_50ms_Services) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    services_mileage_user.o(i.CalcODO_50ms_Services) refers to services_mileage_user.o(.data) for TotalODOTemp
    services_mileage_user.o(i.CalcODO_50ms_Services) refers to services_mileage_user.o(.bss) for g_WriteMileage
    services_mileage_user.o(i.Data_Clear_Trip) refers to services_mileage_user.o(.bss) for g_WriteMileage
    services_mileage_user.o(i.Data_Clear_Trip) refers to services_mileage_user.o(.data) for SaveODOValid
    services_mileage_user.o(i.Data_Mileage_Clear) refers to eeprommanage.o(.text.eeprom_ClearOdoSection) for eeprom_ClearOdoSection
    services_mileage_user.o(i.Data_Mileage_Clear) refers to services_mileage_user.o(i.Mileage_Delay_ms) for Mileage_Delay_ms
    services_mileage_user.o(i.Data_Mileage_Clear) refers to eeprommanage.o(.text.eeprom_WriteRecord) for eeprom_WriteRecord
    services_mileage_user.o(i.Data_Mileage_Clear) refers to services_mileage_user.o(.bss) for g_WriteMileage
    services_mileage_user.o(i.Data_Mileage_Clear) refers to services_mileage_user.o(.data) for TotalODOTemp
    services_mileage_user.o(i.Data_ODO_Read) refers to services_mileage_user.o(.bss) for g_WriteMileage
    services_mileage_user.o(i.Data_Read_Trip) refers to services_mileage_user.o(.bss) for g_WriteMileage
    services_mileage_user.o(i.Mileage_Delay_ms) refers to wdt.o(i.WDT_Restart) for WDT_Restart
    data_gear.o(i.Data_Gear_KL15_Init) refers to data_gear.o(.data) for Gear_Number
    data_gear.o(i.Data_Service_Gear_Processing) refers to data_gear.o(.bss) for GEAR_AD_VALUE
    data_gear.o(i.Data_Service_Gear_Processing) refers to data_gear.o(.constdata) for GEAR_ADResultMIN
    data_gear.o(i.Data_Service_Gear_Processing) refers to data_gear.o(.data) for Gear_Number
    data_gear.o(i.Get_Gear_Mode_Number) refers to data_gear.o(.data) for Gear_Number
    backgroundlight.o(i.AD_SortShort) refers to backgroundlight.o(i.AD_SwapShort) for AD_SwapShort
    backgroundlight.o(i.BackLightDamp) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    backgroundlight.o(i.BackLightDamp) refers to backgroundlight.o(i.SetBackLightOutput) for SetBackLightOutput
    backgroundlight.o(i.BackLightDamp) refers to backgroundlight.o(.data) for BGLCurIgnSt
    backgroundlight.o(i.BackLightDamp) refers to backgroundlight.o(.bss) for BackLightModifyTimer
    backgroundlight.o(i.BackLightDeal) refers to backgroundlight.o(i.SetBacklightDestVal) for SetBacklightDestVal
    backgroundlight.o(i.BackLightDeal) refers to backgroundlight.o(i.SetBacklightCurVal) for SetBacklightCurVal
    backgroundlight.o(i.BackLightDeal) refers to backgroundlight.o(i.SetBacklightMinVal) for SetBacklightMinVal
    backgroundlight.o(i.BackLightDeal) refers to bglinterface.o(i.BGLPwm_Start) for BGLPwm_Start
    backgroundlight.o(i.BackLightDeal) refers to bglinterface.o(i.BGLPwm_Stop) for BGLPwm_Stop
    backgroundlight.o(i.BackLightDeal) refers to backgroundlight.o(.data) for BGLCurIgnSt
    backgroundlight.o(i.BackLightDeal) refers to backgroundlight.o(.bss) for BackupsDuty
    backgroundlight.o(i.BackLightDeal_NTC) refers to backgroundlight.o(i.Calculate_Thermistor) for Calculate_Thermistor
    backgroundlight.o(i.BackLightDeal_NTC) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    backgroundlight.o(i.BackLightDeal_NTC) refers to backgroundlight.o(i.SetBacklightDestVal) for SetBacklightDestVal
    backgroundlight.o(i.BackLightDeal_NTC) refers to backgroundlight.o(.data) for CurBacklightLv
    backgroundlight.o(i.Calculate_Thermistor) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    backgroundlight.o(i.Calculate_Thermistor) refers to backgroundlight.o(i.AD_SortShort) for AD_SortShort
    backgroundlight.o(i.Calculate_Thermistor) refers to backgroundlight.o(.data) for ThermistorIndex
    backgroundlight.o(i.Calculate_Thermistor) refers to backgroundlight.o(.bss) for ThermistorList
    backgroundlight.o(i.SetBackLightOutput) refers to bglinterface.o(i.BGLPwm_Config) for BGLPwm_Config
    backgroundlight.o(i.SetBacklightCurVal) refers to backgroundlight.o(.bss) for BackLightPara
    backgroundlight.o(i.SetBacklightDestVal) refers to backgroundlight.o(.bss) for BackLightPara
    backgroundlight.o(i.SetBacklightMinVal) refers to backgroundlight.o(.bss) for BackLightPara
    bglinterface.o(i.BGLPwm_Config) refers to timera_b_c.o(i.TMB0_PWM_Pin33_Freq_Duty) for TMB0_PWM_Pin33_Freq_Duty
    bglinterface.o(i.BGLPwm_Config) refers to bglinterface.o(.constdata) for PwmChannel
    bglinterface.o(i.BGLPwm_Start) refers to timera_b_c.o(i.TMB0_Start) for TMB0_Start
    bglinterface.o(i.BGLPwm_Start) refers to bglinterface.o(.constdata) for PwmChannel
    bglinterface.o(i.BGLPwm_Stop) refers to timera_b_c.o(i.TMB0_Stop) for TMB0_Stop
    bglinterface.o(i.BGLPwm_Stop) refers to bglinterface.o(.constdata) for PwmChannel
    bglinterface.o(i.BGTask) refers to bglinterface.o(i.SetBGLTheme) for SetBGLTheme
    bglinterface.o(i.BGTask) refers to bglinterface.o(i.SetBGLType) for SetBGLType
    bglinterface.o(i.BGTask) refers to bglinterface.o(i.SetBGLNTCVol) for SetBGLNTCVol
    bglinterface.o(i.BGTask) refers to common_interface.o(i.Common_Get_IG_Sts) for Common_Get_IG_Sts
    bglinterface.o(i.BGTask) refers to system_monitor.o(i.System_FUN_KL30_Status_Get) for System_FUN_KL30_Status_Get
    bglinterface.o(i.BGTask) refers to bglinterface.o(i.BackLightSchedu) for BackLightSchedu
    bglinterface.o(i.BackLightSchedu) refers to bglinterface.o(.data) for CurLcdBackLightCycle
    bglinterface.o(i.BackLightSchedu) refers to bglinterface.o(.bss) for BL_Tmp_PARA
    bglinterface.o(i.Get_Day_Or_Night) refers to bglinterface.o(.data) for DayOrNight
    bglinterface.o(i.ProcessLittleLight) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    bglinterface.o(i.SetBGLLvl) refers to bglinterface.o(i.ProcessLittleLight) for ProcessLittleLight
    bglinterface.o(i.SetBGLLvl) refers to bglinterface.o(.bss) for BLStatePara
    bglinterface.o(i.SetBGLNTCVol) refers to bglinterface.o(.bss) for BLStatePara
    bglinterface.o(i.SetBGLTheme) refers to bglinterface.o(.bss) for BLStatePara
    bglinterface.o(i.SetBGLType) refers to bglinterface.o(.bss) for BLStatePara
    key.o(i.Get_Key1_Line_In_Sts) refers to aw93015.o(i.GET_Key_Prosess) for GET_Key_Prosess
    key.o(i.Get_Key2_Line_In_Sts) refers to aw93015.o(i.GET_Key_Prosess) for GET_Key_Prosess
    key.o(i.Key_Get_Current_Status) refers to key.o(.bss) for KeyStatus
    key.o(i.Key_Get_Status) refers to key.o(.bss) for KeyStatus
    key.o(i.Key_Status_Detect_Service) refers to gpio.o(i.__ARM_common_switch8) for __ARM_common_switch8
    key.o(i.Key_Status_Detect_Service) refers to aeabi_sdivfast.o(.text) for __aeabi_idivmod
    key.o(i.Key_Status_Detect_Service) refers to key.o(.constdata) for KeyAttrTable
    key.o(i.Key_Status_Detect_Service) refers to key.o(.bss) for KeyStatus
    key.o(i.Key_Status_Init) refers to key.o(.bss) for KeyStatus
    key.o(i.Reset_Key_Status) refers to key.o(.bss) for KeyStatus
    key.o(.constdata) refers to key.o(i.Get_Key1_Line_In_Sts) for Get_Key1_Line_In_Sts
    key.o(.constdata) refers to key.o(i.Get_Key2_Line_In_Sts) for Get_Key2_Line_In_Sts
    can_communication_matrix.o(i.Get_ID_101_ECU_Engine_Temperature) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_101_ECU_Engine_Temperature_State) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_101_ECU_Vehicle_Speed) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_111_ISG_Power_Enable) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_111_ISG_Ready) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_111_Sig_ISG_SideStand) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_113_Auto_High_Beam) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_113_Tbatt) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_125_Sig_TCS_SysState) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_125_Sig_TCS_WarningLamp) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_125_Sig_TCS_WorkMode) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_12B_Rear_Speed) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_12B_Rear_Wheel_Speed_Validity) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_401_Sig_ECU_Battery_Voltage) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_402_ECU_DTC1Amnt) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_402_ECU_DTCH1) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_402_ECU_DTCH2) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_402_ECU_DTCL1) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_402_ECU_DTCL2) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_402_ECU_DTCM1) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_402_ECU_DTCM2) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_55C_Sig_ClearTrip) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_55C_Sig_ModifyODOSts) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(i.Get_ID_55C_Sig_ModifyODOValue) refers to can_signal_rx.o(i.CAN_MSG_Read) for CAN_MSG_Read
    can_communication_matrix.o(.constdata) refers to can_user.o(i.Can_Set_Buff_105) for Can_Set_Buff_105
    can_communication_matrix.o(.constdata) refers to can_user.o(i.Can_Set_Buff_51C) for Can_Set_Buff_51C
    can_communication_matrix.o(.constdata) refers to can_user.o(i.Can_Set_Buff_522) for Can_Set_Buff_522
    can_communication_matrix.o(.constdata) refers to can_user.o(i.Can_Set_Buff_523) for Can_Set_Buff_523
    can_communication_matrix.o(.constdata) refers to can_user.o(i.Can_Set_Buff_510) for Can_Set_Buff_510
    can_communication_matrix.o(.constdata) refers to can_user.o(i.Can_Set_Buff_450) for Can_Set_Buff_450
    can_communication_matrix.o(.constdata) refers to can_user.o(i.Can_Set_Buff_515) for Can_Set_Buff_515
    can_user.o(i.APP_CAN_Init) refers to can_signal_tx.o(i.Can_TX_BuffInit) for Can_TX_BuffInit
    can_user.o(i.APP_CAN_Init) refers to can_signal_rx.o(i.Can_RX_BuffInit) for Can_RX_BuffInit
    can_user.o(i.APP_CAN_Init) refers to can_signal_rx.o(i.CAN_RX_SetEnable) for CAN_RX_SetEnable
    can_user.o(i.APP_CAN_Init) refers to can_signal_tx.o(i.CAN_TX_SetEnable) for CAN_TX_SetEnable
    can_user.o(i.APP_CAN_Init) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    can_user.o(i.APP_CAN_Init) refers to can_user.o(i.Can_Write) for Can_Write
    can_user.o(i.APP_CAN_Init) refers to can_communication_matrix.o(.constdata) for st_CANSendAttr
    can_user.o(i.APP_CAN_Init) refers to can_user.o(.bss) for pTXBuff
    can_user.o(i.APP_CAN_Init) refers to can_user.o(.data) for BCM_Module
    can_user.o(i.BatteryVoltageDelayInit) refers to can_user.o(.data) for BatteryClearnflag
    can_user.o(i.CAN_Check_Liandian) refers to can_user.o(.data) for LianDianModuleFlg
    can_user.o(i.CAN_Init) refers to can_signal_tx.o(i.Can_TX_BuffInit) for Can_TX_BuffInit
    can_user.o(i.CAN_Init) refers to can_signal_rx.o(i.Can_RX_BuffInit) for Can_RX_BuffInit
    can_user.o(i.CAN_Init) refers to can_signal_rx.o(i.CAN_RX_SetEnable) for CAN_RX_SetEnable
    can_user.o(i.CAN_Init) refers to can_signal_tx.o(i.CAN_TX_SetEnable) for CAN_TX_SetEnable
    can_user.o(i.CAN_Init) refers to gpio.o(i.PORT_ClrBit) for PORT_ClrBit
    can_user.o(i.CAN_Init) refers to can_user.o(i.Can_Write) for Can_Write
    can_user.o(i.CAN_Init) refers to can_communication_matrix.o(.constdata) for st_CANSendAttr
    can_user.o(i.CAN_Init) refers to can_user.o(.bss) for pTXBuff
    can_user.o(i.CAN_LED_Check_50msTask) refers to system_monitor.o(i.System_FUN_KL15_Status_Get) for System_FUN_KL15_Status_Get
    can_user.o(i.CAN_LED_Check_50msTask) refers to can_user.o(i.Get_TCS_WorkModeFlash) for Get_TCS_WorkModeFlash
    can_user.o(i.CAN_LED_Check_50msTask) refers to can_communication_matrix.o(i.Get_ID_125_Sig_TCS_WorkMode) for Get_ID_125_Sig_TCS_WorkMode
    can_user.o(i.CAN_LED_Check_50msTask) refers to can_user.o(i.Set_TCS_WorkModeFlsh) for Set_TCS_WorkModeFlsh
    can_user.o(i.CAN_LED_Check_50msTask) refers to can_user.o(i.get_ECU_Battery_Voltage) for get_ECU_Battery_Voltage
    can_user.o(i.CAN_LED_Check_50msTask) refers to can_signal_rx.o(i.CAN_MSG_Status) for CAN_MSG_Status
    can_user.o(i.CAN_LED_Check_50msTask) refers to can_user.o(i.SET_LED_ECU_Battery_VoltageFlag) for SET_LED_ECU_Battery_VoltageFlag
    can_user.o(i.CAN_LED_Check_50msTask) refers to can_user.o(.data) for tempclk
    can_user.o(i.CAN_RX_Tick) refers to can_signal_rx.o(i.CanMSg_XMS_Analysis) for CanMSg_XMS_Analysis
    can_user.o(i.CAN_SendAppMesageOpinion) refers to can_signal_tx.o(i.CAN_TX_SetEnable) for CAN_TX_SetEnable
    can_user.o(i.CAN_TX_Tick) refers to can_signal_tx.o(i.Can_Write_Fun) for Can_Write_Fun
    can_user.o(i.Can_BusOffRecover) refers to can_user.o(.data) for BusOffEvent
    can_user.o(i.Can_BusOff_Fun) refers to can.o(i.Get_CH0_BusOffStatus) for Get_CH0_BusOffStatus
    can_user.o(i.Can_BusOff_Fun) refers to can.o(i.bsp_tx_msgbuf_abort) for bsp_tx_msgbuf_abort
    can_user.o(i.Can_BusOff_Fun) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    can_user.o(i.Can_BusOff_Fun) refers to can.o(i.bsp_CAN_BusOff_Recover) for bsp_CAN_BusOff_Recover
    can_user.o(i.Can_BusOff_Fun) refers to can_user.o(i.Can_BusOffRecover) for Can_BusOffRecover
    can_user.o(i.Can_BusOff_Fun) refers to can.o(.data) for CanSendLock
    can_user.o(i.Can_BusOff_Fun) refers to can_user.o(.data) for BusOffEvent
    can_user.o(i.Can_Receive_Msg) refers to can_communication_matrix.o(i.Co_Can_ConvertSubID) for Co_Can_ConvertSubID
    can_user.o(i.Can_Receive_Msg) refers to can_signal_rx.o(i.Co_Can_Buff_Set) for Co_Can_Buff_Set
    can_user.o(i.Can_Set_Buff_105) refers to common_interface.o(i.Common_Get_Disp_E_Speed) for Common_Get_Disp_E_Speed
    can_user.o(i.Can_Set_Buff_105) refers to common_interface.o(i.Common_Get_Disp_V_Speed) for Common_Get_Disp_V_Speed
    can_user.o(i.Can_Set_Buff_105) refers to aeabi_sdivfast.o(.text) for __aeabi_idivmod
    can_user.o(i.Can_Set_Buff_502) refers to line_in.o(i.LINE_IN_Get_TirePressure) for LINE_IN_Get_TirePressure
    can_user.o(i.Can_Set_Buff_510) refers to fuel.o(i.Get_Fuel_Sensor_State) for Get_Fuel_Sensor_State
    can_user.o(i.Can_Set_Buff_510) refers to fuel.o(i.Get_CurFuelSetp) for Get_CurFuelSetp
    can_user.o(i.Can_Set_Buff_510) refers to aeabi_sdivfast.o(.text) for __aeabi_idivmod
    can_user.o(i.Can_Set_Buff_510) refers to fuel.o(.data) for FuelR
    can_user.o(i.Can_Set_Buff_515) refers to can_user.o(i.GetAllDtcFault) for GetAllDtcFault
    can_user.o(i.Can_Set_Buff_515) refers to can_signal_rx.o(i.CAN_MSG_Status) for CAN_MSG_Status
    can_user.o(i.Can_Set_Buff_515) refers to can_user.o(i.get_CoolantTempVal) for get_CoolantTempVal
    can_user.o(i.Can_Set_Buff_515) refers to can_user.o(.data) for HisFaultNum
    can_user.o(i.Can_Set_Buff_515) refers to can_user.o(.bss) for HisFault
    can_user.o(i.Can_Set_Buff_522) refers to services_mileage_user.o(i.Data_ODO_Read) for Data_ODO_Read
    can_user.o(i.Can_Set_Buff_522) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    can_user.o(i.Can_Set_Buff_522) refers to common_interface.o(i.Common_Get_Disp_V_Speed) for Common_Get_Disp_V_Speed
    can_user.o(i.Can_Set_Buff_522) refers to services_mileage_user.o(.data) for ModfyODORemainTimes
    can_user.o(i.Can_Set_Buff_523) refers to services_mileage_user.o(i.Data_Read_Trip) for Data_Read_Trip
    can_user.o(i.Can_Set_Buff_523) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    can_user.o(i.Can_User_Time_Service) refers to common_interface.o(i.Common_Get_IG_Sts) for Common_Get_IG_Sts
    can_user.o(i.Can_User_Time_Service) refers to can_signal_tx.o(i.CAN_TX_SetEnable) for CAN_TX_SetEnable
    can_user.o(i.Can_User_Time_Service) refers to can.o(i.bsp_tx_msgbuf_abort) for bsp_tx_msgbuf_abort
    can_user.o(i.Can_User_Time_Service) refers to can.o(i.bsp_CAN_Sleep) for bsp_CAN_Sleep
    can_user.o(i.Can_User_Time_Service) refers to can_user.o(.data) for Mil_Signal_Time
    can_user.o(i.Can_User_Time_Service) refers to app_service.o(.bss) for DiagnoCtl
    can_user.o(i.Can_Write) refers to gpio.o(i.__ARM_common_switch8) for __ARM_common_switch8
    can_user.o(i.Can_Write) refers to can.o(i.bsp_CANSendFrame) for bsp_CANSendFrame
    can_user.o(i.Can_Write) refers to can.o(.data) for CanSendLock
    can_user.o(i.Can_Write) refers to can_user.o(.data) for CanLibSendFlag
    can_user.o(i.DelfuModuleIn) refers to can_user.o(.data) for DelfuModuleFlg
    can_user.o(i.Diag_Req_Send) refers to can_user.o(i.Get_Bcm_Module) for Get_Bcm_Module
    can_user.o(i.Diag_Req_Send) refers to common_interface.o(i.Common_Get_IG_Sts) for Common_Get_IG_Sts
    can_user.o(i.Diag_Req_Send) refers to can_user.o(i.Get_ReqSilentTimer) for Get_ReqSilentTimer
    can_user.o(i.Diag_Req_Send) refers to gpio.o(i.__ARM_common_switch8) for __ARM_common_switch8
    can_user.o(i.Diag_Req_Send) refers to can_user.o(i.Send_19_0209) for Send_19_0209
    can_user.o(i.Diag_Req_Send) refers to u2_app_service.o(i.Set_UDS_59_MsgRecFlg) for Set_UDS_59_MsgRecFlg
    can_user.o(i.Diag_Req_Send) refers to u2_app_service.o(i.Get_UDS_59_MsgRecFlg) for Get_UDS_59_MsgRecFlg
    can_user.o(i.Diag_Req_Send) refers to can_user.o(i.Send_22_ID0005) for Send_22_ID0005
    can_user.o(i.Diag_Req_Send) refers to u2_app_service.o(i.Set_UDS_62_MsgRecFlg) for Set_UDS_62_MsgRecFlg
    can_user.o(i.Diag_Req_Send) refers to u2_app_service.o(i.Get_UDS_62_MsgRecFlg) for Get_UDS_62_MsgRecFlg
    can_user.o(i.Diag_Req_Send) refers to can_user.o(i.Send_01_01) for Send_01_01
    can_user.o(i.Diag_Req_Send) refers to u2_app_service.o(i.Set_UDS_01_MsgRecFlg) for Set_UDS_01_MsgRecFlg
    can_user.o(i.Diag_Req_Send) refers to u2_app_service.o(i.Get_UDS_01_MsgRecFlg) for Get_UDS_01_MsgRecFlg
    can_user.o(i.Diag_Req_Send) refers to can_user.o(.data) for DTCCurFaultTimes
    can_user.o(i.Diag_Req_Send) refers to can.o(.data) for CanSendLock
    can_user.o(i.Diag_Req_Send) refers to app_service.o(.bss) for DiagnoCtl
    can_user.o(i.DtcFaultInit) refers to can_user.o(.data) for OldDtcAmnt
    can_user.o(i.DtcFaultTimeInit) refers to can_user.o(.data) for DTCCurFaultTimes
    can_user.o(i.GetAllDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTCH1) for Get_ID_402_ECU_DTCH1
    can_user.o(i.GetAllDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTCM1) for Get_ID_402_ECU_DTCM1
    can_user.o(i.GetAllDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTCH2) for Get_ID_402_ECU_DTCH2
    can_user.o(i.GetAllDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTCM2) for Get_ID_402_ECU_DTCM2
    can_user.o(i.GetAllDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTC1Amnt) for Get_ID_402_ECU_DTC1Amnt
    can_user.o(i.GetDtcAmnt) refers to can_user.o(.data) for CurFaultNum
    can_user.o(i.GetDtcDispNum) refers to can_user.o(.bss) for CurFault
    can_user.o(i.GetDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTCH1) for Get_ID_402_ECU_DTCH1
    can_user.o(i.GetDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTCM1) for Get_ID_402_ECU_DTCM1
    can_user.o(i.GetDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTCH2) for Get_ID_402_ECU_DTCH2
    can_user.o(i.GetDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTCM2) for Get_ID_402_ECU_DTCM2
    can_user.o(i.GetDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTC1Amnt) for Get_ID_402_ECU_DTC1Amnt
    can_user.o(i.GetDtcFault) refers to can_user.o(.data) for DTCCurFaultTimes
    can_user.o(i.Get_Bcm_Module) refers to can_user.o(.data) for BCM_Module
    can_user.o(i.Get_CanSleepDelayTime) refers to can_user.o(.data) for CanSleepDelayTime
    can_user.o(i.Get_LED_ECU_Battery_VoltageFlag) refers to can_user.o(.data) for ECU_Battery_VoltageFlag
    can_user.o(i.Get_Mil_Signal_Connect) refers to can_user.o(.data) for Mil_Signal_Connect
    can_user.o(i.Get_RSCAN0Busoff_Status) refers to can_user.o(.data) for RSCAN0Busoff
    can_user.o(i.Get_ReqSilentTimer) refers to can_user.o(.data) for ReqSilentTimer
    can_user.o(i.Get_TCS_WorkModeFlash) refers to can_user.o(.data) for TCS_WorkModeFlsh
    can_user.o(i.LianDianModuleIn) refers to can_user.o(.data) for LianDianModuleFlg
    can_user.o(i.ReqSilentTimer100mSService) refers to can_user.o(.data) for ReqSilentTimer
    can_user.o(i.Reset_Mil_Signal_Time) refers to can_user.o(.data) for Mil_Signal_Time
    can_user.o(i.SET_LED_ECU_Battery_VoltageFlag) refers to can_user.o(.data) for ECU_Battery_VoltageFlag
    can_user.o(i.Send_01_01) refers to can_user.o(i.Can_Write) for Can_Write
    can_user.o(i.Send_19_0209) refers to can_user.o(i.Can_Write) for Can_Write
    can_user.o(i.Send_22_ID0005) refers to can_user.o(i.Can_Write) for Can_Write
    can_user.o(i.SetDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTCH1) for Get_ID_402_ECU_DTCH1
    can_user.o(i.SetDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTCM1) for Get_ID_402_ECU_DTCM1
    can_user.o(i.SetDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTCL1) for Get_ID_402_ECU_DTCL1
    can_user.o(i.SetDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTCH2) for Get_ID_402_ECU_DTCH2
    can_user.o(i.SetDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTCM2) for Get_ID_402_ECU_DTCM2
    can_user.o(i.SetDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTCL2) for Get_ID_402_ECU_DTCL2
    can_user.o(i.SetDtcFault) refers to can_communication_matrix.o(i.Get_ID_402_ECU_DTC1Amnt) for Get_ID_402_ECU_DTC1Amnt
    can_user.o(i.SetDtcFault) refers to rt_memclr.o(.text) for __aeabi_memclr4
    can_user.o(i.SetDtcFault) refers to can_user.o(.data) for OldDtcAmnt
    can_user.o(i.SetDtcFault) refers to u2_app_service.o(.bss) for U2_DiagReciveDTC
    can_user.o(i.SetSendUdsTimeCount_0101) refers to can_user.o(.data) for SendUdsTimeCount_0101
    can_user.o(i.SetSendUdsTimeCount_190209) refers to can_user.o(.data) for SendUdsTimeCount_190209
    can_user.o(i.SetSendUdsTimeCount_220005) refers to can_user.o(.data) for SendUdsTimeCount_220005
    can_user.o(i.Set_CanSleepDelayTime) refers to can_user.o(.data) for CanSleepDelayTime
    can_user.o(i.Set_ReqSilentTimer) refers to can_user.o(.data) for ReqSilentTimer
    can_user.o(i.Set_TCS_WorkModeFlsh) refers to can_user.o(.data) for TCS_WorkModeFlsh
    can_user.o(i.Set_TCS_WorkModeFlshTime) refers to can_user.o(.data) for tempclk
    can_user.o(i.getBUS_OFF_Status) refers to can_user.o(.data) for BusOffEvent
    can_user.o(i.get_CoolantTempVal) refers to can_user.o(i.get_ECU_Temperature_WaterVal) for get_ECU_Temperature_WaterVal
    can_user.o(i.get_Delay_ECU_Battery_Voltage) refers to can_user.o(i.get_ECU_Battery_Voltage) for get_ECU_Battery_Voltage
    can_user.o(i.get_Delay_ECU_Battery_Voltage) refers to can_signal_rx.o(i.CAN_MSG_Status) for CAN_MSG_Status
    can_user.o(i.get_Delay_ECU_Battery_Voltage) refers to can_user.o(.data) for Oldget_ECU_Battery_Voltage
    can_user.o(i.get_ECU_Battery_Voltage) refers to can_communication_matrix.o(i.Get_ID_401_Sig_ECU_Battery_Voltage) for Get_ID_401_Sig_ECU_Battery_Voltage
    can_user.o(i.get_ECU_Temperature_WaterVal) refers to can_communication_matrix.o(i.Get_ID_101_ECU_Engine_Temperature) for Get_ID_101_ECU_Engine_Temperature
    can_user.o(i.get_ECU_Temperature_WaterVal) refers to aeabi_sdivfast.o(.text) for __aeabi_idivmod
    can_user.o(i.get_ECU_Temperature_WaterVal) refers to can_user.o(.data) for Sig_ECU_Temperature_Water
    can_user.o(i.get_ID_ISG_BATT) refers to can_communication_matrix.o(i.Get_ID_113_Tbatt) for Get_ID_113_Tbatt
    can_user.o(i.get_ID_ISG_Power) refers to can_communication_matrix.o(i.Get_ID_111_ISG_Power_Enable) for Get_ID_111_ISG_Power_Enable
    app_telltales.o(i.App_Telltales_AllOFF) refers to app_telltales.o(i.App_Telltales_Ctrl) for App_Telltales_Ctrl
    app_telltales.o(i.App_Telltales_AllON) refers to app_telltales.o(i.App_Telltales_Ctrl) for App_Telltales_Ctrl
    app_telltales.o(i.App_Telltales_Ctrl) refers to app_telltales.o(.constdata) for IS31FL3236_LED_Channel
    app_telltales.o(i.App_Telltales_Ctrl) refers to is31fl3236.o(.bss) for u8IS31Data
    app_service.o(i.App_01_service) refers to can_user.o(i.Reset_Mil_Signal_Time) for Reset_Mil_Signal_Time
    app_service.o(i.App_01_service) refers to can_user.o(i.DelfuModuleIn) for DelfuModuleIn
    app_service.o(i.App_01_service) refers to app_service.o(.bss) for DiagReciveGaugePara
    app_service.o(i.App_10_service) refers to app_serviceproc.o(i.App_ErrorInfoInit) for App_ErrorInfoInit
    app_service.o(i.App_10_service) refers to app_service.o(i.App_SetSessionTimer) for App_SetSessionTimer
    app_service.o(i.App_10_service) refers to flash.o(ram_fetch_code) for EraseSector
    app_service.o(i.App_10_service) refers to app_service.o(.bss) for DiagnoCtl
    app_service.o(i.App_10_service) refers to app_service.o(.data) for Error
    app_service.o(i.App_10_service) refers to tp_layer.o(.bss) for N_RSPData
    app_service.o(i.App_11_service) refers to app_serviceproc.o(i.App_ErrorInfoInit) for App_ErrorInfoInit
    app_service.o(i.App_11_service) refers to app_service.o(.bss) for DiagnoCtl
    app_service.o(i.App_11_service) refers to app_service.o(.data) for Error
    app_service.o(i.App_11_service) refers to tp_layer.o(.bss) for N_RSPData
    app_service.o(i.App_14_service) refers to app_serviceproc.o(i.App_ErrorInfoInit) for App_ErrorInfoInit
    app_service.o(i.App_14_service) refers to app_service.o(.data) for Error
    app_service.o(i.App_14_service) refers to tp_layer.o(.bss) for N_RSPData
    app_service.o(i.App_22_service) refers to app_serviceproc.o(i.App_ErrorInfoInit) for App_ErrorInfoInit
    app_service.o(i.App_22_service) refers to app_serviceproc.o(i.App_Load_DID) for App_Load_DID
    app_service.o(i.App_22_service) refers to app_service.o(.bss) for DiagnoCtl
    app_service.o(i.App_22_service) refers to tp_layer.o(.bss) for N_US_S_MultiData
    app_service.o(i.App_22_service) refers to app_service.o(.data) for MCU_SoftCode
    app_service.o(i.App_27_service) refers to app_serviceproc.o(i.App_ErrorInfoInit) for App_ErrorInfoInit
    app_service.o(i.App_27_service) refers to analog_signals.o(i.ADC_Read_Signal) for ADC_Read_Signal
    app_service.o(i.App_27_service) refers to app_service.o(i.CalculateKey) for CalculateKey
    app_service.o(i.App_27_service) refers to app_service.o(i.App_SetReUnlockTimer) for App_SetReUnlockTimer
    app_service.o(i.App_27_service) refers to app_service.o(.bss) for DiagnoCtl
    app_service.o(i.App_27_service) refers to tp_layer.o(.bss) for N_RSPData
    app_service.o(i.App_27_service) refers to app_service.o(.data) for Error
    app_service.o(i.App_28_service) refers to app_serviceproc.o(i.App_ErrorInfoInit) for App_ErrorInfoInit
    app_service.o(i.App_28_service) refers to app_service.o(.bss) for DiagnoCtl
    app_service.o(i.App_28_service) refers to app_service.o(.data) for Error
    app_service.o(i.App_28_service) refers to tp_layer.o(.bss) for N_RSPData
    app_service.o(i.App_2E_service) refers to app_serviceproc.o(i.App_ErrorInfoInit) for App_ErrorInfoInit
    app_service.o(i.App_2E_service) refers to app_serviceproc.o(i.App_Load_DID) for App_Load_DID
    app_service.o(i.App_2E_service) refers to app_service.o(.bss) for DiagnoCtl
    app_service.o(i.App_2E_service) refers to app_service.o(.data) for Error
    app_service.o(i.App_2E_service) refers to tp_layer.o(.bss) for N_RSPData
    app_service.o(i.App_2F_service) refers to app_serviceproc.o(i.App_ErrorInfoInit) for App_ErrorInfoInit
    app_service.o(i.App_2F_service) refers to app_serviceproc.o(i.App_Load_DID) for App_Load_DID
    app_service.o(i.App_2F_service) refers to app_service.o(.bss) for DiagnoCtl
    app_service.o(i.App_2F_service) refers to app_service.o(.data) for Error
    app_service.o(i.App_2F_service) refers to tp_layer.o(.bss) for N_US_S_MultiData
    app_service.o(i.App_31_service) refers to app_serviceproc.o(i.App_ErrorInfoInit) for App_ErrorInfoInit
    app_service.o(i.App_31_service) refers to app_serviceproc.o(i.App_Load_DID) for App_Load_DID
    app_service.o(i.App_31_service) refers to rt_memcpy.o(.text) for __aeabi_memcpy
    app_service.o(i.App_31_service) refers to app_service.o(.bss) for DiagnoCtl
    app_service.o(i.App_31_service) refers to app_service.o(.data) for Error
    app_service.o(i.App_31_service) refers to tp_layer.o(.bss) for N_RSPData
    app_service.o(i.App_34_service) refers to app_serviceproc.o(i.App_ErrorInfoInit) for App_ErrorInfoInit
    app_service.o(i.App_34_service) refers to app_service.o(.bss) for DiagnoCtl
    app_service.o(i.App_34_service) refers to app_service.o(.data) for Error
    app_service.o(i.App_34_service) refers to tp_layer.o(.bss) for N_RSPData
    app_service.o(i.App_36_service) refers to app_serviceproc.o(i.App_ErrorInfoInit) for App_ErrorInfoInit
    app_service.o(i.App_36_service) refers to app_service.o(.bss) for DiagnoCtl
    app_service.o(i.App_36_service) refers to app_service.o(.data) for Error
    app_service.o(i.App_36_service) refers to tp_layer.o(.bss) for N_RSPData
    app_service.o(i.App_37_service) refers to app_serviceproc.o(i.App_ErrorInfoInit) for App_ErrorInfoInit
    app_service.o(i.App_37_service) refers to app_service.o(.bss) for DiagnoCtl
    app_service.o(i.App_37_service) refers to app_service.o(.data) for Error
    app_service.o(i.App_37_service) refers to tp_layer.o(.bss) for N_RSPData
    app_service.o(i.App_3E_service) refers to app_serviceproc.o(i.App_ErrorInfoInit) for App_ErrorInfoInit
    app_service.o(i.App_3E_service) refers to app_service.o(i.App_SetSessionTimer) for App_SetSessionTimer
    app_service.o(i.App_3E_service) refers to tp_layer.o(.bss) for N_RSPData
    app_service.o(i.App_3E_service) refers to app_service.o(.bss) for DiagClock
    app_service.o(i.App_3E_service) refers to app_service.o(.data) for Error
    app_service.o(i.App_59_service) refers to app_serviceproc.o(i.App_ErrorInfoInit) for App_ErrorInfoInit
    app_service.o(i.App_59_service) refers to app_serviceproc.o(i.App_Load_DID) for App_Load_DID
    app_service.o(i.App_59_service) refers to rt_memclr.o(.text) for __aeabi_memclr4
    app_service.o(i.App_59_service) refers to app_serviceproc.o(i.App_CopyRam) for App_CopyRam
    app_service.o(i.App_59_service) refers to app_service.o(.bss) for DiagReciveDTC
    app_service.o(i.App_85_service) refers to app_serviceproc.o(i.App_ErrorInfoInit) for App_ErrorInfoInit
    app_service.o(i.App_85_service) refers to app_service.o(.bss) for DiagnoCtl
    app_service.o(i.App_85_service) refers to app_service.o(.data) for Error
    app_service.o(i.App_85_service) refers to tp_layer.o(.bss) for N_RSPData
    app_service.o(i.CalculateKeyLv11) refers to app_service.o(.constdata) for XorArray
    app_service.o(i.DiagnosisInit_main) refers to tp_layer.o(i.TP_SetSTminTimer) for TP_SetSTminTimer
    app_service.o(i.DiagnosisInit_main) refers to tp_layer.o(.bss) for N_US_R_MultiData
    app_service.o(i.DiagnosisInit_main) refers to app_service.o(.bss) for Exct_USData
    app_service.o(i.DiagnosisInit_main) refers to link_layer.o(.bss) for LinkDataBuf
    app_service.o(i.DiagnosisInit_main) refers to app_service.o(.data) for Error
    app_service.o(i.Diagnosis_main) refers to tp_layer.o(i.TP_Buffer_handle) for TP_Buffer_handle
    app_service.o(i.Diagnosis_main) refers to tp_layer.o(i.TP_ReciveSF_handle) for TP_ReciveSF_handle
    app_service.o(i.Diagnosis_main) refers to tp_layer.o(i.TP_ReciveMultiF_handle) for TP_ReciveMultiF_handle
    app_service.o(i.Diagnosis_main) refers to tp_layer.o(i.TP_NormalRecFC_handle) for TP_NormalRecFC_handle
    app_service.o(i.Diagnosis_main) refers to tp_layer.o(i.TP_NormalSendFC_Fun) for TP_NormalSendFC_Fun
    app_service.o(i.Diagnosis_main) refers to app_serviceproc.o(i.App_CopyRam) for App_CopyRam
    app_service.o(i.Diagnosis_main) refers to tp_layer.o(i.TP_BsTimerOver) for TP_BsTimerOver
    app_service.o(i.Diagnosis_main) refers to app_service.o(i.App_SessionTimerOver) for App_SessionTimerOver
    app_service.o(i.Diagnosis_main) refers to app_service.o(i.App_ReUnlockTimerOver) for App_ReUnlockTimerOver
    app_service.o(i.Diagnosis_main) refers to app_service.o(i.App_10_service) for App_10_service
    app_service.o(i.Diagnosis_main) refers to app_service.o(i.App_11_service) for App_11_service
    app_service.o(i.Diagnosis_main) refers to app_service.o(i.App_22_service) for App_22_service
    app_service.o(i.Diagnosis_main) refers to app_service.o(i.App_3E_service) for App_3E_service
    app_service.o(i.Diagnosis_main) refers to app_service.o(i.App_85_service) for App_85_service
    app_service.o(i.Diagnosis_main) refers to app_service.o(i.App_28_service) for App_28_service
    app_service.o(i.Diagnosis_main) refers to app_service.o(i.App_27_service) for App_27_service
    app_service.o(i.Diagnosis_main) refers to app_service.o(i.App_2E_service) for App_2E_service
    app_service.o(i.Diagnosis_main) refers to tp_layer.o(i.TP_TransmitPDU) for TP_TransmitPDU
    app_service.o(i.Diagnosis_main) refers to app_serviceproc.o(i.App_11_Reset_handle) for App_11_Reset_handle
    app_service.o(i.Diagnosis_main) refers to link_layer.o(.bss) for LinkData
    app_service.o(i.Diagnosis_main) refers to tp_layer.o(.bss) for N_USSFData
    app_service.o(i.Diagnosis_main) refers to app_service.o(.bss) for Exct_USData
    app_service.o(i.Diagnosis_main) refers to app_service.o(.data) for Error
    app_service.o(i.Get_DiagnoCtl_CommCtl) refers to app_service.o(.bss) for DiagnoCtl
    app_serviceproc.o(i.App_11_Reset_handle) refers to tp_layer.o(.bss) for N_RSPData
    app_serviceproc.o(i.App_11_Reset_handle) refers to app_service.o(.bss) for DiagnoCtl
    app_serviceproc.o(i.App_ErrorInfoInit) refers to app_service.o(.data) for Error
    app_serviceproc.o(i.Diagno_Tick) refers to app_service.o(.bss) for DiagClock
    link_layer.o(i.LK_Link_main) refers to rt_memcpy.o(.text) for __aeabi_memcpy
    link_layer.o(i.LK_Link_main) refers to link_layer.o(.bss) for LinkDataBuf
    tp_layer.o(i.TP_AbnormalInReqFC_handle) refers to tp_layer.o(.bss) for N_US_R_MultiData
    tp_layer.o(i.TP_AbnormalInReqFC_handle) refers to link_layer.o(.bss) for LinkData
    tp_layer.o(i.TP_AbnormalInReqFF_handle) refers to link_layer.o(.bss) for LinkData
    tp_layer.o(i.TP_AbnormalInReqFF_handle) refers to tp_layer.o(.bss) for N_US_R_MultiData
    tp_layer.o(i.TP_AbnormalInResCF_handle) refers to tp_layer.o(.bss) for N_US_S_MultiData
    tp_layer.o(i.TP_AbnormalInResCF_handle) refers to link_layer.o(.bss) for LinkData
    tp_layer.o(i.TP_AbnormalInResFC_handle) refers to tp_layer.o(.bss) for N_US_S_Data_FF
    tp_layer.o(i.TP_AbnormalInResFC_handle) refers to link_layer.o(.bss) for LinkData
    tp_layer.o(i.TP_AbnormalInResSF_handle) refers to tp_layer.o(.bss) for N_US_S_MultiData
    tp_layer.o(i.TP_AbnormalInResSF_handle) refers to link_layer.o(.bss) for LinkData
    tp_layer.o(i.TP_Buffer_handle) refers to rt_memcpy.o(.text) for __aeabi_memcpy
    tp_layer.o(i.TP_Buffer_handle) refers to tp_layer.o(i.TP_AbnormalInResSF_handle) for TP_AbnormalInResSF_handle
    tp_layer.o(i.TP_Buffer_handle) refers to tp_layer.o(i.TP_AbnormalInReqFF_handle) for TP_AbnormalInReqFF_handle
    tp_layer.o(i.TP_Buffer_handle) refers to tp_layer.o(i.TP_UnknownlPDU_handle) for TP_UnknownlPDU_handle
    tp_layer.o(i.TP_Buffer_handle) refers to tp_layer.o(i.TP_AbnormalInResCF_handle) for TP_AbnormalInResCF_handle
    tp_layer.o(i.TP_Buffer_handle) refers to tp_layer.o(i.TP_AbnormalInReqFC_handle) for TP_AbnormalInReqFC_handle
    tp_layer.o(i.TP_Buffer_handle) refers to tp_layer.o(i.TP_AbnormalInResFC_handle) for TP_AbnormalInResFC_handle
    tp_layer.o(i.TP_Buffer_handle) refers to tp_layer.o(i.TP_TooShortDLC_handle) for TP_TooShortDLC_handle
    tp_layer.o(i.TP_Buffer_handle) refers to link_layer.o(.bss) for LinkDataBuf
    tp_layer.o(i.TP_NormalRecFC_handle) refers to tp_layer.o(i.TP_SetBsTimer) for TP_SetBsTimer
    tp_layer.o(i.TP_NormalRecFC_handle) refers to tp_layer.o(i.TP_SetSTminTimer) for TP_SetSTminTimer
    tp_layer.o(i.TP_NormalRecFC_handle) refers to link_layer.o(.bss) for LinkData
    tp_layer.o(i.TP_NormalRecFC_handle) refers to tp_layer.o(.bss) for N_US_S_Data_FF
    tp_layer.o(i.TP_NormalRecFC_handle) refers to app_service.o(.bss) for DiagClock
    tp_layer.o(i.TP_NormalSendFC_Fun) refers to tp_layer.o(i.TP_SetCrTimer) for TP_SetCrTimer
    tp_layer.o(i.TP_NormalSendFC_Fun) refers to tp_layer.o(i.TP_CrTimerOver) for TP_CrTimerOver
    tp_layer.o(i.TP_NormalSendFC_Fun) refers to tp_layer.o(.bss) for N_US_R_MultiData
    tp_layer.o(i.TP_NormalSendFC_Fun) refers to app_service.o(.bss) for DiagnoCtl
    tp_layer.o(i.TP_ReciveMultiF_handle) refers to app_serviceproc.o(i.App_CopyRam) for App_CopyRam
    tp_layer.o(i.TP_ReciveMultiF_handle) refers to tp_layer.o(i.TP_SetCrTimer) for TP_SetCrTimer
    tp_layer.o(i.TP_ReciveMultiF_handle) refers to tp_layer.o(i.TP_CalMsgLen) for TP_CalMsgLen
    tp_layer.o(i.TP_ReciveMultiF_handle) refers to link_layer.o(.bss) for LinkData
    tp_layer.o(i.TP_ReciveMultiF_handle) refers to tp_layer.o(.bss) for N_US_R_MultiData
    tp_layer.o(i.TP_ReciveMultiF_handle) refers to tp_layer.o(.data) for N_RecLen
    tp_layer.o(i.TP_ReciveMultiF_handle) refers to app_service.o(.bss) for DiagClock
    tp_layer.o(i.TP_ReciveSF_handle) refers to app_serviceproc.o(i.App_CopyRam) for App_CopyRam
    tp_layer.o(i.TP_ReciveSF_handle) refers to link_layer.o(.bss) for LinkData
    tp_layer.o(i.TP_ReciveSF_handle) refers to app_service.o(.bss) for Exct_USData
    tp_layer.o(i.TP_ReciveSF_handle) refers to tp_layer.o(.bss) for N_USSFData
    tp_layer.o(i.TP_TooShortDLC_handle) refers to aeabi_sdivfast.o(.text) for __aeabi_idivmod
    tp_layer.o(i.TP_TooShortDLC_handle) refers to tp_layer.o(.bss) for N_US_R_MultiData
    tp_layer.o(i.TP_TransmitNegatePDU) refers to can.o(i.bsp_CANSendFrame) for bsp_CANSendFrame
    tp_layer.o(i.TP_TransmitNegatePDU) refers to tp_layer.o(.bss) for N_US_R_Data_FF
    tp_layer.o(i.TP_TransmitNegatePDU) refers to can.o(.data) for g_bReturn
    tp_layer.o(i.TP_TransmitPDU) refers to app_serviceproc.o(i.App_CopyRam) for App_CopyRam
    tp_layer.o(i.TP_TransmitPDU) refers to link_layer.o(i.LK_FillMsg) for LK_FillMsg
    tp_layer.o(i.TP_TransmitPDU) refers to can.o(i.bsp_CANSendFrame) for bsp_CANSendFrame
    tp_layer.o(i.TP_TransmitPDU) refers to tp_layer.o(i.TP_SetBsTimer) for TP_SetBsTimer
    tp_layer.o(i.TP_TransmitPDU) refers to tp_layer.o(i.TP_STminTimerOver) for TP_STminTimerOver
    tp_layer.o(i.TP_TransmitPDU) refers to aeabi_sdivfast.o(.text) for __aeabi_idivmod
    tp_layer.o(i.TP_TransmitPDU) refers to tp_layer.o(i.TP_SetSTminTimer) for TP_SetSTminTimer
    tp_layer.o(i.TP_TransmitPDU) refers to tp_layer.o(i.TP_TransmitNegatePDU) for TP_TransmitNegatePDU
    tp_layer.o(i.TP_TransmitPDU) refers to tp_layer.o(.bss) for g_txCanMsg
    tp_layer.o(i.TP_TransmitPDU) refers to can.o(.data) for g_bReturn
    tp_layer.o(i.TP_TransmitPDU) refers to app_service.o(.bss) for DiagClock
    tp_layer.o(i.TP_TransmitPDU) refers to app_service.o(.data) for Error
    tp_layer.o(i.TP_UnknownlPDU_handle) refers to link_layer.o(.bss) for LinkData
    tp_layer.o(i.TP_UnknownlPDU_handle) refers to tp_layer.o(.bss) for N_US_S_MultiData
    u2_app_service.o(i.Get_UDS_01_MsgRecFlg) refers to u2_app_service.o(.data) for UDS_01_MsgRecFlg
    u2_app_service.o(i.Get_UDS_59_MsgRecFlg) refers to u2_app_service.o(.data) for UDS_59_MsgRecFlg
    u2_app_service.o(i.Get_UDS_62_MsgRecFlg) refers to u2_app_service.o(.data) for UDS_62_MsgRecFlg
    u2_app_service.o(i.Set_UDS_01_MsgRecFlg) refers to u2_app_service.o(.data) for UDS_01_MsgRecFlg
    u2_app_service.o(i.Set_UDS_59_MsgRecFlg) refers to u2_app_service.o(.data) for UDS_59_MsgRecFlg
    u2_app_service.o(i.Set_UDS_62_MsgRecFlg) refers to u2_app_service.o(.data) for UDS_62_MsgRecFlg
    u2_app_service.o(i.U2_App_01_service) refers to can_user.o(i.Reset_Mil_Signal_Time) for Reset_Mil_Signal_Time
    u2_app_service.o(i.U2_App_01_service) refers to can_user.o(i.SetSendUdsTimeCount_0101) for SetSendUdsTimeCount_0101
    u2_app_service.o(i.U2_App_01_service) refers to can_user.o(i.DelfuModuleIn) for DelfuModuleIn
    u2_app_service.o(i.U2_App_01_service) refers to u2_app_service.o(.bss) for U2_DiagReciveGaugePara
    u2_app_service.o(i.U2_App_01_service) refers to u2_app_service.o(.data) for UDS_01_MsgRecFlg
    u2_app_service.o(i.U2_App_59_service) refers to u2_app_serviceproc.o(i.U2_App_ErrorInfoInit) for U2_App_ErrorInfoInit
    u2_app_service.o(i.U2_App_59_service) refers to u2_app_serviceproc.o(i.U2_App_Load_DID) for U2_App_Load_DID
    u2_app_service.o(i.U2_App_59_service) refers to rt_memclr.o(.text) for __aeabi_memclr4
    u2_app_service.o(i.U2_App_59_service) refers to u2_app_serviceproc.o(i.U2_App_CopyRam) for U2_App_CopyRam
    u2_app_service.o(i.U2_App_59_service) refers to u2_app_service.o(i.U2_App_SetDtcMsgTimer) for U2_App_SetDtcMsgTimer
    u2_app_service.o(i.U2_App_59_service) refers to can_user.o(i.SetSendUdsTimeCount_190209) for SetSendUdsTimeCount_190209
    u2_app_service.o(i.U2_App_59_service) refers to u2_app_service.o(.bss) for U2_DiagReciveDTC
    u2_app_service.o(i.U2_App_59_service) refers to u2_app_service.o(.data) for UDS_59_MsgRecFlg
    u2_app_service.o(i.U2_App_62_service) refers to u2_app_serviceproc.o(i.U2_App_ErrorInfoInit) for U2_App_ErrorInfoInit
    u2_app_service.o(i.U2_App_62_service) refers to u2_app_serviceproc.o(i.U2_App_Load_DID) for U2_App_Load_DID
    u2_app_service.o(i.U2_App_62_service) refers to u2_app_serviceproc.o(i.U2_App_CopyRam) for U2_App_CopyRam
    u2_app_service.o(i.U2_App_62_service) refers to can_user.o(i.SetSendUdsTimeCount_220005) for SetSendUdsTimeCount_220005
    u2_app_service.o(i.U2_App_62_service) refers to u2_app_service.o(.bss) for U2_DiagReciveGaugePara
    u2_app_service.o(i.U2_App_62_service) refers to u2_app_service.o(.data) for UDS_62_MsgRecFlg
    u2_app_service.o(i.U2_DiagnosisInit_main) refers to u2_tp_layer.o(i.U2_TP_SetSTminTimer) for U2_TP_SetSTminTimer
    u2_app_service.o(i.U2_DiagnosisInit_main) refers to u2_tp_layer.o(.bss) for U2_N_US_R_MultiData
    u2_app_service.o(i.U2_DiagnosisInit_main) refers to u2_app_service.o(.bss) for U2_Exct_USData
    u2_app_service.o(i.U2_DiagnosisInit_main) refers to u2_link_layer.o(.bss) for U2_LinkDataBuf
    u2_app_service.o(i.U2_DiagnosisInit_main) refers to u2_app_service.o(.data) for U2_Error
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_tp_layer.o(i.U2_TP_Buffer_handle) for U2_TP_Buffer_handle
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_tp_layer.o(i.U2_TP_ReciveSF_handle) for U2_TP_ReciveSF_handle
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_tp_layer.o(i.U2_TP_ReciveMultiF_handle) for U2_TP_ReciveMultiF_handle
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_tp_layer.o(i.U2_TP_NormalRecFC_handle) for U2_TP_NormalRecFC_handle
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_tp_layer.o(i.U2_TP_NormalSendFC_Fun) for U2_TP_NormalSendFC_Fun
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_app_serviceproc.o(i.U2_App_CopyRam) for U2_App_CopyRam
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_tp_layer.o(i.U2_TP_BsTimerOver) for U2_TP_BsTimerOver
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_app_service.o(i.U2_App_SessionTimerOver) for U2_App_SessionTimerOver
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_app_service.o(i.U2_App_ReUnlockTimerOver) for U2_App_ReUnlockTimerOver
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_app_service.o(i.U2_App_DtcMsgTimerOver) for U2_App_DtcMsgTimerOver
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_app_service.o(i.U2_App_59_service) for U2_App_59_service
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_app_service.o(i.U2_App_62_service) for U2_App_62_service
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_app_service.o(i.U2_App_01_service) for U2_App_01_service
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_tp_layer.o(i.U2_TP_TransmitPDU) for U2_TP_TransmitPDU
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_app_serviceproc.o(i.U2_App_11_Reset_handle) for U2_App_11_Reset_handle
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_link_layer.o(.bss) for U2_LinkData
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_tp_layer.o(.bss) for U2_N_USSFData
    u2_app_service.o(i.U2_Diagnosis_main) refers to u2_app_service.o(.bss) for U2_Exct_USData
    u2_app_serviceproc.o(i.U2_App_ErrorInfoInit) refers to u2_app_service.o(.data) for U2_Error
    u2_app_serviceproc.o(i.U2_Diagno_Tick) refers to u2_app_service.o(.bss) for U2_DiagClock
    u2_link_layer.o(i.U2_LK_Link_main) refers to rt_memcpy.o(.text) for __aeabi_memcpy
    u2_link_layer.o(i.U2_LK_Link_main) refers to can_user.o(i.Get_ReqSilentTimer) for Get_ReqSilentTimer
    u2_link_layer.o(i.U2_LK_Link_main) refers to can_user.o(i.Set_ReqSilentTimer) for Set_ReqSilentTimer
    u2_link_layer.o(i.U2_LK_Link_main) refers to u2_link_layer.o(.bss) for U2_LinkDataBuf
    u2_tp_layer.o(i.U2_TP_AbnormalInReqFC_handle) refers to u2_tp_layer.o(.bss) for U2_N_US_R_MultiData
    u2_tp_layer.o(i.U2_TP_AbnormalInReqFC_handle) refers to u2_link_layer.o(.bss) for U2_LinkData
    u2_tp_layer.o(i.U2_TP_AbnormalInReqFF_handle) refers to u2_link_layer.o(.bss) for U2_LinkData
    u2_tp_layer.o(i.U2_TP_AbnormalInReqFF_handle) refers to u2_tp_layer.o(.bss) for U2_N_US_R_MultiData
    u2_tp_layer.o(i.U2_TP_AbnormalInResCF_handle) refers to u2_tp_layer.o(.bss) for U2_N_US_S_MultiData
    u2_tp_layer.o(i.U2_TP_AbnormalInResCF_handle) refers to u2_link_layer.o(.bss) for U2_LinkData
    u2_tp_layer.o(i.U2_TP_AbnormalInResFC_handle) refers to u2_tp_layer.o(.bss) for U2_N_US_S_Data_FF
    u2_tp_layer.o(i.U2_TP_AbnormalInResFC_handle) refers to u2_link_layer.o(.bss) for U2_LinkData
    u2_tp_layer.o(i.U2_TP_AbnormalInResSF_handle) refers to u2_tp_layer.o(.bss) for U2_N_US_S_MultiData
    u2_tp_layer.o(i.U2_TP_AbnormalInResSF_handle) refers to u2_link_layer.o(.bss) for U2_LinkData
    u2_tp_layer.o(i.U2_TP_Buffer_handle) refers to rt_memcpy.o(.text) for __aeabi_memcpy
    u2_tp_layer.o(i.U2_TP_Buffer_handle) refers to u2_tp_layer.o(i.U2_TP_AbnormalInResSF_handle) for U2_TP_AbnormalInResSF_handle
    u2_tp_layer.o(i.U2_TP_Buffer_handle) refers to u2_tp_layer.o(i.U2_TP_AbnormalInReqFF_handle) for U2_TP_AbnormalInReqFF_handle
    u2_tp_layer.o(i.U2_TP_Buffer_handle) refers to u2_tp_layer.o(i.U2_TP_UnknownlPDU_handle) for U2_TP_UnknownlPDU_handle
    u2_tp_layer.o(i.U2_TP_Buffer_handle) refers to u2_tp_layer.o(i.U2_TP_AbnormalInResCF_handle) for U2_TP_AbnormalInResCF_handle
    u2_tp_layer.o(i.U2_TP_Buffer_handle) refers to u2_tp_layer.o(i.U2_TP_AbnormalInReqFC_handle) for U2_TP_AbnormalInReqFC_handle
    u2_tp_layer.o(i.U2_TP_Buffer_handle) refers to u2_tp_layer.o(i.U2_TP_AbnormalInResFC_handle) for U2_TP_AbnormalInResFC_handle
    u2_tp_layer.o(i.U2_TP_Buffer_handle) refers to u2_tp_layer.o(i.U2_TP_TooShortDLC_handle) for U2_TP_TooShortDLC_handle
    u2_tp_layer.o(i.U2_TP_Buffer_handle) refers to u2_link_layer.o(.bss) for U2_LinkDataBuf
    u2_tp_layer.o(i.U2_TP_NormalRecFC_handle) refers to u2_tp_layer.o(i.U2_TP_SetBsTimer) for U2_TP_SetBsTimer
    u2_tp_layer.o(i.U2_TP_NormalRecFC_handle) refers to u2_tp_layer.o(i.U2_TP_SetSTminTimer) for U2_TP_SetSTminTimer
    u2_tp_layer.o(i.U2_TP_NormalRecFC_handle) refers to u2_link_layer.o(.bss) for U2_LinkData
    u2_tp_layer.o(i.U2_TP_NormalRecFC_handle) refers to u2_tp_layer.o(.bss) for U2_N_US_S_Data_FF
    u2_tp_layer.o(i.U2_TP_NormalRecFC_handle) refers to u2_app_service.o(.bss) for U2_DiagClock
    u2_tp_layer.o(i.U2_TP_NormalSendFC_Fun) refers to u2_tp_layer.o(i.U2_TP_SetCrTimer) for U2_TP_SetCrTimer
    u2_tp_layer.o(i.U2_TP_NormalSendFC_Fun) refers to u2_tp_layer.o(i.U2_TP_CrTimerOver) for U2_TP_CrTimerOver
    u2_tp_layer.o(i.U2_TP_NormalSendFC_Fun) refers to u2_tp_layer.o(.bss) for U2_N_US_R_MultiData
    u2_tp_layer.o(i.U2_TP_NormalSendFC_Fun) refers to u2_app_service.o(.bss) for U2_DiagnoCtl
    u2_tp_layer.o(i.U2_TP_ReciveMultiF_handle) refers to u2_app_serviceproc.o(i.U2_App_CopyRam) for U2_App_CopyRam
    u2_tp_layer.o(i.U2_TP_ReciveMultiF_handle) refers to u2_tp_layer.o(i.U2_TP_SetCrTimer) for U2_TP_SetCrTimer
    u2_tp_layer.o(i.U2_TP_ReciveMultiF_handle) refers to u2_tp_layer.o(i.U2_TP_CalMsgLen) for U2_TP_CalMsgLen
    u2_tp_layer.o(i.U2_TP_ReciveMultiF_handle) refers to u2_link_layer.o(.bss) for U2_LinkData
    u2_tp_layer.o(i.U2_TP_ReciveMultiF_handle) refers to u2_tp_layer.o(.bss) for U2_N_US_R_MultiData
    u2_tp_layer.o(i.U2_TP_ReciveMultiF_handle) refers to u2_tp_layer.o(.data) for U2_N_RecLen
    u2_tp_layer.o(i.U2_TP_ReciveMultiF_handle) refers to u2_app_service.o(.bss) for U2_DiagClock
    u2_tp_layer.o(i.U2_TP_ReciveSF_handle) refers to u2_app_serviceproc.o(i.U2_App_CopyRam) for U2_App_CopyRam
    u2_tp_layer.o(i.U2_TP_ReciveSF_handle) refers to u2_link_layer.o(.bss) for U2_LinkData
    u2_tp_layer.o(i.U2_TP_ReciveSF_handle) refers to u2_app_service.o(.bss) for U2_Exct_USData
    u2_tp_layer.o(i.U2_TP_ReciveSF_handle) refers to u2_tp_layer.o(.bss) for U2_N_USSFData
    u2_tp_layer.o(i.U2_TP_TooShortDLC_handle) refers to aeabi_sdivfast.o(.text) for __aeabi_idivmod
    u2_tp_layer.o(i.U2_TP_TooShortDLC_handle) refers to u2_tp_layer.o(.bss) for U2_N_US_R_MultiData
    u2_tp_layer.o(i.U2_TP_TransmitNegatePDU) refers to can.o(i.bsp_CANSendFrame) for bsp_CANSendFrame
    u2_tp_layer.o(i.U2_TP_TransmitNegatePDU) refers to u2_tp_layer.o(.bss) for U2_N_US_R_Data_FF
    u2_tp_layer.o(i.U2_TP_TransmitNegatePDU) refers to can.o(.data) for g_bReturn
    u2_tp_layer.o(i.U2_TP_TransmitPDU) refers to u2_app_serviceproc.o(i.U2_App_CopyRam) for U2_App_CopyRam
    u2_tp_layer.o(i.U2_TP_TransmitPDU) refers to u2_link_layer.o(i.U2_LK_FillMsg) for U2_LK_FillMsg
    u2_tp_layer.o(i.U2_TP_TransmitPDU) refers to can.o(i.bsp_CANSendFrame) for bsp_CANSendFrame
    u2_tp_layer.o(i.U2_TP_TransmitPDU) refers to u2_tp_layer.o(i.U2_TP_SetBsTimer) for U2_TP_SetBsTimer
    u2_tp_layer.o(i.U2_TP_TransmitPDU) refers to u2_tp_layer.o(i.U2_TP_STminTimerOver) for U2_TP_STminTimerOver
    u2_tp_layer.o(i.U2_TP_TransmitPDU) refers to aeabi_sdivfast.o(.text) for __aeabi_idivmod
    u2_tp_layer.o(i.U2_TP_TransmitPDU) refers to u2_tp_layer.o(i.U2_TP_SetSTminTimer) for U2_TP_SetSTminTimer
    u2_tp_layer.o(i.U2_TP_TransmitPDU) refers to u2_tp_layer.o(i.U2_TP_TransmitNegatePDU) for U2_TP_TransmitNegatePDU
    u2_tp_layer.o(i.U2_TP_TransmitPDU) refers to u2_tp_layer.o(.bss) for U2_g_txCanMsg
    u2_tp_layer.o(i.U2_TP_TransmitPDU) refers to can.o(.data) for g_bReturn
    u2_tp_layer.o(i.U2_TP_TransmitPDU) refers to u2_app_service.o(.bss) for U2_DiagClock
    u2_tp_layer.o(i.U2_TP_TransmitPDU) refers to u2_app_service.o(.data) for U2_Error
    u2_tp_layer.o(i.U2_TP_UnknownlPDU_handle) refers to u2_link_layer.o(.bss) for U2_LinkData
    u2_tp_layer.o(i.U2_TP_UnknownlPDU_handle) refers to u2_tp_layer.o(.bss) for U2_N_US_S_MultiData
    isr_bat32a239.o(i.CAN0Rec_Interrupt) refers to can.o(i.bsp_CAN0_Rev_isr) for bsp_CAN0_Rev_isr
    isr_bat32a239.o(i.CAN0Trx_Interrupt) refers to can.o(i.bsp_CAN0_Tx_isr) for bsp_CAN0_Tx_isr
    isr_bat32a239.o(i.IRQ00_Handler) refers to isr_bat32a239.o(i.lvi_interrupt) for lvi_interrupt
    isr_bat32a239.o(i.IRQ00_Handler) refers to isr_bat32a239.o(i.osdc_interrupt) for osdc_interrupt
    isr_bat32a239.o(i.IRQ00_Handler) refers to isr_bat32a239.o(i.ocrv_interrupt) for ocrv_interrupt
    isr_bat32a239.o(i.IRQ01_Handler) refers to intp_user.o(i.intp0_interrupt) for intp0_interrupt
    isr_bat32a239.o(i.IRQ01_Handler) refers to intp_user.o(i.intp6_interrupt) for intp6_interrupt
    isr_bat32a239.o(i.IRQ02_Handler) refers to intp_user.o(i.intp1_interrupt) for intp1_interrupt
    isr_bat32a239.o(i.IRQ02_Handler) refers to intp_user.o(i.intp7_interrupt) for intp7_interrupt
    isr_bat32a239.o(i.IRQ03_Handler) refers to intp_user.o(i.intp2_interrupt) for intp2_interrupt
    isr_bat32a239.o(i.IRQ03_Handler) refers to intp_user.o(i.intp8_interrupt) for intp8_interrupt
    isr_bat32a239.o(i.IRQ04_Handler) refers to intp_user.o(i.intp3_interrupt) for intp3_interrupt
    isr_bat32a239.o(i.IRQ04_Handler) refers to intp_user.o(i.intp9_interrupt) for intp9_interrupt
    isr_bat32a239.o(i.IRQ05_Handler) refers to intp_user.o(i.intp4_interrupt) for intp4_interrupt
    isr_bat32a239.o(i.IRQ05_Handler) refers to intp_user.o(i.intp10_interrupt) for intp10_interrupt
    isr_bat32a239.o(i.IRQ06_Handler) refers to intp_user.o(i.intp5_interrupt) for intp5_interrupt
    isr_bat32a239.o(i.IRQ06_Handler) refers to intp_user.o(i.intp11_interrupt) for intp11_interrupt
    isr_bat32a239.o(i.IRQ07_Handler) refers to sci_user.o(i.iic20_interrupt) for iic20_interrupt
    isr_bat32a239.o(i.IRQ07_Handler) refers to sci_user.o(i.uart3_interrupt_send) for uart3_interrupt_send
    isr_bat32a239.o(i.IRQ08_Handler) refers to sci_user.o(i.iic21_interrupt) for iic21_interrupt
    isr_bat32a239.o(i.IRQ08_Handler) refers to sci_user.o(i.uart3_interrupt_receive) for uart3_interrupt_receive
    isr_bat32a239.o(i.IRQ09_Handler) refers to isr_bat32a239.o(i.sre2_interrupt) for sre2_interrupt
    isr_bat32a239.o(i.IRQ09_Handler) refers to isr_bat32a239.o(i.CAN0Err_Interrupt) for CAN0Err_Interrupt
    isr_bat32a239.o(i.IRQ10_Handler) refers to sci_user.o(i.uart0_interrupt_send) for uart0_interrupt_send
    isr_bat32a239.o(i.IRQ11_Handler) refers to sci_user.o(i.uart0_interrupt_receive) for uart0_interrupt_receive
    isr_bat32a239.o(i.IRQ12_Handler) refers to isr_bat32a239.o(i.sre0_interrupt) for sre0_interrupt
    isr_bat32a239.o(i.IRQ12_Handler) refers to isr_bat32a239.o(i.tm01h_interrupt) for tm01h_interrupt
    isr_bat32a239.o(i.IRQ13_Handler) refers to sci_user.o(i.uart1_interrupt_send) for uart1_interrupt_send
    isr_bat32a239.o(i.IRQ14_Handler) refers to sci_user.o(i.uart1_interrupt_receive) for uart1_interrupt_receive
    isr_bat32a239.o(i.IRQ15_Handler) refers to isr_bat32a239.o(i.sre1_interrupt) for sre1_interrupt
    isr_bat32a239.o(i.IRQ15_Handler) refers to isr_bat32a239.o(i.tm03h_interrupt) for tm03h_interrupt
    isr_bat32a239.o(i.IRQ16_Handler) refers to isr_bat32a239.o(i.iica0_interrupt) for iica0_interrupt
    isr_bat32a239.o(i.IRQ16_Handler) refers to isr_bat32a239.o(i.div_interrupt) for div_interrupt
    isr_bat32a239.o(i.IRQ16_Handler) refers to isr_bat32a239.o(i.iica1_interrupt) for iica1_interrupt
    isr_bat32a239.o(i.IRQ17_Handler) refers to isr_bat32a239.o(i.tm40_channel0_interrupt) for tm40_channel0_interrupt
    isr_bat32a239.o(i.IRQ17_Handler) refers to isr_bat32a239.o(i.tm81_channel10_interrupt) for tm81_channel10_interrupt
    isr_bat32a239.o(i.IRQ17_Handler) refers to isr_bat32a239.o(i.tm81_channel14_interrupt) for tm81_channel14_interrupt
    isr_bat32a239.o(i.IRQ18_Handler) refers to isr_bat32a239.o(i.tm40_channel1_interrupt) for tm40_channel1_interrupt
    isr_bat32a239.o(i.IRQ18_Handler) refers to isr_bat32a239.o(i.tm81_channel11_interrupt) for tm81_channel11_interrupt
    isr_bat32a239.o(i.IRQ18_Handler) refers to isr_bat32a239.o(i.tm81_channel15_interrupt) for tm81_channel15_interrupt
    isr_bat32a239.o(i.IRQ19_Handler) refers to isr_bat32a239.o(i.tm40_channel2_interrupt) for tm40_channel2_interrupt
    isr_bat32a239.o(i.IRQ19_Handler) refers to isr_bat32a239.o(i.tm81_channel12_interrupt) for tm81_channel12_interrupt
    isr_bat32a239.o(i.IRQ19_Handler) refers to isr_bat32a239.o(i.tm81_channel16_interrupt) for tm81_channel16_interrupt
    isr_bat32a239.o(i.IRQ20_Handler) refers to isr_bat32a239.o(i.tm40_channel3_interrupt) for tm40_channel3_interrupt
    isr_bat32a239.o(i.IRQ20_Handler) refers to isr_bat32a239.o(i.tm81_channel13_interrupt) for tm81_channel13_interrupt
    isr_bat32a239.o(i.IRQ20_Handler) refers to isr_bat32a239.o(i.tm81_channel17_interrupt) for tm81_channel17_interrupt
    isr_bat32a239.o(i.IRQ21_Handler) refers to isr_bat32a239.o(i.adc_interrupt) for adc_interrupt
    isr_bat32a239.o(i.IRQ22_Handler) refers to isr_bat32a239.o(i.rtc_interrupt) for rtc_interrupt
    isr_bat32a239.o(i.IRQ22_Handler) refers to isr_bat32a239.o(i.it_interrupt) for it_interrupt
    isr_bat32a239.o(i.IRQ23_Handler) refers to isr_bat32a239.o(i.key_interrupt) for key_interrupt
    isr_bat32a239.o(i.IRQ23_Handler) refers to isr_bat32a239.o(i.CAN0Rec_Interrupt) for CAN0Rec_Interrupt
    isr_bat32a239.o(i.IRQ24_Handler) refers to isr_bat32a239.o(i.cmp0_interrupt) for cmp0_interrupt
    isr_bat32a239.o(i.IRQ24_Handler) refers to isr_bat32a239.o(i.CAN0Wup_Interrupt) for CAN0Wup_Interrupt
    isr_bat32a239.o(i.IRQ25_Handler) refers to isr_bat32a239.o(i.cmp1_interrupt) for cmp1_interrupt
    isr_bat32a239.o(i.IRQ25_Handler) refers to isr_bat32a239.o(i.CAN0Trx_Interrupt) for CAN0Trx_Interrupt
    isr_bat32a239.o(i.IRQ26_Handler) refers to isr_bat32a239.o(i.tma0_interrupt) for tma0_interrupt
    isr_bat32a239.o(i.IRQ26_Handler) refers to isr_bat32a239.o(i.CAN1Err_Interrupt) for CAN1Err_Interrupt
    isr_bat32a239.o(i.IRQ27_Handler) refers to isr_bat32a239.o(i.tmm0_interrupt) for tmm0_interrupt
    isr_bat32a239.o(i.IRQ28_Handler) refers to isr_bat32a239.o(i.tmm1_interrupt) for tmm1_interrupt
    isr_bat32a239.o(i.IRQ29_Handler) refers to isr_bat32a239.o(i.tmb0_interrupt) for tmb0_interrupt
    isr_bat32a239.o(i.IRQ29_Handler) refers to isr_bat32a239.o(i.CAN1Rec_Interrupt) for CAN1Rec_Interrupt
    isr_bat32a239.o(i.IRQ30_Handler) refers to isr_bat32a239.o(i.tmc_interrupt) for tmc_interrupt
    isr_bat32a239.o(i.IRQ30_Handler) refers to isr_bat32a239.o(i.CAN1Wup_Interrupt) for CAN1Wup_Interrupt
    isr_bat32a239.o(i.IRQ31_Handler) refers to isr_bat32a239.o(i.flash_interrupt) for flash_interrupt
    isr_bat32a239.o(i.IRQ31_Handler) refers to isr_bat32a239.o(i.CAN1Trx_Interrupt) for CAN1Trx_Interrupt
    isr_bat32a239.o(i.tm40_channel1_interrupt) refers to tim4.o(i.bsp_tim4_01_isr_Handler) for bsp_tim4_01_isr_Handler
    isr_bat32a239.o(i.tm40_channel2_interrupt) refers to tim4.o(i.bsp_tim4_02_isr_Handler) for bsp_tim4_02_isr_Handler
    startup_bat32a239.o(STACK) refers (Special) to heapauxi.o(.text) for __use_two_region_memory
    startup_bat32a239.o(HEAP) refers (Special) to heapauxi.o(.text) for __use_two_region_memory
    startup_bat32a239.o(RESET) refers (Special) to heapauxi.o(.text) for __use_two_region_memory
    startup_bat32a239.o(RESET) refers to startup_bat32a239.o(STACK) for __initial_sp
    startup_bat32a239.o(RESET) refers to startup_bat32a239.o(.text) for Reset_Handler
    startup_bat32a239.o(RESET) refers to sys_tick.o(i.SysTick_Handler) for SysTick_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ00_Handler) for IRQ00_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ01_Handler) for IRQ01_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ02_Handler) for IRQ02_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ03_Handler) for IRQ03_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ04_Handler) for IRQ04_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ05_Handler) for IRQ05_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ06_Handler) for IRQ06_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ07_Handler) for IRQ07_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ08_Handler) for IRQ08_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ09_Handler) for IRQ09_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ10_Handler) for IRQ10_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ11_Handler) for IRQ11_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ12_Handler) for IRQ12_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ13_Handler) for IRQ13_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ14_Handler) for IRQ14_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ15_Handler) for IRQ15_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ16_Handler) for IRQ16_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ17_Handler) for IRQ17_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ18_Handler) for IRQ18_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ19_Handler) for IRQ19_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ20_Handler) for IRQ20_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ21_Handler) for IRQ21_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ22_Handler) for IRQ22_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ23_Handler) for IRQ23_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ24_Handler) for IRQ24_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ25_Handler) for IRQ25_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ26_Handler) for IRQ26_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ27_Handler) for IRQ27_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ28_Handler) for IRQ28_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ29_Handler) for IRQ29_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ30_Handler) for IRQ30_Handler
    startup_bat32a239.o(RESET) refers to isr_bat32a239.o(i.IRQ31_Handler) for IRQ31_Handler
    startup_bat32a239.o(.text) refers (Special) to heapauxi.o(.text) for __use_two_region_memory
    startup_bat32a239.o(.text) refers to system_bat32a239.o(i.SystemInit) for SystemInit
    startup_bat32a239.o(.text) refers to __main.o(!!!main) for __main
    startup_bat32a239.o(.text) refers to startup_bat32a239.o(HEAP) for Heap_Mem
    startup_bat32a239.o(.text) refers to startup_bat32a239.o(STACK) for Stack_Mem
    system_bat32a239.o(i.CLK_GetCoreFreq) refers to system_bat32a239.o(i.CLK_GetfIHFreq) for CLK_GetfIHFreq
    system_bat32a239.o(i.CLK_GetCoreFreq) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    system_bat32a239.o(i.CLK_GetfIHFreq) refers to gpio.o(i.__ARM_common_switch8) for __ARM_common_switch8
    system_bat32a239.o(i.SystemCoreClockUpdate) refers to system_bat32a239.o(i.CLK_GetCoreFreq) for CLK_GetCoreFreq
    system_bat32a239.o(i.SystemCoreClockUpdate) refers to system_bat32a239.o(.data) for SystemCoreClock
    system_bat32a239.o(i.SystemInit) refers to system_bat32a239.o(i.CLK_GetCoreFreq) for CLK_GetCoreFreq
    system_bat32a239.o(i.SystemInit) refers to system_bat32a239.o(.data) for SystemCoreClock
    eeprommanage.o(.ARM.exidx.text.eeprom_getVersion) refers to eeprommanage.o(.text.eeprom_getVersion) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_1ms_timeCount) refers to eeprommanage.o(.bss.tWR_count) for [Anonymous Symbol]
    eeprommanage.o(.ARM.exidx.text.eeprom_1ms_timeCount) refers to eeprommanage.o(.text.eeprom_1ms_timeCount) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_SetParameter) refers to eeprommanage.o(.bss.MemoryConfig.1) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_SetParameter) refers to eeprommanage.o(.bss.MemoryConfig.0) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_SetParameter) refers to eeprommanage.o(.bss.MemoryConfig.2) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_SetParameter) refers to eeprommanage.o(.bss.memoryOdo) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_SetParameter) refers to eeprommanage.o(.bss.MemoryConfig.3) for [Anonymous Symbol]
    eeprommanage.o(.ARM.exidx.text.eeprom_SetParameter) refers to eeprommanage.o(.text.eeprom_SetParameter) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_getOdoLastWriteValue) refers to eeprommanage.o(.bss.memoryOdo) for [Anonymous Symbol]
    eeprommanage.o(.ARM.exidx.text.eeprom_getOdoLastWriteValue) refers to eeprommanage.o(.text.eeprom_getOdoLastWriteValue) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_getOdoCurWriteAddress) refers to eeprommanage.o(.bss.OdoValidAddress) for OdoValidAddress
    eeprommanage.o(.ARM.exidx.text.eeprom_getOdoCurWriteAddress) refers to eeprommanage.o(.text.eeprom_getOdoCurWriteAddress) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_getWriteState) refers to eeprommanage.o(.bss.writeState) for [Anonymous Symbol]
    eeprommanage.o(.ARM.exidx.text.eeprom_getWriteState) refers to eeprommanage.o(.text.eeprom_getWriteState) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_getReadState) refers to eeprommanage.o(.bss.readState) for [Anonymous Symbol]
    eeprommanage.o(.ARM.exidx.text.eeprom_getReadState) refers to eeprommanage.o(.text.eeprom_getReadState) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_ReadRecord) refers to eeprommanage.o(.text.ee_IIC_SequentialRead) for ee_IIC_SequentialRead
    eeprommanage.o(.text.eeprom_ReadRecord) refers to eeprommanage.o(.bss.readState) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_ReadRecord) refers to eeprommanage.o(.bss.MemoryConfig.0) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_ReadRecord) refers to eeprommanage.o(.bss.readDebugState) for [Anonymous Symbol]
    eeprommanage.o(.ARM.exidx.text.eeprom_ReadRecord) refers to eeprommanage.o(.text.eeprom_ReadRecord) for [Anonymous Symbol]
    eeprommanage.o(.text.ee_IIC_SequentialRead) refers to eeprommanage.o(.text.ee_IIC_Stop) for ee_IIC_Stop
    eeprommanage.o(.text.ee_IIC_SequentialRead) refers to eeprommanage.o(.text.ee_IIC_Start) for ee_IIC_Start
    eeprommanage.o(.text.ee_IIC_SequentialRead) refers to eeprommanage.o(.text.ee_IIC_SendByte) for ee_IIC_SendByte
    eeprommanage.o(.text.ee_IIC_SequentialRead) refers to eeprommanage.o(.text.ee_IIC_WaitAck) for ee_IIC_WaitAck
    eeprommanage.o(.text.ee_IIC_SequentialRead) refers to eeprommanage.o(.text.ee_IIC_Read_8bit) for ee_IIC_Read_8bit
    eeprommanage.o(.text.ee_IIC_SequentialRead) refers to eeprommanage.o(.text.ee_IIC_ACK) for ee_IIC_ACK
    eeprommanage.o(.text.ee_IIC_SequentialRead) refers to eeprommanage.o(.text.ee_IIC_NACK) for ee_IIC_NACK
    eeprommanage.o(.ARM.exidx.text.ee_IIC_SequentialRead) refers to eeprommanage.o(.text.ee_IIC_SequentialRead) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteRecord) refers to eemanager_interface.o(i.EE_FeedDog) for EE_FeedDog
    eeprommanage.o(.text.eeprom_WriteRecord) refers to eeprommanage.o(.text.ee_IIC_SequentialWrite) for ee_IIC_SequentialWrite
    eeprommanage.o(.text.eeprom_WriteRecord) refers to eeprommanage.o(.bss.writeState) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteRecord) refers to eeprommanage.o(.bss.MemoryConfig.3) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteRecord) refers to eeprommanage.o(.bss.writeDebugState) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteRecord) refers to eeprommanage.o(.bss.writeWaitTime) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteRecord) refers to eeprommanage.o(.bss.tWR_count) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteRecord) refers to eeprommanage.o(.bss.write_pos) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteRecord) refers to eeprommanage.o(.bss.MemoryConfig.0) for [Anonymous Symbol]
    eeprommanage.o(.ARM.exidx.text.eeprom_WriteRecord) refers to eeprommanage.o(.text.eeprom_WriteRecord) for [Anonymous Symbol]
    eeprommanage.o(.text.ee_IIC_SequentialWrite) refers to eeprommanage.o(.text.ee_IIC_Stop) for ee_IIC_Stop
    eeprommanage.o(.text.ee_IIC_SequentialWrite) refers to eeprommanage.o(.text.ee_IIC_Start) for ee_IIC_Start
    eeprommanage.o(.text.ee_IIC_SequentialWrite) refers to eeprommanage.o(.text.ee_IIC_SendByte) for ee_IIC_SendByte
    eeprommanage.o(.text.ee_IIC_SequentialWrite) refers to eeprommanage.o(.text.ee_IIC_WaitAck) for ee_IIC_WaitAck
    eeprommanage.o(.ARM.exidx.text.ee_IIC_SequentialWrite) refers to eeprommanage.o(.text.ee_IIC_SequentialWrite) for [Anonymous Symbol]
    eeprommanage.o(.ARM.exidx.text.eeprom_CreateCRC_8_Num) refers to eeprommanage.o(.text.eeprom_CreateCRC_8_Num) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_OdoDecryption) refers to eeprommanage.o(.text.eeprom_CreateCRC_8_Num) for eeprom_CreateCRC_8_Num
    eeprommanage.o(.ARM.exidx.text.eeprom_OdoDecryption) refers to eeprommanage.o(.text.eeprom_OdoDecryption) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_OdoEncryption) refers to eeprommanage.o(.text.eeprom_CreateCRC_8_Num) for eeprom_CreateCRC_8_Num
    eeprommanage.o(.ARM.exidx.text.eeprom_OdoEncryption) refers to eeprommanage.o(.text.eeprom_OdoEncryption) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteODO) refers to eemanager_interface.o(i.EE_FeedDog) for EE_FeedDog
    eeprommanage.o(.text.eeprom_WriteODO) refers to eeprommanage.o(.text.eeprom_ReadODO) for eeprom_ReadODO
    eeprommanage.o(.text.eeprom_WriteODO) refers to eeprommanage.o(.text.eeprom_OdoEncryption) for eeprom_OdoEncryption
    eeprommanage.o(.text.eeprom_WriteODO) refers to eeprommanage.o(.text.ee_IIC_SequentialWrite) for ee_IIC_SequentialWrite
    eeprommanage.o(.text.eeprom_WriteODO) refers to aeabi_sdivfast.o(.text) for __aeabi_uidivmod
    eeprommanage.o(.text.eeprom_WriteODO) refers to eeprommanage.o(.bss.writeState) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteODO) refers to eeprommanage.o(.bss.MemoryConfig.2) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteODO) refers to eeprommanage.o(.bss.writeDebugState) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteODO) refers to eeprommanage.o(.bss.IsReadOdoState) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteODO) refers to eeprommanage.o(.bss.writeWaitTime) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteODO) refers to eeprommanage.o(.bss.tWR_count) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteODO) refers to eeprommanage.o(.bss.OdoValidAddress) for OdoValidAddress
    eeprommanage.o(.text.eeprom_WriteODO) refers to eeprommanage.o(.bss.memIgnState) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteODO) refers to eeprommanage.o(.bss.MemoryConfig.1) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteODO) refers to eeprommanage.o(.bss.memoryOdo) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_WriteODO) refers to eeprommanage.o(.bss.writeBakEnable) for [Anonymous Symbol]
    eeprommanage.o(.ARM.exidx.text.eeprom_WriteODO) refers to eeprommanage.o(.text.eeprom_WriteODO) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_ReadODO) refers to eemanager_interface.o(i.eeprom_comm_DelayUs) for eeprom_comm_DelayUs
    eeprommanage.o(.text.eeprom_ReadODO) refers to eemanager_interface.o(i.EE_FeedDog) for EE_FeedDog
    eeprommanage.o(.text.eeprom_ReadODO) refers to eeprommanage.o(.text.ee_IIC_SequentialRead) for ee_IIC_SequentialRead
    eeprommanage.o(.text.eeprom_ReadODO) refers to eeprommanage.o(.text.eeprom_OdoDecryption) for eeprom_OdoDecryption
    eeprommanage.o(.text.eeprom_ReadODO) refers to rt_memcpy.o(.text) for __aeabi_memcpy
    eeprommanage.o(.text.eeprom_ReadODO) refers to eeprommanage.o(.bss.MemoryConfig.2) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_ReadODO) refers to eeprommanage.o(.bss.OdoValidAddress) for OdoValidAddress
    eeprommanage.o(.text.eeprom_ReadODO) refers to eeprommanage.o(.bss.IsReadOdoState) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_ReadODO) refers to eeprommanage.o(.bss.MemoryConfig.1) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_ReadODO) refers to eeprommanage.o(.bss.memoryOdo) for [Anonymous Symbol]
    eeprommanage.o(.ARM.exidx.text.eeprom_ReadODO) refers to eeprommanage.o(.text.eeprom_ReadODO) for [Anonymous Symbol]
    eeprommanage.o(.text.eeprom_ClearOdoSection) refers to eemanager_interface.o(i.EE_FeedDog) for EE_FeedDog
    eeprommanage.o(.text.eeprom_ClearOdoSection) refers to eeprommanage.o(.text.ee_IIC_SequentialWrite) for ee_IIC_SequentialWrite
    eeprommanage.o(.text.eeprom_ClearOdoSection) refers to eemanager_interface.o(i.eeprom_comm_DelayUs) for eeprom_comm_DelayUs
    eeprommanage.o(.text.eeprom_ClearOdoSection) refers to eeprommanage.o(.bss.OdoValidAddress) for OdoValidAddress
    eeprommanage.o(.ARM.exidx.text.eeprom_ClearOdoSection) refers to eeprommanage.o(.text.eeprom_ClearOdoSection) for [Anonymous Symbol]
    eeprommanage.o(.text.ee_IIC_Start) refers to eemanager_interface.o(i.EE_SDA_OutConfig) for EE_SDA_OutConfig
    eeprommanage.o(.text.ee_IIC_Start) refers to eemanager_interface.o(i.eeprom_comm_DelayUs) for eeprom_comm_DelayUs
    eeprommanage.o(.text.ee_IIC_Start) refers to eemanager_interface.o(i.EE_SCL_OUT) for EE_SCL_OUT
    eeprommanage.o(.text.ee_IIC_Start) refers to eemanager_interface.o(i.EE_SDA_OUT) for EE_SDA_OUT
    eeprommanage.o(.ARM.exidx.text.ee_IIC_Start) refers to eeprommanage.o(.text.ee_IIC_Start) for [Anonymous Symbol]
    eeprommanage.o(.text.ee_IIC_Stop) refers to eemanager_interface.o(i.EE_SDA_OutConfig) for EE_SDA_OutConfig
    eeprommanage.o(.text.ee_IIC_Stop) refers to eemanager_interface.o(i.eeprom_comm_DelayUs) for eeprom_comm_DelayUs
    eeprommanage.o(.text.ee_IIC_Stop) refers to eemanager_interface.o(i.EE_SCL_OUT) for EE_SCL_OUT
    eeprommanage.o(.text.ee_IIC_Stop) refers to eemanager_interface.o(i.EE_SDA_OUT) for EE_SDA_OUT
    eeprommanage.o(.ARM.exidx.text.ee_IIC_Stop) refers to eeprommanage.o(.text.ee_IIC_Stop) for [Anonymous Symbol]
    eeprommanage.o(.text.ee_IIC_ACK) refers to eemanager_interface.o(i.EE_SDA_OutConfig) for EE_SDA_OutConfig
    eeprommanage.o(.text.ee_IIC_ACK) refers to eemanager_interface.o(i.eeprom_comm_DelayUs) for eeprom_comm_DelayUs
    eeprommanage.o(.text.ee_IIC_ACK) refers to eemanager_interface.o(i.EE_SDA_OUT) for EE_SDA_OUT
    eeprommanage.o(.text.ee_IIC_ACK) refers to eemanager_interface.o(i.EE_SCL_OUT) for EE_SCL_OUT
    eeprommanage.o(.ARM.exidx.text.ee_IIC_ACK) refers to eeprommanage.o(.text.ee_IIC_ACK) for [Anonymous Symbol]
    eeprommanage.o(.text.ee_IIC_NACK) refers to eemanager_interface.o(i.EE_SDA_OutConfig) for EE_SDA_OutConfig
    eeprommanage.o(.text.ee_IIC_NACK) refers to eemanager_interface.o(i.eeprom_comm_DelayUs) for eeprom_comm_DelayUs
    eeprommanage.o(.text.ee_IIC_NACK) refers to eemanager_interface.o(i.EE_SDA_OUT) for EE_SDA_OUT
    eeprommanage.o(.text.ee_IIC_NACK) refers to eemanager_interface.o(i.EE_SCL_OUT) for EE_SCL_OUT
    eeprommanage.o(.ARM.exidx.text.ee_IIC_NACK) refers to eeprommanage.o(.text.ee_IIC_NACK) for [Anonymous Symbol]
    eeprommanage.o(.text.ee_IIC_WaitAck) refers to eemanager_interface.o(i.EE_SDA_InConfig) for EE_SDA_InConfig
    eeprommanage.o(.text.ee_IIC_WaitAck) refers to eemanager_interface.o(i.eeprom_comm_DelayUs) for eeprom_comm_DelayUs
    eeprommanage.o(.text.ee_IIC_WaitAck) refers to eemanager_interface.o(i.EE_SCL_OUT) for EE_SCL_OUT
    eeprommanage.o(.text.ee_IIC_WaitAck) refers to eemanager_interface.o(i.EE_SDA_GetValue) for EE_SDA_GetValue
    eeprommanage.o(.text.ee_IIC_WaitAck) refers to eemanager_interface.o(i.EE_FeedDog) for EE_FeedDog
    eeprommanage.o(.ARM.exidx.text.ee_IIC_WaitAck) refers to eeprommanage.o(.text.ee_IIC_WaitAck) for [Anonymous Symbol]
    eeprommanage.o(.text.ee_IIC_SendByte) refers to eemanager_interface.o(i.EE_SCL_OUT) for EE_SCL_OUT
    eeprommanage.o(.text.ee_IIC_SendByte) refers to eemanager_interface.o(i.EE_SDA_OutConfig) for EE_SDA_OutConfig
    eeprommanage.o(.text.ee_IIC_SendByte) refers to eemanager_interface.o(i.eeprom_comm_DelayUs) for eeprom_comm_DelayUs
    eeprommanage.o(.text.ee_IIC_SendByte) refers to eemanager_interface.o(i.EE_SDA_OUT) for EE_SDA_OUT
    eeprommanage.o(.ARM.exidx.text.ee_IIC_SendByte) refers to eeprommanage.o(.text.ee_IIC_SendByte) for [Anonymous Symbol]
    eeprommanage.o(.text.ee_IIC_RandomReadByte) refers to eeprommanage.o(.text.ee_IIC_Start) for ee_IIC_Start
    eeprommanage.o(.text.ee_IIC_RandomReadByte) refers to eeprommanage.o(.text.ee_IIC_SendByte) for ee_IIC_SendByte
    eeprommanage.o(.text.ee_IIC_RandomReadByte) refers to eeprommanage.o(.text.ee_IIC_WaitAck) for ee_IIC_WaitAck
    eeprommanage.o(.text.ee_IIC_RandomReadByte) refers to eeprommanage.o(.text.ee_IIC_Read_8bit) for ee_IIC_Read_8bit
    eeprommanage.o(.text.ee_IIC_RandomReadByte) refers to eeprommanage.o(.text.ee_IIC_NACK) for ee_IIC_NACK
    eeprommanage.o(.text.ee_IIC_RandomReadByte) refers to eeprommanage.o(.text.ee_IIC_Stop) for ee_IIC_Stop
    eeprommanage.o(.ARM.exidx.text.ee_IIC_RandomReadByte) refers to eeprommanage.o(.text.ee_IIC_RandomReadByte) for [Anonymous Symbol]
    eeprommanage.o(.text.ee_IIC_Read_8bit) refers to eemanager_interface.o(i.EE_SDA_InConfig) for EE_SDA_InConfig
    eeprommanage.o(.text.ee_IIC_Read_8bit) refers to eemanager_interface.o(i.eeprom_comm_DelayUs) for eeprom_comm_DelayUs
    eeprommanage.o(.text.ee_IIC_Read_8bit) refers to eemanager_interface.o(i.EE_SCL_OUT) for EE_SCL_OUT
    eeprommanage.o(.text.ee_IIC_Read_8bit) refers to eemanager_interface.o(i.EE_SDA_GetValue) for EE_SDA_GetValue
    eeprommanage.o(.ARM.exidx.text.ee_IIC_Read_8bit) refers to eeprommanage.o(.text.ee_IIC_Read_8bit) for [Anonymous Symbol]
    can_signal_rx.o(i.CAN_MSG_Read) refers to can_signal_rx.o(.bss) for CanRXMsgOp
    can_signal_rx.o(i.CAN_MSG_Status) refers to can_signal_rx.o(.bss) for CanRXMsgOp
    can_signal_rx.o(i.CAN_RX_DiagCtrlEnable) refers to can_signal_rx.o(.data) for u8CAN_RX_ENABLE
    can_signal_rx.o(i.CAN_RX_DiagCtrlRelease) refers to can_signal_rx.o(.data) for u8CAN_RX_ENABLE
    can_signal_rx.o(i.CAN_RX_ReadEnableSts) refers to can_signal_rx.o(.data) for u8CAN_RX_ENABLE
    can_signal_rx.o(i.CAN_RX_SetEnable) refers to can_signal_rx.o(.data) for u8CAN_RX_ENABLE
    can_signal_rx.o(i.CanMSg_XMS_Analysis) refers to can_signal_rx.o(.data) for u8CAN_RX_ENABLE
    can_signal_rx.o(i.CanMSg_XMS_Analysis) refers to can_signal_rx.o(.bss) for CanRXMsgOp
    can_signal_rx.o(i.Can_RX_BuffInit) refers to can_signal_rx.o(.bss) for CanRXMsgOp
    can_signal_rx.o(i.Can_RX_BuffInit) refers to can_signal_rx.o(.data) for u8CAN_RX_ENABLE
    can_signal_rx.o(i.Can_RX_ResetAllTimer) refers to can_signal_rx.o(.bss) for CanRXMsgOp
    can_signal_rx.o(i.Can_RX_ResetTimer) refers to can_signal_rx.o(.bss) for CanRXMsgOp
    can_signal_rx.o(i.Co_Can_Buff_Set) refers to can_signal_rx.o(.bss) for CanRXMsgOp
    can_signal_tx.o(i.CAN_TX_DiagCtrlEnable) refers to can_signal_tx.o(.data) for u8CAN_TX_ENABLE
    can_signal_tx.o(i.CAN_TX_DiagCtrlRelease) refers to can_signal_tx.o(.data) for u8CAN_TX_ENABLE
    can_signal_tx.o(i.CAN_TX_ReadEnableSts) refers to can_signal_tx.o(.data) for u8CAN_TX_ENABLE
    can_signal_tx.o(i.CAN_TX_SetEnable) refers to can_signal_tx.o(.data) for u8CAN_TX_ENABLE
    can_signal_tx.o(i.Can_Msg_TX_FastInitCycle) refers to can_signal_tx.o(.bss) for CanMsgTxOp
    can_signal_tx.o(i.Can_Msg_TX_SUCCESS) refers to can_signal_tx.o(.bss) for CanMsgTxOp
    can_signal_tx.o(i.Can_Msg_Tx_Overwrite) refers to can_signal_tx.o(.bss) for CanMsgTxOp
    can_signal_tx.o(i.Can_TX_BuffInit) refers to can_signal_tx.o(.bss) for CanMsgTxOp
    can_signal_tx.o(i.Can_TX_BuffInit) refers to can_signal_tx.o(.data) for u8CAN_TX_ENABLE
    can_signal_tx.o(i.Can_Write_Fun) refers to can_signal_tx.o(.data) for u8CAN_TX_ENABLE
    can_signal_tx.o(i.Can_Write_Fun) refers to can_signal_tx.o(.bss) for CanMsgTxOp
    telltales_lib.o(i.Get_TelltalesLedSts) refers to telltales_lib.o(.bss) for LED_Operate
    telltales_lib.o(i.Telltales_DiagCtrl) refers to telltales_lib.o(.bss) for LED_Operate
    telltales_lib.o(i.Telltales_DiagRelease) refers to telltales_lib.o(.bss) for LED_Operate
    telltales_lib.o(i.Telltales_IG_OFF_Work) refers to telltales_lib.o(.bss) for LED_Operate
    telltales_lib.o(i.Telltales_IG_ON_Work) refers to telltales_lib.o(.bss) for LED_Operate
    telltales_lib.o(i.Telltales_KL15_Init) refers to telltales_lib.o(.bss) for LED_Operate
    telltales_lib.o(i.Telltales_KL30_Wakeup_Init) refers to telltales_lib.o(.bss) for LED_Operate
    telltales_lib.o(i.Telltales_Management) refers to telltales_lib.o(i.Telltales_IG_OFF_Work) for Telltales_IG_OFF_Work
    telltales_lib.o(i.Telltales_Management) refers to telltales_lib.o(i.Telltales_IG_ON_Work) for Telltales_IG_ON_Work
    telltales_lib.o(i.Telltales_Management) refers to telltales_lib.o(.bss) for LED_Operate
    telltales_lib.o(i.Telltales_SetCheckFinish) refers to telltales_lib.o(.bss) for LED_Operate
    telltales_lib.o(i.Test_LED_AllLight) refers to telltales_lib.o(.bss) for LED_Operate
    rt_memcpy.o(.text) refers to rt_memcpy.o(.emb_text) for __aeabi_memcpy4
    __main.o(!!!main) refers to __rtentry.o(.ARM.Collect$$rtentry$$00000000) for __rt_entry
    __rtentry.o(.ARM.Collect$$rtentry$$00000000) refers (Special) to __rtentry2.o(.ARM.Collect$$rtentry$$0000000A) for __rt_entry_li
    __rtentry.o(.ARM.Collect$$rtentry$$00000000) refers (Special) to __rtentry2.o(.ARM.Collect$$rtentry$$0000000D) for __rt_entry_main
    __rtentry.o(.ARM.Collect$$rtentry$$00000000) refers (Special) to __rtentry2.o(.ARM.Collect$$rtentry$$0000000C) for __rt_entry_postli_1
    __rtentry.o(.ARM.Collect$$rtentry$$00000000) refers (Special) to __rtentry2.o(.ARM.Collect$$rtentry$$00000009) for __rt_entry_postsh_1
    __rtentry.o(.ARM.Collect$$rtentry$$00000000) refers (Special) to __rtentry2.o(.ARM.Collect$$rtentry$$00000002) for __rt_entry_presh_1
    __rtentry.o(.ARM.Collect$$rtentry$$00000000) refers (Special) to __rtentry4.o(.ARM.Collect$$rtentry$$00000004) for __rt_entry_sh
    aeabi_idiv0_sigfpe.o(.text) refers to rt_div0.o(.text) for __rt_div0
    aeabi_ldiv0_sigfpe.o(.text) refers to rt_div0.o(.text) for __rt_div0
    __rtentry2.o(.ARM.Collect$$rtentry$$00000008) refers to boardinit2.o(.text) for _platform_post_stackheap_init
    __rtentry2.o(.ARM.Collect$$rtentry$$0000000A) refers to libinit.o(.ARM.Collect$$libinit$$00000000) for __rt_lib_init
    __rtentry2.o(.ARM.Collect$$rtentry$$0000000B) refers to boardinit3.o(.text) for _platform_post_lib_init
    __rtentry2.o(.ARM.Collect$$rtentry$$0000000D) refers to main.o(i.main) for main
    __rtentry2.o(.ARM.Collect$$rtentry$$0000000D) refers to exit.o(.text) for exit
    __rtentry2.o(.ARM.exidx) refers to __rtentry2.o(.ARM.Collect$$rtentry$$00000001) for .ARM.Collect$$rtentry$$00000001
    __rtentry2.o(.ARM.exidx) refers to __rtentry2.o(.ARM.Collect$$rtentry$$00000008) for .ARM.Collect$$rtentry$$00000008
    __rtentry2.o(.ARM.exidx) refers to __rtentry2.o(.ARM.Collect$$rtentry$$0000000A) for .ARM.Collect$$rtentry$$0000000A
    __rtentry2.o(.ARM.exidx) refers to __rtentry2.o(.ARM.Collect$$rtentry$$0000000B) for .ARM.Collect$$rtentry$$0000000B
    __rtentry2.o(.ARM.exidx) refers to __rtentry2.o(.ARM.Collect$$rtentry$$0000000D) for .ARM.Collect$$rtentry$$0000000D
    __rtentry4.o(.ARM.Collect$$rtentry$$00000004) refers to sys_stackheap_outer.o(.text) for __user_setup_stackheap
    __rtentry4.o(.ARM.exidx) refers to __rtentry4.o(.ARM.Collect$$rtentry$$00000004) for .ARM.Collect$$rtentry$$00000004
    rt_div0.o(.text) refers to defsig_fpe_outer.o(.text) for __rt_SIGFPE
    sys_stackheap_outer.o(.text) refers to libspace.o(.text) for __user_perproc_libspace
    sys_stackheap_outer.o(.text) refers to startup_bat32a239.o(.text) for __user_initial_stackheap
    sys_stackheap_outer.o(__vectab_stack_and_reset_area) refers to tempstk.o(.text) for __temporary_stack_top
    sys_stackheap_outer.o(__vectab_stack_and_reset_area) refers to __main.o(!!!main) for __main
    exit.o(.text) refers to rtexit.o(.ARM.Collect$$rtexit$$00000000) for __rt_exit
    defsig_fpe_outer.o(.text) refers to defsig_fpe_inner.o(.text) for __rt_SIGFPE_inner
    defsig_fpe_outer.o(.text) refers to defsig_exit.o(.text) for __sig_exit
    defsig_fpe_formal.o(.text) refers to rt_raise.o(.text) for __rt_raise
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$0000002E) for __rt_lib_init_alloca_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$0000002C) for __rt_lib_init_argv_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$0000001B) for __rt_lib_init_atexit_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000021) for __rt_lib_init_clock_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000032) for __rt_lib_init_cpp_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000030) for __rt_lib_init_exceptions_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000002) for __rt_lib_init_fp_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$0000001F) for __rt_lib_init_fp_trap_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000023) for __rt_lib_init_getenv_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$0000000A) for __rt_lib_init_heap_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000011) for __rt_lib_init_lc_collate_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000013) for __rt_lib_init_lc_ctype_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000015) for __rt_lib_init_lc_monetary_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000017) for __rt_lib_init_lc_numeric_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000019) for __rt_lib_init_lc_time_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000004) for __rt_lib_init_preinit_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$0000000E) for __rt_lib_init_rand_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000033) for __rt_lib_init_return
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$0000001D) for __rt_lib_init_signal_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$00000025) for __rt_lib_init_stdio_1
    libinit.o(.ARM.Collect$$libinit$$00000000) refers (Special) to libinit2.o(.ARM.Collect$$libinit$$0000000C) for __rt_lib_init_user_alloc_1
    libspace.o(.text) refers to libspace.o(.bss) for __libspace_start
    rtexit.o(.ARM.Collect$$rtexit$$00000000) refers (Special) to rtexit2.o(.ARM.Collect$$rtexit$$00000004) for __rt_exit_exit
    rtexit.o(.ARM.Collect$$rtexit$$00000000) refers (Special) to rtexit2.o(.ARM.Collect$$rtexit$$00000003) for __rt_exit_ls
    rtexit.o(.ARM.Collect$$rtexit$$00000000) refers (Special) to rtexit2.o(.ARM.Collect$$rtexit$$00000002) for __rt_exit_prels_1
    rtexit.o(.ARM.exidx) refers (Special) to rtexit2.o(.ARM.Collect$$rtexit$$00000004) for __rt_exit_exit
    rtexit.o(.ARM.exidx) refers (Special) to rtexit2.o(.ARM.Collect$$rtexit$$00000003) for __rt_exit_ls
    rtexit.o(.ARM.exidx) refers (Special) to rtexit2.o(.ARM.Collect$$rtexit$$00000002) for __rt_exit_prels_1
    rtexit.o(.ARM.exidx) refers to rtexit.o(.ARM.Collect$$rtexit$$00000000) for .ARM.Collect$$rtexit$$00000000
    rt_raise.o(.text) refers to __raise.o(.text) for __raise
    rt_raise.o(.text) refers to sys_exit.o(.text) for _sys_exit
    defsig_exit.o(.text) refers to sys_exit.o(.text) for _sys_exit
    defsig_fpe_inner.o(.text) refers to defsig_general.o(.text) for __default_signal_display
    libinit2.o(.ARM.Collect$$libinit$$00000010) refers to libinit2.o(.ARM.Collect$$libinit$$0000000F) for .ARM.Collect$$libinit$$0000000F
    libinit2.o(.ARM.Collect$$libinit$$00000012) refers to libinit2.o(.ARM.Collect$$libinit$$0000000F) for .ARM.Collect$$libinit$$0000000F
    libinit2.o(.ARM.Collect$$libinit$$00000014) refers to libinit2.o(.ARM.Collect$$libinit$$0000000F) for .ARM.Collect$$libinit$$0000000F
    libinit2.o(.ARM.Collect$$libinit$$00000016) refers to libinit2.o(.ARM.Collect$$libinit$$0000000F) for .ARM.Collect$$libinit$$0000000F
    libinit2.o(.ARM.Collect$$libinit$$00000018) refers to libinit2.o(.ARM.Collect$$libinit$$0000000F) for .ARM.Collect$$libinit$$0000000F
    libinit2.o(.ARM.Collect$$libinit$$00000026) refers to argv_veneer.o(.text) for __ARM_argv_veneer
    libinit2.o(.ARM.Collect$$libinit$$00000027) refers to argv_veneer.o(.text) for __ARM_argv_veneer
    sys_exit.o(.text) refers (Special) to use_no_semi.o(.text) for __I$use$semihosting
    sys_exit.o(.text) refers (Special) to indicate_semi.o(.text) for __semihosting_library_function
    rtexit2.o(.ARM.Collect$$rtexit$$00000003) refers to libshutdown.o(.ARM.Collect$$libshutdown$$00000000) for __rt_lib_shutdown
    rtexit2.o(.ARM.Collect$$rtexit$$00000004) refers to sys_exit.o(.text) for _sys_exit
    rtexit2.o(.ARM.exidx) refers to rtexit2.o(.ARM.Collect$$rtexit$$00000001) for .ARM.Collect$$rtexit$$00000001
    rtexit2.o(.ARM.exidx) refers to rtexit2.o(.ARM.Collect$$rtexit$$00000003) for .ARM.Collect$$rtexit$$00000003
    rtexit2.o(.ARM.exidx) refers to rtexit2.o(.ARM.Collect$$rtexit$$00000004) for .ARM.Collect$$rtexit$$00000004
    __raise.o(.text) refers to defsig.o(CL$$defsig) for __default_signal_handler
    defsig_general.o(.text) refers to sys_wrch.o(.text) for _ttywrch
    sys_wrch.o(.text) refers (Special) to use_no_semi.o(.text) for __I$use$semihosting
    sys_wrch.o(.text) refers (Special) to indicate_semi.o(.text) for __semihosting_library_function
    defsig.o(CL$$defsig) refers to defsig_fpe_inner.o(.text) for __rt_SIGFPE_inner
    defsig.o(CL$$defsig) refers to defsig_rtmem_inner.o(.text) for __rt_SIGRTMEM_inner
    _get_argv_nomalloc.o(.text) refers (Special) to hrguard.o(.text) for __heap_region$guard
    _get_argv_nomalloc.o(.text) refers to defsig_rtmem_outer.o(.text) for __rt_SIGRTMEM
    _get_argv_nomalloc.o(.text) refers to sys_command.o(.text) for _sys_command_string
    libshutdown.o(.ARM.Collect$$libshutdown$$00000000) refers (Special) to libshutdown2.o(.ARM.Collect$$libshutdown$$00000004) for __rt_lib_shutdown_cpp_1
    libshutdown.o(.ARM.Collect$$libshutdown$$00000000) refers (Special) to libshutdown2.o(.ARM.Collect$$libshutdown$$00000002) for __rt_lib_shutdown_fini_1
    libshutdown.o(.ARM.Collect$$libshutdown$$00000000) refers (Special) to libshutdown2.o(.ARM.Collect$$libshutdown$$00000009) for __rt_lib_shutdown_fp_trap_1
    libshutdown.o(.ARM.Collect$$libshutdown$$00000000) refers (Special) to libshutdown2.o(.ARM.Collect$$libshutdown$$00000011) for __rt_lib_shutdown_heap_1
    libshutdown.o(.ARM.Collect$$libshutdown$$00000000) refers (Special) to libshutdown2.o(.ARM.Collect$$libshutdown$$00000012) for __rt_lib_shutdown_return
    libshutdown.o(.ARM.Collect$$libshutdown$$00000000) refers (Special) to libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C) for __rt_lib_shutdown_signal_1
    libshutdown.o(.ARM.Collect$$libshutdown$$00000000) refers (Special) to libshutdown2.o(.ARM.Collect$$libshutdown$$00000006) for __rt_lib_shutdown_stdio_1
    libshutdown.o(.ARM.Collect$$libshutdown$$00000000) refers (Special) to libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E) for __rt_lib_shutdown_user_alloc_1
    sys_command.o(.text) refers (Special) to use_no_semi.o(.text) for __I$use$semihosting
    sys_command.o(.text) refers (Special) to indicate_semi.o(.text) for __semihosting_library_function
    defsig_abrt_inner.o(.text) refers to defsig_general.o(.text) for __default_signal_display
    defsig_rtred_inner.o(.text) refers to defsig_general.o(.text) for __default_signal_display
    defsig_rtmem_inner.o(.text) refers to defsig_general.o(.text) for __default_signal_display
    defsig_rtmem_outer.o(.text) refers to defsig_rtmem_inner.o(.text) for __rt_SIGRTMEM_inner
    defsig_rtmem_outer.o(.text) refers to defsig_exit.o(.text) for __sig_exit
    defsig_rtmem_formal.o(.text) refers to rt_raise.o(.text) for __rt_raise
    defsig_stak_inner.o(.text) refers to defsig_general.o(.text) for __default_signal_display
    defsig_pvfn_inner.o(.text) refers to defsig_general.o(.text) for __default_signal_display
    defsig_cppl_inner.o(.text) refers to defsig_general.o(.text) for __default_signal_display
    defsig_segv_inner.o(.text) refers to defsig_general.o(.text) for __default_signal_display
    defsig_other.o(.text) refers to defsig_general.o(.text) for __default_signal_display


==============================================================================

Removing Unused input sections from the image.

    Removing gpio.o(.rev16_text), (4 bytes).
    Removing gpio.o(.revsh_text), (4 bytes).
    Removing gpio.o(i.GPIO_Get_Value), (6 bytes).
    Removing gpio.o(i.GPIO_Input_Enable), (32 bytes).
    Removing gpio.o(i.GPIO_Nch_OpenDrain), (20 bytes).
    Removing gpio.o(i.GPIO_Output_Enable), (32 bytes).
    Removing gpio.o(i.GPIO_PullUp_Disable), (20 bytes).
    Removing gpio.o(i.GPIO_PullUp_Enable), (20 bytes).
    Removing gpio.o(i.GPIO_Set_Value), (4 bytes).
    Removing gpio.o(i.GPIO_Ttl_Input), (20 bytes).
    Removing gpio.o(i.PORT_ToggleBit), (36 bytes).
    Removing wdt.o(.rev16_text), (4 bytes).
    Removing wdt.o(.revsh_text), (4 bytes).
    Removing sys_tick.o(.rev16_text), (4 bytes).
    Removing sys_tick.o(.revsh_text), (4 bytes).
    Removing sys_tick.o(i.Sys_Tick_Timer_Call_Back_Reg), (16 bytes).
    Removing adc.o(.rev16_text), (4 bytes).
    Removing adc.o(.revsh_text), (4 bytes).
    Removing adc.o(i.ADC_Converse), (132 bytes).
    Removing adc.o(i.ADC_MidAvg_Filter), (116 bytes).
    Removing adc.o(i.ADC_SelfTest), (160 bytes).
    Removing adc.o(i.ADC_Set_Clock), (36 bytes).
    Removing adc.o(i.ADC_Set_HardTrigger), (52 bytes).
    Removing adc.o(i.ADC_Set_OperationOff), (20 bytes).
    Removing adc.o(i.ADC_Set_OperationOn), (20 bytes).
    Removing adc.o(i.ADC_Set_RefVoltage), (60 bytes).
    Removing analog_circuits.o(.rev16_text), (4 bytes).
    Removing analog_circuits.o(.revsh_text), (4 bytes).
    Removing analog_circuits.o(i.ADC_Res_Calc_Circuit102), (304 bytes).
    Removing analog_circuits.o(i.ADC_Res_Calc_Circuit103), (368 bytes).
    Removing analog_circuits.o(i.ADC_Res_Calc_Circuit201), (176 bytes).
    Removing analog_circuits.o(i.ADC_Res_Calc_Circuit202), (248 bytes).
    Removing analog_circuits.o(i.ADC_Res_Calc_Circuit203), (324 bytes).
    Removing analog_circuits.o(i.ADC_Res_Calc_Circuit301), (96 bytes).
    Removing analog_circuits.o(i.ADC_Res_Calc_Circuit302), (136 bytes).
    Removing analog_circuits.o(i.ADC_Res_Calc_Circuit303), (232 bytes).
    Removing analog_circuits.o(i.ADC_VRef_Calibrate), (60 bytes).
    Removing analog_signals.o(.rev16_text), (4 bytes).
    Removing analog_signals.o(.revsh_text), (4 bytes).
    Removing sci.o(.rev16_text), (4 bytes).
    Removing sci.o(.revsh_text), (4 bytes).
    Removing sci.o(i.IIC00_Init), (208 bytes).
    Removing sci.o(i.IIC00_MasterReceive), (132 bytes).
    Removing sci.o(i.IIC00_MasterSend), (120 bytes).
    Removing sci.o(i.IIC00_StartCondition), (88 bytes).
    Removing sci.o(i.IIC00_Stop), (36 bytes).
    Removing sci.o(i.IIC00_StopCondition), (108 bytes).
    Removing sci.o(i.IIC01_Init), (172 bytes).
    Removing sci.o(i.IIC01_MasterReceive), (124 bytes).
    Removing sci.o(i.IIC01_MasterSend), (112 bytes).
    Removing sci.o(i.IIC01_StartCondition), (92 bytes).
    Removing sci.o(i.IIC01_Stop), (40 bytes).
    Removing sci.o(i.IIC01_StopCondition), (100 bytes).
    Removing sci.o(i.IIC10_Init), (212 bytes).
    Removing sci.o(i.IIC10_MasterReceive), (132 bytes).
    Removing sci.o(i.IIC10_MasterSend), (120 bytes).
    Removing sci.o(i.IIC10_StartCondition), (92 bytes).
    Removing sci.o(i.IIC10_Stop), (40 bytes).
    Removing sci.o(i.IIC10_StopCondition), (108 bytes).
    Removing sci.o(i.IIC11_Init), (216 bytes).
    Removing sci.o(i.IIC11_MasterReceive), (124 bytes).
    Removing sci.o(i.IIC11_MasterSend), (112 bytes).
    Removing sci.o(i.IIC11_StartCondition), (92 bytes).
    Removing sci.o(i.IIC11_Stop), (40 bytes).
    Removing sci.o(i.IIC11_StopCondition), (100 bytes).
    Removing sci.o(i.IIC20_Init), (204 bytes).
    Removing sci.o(i.IIC20_MasterReceive), (132 bytes).
    Removing sci.o(i.IIC20_MasterSend), (120 bytes).
    Removing sci.o(i.IIC20_StartCondition), (88 bytes).
    Removing sci.o(i.IIC21_Init), (168 bytes).
    Removing sci.o(i.IIC21_MasterReceive), (124 bytes).
    Removing sci.o(i.IIC21_MasterSend), (112 bytes).
    Removing sci.o(i.IIC21_StartCondition), (92 bytes).
    Removing sci.o(i.IIC30_Init), (176 bytes).
    Removing sci.o(i.IIC30_MasterReceive), (132 bytes).
    Removing sci.o(i.IIC30_MasterSend), (120 bytes).
    Removing sci.o(i.IIC30_StartCondition), (88 bytes).
    Removing sci.o(i.IIC30_Stop), (36 bytes).
    Removing sci.o(i.IIC30_StopCondition), (108 bytes).
    Removing sci.o(i.IIC31_Init), (168 bytes).
    Removing sci.o(i.IIC31_MasterReceive), (124 bytes).
    Removing sci.o(i.IIC31_MasterSend), (112 bytes).
    Removing sci.o(i.IIC31_StartCondition), (92 bytes).
    Removing sci.o(i.IIC31_Stop), (40 bytes).
    Removing sci.o(i.IIC31_StopCondition), (100 bytes).
    Removing sci.o(i.SPI00_MasterInit), (336 bytes).
    Removing sci.o(i.SPI00_MasterReceive), (216 bytes).
    Removing sci.o(i.SPI00_MasterSend), (200 bytes).
    Removing sci.o(i.SPI00_MasterSendReceive), (240 bytes).
    Removing sci.o(i.SPI00_SlaveInit), (244 bytes).
    Removing sci.o(i.SPI00_SlaveReceive), (164 bytes).
    Removing sci.o(i.SPI00_SlaveSend), (196 bytes).
    Removing sci.o(i.SPI00_Start), (80 bytes).
    Removing sci.o(i.SPI00_Stop), (72 bytes).
    Removing sci.o(i.SPI01_MasterInit), (284 bytes).
    Removing sci.o(i.SPI01_MasterReceive), (88 bytes).
    Removing sci.o(i.SPI01_MasterSend), (104 bytes).
    Removing sci.o(i.SPI01_SlaveInit), (168 bytes).
    Removing sci.o(i.SPI01_SlaveReceive), (88 bytes).
    Removing sci.o(i.SPI01_SlaveSend), (104 bytes).
    Removing sci.o(i.SPI01_SlaveSendReceive), (108 bytes).
    Removing sci.o(i.SPI01_Start), (80 bytes).
    Removing sci.o(i.SPI01_Stop), (84 bytes).
    Removing sci.o(i.SPI10_MasterInit), (364 bytes).
    Removing sci.o(i.SPI10_MasterReceive), (228 bytes).
    Removing sci.o(i.SPI10_MasterSend), (196 bytes).
    Removing sci.o(i.SPI10_MasterSendReceive), (248 bytes).
    Removing sci.o(i.SPI10_SlaveInit), (224 bytes).
    Removing sci.o(i.SPI10_SlaveReceive), (164 bytes).
    Removing sci.o(i.SPI10_SlaveSend), (192 bytes).
    Removing sci.o(i.SPI10_Start), (80 bytes).
    Removing sci.o(i.SPI10_Stop), (84 bytes).
    Removing sci.o(i.SPI11_MasterInit), (364 bytes).
    Removing sci.o(i.SPI11_MasterReceive), (236 bytes).
    Removing sci.o(i.SPI11_MasterSend), (200 bytes).
    Removing sci.o(i.SPI11_SlaveInit), (224 bytes).
    Removing sci.o(i.SPI11_SlaveReceive), (168 bytes).
    Removing sci.o(i.SPI11_SlaveSend), (200 bytes).
    Removing sci.o(i.SPI11_SlaveSendReceive), (236 bytes).
    Removing sci.o(i.SPI11_Start), (80 bytes).
    Removing sci.o(i.SPI11_Stop), (84 bytes).
    Removing sci.o(i.SPI20_MasterInit), (328 bytes).
    Removing sci.o(i.SPI20_MasterReceive), (76 bytes).
    Removing sci.o(i.SPI20_MasterSend), (72 bytes).
    Removing sci.o(i.SPI20_SlaveInit), (216 bytes).
    Removing sci.o(i.SPI20_SlaveReceive), (88 bytes).
    Removing sci.o(i.SPI20_SlaveSend), (104 bytes).
    Removing sci.o(i.SPI20_Start), (80 bytes).
    Removing sci.o(i.SPI20_Stop), (72 bytes).
    Removing sci.o(i.SPI21_MasterInit), (260 bytes).
    Removing sci.o(i.SPI21_MasterReceive), (88 bytes).
    Removing sci.o(i.SPI21_MasterSend), (108 bytes).
    Removing sci.o(i.SPI21_MasterSendReceive), (112 bytes).
    Removing sci.o(i.SPI21_SlaveInit), (160 bytes).
    Removing sci.o(i.SPI21_SlaveReceive), (88 bytes).
    Removing sci.o(i.SPI21_SlaveSend), (104 bytes).
    Removing sci.o(i.SPI21_Start), (80 bytes).
    Removing sci.o(i.SPI21_Stop), (76 bytes).
    Removing sci.o(i.SPI30_MasterInit), (288 bytes).
    Removing sci.o(i.SPI30_MasterReceive), (76 bytes).
    Removing sci.o(i.SPI30_MasterSend), (72 bytes).
    Removing sci.o(i.SPI30_SlaveInit), (176 bytes).
    Removing sci.o(i.SPI30_SlaveReceive), (88 bytes).
    Removing sci.o(i.SPI30_SlaveSend), (104 bytes).
    Removing sci.o(i.SPI30_Start), (80 bytes).
    Removing sci.o(i.SPI30_Stop), (72 bytes).
    Removing sci.o(i.SPI31_MasterInit), (260 bytes).
    Removing sci.o(i.SPI31_MasterReceive), (88 bytes).
    Removing sci.o(i.SPI31_MasterSend), (108 bytes).
    Removing sci.o(i.SPI31_MasterSendReceive), (112 bytes).
    Removing sci.o(i.SPI31_SlaveInit), (160 bytes).
    Removing sci.o(i.SPI31_SlaveReceive), (88 bytes).
    Removing sci.o(i.SPI31_SlaveSend), (104 bytes).
    Removing sci.o(i.SPI31_Start), (80 bytes).
    Removing sci.o(i.SPI31_Stop), (76 bytes).
    Removing sci.o(i.UART0_BaudRate), (100 bytes).
    Removing sci.o(i.UART0_Init), (260 bytes).
    Removing sci.o(i.UART0_Receive), (28 bytes).
    Removing sci.o(i.UART0_Receive_Int), (44 bytes).
    Removing sci.o(i.UART0_Send), (28 bytes).
    Removing sci.o(i.UART1_BaudRate), (80 bytes).
    Removing sci.o(i.UART1_Init), (304 bytes).
    Removing sci.o(i.UART1_Receive), (44 bytes).
    Removing sci.o(i.UART1_Send), (68 bytes).
    Removing sci.o(i.UART1_Start), (80 bytes).
    Removing sci.o(i.UART1_Stop), (60 bytes).
    Removing sci.o(i.UART2_BaudRate), (80 bytes).
    Removing sci.o(i.UART2_Init), (348 bytes).
    Removing sci.o(i.UART2_Receive), (44 bytes).
    Removing sci.o(i.UART2_Send), (68 bytes).
    Removing sci.o(i.UART2_Start), (88 bytes).
    Removing sci.o(i.UART2_Stop), (68 bytes).
    Removing sci.o(i.UART3_BaudRate), (80 bytes).
    Removing sci.o(i.UART3_Init), (308 bytes).
    Removing sci.o(i.UART3_Receive), (44 bytes).
    Removing sci.o(i.UART3_Send), (68 bytes).
    Removing sci.o(i.UART3_Sendbyte), (28 bytes).
    Removing sci.o(i.UART3_Start), (72 bytes).
    Removing sci.o(i.UART3_Stop), (68 bytes).
    Removing sci.o(i.UART_BaudRateCal), (120 bytes).
    Removing sci.o(i.__NVIC_ClearPendingIRQ), (24 bytes).
    Removing sci.o(i.__NVIC_SetPriority), (120 bytes).
    Removing sci.o(.constdata), (32 bytes).
    Removing sci_user.o(.rev16_text), (4 bytes).
    Removing sci_user.o(.revsh_text), (4 bytes).
    Removing sci_user.o(i.Get_Uart2_State), (12 bytes).
    Removing sci_user.o(i.UART_Ch2_Send_Multiple_Byte), (88 bytes).
    Removing sci_user.o(i.iic00_callback_master_error), (2 bytes).
    Removing sci_user.o(i.iic00_callback_master_receiveend), (20 bytes).
    Removing sci_user.o(i.iic00_callback_master_sendend), (20 bytes).
    Removing sci_user.o(i.iic00_interrupt), (388 bytes).
    Removing sci_user.o(i.iic01_callback_master_error), (2 bytes).
    Removing sci_user.o(i.iic01_callback_master_receiveend), (20 bytes).
    Removing sci_user.o(i.iic01_callback_master_sendend), (20 bytes).
    Removing sci_user.o(i.iic01_interrupt), (388 bytes).
    Removing sci_user.o(i.iic30_callback_master_error), (2 bytes).
    Removing sci_user.o(i.iic30_callback_master_receiveend), (20 bytes).
    Removing sci_user.o(i.iic30_callback_master_sendend), (20 bytes).
    Removing sci_user.o(i.iic30_interrupt), (372 bytes).
    Removing sci_user.o(i.iic31_callback_master_error), (2 bytes).
    Removing sci_user.o(i.iic31_callback_master_receiveend), (20 bytes).
    Removing sci_user.o(i.iic31_callback_master_sendend), (20 bytes).
    Removing sci_user.o(i.iic31_interrupt), (372 bytes).
    Removing sci_user.o(i.spi00_callback_error), (2 bytes).
    Removing sci_user.o(i.spi00_callback_receiveend), (12 bytes).
    Removing sci_user.o(i.spi00_callback_sendend), (12 bytes).
    Removing sci_user.o(i.spi00_interrupt), (312 bytes).
    Removing sci_user.o(i.spi01_callback_error), (2 bytes).
    Removing sci_user.o(i.spi01_callback_receiveend), (20 bytes).
    Removing sci_user.o(i.spi01_callback_sendend), (20 bytes).
    Removing sci_user.o(i.spi01_interrupt), (312 bytes).
    Removing sci_user.o(i.spi10_callback_error), (2 bytes).
    Removing sci_user.o(i.spi10_callback_receiveend), (12 bytes).
    Removing sci_user.o(i.spi10_callback_sendend), (12 bytes).
    Removing sci_user.o(i.spi10_interrupt), (312 bytes).
    Removing sci_user.o(i.spi11_callback_error), (2 bytes).
    Removing sci_user.o(i.spi11_callback_receiveend), (20 bytes).
    Removing sci_user.o(i.spi11_callback_sendend), (20 bytes).
    Removing sci_user.o(i.spi11_interrupt), (312 bytes).
    Removing sci_user.o(i.spi20_callback_error), (2 bytes).
    Removing sci_user.o(i.spi20_callback_receiveend), (12 bytes).
    Removing sci_user.o(i.spi20_callback_sendend), (12 bytes).
    Removing sci_user.o(i.spi20_interrupt), (312 bytes).
    Removing sci_user.o(i.spi21_callback_error), (2 bytes).
    Removing sci_user.o(i.spi21_callback_receiveend), (12 bytes).
    Removing sci_user.o(i.spi21_callback_sendend), (12 bytes).
    Removing sci_user.o(i.spi21_interrupt), (312 bytes).
    Removing sci_user.o(i.spi30_callback_error), (2 bytes).
    Removing sci_user.o(i.spi30_callback_receiveend), (12 bytes).
    Removing sci_user.o(i.spi30_callback_sendend), (12 bytes).
    Removing sci_user.o(i.spi30_interrupt), (312 bytes).
    Removing sci_user.o(i.spi31_callback_error), (2 bytes).
    Removing sci_user.o(i.spi31_callback_receiveend), (12 bytes).
    Removing sci_user.o(i.spi31_callback_sendend), (12 bytes).
    Removing sci_user.o(i.spi31_interrupt), (312 bytes).
    Removing sci_user.o(i.uart0_callback_error), (2 bytes).
    Removing sci_user.o(i.uart0_callback_receiveend), (2 bytes).
    Removing sci_user.o(i.uart0_callback_softwareoverrun), (2 bytes).
    Removing sci_user.o(i.uart2_Get_0x10_Rev_Flag), (12 bytes).
    Removing sci_user.o(i.uart2_User_KL30_Init), (16 bytes).
    Removing sci_user.o(i.uart2_callback_error), (16 bytes).
    Removing sci_user.o(i.uart2_callback_receiveend), (2 bytes).
    Removing sci_user.o(i.uart2_callback_sendend), (12 bytes).
    Removing sci_user.o(i.uart2_interrupt_receive), (44 bytes).
    Removing sci_user.o(i.uart2_interrupt_send), (76 bytes).
    Removing clk.o(.rev16_text), (4 bytes).
    Removing clk.o(.revsh_text), (4 bytes).
    Removing clk.o(i.CLK_Hoco_Start), (20 bytes).
    Removing clk.o(i.CLK_Hoco_Stop), (20 bytes).
    Removing clk.o(i.CLK_MainOsc_Setting), (72 bytes).
    Removing clk.o(i.CLK_MainOsc_Start), (20 bytes).
    Removing clk.o(i.CLK_MainOsc_Stop), (20 bytes).
    Removing clk.o(i.CLK_PLL_Stop), (12 bytes).
    Removing clk.o(i.CLK_SubOsc_Setting), (84 bytes).
    Removing clk.o(i.CLK_SubOsc_Start), (20 bytes).
    Removing clk.o(i.CLK_SubOsc_Stop), (20 bytes).
    Removing intp.o(.rev16_text), (4 bytes).
    Removing intp.o(.revsh_text), (4 bytes).
    Removing intp.o(i.INTP_Stop), (260 bytes).
    Removing intp_user.o(.rev16_text), (4 bytes).
    Removing intp_user.o(.revsh_text), (4 bytes).
    Removing tim4.o(.rev16_text), (4 bytes).
    Removing tim4.o(.revsh_text), (4 bytes).
    Removing tim4.o(i.Capture_Init), (424 bytes).
    Removing tim4.o(i.Timer4_Init), (2 bytes).
    Removing rtc.o(.rev16_text), (4 bytes).
    Removing rtc.o(.revsh_text), (4 bytes).
    Removing timera_b_c.o(.rev16_text), (4 bytes).
    Removing timera_b_c.o(.revsh_text), (4 bytes).
    Removing timera_b_c.o(i.TMA0_Start), (40 bytes).
    Removing timera_b_c.o(i.TMA0_Stop), (40 bytes).
    Removing timera_b_c.o(i.TMB0_Stop), (88 bytes).
    Removing timera_b_c.o(i.bsp_TMA0_IntervalTimer), (92 bytes).
    Removing can.o(.rev16_text), (4 bytes).
    Removing can.o(.revsh_text), (4 bytes).
    Removing can.o(i.CAN0_Get_Wake_Up_Flag), (24 bytes).
    Removing can.o(i.GetBusOffState), (100 bytes).
    Removing bu98r10.o(.rev16_text), (4 bytes).
    Removing bu98r10.o(.revsh_text), (4 bytes).
    Removing bu98r10.o(i.BU98R10_0_Command_Write), (152 bytes).
    Removing bu98r10.o(i.BU98R10_0_Data_Write), (152 bytes).
    Removing bu98r10.o(i.BU98R10_1_Command_Write), (152 bytes).
    Removing bu98r10.o(i.BU98R10_1_Data_Write), (152 bytes).
    Removing bu98r10.o(i.BU98R10_All_ReadRam), (464 bytes).
    Removing seg_lcd.o(.rev16_text), (4 bytes).
    Removing seg_lcd.o(.revsh_text), (4 bytes).
    Removing seg_lcd.o(i.Conv_Single_DECHEX), (50 bytes).
    Removing seg_lcd.o(i.SEG_LCD_BatteryErr_Display), (1948 bytes).
    Removing seg_lcd.o(i.SEG_LCD_FaultCode_Display), (2084 bytes).
    Removing seg_lcd.o(i.SEG_LCD_TSC), (24 bytes).
    Removing flash.o(.rev16_text), (4 bytes).
    Removing flash.o(.revsh_text), (4 bytes).
    Removing is31fl3236.o(.rev16_text), (4 bytes).
    Removing is31fl3236.o(.revsh_text), (4 bytes).
    Removing is31fl3236.o(i.IS31FL3236_Clear), (48 bytes).
    Removing is31fl3236.o(i.extend_CheckChips), (2 bytes).
    Removing aw93015.o(.rev16_text), (4 bytes).
    Removing aw93015.o(.revsh_text), (4 bytes).
    Removing aw93015.o(i.bsp_IIC2_NACK), (32 bytes).
    Removing aw93015.o(i.bsp_IIC_delay), (28 bytes).
    Removing is31_iic_master.o(.rev16_text), (4 bytes).
    Removing is31_iic_master.o(.revsh_text), (4 bytes).
    Removing is31_iic_master.o(i.IS31_IIC_NACK), (50 bytes).
    Removing is31_iic_master.o(i.IS31_IIC_SCL_Dir_In), (96 bytes).
    Removing is31_iic_master.o(i.Simulated_Release_SCL), (16 bytes).
    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing main.o(.data), (1 bytes).
    Removing tasks.o(.rev16_text), (4 bytes).
    Removing tasks.o(.revsh_text), (4 bytes).
    Removing tasks.o(i.APP_Startup_Init), (2 bytes).
    Removing tasks.o(i.Sys_Sleep_Mode_Tasks), (2 bytes).
    Removing tasks.o(.constdata), (20 bytes).
    Removing tasks.o(.data), (12 bytes).
    Removing sys_scheduler.o(.rev16_text), (4 bytes).
    Removing sys_scheduler.o(.revsh_text), (4 bytes).
    Removing init.o(.rev16_text), (4 bytes).
    Removing init.o(.revsh_text), (4 bytes).
    Removing init.o(i.Sys_Sleep_Init), (2 bytes).
    Removing init.o(i.Sys_Startup_Pre_Init), (2 bytes).
    Removing init.o(i.Sys_Wakeup_Init), (2 bytes).
    Removing line_in.o(.rev16_text), (4 bytes).
    Removing line_in.o(.revsh_text), (4 bytes).
    Removing line_in.o(i.Line_In_SetPowerSt), (12 bytes).
    Removing powermanagement.o(.rev16_text), (4 bytes).
    Removing powermanagement.o(.revsh_text), (4 bytes).
    Removing powermanagement.o(i.Get_PwrLibVersion), (4 bytes).
    Removing powermanagement_user.o(.rev16_text), (4 bytes).
    Removing powermanagement_user.o(.revsh_text), (4 bytes).
    Removing powermanagement_user.o(.constdata), (20 bytes).
    Removing system_monitor.o(.rev16_text), (4 bytes).
    Removing system_monitor.o(.revsh_text), (4 bytes).
    Removing system_monitor.o(i.Read_KL30_ConvertFinish), (12 bytes).
    Removing system_monitor.o(i.System_NM_KL15_Status_Get), (12 bytes).
    Removing system_monitor.o(i.System_NM_KL30_Status_Get), (12 bytes).
    Removing system_monitor_user.o(.rev16_text), (4 bytes).
    Removing system_monitor_user.o(.revsh_text), (4 bytes).
    Removing system_monitor_user.o(.data), (4 bytes).
    Removing rte_adc.o(.rev16_text), (4 bytes).
    Removing rte_adc.o(.revsh_text), (4 bytes).
    Removing rte_adc.o(i.RTE_ADC_Init), (8 bytes).
    Removing rte_adc.o(i.RTE_ForceRead_FUEL1_Voltage), (16 bytes).
    Removing rte_adc.o(i.RTE_ForceRead_FUEL_VREF_Voltage), (16 bytes).
    Removing rte_adc.o(i.RTE_Read_FUEL1_Valid), (16 bytes).
    Removing rte_adc.o(i.RTE_Read_FUEL1_Voltage), (16 bytes).
    Removing rte_adc.o(i.RTE_Read_FUEL_VREF_Valid), (16 bytes).
    Removing rte_adc.o(i.RTE_Read_FUEL_VREF_Voltage), (16 bytes).
    Removing common_interface.o(.rev16_text), (4 bytes).
    Removing common_interface.o(.revsh_text), (4 bytes).
    Removing common_interface.o(i.Common_BlockDelay), (56 bytes).
    Removing common_interface.o(i.Common_Get_Act_E_Speed), (12 bytes).
    Removing common_interface.o(i.Common_Get_Act_E_Speed_Valid), (12 bytes).
    Removing common_interface.o(i.Common_Get_Act_RV_Speed), (12 bytes).
    Removing common_interface.o(i.Common_Get_Act_V_Speed), (12 bytes).
    Removing common_interface.o(i.Common_Get_Act_V_Speed_Valid), (12 bytes).
    Removing common_interface.o(i.Common_Get_Disp_E_Speed_Valid), (12 bytes).
    Removing common_interface.o(i.Common_Get_Disp_RV_Speed), (12 bytes).
    Removing common_interface.o(i.Common_Get_Disp_V_Speed_Valid), (12 bytes).
    Removing common_interface.o(i.Common_Get_E_Speed_TEST), (12 bytes).
    Removing common_interface.o(i.Common_Get_Fuel_TEST), (12 bytes).
    Removing common_interface.o(i.Common_Get_Gauges_Disp_E_Speed), (12 bytes).
    Removing common_interface.o(i.Common_Get_Temp_TEST), (12 bytes).
    Removing common_interface.o(i.Common_Get_V_Speed_TEST), (12 bytes).
    Removing common_interface.o(i.Common_ReadRollingCounter), (12 bytes).
    Removing common_interface.o(i.Common_RollingCounterAdd), (16 bytes).
    Removing common_interface.o(i.Common_RollingCounterClear), (12 bytes).
    Removing common_interface.o(i.Common_Set_Act_E_Speed), (12 bytes).
    Removing common_interface.o(i.Common_Set_Act_E_Speed_Valid), (12 bytes).
    Removing common_interface.o(i.Common_Set_Act_V_Speed), (12 bytes).
    Removing common_interface.o(i.Common_Set_Act_V_Speed_Valid), (12 bytes).
    Removing common_interface.o(i.Common_Set_DispMode), (12 bytes).
    Removing common_interface.o(i.Common_Set_Disp_E_Speed), (12 bytes).
    Removing common_interface.o(i.Common_Set_Disp_E_Speed_Valid), (12 bytes).
    Removing common_interface.o(i.Common_Set_Disp_V_Speed), (12 bytes).
    Removing common_interface.o(i.Common_Set_Disp_V_Speed_Valid), (12 bytes).
    Removing common_interface.o(i.Common_Set_Gauges_E_Speed), (12 bytes).
    Removing mcu_core_protocol.o(.rev16_text), (4 bytes).
    Removing mcu_core_protocol.o(.revsh_text), (4 bytes).
    Removing mcu_core_protocol.o(i.Check_Event_Msg), (100 bytes).
    Removing mcu_core_protocol.o(i.Disable_Cyc_Msg), (24 bytes).
    Removing mcu_core_protocol.o(i.GetSocDispSts), (12 bytes).
    Removing mcu_core_protocol.o(i.Get_Event_Msg_Queue_Length), (12 bytes).
    Removing mcu_core_protocol.o(i.MCU_Send_Service), (184 bytes).
    Removing mcu_core_protocol.o(i.Send_Event_Msg), (148 bytes).
    Removing mcu_core_protocol.o(i.Send_To_Core), (132 bytes).
    Removing mcu_core_protocol.o(i.SetUartRxMsg_0x12), (28 bytes).
    Removing mcu_core_protocol.o(i.TFT_CreateCRCCheckSum), (72 bytes).
    Removing mcu_core_protocol.o(.constdata), (512 bytes).
    Removing telltales_user.o(.rev16_text), (4 bytes).
    Removing telltales_user.o(.revsh_text), (4 bytes).
    Removing telltales_user.o(.data), (6 bytes).
    Removing flash_synchronizer.o(.rev16_text), (4 bytes).
    Removing flash_synchronizer.o(.revsh_text), (4 bytes).
    Removing flash_synchronizer.o(i.Common_Get_Sync_Signal_Num), (12 bytes).
    Removing fuel.o(.rev16_text), (4 bytes).
    Removing fuel.o(.revsh_text), (4 bytes).
    Removing fuel.o(i.Get_Fuel_Disp_Byte), (108 bytes).
    Removing eemanager_interface.o(.rev16_text), (4 bytes).
    Removing eemanager_interface.o(.revsh_text), (4 bytes).
    Removing services_mileage_user.o(.rev16_text), (4 bytes).
    Removing services_mileage_user.o(.revsh_text), (4 bytes).
    Removing services_mileage_user.o(i.CalcODOIgnOffInit), (12 bytes).
    Removing services_mileage_user.o(i.CalcODO_50ms_Services), (212 bytes).
    Removing services_mileage_user.o(i.Data_Mileage_Clear), (56 bytes).
    Removing data_gear.o(.rev16_text), (4 bytes).
    Removing data_gear.o(.revsh_text), (4 bytes).
    Removing data_gear.o(i.Data_Service_Gear_Processing), (512 bytes).
    Removing data_gear.o(i.Get_Gear_Mode_Number), (12 bytes).
    Removing data_gear.o(.bss), (22 bytes).
    Removing data_gear.o(.constdata), (28 bytes).
    Removing backgroundlight.o(.rev16_text), (4 bytes).
    Removing backgroundlight.o(.revsh_text), (4 bytes).
    Removing backgroundlight.o(i.AD_SortShort), (48 bytes).
    Removing backgroundlight.o(i.AD_SwapShort), (20 bytes).
    Removing backgroundlight.o(i.BackLightDeal), (408 bytes).
    Removing backgroundlight.o(i.BackLightDeal_NTC), (268 bytes).
    Removing backgroundlight.o(i.Calculate_Thermistor), (160 bytes).
    Removing backgroundlight.o(i.SetBacklightCurVal), (16 bytes).
    Removing backgroundlight.o(i.SetBacklightDestVal), (16 bytes).
    Removing backgroundlight.o(i.SetBacklightMinVal), (16 bytes).
    Removing bglinterface.o(.rev16_text), (4 bytes).
    Removing bglinterface.o(.revsh_text), (4 bytes).
    Removing bglinterface.o(i.BGLPwm_Start), (24 bytes).
    Removing bglinterface.o(i.BGLPwm_Stop), (24 bytes).
    Removing bglinterface.o(i.ProcessLittleLight), (32 bytes).
    Removing bglinterface.o(i.SetBGLLvl), (72 bytes).
    Removing key.o(.rev16_text), (4 bytes).
    Removing key.o(.revsh_text), (4 bytes).
    Removing key.o(i.Key_Get_Current_Status), (16 bytes).
    Removing key.o(i.Key_Get_Status), (28 bytes).
    Removing key.o(i.Reset_Key_Status), (40 bytes).
    Removing can_communication_matrix.o(.rev16_text), (4 bytes).
    Removing can_communication_matrix.o(.revsh_text), (4 bytes).
    Removing can_communication_matrix.o(i.Get_ID_101_ECU_Engine_Temperature_State), (14 bytes).
    Removing can_communication_matrix.o(i.Get_ID_101_ECU_Vehicle_Speed), (12 bytes).
    Removing can_communication_matrix.o(i.Get_ID_111_ISG_Power_Enable), (16 bytes).
    Removing can_communication_matrix.o(i.Get_ID_113_Auto_High_Beam), (14 bytes).
    Removing can_communication_matrix.o(i.Get_ID_113_Tbatt), (12 bytes).
    Removing can_communication_matrix.o(i.Get_ID_125_Sig_TCS_SysState), (16 bytes).
    Removing can_communication_matrix.o(i.Get_ID_125_Sig_TCS_WarningLamp), (16 bytes).
    Removing can_communication_matrix.o(i.Get_ID_12B_Rear_Speed), (26 bytes).
    Removing can_communication_matrix.o(i.Get_ID_12B_Rear_Wheel_Speed_Validity), (16 bytes).
    Removing can_user.o(.rev16_text), (4 bytes).
    Removing can_user.o(.revsh_text), (4 bytes).
    Removing can_user.o(i.CAN_Check_Liandian), (44 bytes).
    Removing can_user.o(i.CAN_Init), (68 bytes).
    Removing can_user.o(i.CAN_SendAppMesageOpinion), (10 bytes).
    Removing can_user.o(i.Can_Set_Buff_502), (36 bytes).
    Removing can_user.o(i.DtcFaultTimeInit), (12 bytes).
    Removing can_user.o(i.GetDtcFault), (252 bytes).
    Removing can_user.o(i.Get_CanSleepDelayTime), (12 bytes).
    Removing can_user.o(i.Get_Mil_Signal_Connect), (12 bytes).
    Removing can_user.o(i.LianDianModuleIn), (12 bytes).
    Removing can_user.o(i.Set_TCS_WorkModeFlshTime), (12 bytes).
    Removing can_user.o(i.Test), (2 bytes).
    Removing can_user.o(i.getBUS_OFF_Status), (12 bytes).
    Removing can_user.o(i.get_Delay_ECU_Battery_Voltage), (116 bytes).
    Removing can_user.o(i.get_ID_ISG_BATT), (26 bytes).
    Removing can_user.o(i.get_ID_ISG_Power), (18 bytes).
    Removing can_user.o(i.swap32), (52 bytes).
    Removing app_telltales.o(.rev16_text), (4 bytes).
    Removing app_telltales.o(.revsh_text), (4 bytes).
    Removing app_telltales.o(i.App_Telltales_AllON), (26 bytes).
    Removing app_service.o(.rev16_text), (4 bytes).
    Removing app_service.o(.revsh_text), (4 bytes).
    Removing app_service.o(i.App_01_service), (44 bytes).
    Removing app_service.o(i.App_14_service), (60 bytes).
    Removing app_service.o(i.App_2F_service), (176 bytes).
    Removing app_service.o(i.App_31_service), (472 bytes).
    Removing app_service.o(i.App_34_service), (128 bytes).
    Removing app_service.o(i.App_36_service), (120 bytes).
    Removing app_service.o(i.App_37_service), (108 bytes).
    Removing app_service.o(i.App_59_service), (64 bytes).
    Removing app_service.o(i.App_Load_DTCNum), (34 bytes).
    Removing app_service.o(i.App_SequenceTimerOver), (36 bytes).
    Removing app_service.o(i.App_SetSequenceTimer), (14 bytes).
    Removing app_service.o(i.CalculateKeyLv11), (124 bytes).
    Removing app_service.o(i.Get_DiagnoCtl_CommCtl), (12 bytes).
    Removing app_service.o(.constdata), (4 bytes).
    Removing app_serviceproc.o(.rev16_text), (4 bytes).
    Removing app_serviceproc.o(.revsh_text), (4 bytes).
    Removing app_serviceproc.o(i.App_CreateCRCCheckSum), (58 bytes).
    Removing link_layer.o(.rev16_text), (4 bytes).
    Removing link_layer.o(.revsh_text), (4 bytes).
    Removing tp_layer.o(.rev16_text), (4 bytes).
    Removing tp_layer.o(.revsh_text), (4 bytes).
    Removing u2_app_service.o(.rev16_text), (4 bytes).
    Removing u2_app_service.o(.revsh_text), (4 bytes).
    Removing u2_app_service.o(i.U2_App_10_service), (2 bytes).
    Removing u2_app_service.o(i.U2_App_11_service), (2 bytes).
    Removing u2_app_service.o(i.U2_App_14_service), (2 bytes).
    Removing u2_app_service.o(i.U2_App_27_service), (2 bytes).
    Removing u2_app_service.o(i.U2_App_28_service), (2 bytes).
    Removing u2_app_service.o(i.U2_App_2E_service), (2 bytes).
    Removing u2_app_service.o(i.U2_App_2F_service), (2 bytes).
    Removing u2_app_service.o(i.U2_App_31_service), (2 bytes).
    Removing u2_app_service.o(i.U2_App_34_service), (2 bytes).
    Removing u2_app_service.o(i.U2_App_36_service), (2 bytes).
    Removing u2_app_service.o(i.U2_App_37_service), (2 bytes).
    Removing u2_app_service.o(i.U2_App_3E_service), (2 bytes).
    Removing u2_app_service.o(i.U2_App_85_service), (2 bytes).
    Removing u2_app_service.o(i.U2_App_Load_DTCNum), (34 bytes).
    Removing u2_app_service.o(i.U2_App_SequenceTimerOver), (36 bytes).
    Removing u2_app_service.o(i.U2_App_SetReUnlockTimer), (14 bytes).
    Removing u2_app_service.o(i.U2_App_SetSequenceTimer), (14 bytes).
    Removing u2_app_service.o(i.U2_App_SetSessionTimer), (14 bytes).
    Removing u2_app_serviceproc.o(.rev16_text), (4 bytes).
    Removing u2_app_serviceproc.o(.revsh_text), (4 bytes).
    Removing u2_app_serviceproc.o(i.U2_App_CreateCRCCheckSum), (58 bytes).
    Removing u2_link_layer.o(.rev16_text), (4 bytes).
    Removing u2_link_layer.o(.revsh_text), (4 bytes).
    Removing u2_tp_layer.o(.rev16_text), (4 bytes).
    Removing u2_tp_layer.o(.revsh_text), (4 bytes).
    Removing isr_bat32a239.o(.rev16_text), (4 bytes).
    Removing isr_bat32a239.o(.revsh_text), (4 bytes).
    Removing isr_bat32a239.o(i.iic00_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.iic01_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.iic10_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.iic11_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.iic20_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.iic21_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.iic30_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.iic31_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.intp0_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.intp10_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.intp11_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.intp1_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.intp2_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.intp3_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.intp4_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.intp5_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.intp6_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.intp7_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.intp8_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.intp9_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.spi00_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.spi01_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.spi10_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.spi11_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.spi20_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.spi21_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.spi30_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.spi31_interrupt), (12 bytes).
    Removing isr_bat32a239.o(i.uart0_interrupt_receive), (12 bytes).
    Removing isr_bat32a239.o(i.uart0_interrupt_send), (12 bytes).
    Removing isr_bat32a239.o(i.uart1_interrupt_receive), (12 bytes).
    Removing isr_bat32a239.o(i.uart1_interrupt_send), (12 bytes).
    Removing isr_bat32a239.o(i.uart2_interrupt_receive), (12 bytes).
    Removing isr_bat32a239.o(i.uart2_interrupt_send), (12 bytes).
    Removing isr_bat32a239.o(i.uart3_interrupt_receive), (12 bytes).
    Removing isr_bat32a239.o(i.uart3_interrupt_send), (12 bytes).
    Removing system_bat32a239.o(.rev16_text), (4 bytes).
    Removing system_bat32a239.o(.revsh_text), (4 bytes).
    Removing eeprommanage.o(.text), (0 bytes).
    Removing eeprommanage.o(.text.eeprom_getVersion), (68 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.eeprom_getVersion), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.eeprom_1ms_timeCount), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.eeprom_SetParameter), (8 bytes).
    Removing eeprommanage.o(.text.eeprom_getOdoLastWriteValue), (12 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.eeprom_getOdoLastWriteValue), (8 bytes).
    Removing eeprommanage.o(.text.eeprom_getOdoCurWriteAddress), (12 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.eeprom_getOdoCurWriteAddress), (8 bytes).
    Removing eeprommanage.o(.text.eeprom_getWriteState), (12 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.eeprom_getWriteState), (8 bytes).
    Removing eeprommanage.o(.text.eeprom_getReadState), (16 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.eeprom_getReadState), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.eeprom_ReadRecord), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.ee_IIC_SequentialRead), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.eeprom_WriteRecord), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.ee_IIC_SequentialWrite), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.eeprom_CreateCRC_8_Num), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.eeprom_OdoDecryption), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.eeprom_OdoEncryption), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.eeprom_WriteODO), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.eeprom_ReadODO), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.eeprom_ClearOdoSection), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.ee_IIC_Start), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.ee_IIC_Stop), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.ee_IIC_ACK), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.ee_IIC_NACK), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.ee_IIC_WaitAck), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.ee_IIC_SendByte), (8 bytes).
    Removing eeprommanage.o(.text.ee_IIC_RandomReadByte), (84 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.ee_IIC_RandomReadByte), (8 bytes).
    Removing eeprommanage.o(.ARM.exidx.text.ee_IIC_Read_8bit), (8 bytes).
    Removing can_signal_rx.o(i.CAN_RX_DiagCtrlEnable), (20 bytes).
    Removing can_signal_rx.o(i.CAN_RX_DiagCtrlRelease), (20 bytes).
    Removing can_signal_rx.o(i.CAN_RX_ReadEnableSts), (12 bytes).
    Removing can_signal_rx.o(i.Can_RX_ResetAllTimer), (36 bytes).
    Removing can_signal_rx.o(i.Can_RX_ResetTimer), (28 bytes).
    Removing can_signal_rx.o(i.Read_CAN_RX_Version), (4 bytes).
    Removing can_signal_rx.o(.constdata), (21 bytes).
    Removing can_signal_tx.o(i.CAN_TX_DiagCtrlEnable), (20 bytes).
    Removing can_signal_tx.o(i.CAN_TX_DiagCtrlRelease), (20 bytes).
    Removing can_signal_tx.o(i.CAN_TX_ReadEnableSts), (12 bytes).
    Removing can_signal_tx.o(i.Can_Msg_TX_FastInitCycle), (36 bytes).
    Removing can_signal_tx.o(i.Can_Msg_TX_SUCCESS), (48 bytes).
    Removing can_signal_tx.o(i.Can_Msg_Tx_Overwrite), (76 bytes).
    Removing can_signal_tx.o(i.Read_CAN_TX_Version), (4 bytes).
    Removing telltales_lib.o(i.Get_TelltalesLedSts), (20 bytes).
    Removing telltales_lib.o(i.Tel_VersionGet), (4 bytes).
    Removing telltales_lib.o(i.Telltales_DiagCtrl), (52 bytes).
    Removing telltales_lib.o(i.Telltales_DiagRelease), (40 bytes).
    Removing telltales_lib.o(i.Telltales_SetCheckFinish), (24 bytes).
    Removing telltales_lib.o(i.Test_LED_AllLight), (60 bytes).
    Removing is31_iic_master.o(i.bsp_IIC_nop), (4 bytes).

606 unused section(s) (total 40984 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    RESET                                    0x00000000   Section      192  startup_bat32a239.o(RESET)
    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/angel/boardlib.s                 0x00000000   Number         0  boardinit1.o ABSOLUTE
    ../clib/angel/boardlib.s                 0x00000000   Number         0  boardinit2.o ABSOLUTE
    ../clib/angel/boardlib.s                 0x00000000   Number         0  boardinit3.o ABSOLUTE
    ../clib/angel/boardlib.s                 0x00000000   Number         0  boardshut.o ABSOLUTE
    ../clib/angel/handlers.s                 0x00000000   Number         0  __scatter_zi.o ABSOLUTE
    ../clib/angel/kernel.s                   0x00000000   Number         0  rtexit.o ABSOLUTE
    ../clib/angel/kernel.s                   0x00000000   Number         0  rtexit2.o ABSOLUTE
    ../clib/angel/kernel.s                   0x00000000   Number         0  __rtentry4.o ABSOLUTE
    ../clib/angel/kernel.s                   0x00000000   Number         0  __rtentry2.o ABSOLUTE
    ../clib/angel/kernel.s                   0x00000000   Number         0  __rtentry.o ABSOLUTE
    ../clib/angel/rt.s                       0x00000000   Number         0  rt_raise.o ABSOLUTE
    ../clib/angel/rt.s                       0x00000000   Number         0  rt_div0.o ABSOLUTE
    ../clib/angel/rt.s                       0x00000000   Number         0  aeabi_ldiv0_sigfpe.o ABSOLUTE
    ../clib/angel/rt.s                       0x00000000   Number         0  aeabi_ldiv0.o ABSOLUTE
    ../clib/angel/rt.s                       0x00000000   Number         0  aeabi_idiv0_sigfpe.o ABSOLUTE
    ../clib/angel/rt.s                       0x00000000   Number         0  aeabi_idiv0.o ABSOLUTE
    ../clib/angel/scatterp.s                 0x00000000   Number         0  __scatter.o ABSOLUTE
    ../clib/angel/startup.s                  0x00000000   Number         0  __main.o ABSOLUTE
    ../clib/angel/sys.s                      0x00000000   Number         0  libspace.o ABSOLUTE
    ../clib/angel/sys.s                      0x00000000   Number         0  tempstk.o ABSOLUTE
    ../clib/angel/sys.s                      0x00000000   Number         0  use_no_semi.o ABSOLUTE
    ../clib/angel/sys.s                      0x00000000   Number         0  indicate_semi.o ABSOLUTE
    ../clib/angel/sys.s                      0x00000000   Number         0  sys_stackheap_outer.o ABSOLUTE
    ../clib/angel/sysapp.c                   0x00000000   Number         0  sys_exit.o ABSOLUTE
    ../clib/angel/sysapp.c                   0x00000000   Number         0  sys_wrch.o ABSOLUTE
    ../clib/angel/sysapp.c                   0x00000000   Number         0  sys_command.o ABSOLUTE
    ../clib/armsys.c                         0x00000000   Number         0  argv_veneer.o ABSOLUTE
    ../clib/armsys.c                         0x00000000   Number         0  no_argv.o ABSOLUTE
    ../clib/armsys.c                         0x00000000   Number         0  _get_argv_nomalloc.o ABSOLUTE
    ../clib/division.c                       0x00000000   Number         0  lludiv.o ABSOLUTE
    ../clib/division.s                       0x00000000   Number         0  aeabi_sdivfast.o ABSOLUTE
    ../clib/division.s                       0x00000000   Number         0  aeabi_sdivfast_div0.o ABSOLUTE
    ../clib/heapalloc.c                      0x00000000   Number         0  hrguard.o ABSOLUTE
    ../clib/heapaux.c                        0x00000000   Number         0  heapauxi.o ABSOLUTE
    ../clib/libinit.s                        0x00000000   Number         0  libshutdown.o ABSOLUTE
    ../clib/libinit.s                        0x00000000   Number         0  libinit.o ABSOLUTE
    ../clib/libinit.s                        0x00000000   Number         0  libshutdown2.o ABSOLUTE
    ../clib/libinit.s                        0x00000000   Number         0  libinit2.o ABSOLUTE
    ../clib/longlong.c                       0x00000000   Number         0  llmul.o ABSOLUTE
    ../clib/memcpset.c                       0x00000000   Number         0  rt_memclr.o ABSOLUTE
    ../clib/memcpset.c                       0x00000000   Number         0  rt_memcpy.o ABSOLUTE
    ../clib/memcpset.c                       0x00000000   Number         0  rt_memcpy.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_fpe_outer.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_fpe_formal.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  __raise.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_segv_inner.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_stak_inner.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_rtmem_outer.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_general.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_exit.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_rtmem_formal.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_pvfn_inner.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_other.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_cppl_inner.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_abrt_inner.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_rtred_inner.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_rtmem_inner.o ABSOLUTE
    ../clib/signal.c                         0x00000000   Number         0  defsig_fpe_inner.o ABSOLUTE
    ../clib/signal.s                         0x00000000   Number         0  defsig.o ABSOLUTE
    ../clib/stdlib.c                         0x00000000   Number         0  exit.o ABSOLUTE
    ../fplib/cfplib/fpinit.c                 0x00000000   Number         0  fpinit.o ABSOLUTE
    ..\src\CAN_Signal_Rx.c                   0x00000000   Number         0  can_signal_rx.o ABSOLUTE
    ..\src\CAN_Signal_Tx.c                   0x00000000   Number         0  can_signal_tx.o ABSOLUTE
    ..\src\Telltales_Lib.c                   0x00000000   Number         0  telltales_lib.o ABSOLUTE
    RTE\Device\BAT32A239KK64FB\isr_BAT32A239.c 0x00000000   Number         0  isr_bat32a239.o ABSOLUTE
    RTE\Device\BAT32A239KK64FB\startup_BAT32A239.s 0x00000000   Number         0  startup_bat32a239.o ABSOLUTE
    RTE\Device\BAT32A239KK64FB\system_BAT32A239.c 0x00000000   Number         0  system_bat32a239.o ABSOLUTE
    RTE\\Device\\BAT32A239KK64FB\\isr_BAT32A239.c 0x00000000   Number         0  isr_bat32a239.o ABSOLUTE
    RTE\\Device\\BAT32A239KK64FB\\system_BAT32A239.c 0x00000000   Number         0  system_bat32a239.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    eepromManage.c                           0x00000000   Number         0  eeprommanage.o ABSOLUTE
    source\Application\APPCan\CAN_Communication_Matrix.c 0x00000000   Number         0  can_communication_matrix.o ABSOLUTE
    source\Application\APPCan\CAN_User.c     0x00000000   Number         0  can_user.o ABSOLUTE
    source\Application\BackLight\BGLInterface.c 0x00000000   Number         0  bglinterface.o ABSOLUTE
    source\Application\BackLight\BackGroundLight.c 0x00000000   Number         0  backgroundlight.o ABSOLUTE
    source\Application\DataProcessor\Data_Gear.c 0x00000000   Number         0  data_gear.o ABSOLUTE
    source\Application\DataProcessor\Services_Mileage_User.c 0x00000000   Number         0  services_mileage_user.o ABSOLUTE
    source\Application\Eeprom\eeManager_Interface.c 0x00000000   Number         0  eemanager_interface.o ABSOLUTE
    source\Application\Fuel\Fuel.c           0x00000000   Number         0  fuel.o ABSOLUTE
    source\Application\Key\Key.c             0x00000000   Number         0  key.o ABSOLUTE
    source\Application\LINE_IN\Line_In.c     0x00000000   Number         0  line_in.o ABSOLUTE
    source\Application\MCU_Core_Protocol\MCU_Core_Protocol.c 0x00000000   Number         0  mcu_core_protocol.o ABSOLUTE
    source\Application\PowerManagement\PowerManagement.c 0x00000000   Number         0  powermanagement.o ABSOLUTE
    source\Application\PowerManagement\PowerManagement_user.c 0x00000000   Number         0  powermanagement_user.o ABSOLUTE
    source\Application\PowerManagement\System_Monitor.c 0x00000000   Number         0  system_monitor.o ABSOLUTE
    source\Application\PowerManagement\System_Monitor_user.c 0x00000000   Number         0  system_monitor_user.o ABSOLUTE
    source\Application\RTE\Common_Interface.c 0x00000000   Number         0  common_interface.o ABSOLUTE
    source\Application\RTE\RTE_ADC.c         0x00000000   Number         0  rte_adc.o ABSOLUTE
    source\Application\Telltales\Flash_synchronizer.c 0x00000000   Number         0  flash_synchronizer.o ABSOLUTE
    source\Application\Telltales\Telltales_user.c 0x00000000   Number         0  telltales_user.o ABSOLUTE
    source\Application\Telltales\app_Telltales.c 0x00000000   Number         0  app_telltales.o ABSOLUTE
    source\Driver\src\AW93015.c              0x00000000   Number         0  aw93015.o ABSOLUTE
    source\Driver\src\Analog_Circuits.c      0x00000000   Number         0  analog_circuits.o ABSOLUTE
    source\Driver\src\Analog_Signals.c       0x00000000   Number         0  analog_signals.o ABSOLUTE
    source\Driver\src\BU98R10.C              0x00000000   Number         0  bu98r10.o ABSOLUTE
    source\Driver\src\IS31FL3236.c           0x00000000   Number         0  is31fl3236.o ABSOLUTE
    source\Driver\src\IS31_IIC_Master.c      0x00000000   Number         0  is31_iic_master.o ABSOLUTE
    source\Driver\src\SEG_LCD.c              0x00000000   Number         0  seg_lcd.o ABSOLUTE
    source\Driver\src\Sys_Tick.c             0x00000000   Number         0  sys_tick.o ABSOLUTE
    source\Driver\src\adc.c                  0x00000000   Number         0  adc.o ABSOLUTE
    source\Driver\src\can.c                  0x00000000   Number         0  can.o ABSOLUTE
    source\Driver\src\clk.c                  0x00000000   Number         0  clk.o ABSOLUTE
    source\Driver\src\flash.c                0x00000000   Number         0  flash.o ABSOLUTE
    source\Driver\src\gpio.c                 0x00000000   Number         0  gpio.o ABSOLUTE
    source\Driver\src\intp.c                 0x00000000   Number         0  intp.o ABSOLUTE
    source\Driver\src\intp_user.c            0x00000000   Number         0  intp_user.o ABSOLUTE
    source\Driver\src\rtc.c                  0x00000000   Number         0  rtc.o ABSOLUTE
    source\Driver\src\sci.c                  0x00000000   Number         0  sci.o ABSOLUTE
    source\Driver\src\sci_user.c             0x00000000   Number         0  sci_user.o ABSOLUTE
    source\Driver\src\tim4.c                 0x00000000   Number         0  tim4.o ABSOLUTE
    source\Driver\src\timerA_B_C.c           0x00000000   Number         0  timera_b_c.o ABSOLUTE
    source\Driver\src\wdt.c                  0x00000000   Number         0  wdt.o ABSOLUTE
    source\System\init.c                     0x00000000   Number         0  init.o ABSOLUTE
    source\System\main.c                     0x00000000   Number         0  main.o ABSOLUTE
    source\System\sys_scheduler.c            0x00000000   Number         0  sys_scheduler.o ABSOLUTE
    source\System\tasks.c                    0x00000000   Number         0  tasks.o ABSOLUTE
    source\UDS2\U2_Link_Layer.c              0x00000000   Number         0  u2_link_layer.o ABSOLUTE
    source\UDS2\U2_TP_Layer.c                0x00000000   Number         0  u2_tp_layer.o ABSOLUTE
    source\UDS2\U2_app_Service.c             0x00000000   Number         0  u2_app_service.o ABSOLUTE
    source\UDS2\U2_app_ServiceProc.c         0x00000000   Number         0  u2_app_serviceproc.o ABSOLUTE
    source\UDS\Link_Layer.c                  0x00000000   Number         0  link_layer.o ABSOLUTE
    source\UDS\TP_Layer.c                    0x00000000   Number         0  tp_layer.o ABSOLUTE
    source\UDS\app_Service.c                 0x00000000   Number         0  app_service.o ABSOLUTE
    source\UDS\app_ServiceProc.c             0x00000000   Number         0  app_serviceproc.o ABSOLUTE
    source\\Application\\APPCan\\CAN_Communication_Matrix.c 0x00000000   Number         0  can_communication_matrix.o ABSOLUTE
    source\\Application\\APPCan\\CAN_User.c  0x00000000   Number         0  can_user.o ABSOLUTE
    source\\Application\\BackLight\\BGLInterface.c 0x00000000   Number         0  bglinterface.o ABSOLUTE
    source\\Application\\BackLight\\BackGroundLight.c 0x00000000   Number         0  backgroundlight.o ABSOLUTE
    source\\Application\\DataProcessor\\Data_Gear.c 0x00000000   Number         0  data_gear.o ABSOLUTE
    source\\Application\\DataProcessor\\Services_Mileage_User.c 0x00000000   Number         0  services_mileage_user.o ABSOLUTE
    source\\Application\\Eeprom\\eeManager_Interface.c 0x00000000   Number         0  eemanager_interface.o ABSOLUTE
    source\\Application\\Fuel\\Fuel.c        0x00000000   Number         0  fuel.o ABSOLUTE
    source\\Application\\Key\\Key.c          0x00000000   Number         0  key.o ABSOLUTE
    source\\Application\\LINE_IN\\Line_In.c  0x00000000   Number         0  line_in.o ABSOLUTE
    source\\Application\\MCU_Core_Protocol\\MCU_Core_Protocol.c 0x00000000   Number         0  mcu_core_protocol.o ABSOLUTE
    source\\Application\\PowerManagement\\PowerManagement.c 0x00000000   Number         0  powermanagement.o ABSOLUTE
    source\\Application\\PowerManagement\\PowerManagement_user.c 0x00000000   Number         0  powermanagement_user.o ABSOLUTE
    source\\Application\\PowerManagement\\System_Monitor.c 0x00000000   Number         0  system_monitor.o ABSOLUTE
    source\\Application\\PowerManagement\\System_Monitor_user.c 0x00000000   Number         0  system_monitor_user.o ABSOLUTE
    source\\Application\\RTE\\Common_Interface.c 0x00000000   Number         0  common_interface.o ABSOLUTE
    source\\Application\\RTE\\RTE_ADC.c      0x00000000   Number         0  rte_adc.o ABSOLUTE
    source\\Application\\Telltales\\Flash_synchronizer.c 0x00000000   Number         0  flash_synchronizer.o ABSOLUTE
    source\\Application\\Telltales\\Telltales_user.c 0x00000000   Number         0  telltales_user.o ABSOLUTE
    source\\Application\\Telltales\\app_Telltales.c 0x00000000   Number         0  app_telltales.o ABSOLUTE
    source\\Driver\\src\\AW93015.c           0x00000000   Number         0  aw93015.o ABSOLUTE
    source\\Driver\\src\\Analog_Circuits.c   0x00000000   Number         0  analog_circuits.o ABSOLUTE
    source\\Driver\\src\\Analog_Signals.c    0x00000000   Number         0  analog_signals.o ABSOLUTE
    source\\Driver\\src\\BU98R10.C           0x00000000   Number         0  bu98r10.o ABSOLUTE
    source\\Driver\\src\\IS31FL3236.c        0x00000000   Number         0  is31fl3236.o ABSOLUTE
    source\\Driver\\src\\IS31_IIC_Master.c   0x00000000   Number         0  is31_iic_master.o ABSOLUTE
    source\\Driver\\src\\SEG_LCD.c           0x00000000   Number         0  seg_lcd.o ABSOLUTE
    source\\Driver\\src\\Sys_Tick.c          0x00000000   Number         0  sys_tick.o ABSOLUTE
    source\\Driver\\src\\adc.c               0x00000000   Number         0  adc.o ABSOLUTE
    source\\Driver\\src\\can.c               0x00000000   Number         0  can.o ABSOLUTE
    source\\Driver\\src\\clk.c               0x00000000   Number         0  clk.o ABSOLUTE
    source\\Driver\\src\\flash.c             0x00000000   Number         0  flash.o ABSOLUTE
    source\\Driver\\src\\gpio.c              0x00000000   Number         0  gpio.o ABSOLUTE
    source\\Driver\\src\\intp.c              0x00000000   Number         0  intp.o ABSOLUTE
    source\\Driver\\src\\intp_user.c         0x00000000   Number         0  intp_user.o ABSOLUTE
    source\\Driver\\src\\rtc.c               0x00000000   Number         0  rtc.o ABSOLUTE
    source\\Driver\\src\\sci.c               0x00000000   Number         0  sci.o ABSOLUTE
    source\\Driver\\src\\sci_user.c          0x00000000   Number         0  sci_user.o ABSOLUTE
    source\\Driver\\src\\tim4.c              0x00000000   Number         0  tim4.o ABSOLUTE
    source\\Driver\\src\\timerA_B_C.c        0x00000000   Number         0  timera_b_c.o ABSOLUTE
    source\\Driver\\src\\wdt.c               0x00000000   Number         0  wdt.o ABSOLUTE
    source\\System\\init.c                   0x00000000   Number         0  init.o ABSOLUTE
    source\\System\\main.c                   0x00000000   Number         0  main.o ABSOLUTE
    source\\System\\sys_scheduler.c          0x00000000   Number         0  sys_scheduler.o ABSOLUTE
    source\\System\\tasks.c                  0x00000000   Number         0  tasks.o ABSOLUTE
    source\\UDS2\\U2_Link_Layer.c            0x00000000   Number         0  u2_link_layer.o ABSOLUTE
    source\\UDS2\\U2_TP_Layer.c              0x00000000   Number         0  u2_tp_layer.o ABSOLUTE
    source\\UDS2\\U2_app_Service.c           0x00000000   Number         0  u2_app_service.o ABSOLUTE
    source\\UDS2\\U2_app_ServiceProc.c       0x00000000   Number         0  u2_app_serviceproc.o ABSOLUTE
    source\\UDS\\Link_Layer.c                0x00000000   Number         0  link_layer.o ABSOLUTE
    source\\UDS\\TP_Layer.c                  0x00000000   Number         0  tp_layer.o ABSOLUTE
    source\\UDS\\app_Service.c               0x00000000   Number         0  app_service.o ABSOLUTE
    source\\UDS\\app_ServiceProc.c           0x00000000   Number         0  app_serviceproc.o ABSOLUTE
    .ARM.__AT_0x000000C0                     0x000000c0   Section        4  system_bat32a239.o(.ARM.__AT_0x000000C0)
    __tagsym$$used                           0x000000c0   Number         0  system_bat32a239.o(.ARM.__AT_0x000000C0)
    !!!main                                  0x000000c4   Section        8  __main.o(!!!main)
    !!!scatter                               0x000000cc   Section       60  __scatter.o(!!!scatter)
    !!handler_zi                             0x00000108   Section       28  __scatter_zi.o(!!handler_zi)
    .ARM.Collect$$libinit$$00000000          0x00000124   Section        2  libinit.o(.ARM.Collect$$libinit$$00000000)
    .ARM.Collect$$libinit$$00000002          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000002)
    .ARM.Collect$$libinit$$00000004          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000004)
    .ARM.Collect$$libinit$$0000000A          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$0000000A)
    .ARM.Collect$$libinit$$0000000C          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$0000000C)
    .ARM.Collect$$libinit$$0000000E          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$0000000E)
    .ARM.Collect$$libinit$$00000011          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000011)
    .ARM.Collect$$libinit$$00000013          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000013)
    .ARM.Collect$$libinit$$00000015          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000015)
    .ARM.Collect$$libinit$$00000017          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000017)
    .ARM.Collect$$libinit$$00000019          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000019)
    .ARM.Collect$$libinit$$0000001B          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$0000001B)
    .ARM.Collect$$libinit$$0000001D          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$0000001D)
    .ARM.Collect$$libinit$$0000001F          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$0000001F)
    .ARM.Collect$$libinit$$00000021          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000021)
    .ARM.Collect$$libinit$$00000023          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000023)
    .ARM.Collect$$libinit$$00000025          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000025)
    .ARM.Collect$$libinit$$0000002C          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$0000002C)
    .ARM.Collect$$libinit$$0000002E          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$0000002E)
    .ARM.Collect$$libinit$$00000030          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000030)
    .ARM.Collect$$libinit$$00000032          0x00000126   Section        0  libinit2.o(.ARM.Collect$$libinit$$00000032)
    .ARM.Collect$$libinit$$00000033          0x00000126   Section        2  libinit2.o(.ARM.Collect$$libinit$$00000033)
    .ARM.Collect$$libshutdown$$00000000      0x00000128   Section        2  libshutdown.o(.ARM.Collect$$libshutdown$$00000000)
    .ARM.Collect$$libshutdown$$00000002      0x0000012a   Section        0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000002)
    .ARM.Collect$$libshutdown$$00000004      0x0000012a   Section        0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000004)
    .ARM.Collect$$libshutdown$$00000006      0x0000012a   Section        0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000006)
    .ARM.Collect$$libshutdown$$00000009      0x0000012a   Section        0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000009)
    .ARM.Collect$$libshutdown$$0000000C      0x0000012a   Section        0  libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C)
    .ARM.Collect$$libshutdown$$0000000E      0x0000012a   Section        0  libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E)
    .ARM.Collect$$libshutdown$$00000011      0x0000012a   Section        0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000011)
    .ARM.Collect$$libshutdown$$00000012      0x0000012a   Section        2  libshutdown2.o(.ARM.Collect$$libshutdown$$00000012)
    .ARM.Collect$$rtentry$$00000000          0x0000012c   Section        0  __rtentry.o(.ARM.Collect$$rtentry$$00000000)
    .ARM.Collect$$rtentry$$00000002          0x0000012c   Section        0  __rtentry2.o(.ARM.Collect$$rtentry$$00000002)
    .ARM.Collect$$rtentry$$00000004          0x0000012c   Section        6  __rtentry4.o(.ARM.Collect$$rtentry$$00000004)
    .ARM.Collect$$rtentry$$00000009          0x00000132   Section        0  __rtentry2.o(.ARM.Collect$$rtentry$$00000009)
    .ARM.Collect$$rtentry$$0000000A          0x00000132   Section        4  __rtentry2.o(.ARM.Collect$$rtentry$$0000000A)
    .ARM.Collect$$rtentry$$0000000C          0x00000136   Section        0  __rtentry2.o(.ARM.Collect$$rtentry$$0000000C)
    .ARM.Collect$$rtentry$$0000000D          0x00000136   Section        8  __rtentry2.o(.ARM.Collect$$rtentry$$0000000D)
    .ARM.Collect$$rtexit$$00000000           0x0000013e   Section        2  rtexit.o(.ARM.Collect$$rtexit$$00000000)
    .ARM.Collect$$rtexit$$00000002           0x00000140   Section        0  rtexit2.o(.ARM.Collect$$rtexit$$00000002)
    .ARM.Collect$$rtexit$$00000003           0x00000140   Section        4  rtexit2.o(.ARM.Collect$$rtexit$$00000003)
    .ARM.Collect$$rtexit$$00000004           0x00000144   Section        6  rtexit2.o(.ARM.Collect$$rtexit$$00000004)
    .emb_text                                0x0000014c   Section       56  rt_memcpy.o(.emb_text)
    .text                                    0x00000184   Section      128  startup_bat32a239.o(.text)
    .text                                    0x00000204   Section        0  llmul.o(.text)
    .text                                    0x00000234   Section        0  lludiv.o(.text)
    .text                                    0x00000336   Section        0  rt_memcpy.o(.text)
    .text                                    0x000003b8   Section        0  rt_memclr.o(.text)
    .text                                    0x000003f8   Section      488  aeabi_sdivfast.o(.text)
    .text                                    0x000005e0   Section        0  heapauxi.o(.text)
    .text                                    0x000005e6   Section       62  sys_stackheap_outer.o(.text)
    .text                                    0x00000624   Section        0  exit.o(.text)
    .text                                    0x00000634   Section        8  libspace.o(.text)
    .text                                    0x0000063c   Section        0  sys_exit.o(.text)
    .text                                    0x00000648   Section        2  use_no_semi.o(.text)
    .text                                    0x0000064a   Section        0  indicate_semi.o(.text)
    .text                                    0x0000064a   Section        0  __dczerorl2.o(.text)
    [Anonymous Symbol]                       0x000006a0   Section        0  eeprommanage.o(.text.ee_IIC_ACK)
    [Anonymous Symbol]                       0x000006e4   Section        0  eeprommanage.o(.text.ee_IIC_NACK)
    [Anonymous Symbol]                       0x0000071a   Section        0  eeprommanage.o(.text.ee_IIC_Read_8bit)
    [Anonymous Symbol]                       0x00000768   Section        0  eeprommanage.o(.text.ee_IIC_SendByte)
    [Anonymous Symbol]                       0x000007be   Section        0  eeprommanage.o(.text.ee_IIC_SequentialRead)
    [Anonymous Symbol]                       0x00000848   Section        0  eeprommanage.o(.text.ee_IIC_SequentialWrite)
    [Anonymous Symbol]                       0x000008b0   Section        0  eeprommanage.o(.text.ee_IIC_Start)
    [Anonymous Symbol]                       0x000008f4   Section        0  eeprommanage.o(.text.ee_IIC_Stop)
    [Anonymous Symbol]                       0x00000938   Section        0  eeprommanage.o(.text.ee_IIC_WaitAck)
    __arm_cp.21_0                            0x00000980   Number         4  eeprommanage.o(.text.ee_IIC_WaitAck)
    [Anonymous Symbol]                       0x00000984   Section        0  eeprommanage.o(.text.eeprom_1ms_timeCount)
    __arm_cp.1_0                             0x00000994   Number         4  eeprommanage.o(.text.eeprom_1ms_timeCount)
    [Anonymous Symbol]                       0x00000998   Section        0  eeprommanage.o(.text.eeprom_ClearOdoSection)
    __arm_cp.16_0                            0x000009e8   Number         4  eeprommanage.o(.text.eeprom_ClearOdoSection)
    __arm_cp.16_1                            0x000009ec   Number         4  eeprommanage.o(.text.eeprom_ClearOdoSection)
    [Anonymous Symbol]                       0x000009f0   Section        0  eeprommanage.o(.text.eeprom_CreateCRC_8_Num)
    [Anonymous Symbol]                       0x00000a34   Section        0  eeprommanage.o(.text.eeprom_OdoDecryption)
    [Anonymous Symbol]                       0x00000b52   Section        0  eeprommanage.o(.text.eeprom_OdoEncryption)
    [Anonymous Symbol]                       0x00000c5c   Section        0  eeprommanage.o(.text.eeprom_ReadODO)
    __arm_cp.15_0                            0x00000e38   Number         4  eeprommanage.o(.text.eeprom_ReadODO)
    __arm_cp.15_1                            0x00000e3c   Number         4  eeprommanage.o(.text.eeprom_ReadODO)
    __arm_cp.15_2                            0x00000e40   Number         4  eeprommanage.o(.text.eeprom_ReadODO)
    __arm_cp.15_3                            0x00000e44   Number         4  eeprommanage.o(.text.eeprom_ReadODO)
    __arm_cp.15_4                            0x00000e48   Number         4  eeprommanage.o(.text.eeprom_ReadODO)
    __arm_cp.15_5                            0x00000e4c   Number         4  eeprommanage.o(.text.eeprom_ReadODO)
    [Anonymous Symbol]                       0x00000e50   Section        0  eeprommanage.o(.text.eeprom_ReadRecord)
    __arm_cp.7_0                             0x00000ee0   Number         4  eeprommanage.o(.text.eeprom_ReadRecord)
    __arm_cp.7_1                             0x00000ee4   Number         4  eeprommanage.o(.text.eeprom_ReadRecord)
    __arm_cp.7_2                             0x00000ee8   Number         4  eeprommanage.o(.text.eeprom_ReadRecord)
    [Anonymous Symbol]                       0x00000eec   Section        0  eeprommanage.o(.text.eeprom_SetParameter)
    __arm_cp.2_0                             0x00000f18   Number         4  eeprommanage.o(.text.eeprom_SetParameter)
    __arm_cp.2_1                             0x00000f1c   Number         4  eeprommanage.o(.text.eeprom_SetParameter)
    __arm_cp.2_2                             0x00000f20   Number         4  eeprommanage.o(.text.eeprom_SetParameter)
    __arm_cp.2_3                             0x00000f24   Number         4  eeprommanage.o(.text.eeprom_SetParameter)
    __arm_cp.2_4                             0x00000f28   Number         4  eeprommanage.o(.text.eeprom_SetParameter)
    [Anonymous Symbol]                       0x00000f2c   Section        0  eeprommanage.o(.text.eeprom_WriteODO)
    __arm_cp.14_0                            0x00001198   Number         4  eeprommanage.o(.text.eeprom_WriteODO)
    __arm_cp.14_1                            0x0000119c   Number         4  eeprommanage.o(.text.eeprom_WriteODO)
    __arm_cp.14_2                            0x000011a0   Number         4  eeprommanage.o(.text.eeprom_WriteODO)
    __arm_cp.14_3                            0x000011a4   Number         4  eeprommanage.o(.text.eeprom_WriteODO)
    __arm_cp.14_4                            0x000011a8   Number         4  eeprommanage.o(.text.eeprom_WriteODO)
    __arm_cp.14_5                            0x000011ac   Number         4  eeprommanage.o(.text.eeprom_WriteODO)
    __arm_cp.14_6                            0x000011b0   Number         4  eeprommanage.o(.text.eeprom_WriteODO)
    __arm_cp.14_7                            0x000011b4   Number         4  eeprommanage.o(.text.eeprom_WriteODO)
    __arm_cp.14_8                            0x000011b8   Number         4  eeprommanage.o(.text.eeprom_WriteODO)
    __arm_cp.14_9                            0x000011bc   Number         4  eeprommanage.o(.text.eeprom_WriteODO)
    __arm_cp.14_10                           0x000011c0   Number         4  eeprommanage.o(.text.eeprom_WriteODO)
    __arm_cp.14_11                           0x000011c4   Number         4  eeprommanage.o(.text.eeprom_WriteODO)
    __arm_cp.14_12                           0x000011c8   Number         4  eeprommanage.o(.text.eeprom_WriteODO)
    [Anonymous Symbol]                       0x000011cc   Section        0  eeprommanage.o(.text.eeprom_WriteRecord)
    __arm_cp.9_0                             0x000012e0   Number         4  eeprommanage.o(.text.eeprom_WriteRecord)
    __arm_cp.9_1                             0x000012e4   Number         4  eeprommanage.o(.text.eeprom_WriteRecord)
    __arm_cp.9_2                             0x000012e8   Number         4  eeprommanage.o(.text.eeprom_WriteRecord)
    __arm_cp.9_3                             0x000012ec   Number         4  eeprommanage.o(.text.eeprom_WriteRecord)
    __arm_cp.9_4                             0x000012f0   Number         4  eeprommanage.o(.text.eeprom_WriteRecord)
    __arm_cp.9_5                             0x000012f4   Number         4  eeprommanage.o(.text.eeprom_WriteRecord)
    __arm_cp.9_6                             0x000012f8   Number         4  eeprommanage.o(.text.eeprom_WriteRecord)
    __arm_cp.9_7                             0x000012fc   Number         4  eeprommanage.o(.text.eeprom_WriteRecord)
    i.ADC_Conv_Single_Channel                0x00001300   Section        0  analog_signals.o(i.ADC_Conv_Single_Channel)
    i.ADC_Data_Calibrate                     0x00001470   Section        0  analog_circuits.o(i.ADC_Data_Calibrate)
    i.ADC_Get_Conversion_Result              0x000014a4   Section        0  adc.o(i.ADC_Get_Conversion_Result)
    i.ADC_Get_Conversion_Status              0x000014d0   Section        0  adc.o(i.ADC_Get_Conversion_Status)
    i.ADC_Init                               0x000014dc   Section        0  adc.o(i.ADC_Init)
    i.ADC_Input_Voltage_Calc                 0x00001598   Section        0  analog_circuits.o(i.ADC_Input_Voltage_Calc)
    i.ADC_Read_Signal                        0x000015cc   Section        0  analog_signals.o(i.ADC_Read_Signal)
    i.ADC_Read_Signal_Valid                  0x000015e4   Section        0  analog_signals.o(i.ADC_Read_Signal_Valid)
    i.ADC_Res_Calc_Circuit101                0x000015fc   Section        0  analog_circuits.o(i.ADC_Res_Calc_Circuit101)
    i.ADC_Start                              0x000016a8   Section        0  adc.o(i.ADC_Start)
    i.ADC_Start_Conversion                   0x000016dc   Section        0  adc.o(i.ADC_Start_Conversion)
    i.ADC_Stop                               0x00001704   Section        0  adc.o(i.ADC_Stop)
    i.ADC_Stop_Conversion                    0x00001734   Section        0  adc.o(i.ADC_Stop_Conversion)
    i.ADC_Voltage_Calc_Circuit101            0x0000173c   Section        0  analog_circuits.o(i.ADC_Voltage_Calc_Circuit101)
    i.ADC_Voltage_Calc_Circuit102            0x00001754   Section        0  analog_circuits.o(i.ADC_Voltage_Calc_Circuit102)
    i.APP_CAN_Init                           0x000017dc   Section        0  can_user.o(i.APP_CAN_Init)
    i.Analog_Signal_Conv_Init                0x00001844   Section        0  analog_signals.o(i.Analog_Signal_Conv_Init)
    i.Analog_Signal_Conv_Real_Time_Run       0x000018a4   Section        0  adc.o(i.Analog_Signal_Conv_Real_Time_Run)
    i.Analog_Signal_Conv_Service             0x00001910   Section        0  analog_signals.o(i.Analog_Signal_Conv_Service)
    i.Analog_Signal_Conv_Stop                0x00001b64   Section        0  analog_signals.o(i.Analog_Signal_Conv_Stop)
    i.App_10_service                         0x00001ba0   Section        0  app_service.o(i.App_10_service)
    i.App_11_Reset_handle                    0x00001e28   Section        0  app_serviceproc.o(i.App_11_Reset_handle)
    i.App_11_service                         0x00001e7c   Section        0  app_service.o(i.App_11_service)
    i.App_22_service                         0x00001f58   Section        0  app_service.o(i.App_22_service)
    i.App_27_service                         0x000021b4   Section        0  app_service.o(i.App_27_service)
    i.App_28_service                         0x00002500   Section        0  app_service.o(i.App_28_service)
    i.App_2E_service                         0x000025cc   Section        0  app_service.o(i.App_2E_service)
    i.App_3E_service                         0x00002688   Section        0  app_service.o(i.App_3E_service)
    i.App_85_service                         0x00002718   Section        0  app_service.o(i.App_85_service)
    i.App_CopyRam                            0x000027e0   Section        0  app_serviceproc.o(i.App_CopyRam)
    i.App_ErrorInfoInit                      0x000027f8   Section        0  app_serviceproc.o(i.App_ErrorInfoInit)
    i.App_Load_DID                           0x0000280c   Section        0  app_serviceproc.o(i.App_Load_DID)
    i.App_ReUnlockTimerOver                  0x00002822   Section        0  app_service.o(i.App_ReUnlockTimerOver)
    i.App_SessionTimerOver                   0x00002846   Section        0  app_service.o(i.App_SessionTimerOver)
    i.App_SetReUnlockTimer                   0x0000286a   Section        0  app_service.o(i.App_SetReUnlockTimer)
    i.App_SetSessionTimer                    0x00002878   Section        0  app_service.o(i.App_SetSessionTimer)
    i.App_Telltales_AllOFF                   0x00002886   Section        0  app_telltales.o(i.App_Telltales_AllOFF)
    i.App_Telltales_Ctrl                     0x000028a0   Section        0  app_telltales.o(i.App_Telltales_Ctrl)
    i.BGLPwm_Config                          0x000028d0   Section        0  bglinterface.o(i.BGLPwm_Config)
    i.BGTask                                 0x000028f0   Section        0  bglinterface.o(i.BGTask)
    i.BU98R10_All_Command_Write              0x00002940   Section        0  bu98r10.o(i.BU98R10_All_Command_Write)
    i.BU98R10_All_Data_Write                 0x00002a38   Section        0  bu98r10.o(i.BU98R10_All_Data_Write)
    i.BU98R10_Init                           0x00002b40   Section        0  bu98r10.o(i.BU98R10_Init)
    i.BU98R10_Shutdown                       0x00002c60   Section        0  bu98r10.o(i.BU98R10_Shutdown)
    i.BU98R10_Update_Request                 0x00002c6c   Section        0  bu98r10.o(i.BU98R10_Update_Request)
    i.BU98R10_Update_Service                 0x00002c88   Section        0  bu98r10.o(i.BU98R10_Update_Service)
    i.BackLightDamp                          0x00002dc0   Section        0  backgroundlight.o(i.BackLightDamp)
    i.BackLightSchedu                        0x00003058   Section        0  bglinterface.o(i.BackLightSchedu)
    i.BatteryVoltageDelayInit                0x0000309c   Section        0  can_user.o(i.BatteryVoltageDelayInit)
    i.CAN0Err_Interrupt                      0x000030b4   Section        0  isr_bat32a239.o(i.CAN0Err_Interrupt)
    i.CAN0Rec_Interrupt                      0x000030c0   Section        0  isr_bat32a239.o(i.CAN0Rec_Interrupt)
    i.CAN0Trx_Interrupt                      0x000030c8   Section        0  isr_bat32a239.o(i.CAN0Trx_Interrupt)
    i.CAN0Wup_Interrupt                      0x000030d0   Section        0  isr_bat32a239.o(i.CAN0Wup_Interrupt)
    i.CAN1Err_Interrupt                      0x000030dc   Section        0  isr_bat32a239.o(i.CAN1Err_Interrupt)
    i.CAN1Rec_Interrupt                      0x000030e8   Section        0  isr_bat32a239.o(i.CAN1Rec_Interrupt)
    i.CAN1Trx_Interrupt                      0x000030f4   Section        0  isr_bat32a239.o(i.CAN1Trx_Interrupt)
    i.CAN1Wup_Interrupt                      0x00003100   Section        0  isr_bat32a239.o(i.CAN1Wup_Interrupt)
    i.CAN_LED_Check_50msTask                 0x0000310c   Section        0  can_user.o(i.CAN_LED_Check_50msTask)
    i.CAN_MSG_Read                           0x000031b4   Section        0  can_signal_rx.o(i.CAN_MSG_Read)
    i.CAN_MSG_Status                         0x000031e0   Section        0  can_signal_rx.o(i.CAN_MSG_Status)
    i.CAN_RX_SetEnable                       0x00003200   Section        0  can_signal_rx.o(i.CAN_RX_SetEnable)
    i.CAN_RX_Tick                            0x00003218   Section        0  can_user.o(i.CAN_RX_Tick)
    i.CAN_TX_SetEnable                       0x00003224   Section        0  can_signal_tx.o(i.CAN_TX_SetEnable)
    i.CAN_TX_Tick                            0x0000323c   Section        0  can_user.o(i.CAN_TX_Tick)
    i.CLK_GetCoreFreq                        0x00003248   Section        0  system_bat32a239.o(i.CLK_GetCoreFreq)
    i.CLK_GetfIHFreq                         0x000032ec   Section        0  system_bat32a239.o(i.CLK_GetfIHFreq)
    i.CLK_Osc_Setting                        0x0000339c   Section        0  clk.o(i.CLK_Osc_Setting)
    i.CLK_PLL_Setting                        0x00003420   Section        0  clk.o(i.CLK_PLL_Setting)
    i.CLK_PLL_Start                          0x00003464   Section        0  clk.o(i.CLK_PLL_Start)
    i.CalcODOKL15Init                        0x00003488   Section        0  services_mileage_user.o(i.CalcODOKL15Init)
    i.CalcODOKL30Init                        0x00003494   Section        0  services_mileage_user.o(i.CalcODOKL30Init)
    i.CalcODO_100ms_Services                 0x00003508   Section        0  services_mileage_user.o(i.CalcODO_100ms_Services)
    i.CalculateKey                           0x000036f0   Section        0  app_service.o(i.CalculateKey)
    i.CanMSg_XMS_Analysis                    0x0000376c   Section        0  can_signal_rx.o(i.CanMSg_XMS_Analysis)
    i.Can_BusOffRecover                      0x00003934   Section        0  can_user.o(i.Can_BusOffRecover)
    i.Can_BusOff_Fun                         0x00003950   Section        0  can_user.o(i.Can_BusOff_Fun)
    i.Can_RX_BuffInit                        0x00003a24   Section        0  can_signal_rx.o(i.Can_RX_BuffInit)
    i.Can_Receive_Msg                        0x00003ad0   Section        0  can_user.o(i.Can_Receive_Msg)
    i.Can_Set_Buff_105                       0x00003aec   Section        0  can_user.o(i.Can_Set_Buff_105)
    i.Can_Set_Buff_450                       0x00003b30   Section        0  can_user.o(i.Can_Set_Buff_450)
    i.Can_Set_Buff_510                       0x00003b48   Section        0  can_user.o(i.Can_Set_Buff_510)
    i.Can_Set_Buff_515                       0x00003ba8   Section        0  can_user.o(i.Can_Set_Buff_515)
    i.Can_Set_Buff_51C                       0x00003d4c   Section        0  can_user.o(i.Can_Set_Buff_51C)
    i.Can_Set_Buff_522                       0x00003d6c   Section        0  can_user.o(i.Can_Set_Buff_522)
    i.Can_Set_Buff_523                       0x00003e6c   Section        0  can_user.o(i.Can_Set_Buff_523)
    i.Can_TX_BuffInit                        0x00003f78   Section        0  can_signal_tx.o(i.Can_TX_BuffInit)
    i.Can_User_Time_Service                  0x00004130   Section        0  can_user.o(i.Can_User_Time_Service)
    i.Can_Write                              0x000041bc   Section        0  can_user.o(i.Can_Write)
    i.Can_Write_Fun                          0x000042cc   Section        0  can_signal_tx.o(i.Can_Write_Fun)
    i.Capture_Stop                           0x0000465c   Section        0  tim4.o(i.Capture_Stop)
    i.Clock_Init                             0x00004804   Section        0  clk.o(i.Clock_Init)
    i.Co_Can_Buff_Set                        0x00004844   Section        0  can_signal_rx.o(i.Co_Can_Buff_Set)
    i.Co_Can_ConvertSubID                    0x000048c0   Section        0  can_communication_matrix.o(i.Co_Can_ConvertSubID)
    i.Common_DataInit                        0x00004924   Section        0  common_interface.o(i.Common_DataInit)
    i.Common_GetIgnOffTime                   0x000049b0   Section        0  common_interface.o(i.Common_GetIgnOffTime)
    i.Common_GetIgnOnTime                    0x000049bc   Section        0  common_interface.o(i.Common_GetIgnOnTime)
    i.Common_Get_DispMode                    0x000049c8   Section        0  common_interface.o(i.Common_Get_DispMode)
    i.Common_Get_Disp_E_Speed                0x000049d4   Section        0  common_interface.o(i.Common_Get_Disp_E_Speed)
    i.Common_Get_Disp_V_Speed                0x000049e0   Section        0  common_interface.o(i.Common_Get_Disp_V_Speed)
    i.Common_Get_IG_Sts                      0x000049ec   Section        0  common_interface.o(i.Common_Get_IG_Sts)
    i.Common_Get_Language                    0x000049f8   Section        0  common_interface.o(i.Common_Get_Language)
    i.Common_Input_Para                      0x00004a04   Section        0  common_interface.o(i.Common_Input_Para)
    i.Common_SetSelfcheckStart               0x00004a64   Section        0  common_interface.o(i.Common_SetSelfcheckStart)
    i.Common_Set_IG_Sts                      0x00004a70   Section        0  common_interface.o(i.Common_Set_IG_Sts)
    i.Data_Clear_Trip                        0x00004a7c   Section        0  services_mileage_user.o(i.Data_Clear_Trip)
    i.Data_Gear_KL15_Init                    0x00004aac   Section        0  data_gear.o(i.Data_Gear_KL15_Init)
    i.Data_Gear_KL30_Init                    0x00004ab8   Section        0  data_gear.o(i.Data_Gear_KL30_Init)
    i.Data_ODO_Read                          0x00004abc   Section        0  services_mileage_user.o(i.Data_ODO_Read)
    i.Data_Read_Trip                         0x00004ac8   Section        0  services_mileage_user.o(i.Data_Read_Trip)
    i.DelfuModuleIn                          0x00004ae4   Section        0  can_user.o(i.DelfuModuleIn)
    i.Diag_Req_Send                          0x00004af0   Section        0  can_user.o(i.Diag_Req_Send)
    i.Diagno_Tick                            0x00004c6c   Section        0  app_serviceproc.o(i.Diagno_Tick)
    i.DiagnosisInit_main                     0x00004d58   Section        0  app_service.o(i.DiagnosisInit_main)
    i.Diagnosis_main                         0x00004de4   Section        0  app_service.o(i.Diagnosis_main)
    i.Drive_Info_Display_Update_Service      0x00005080   Section        0  mcu_core_protocol.o(i.Drive_Info_Display_Update_Service)
    i.DtcFaultInit                           0x00005148   Section        0  can_user.o(i.DtcFaultInit)
    i.EE_FeedDog                             0x00005164   Section        0  eemanager_interface.o(i.EE_FeedDog)
    i.EE_NOP                                 0x0000516c   Section        0  eemanager_interface.o(i.EE_NOP)
    i.EE_SCL_OUT                             0x00005170   Section        0  eemanager_interface.o(i.EE_SCL_OUT)
    i.EE_SCL_OutConfig                       0x0000518c   Section        0  eemanager_interface.o(i.EE_SCL_OutConfig)
    i.EE_SDA_GetValue                        0x0000519a   Section        0  eemanager_interface.o(i.EE_SDA_GetValue)
    i.EE_SDA_InConfig                        0x000051b0   Section        0  eemanager_interface.o(i.EE_SDA_InConfig)
    i.EE_SDA_OUT                             0x000051be   Section        0  eemanager_interface.o(i.EE_SDA_OUT)
    i.EE_SDA_OutConfig                       0x000051da   Section        0  eemanager_interface.o(i.EE_SDA_OutConfig)
    i.Enable_Cyc_Msg                         0x000051e8   Section        0  mcu_core_protocol.o(i.Enable_Cyc_Msg)
    i.Flash_Sync_Signal_Generation_Service   0x00005200   Section        0  flash_synchronizer.o(i.Flash_Sync_Signal_Generation_Service)
    i.Fuel_Cal_Sevice                        0x00005288   Section        0  fuel.o(i.Fuel_Cal_Sevice)
    i.Fuel_Gauges_Cal                        0x000052a0   Section        0  fuel.o(i.Fuel_Gauges_Cal)
    i.Fuel_KL15_Init                         0x0000555c   Section        0  fuel.o(i.Fuel_KL15_Init)
    i.Fuel_KL30_Init                         0x000055c0   Section        0  fuel.o(i.Fuel_KL30_Init)
    i.Fuel_R_Cal                             0x000055cc   Section        0  fuel.o(i.Fuel_R_Cal)
    i.Fuel_State_Check                       0x000056a8   Section        0  fuel.o(i.Fuel_State_Check)
    i.GET_Key_Prosess                        0x000057b8   Section        0  aw93015.o(i.GET_Key_Prosess)
    i.GPIO_Init                              0x00005818   Section        0  gpio.o(i.GPIO_Init)
    i.GetAllDtcFault                         0x00005dd4   Section        0  can_user.o(i.GetAllDtcFault)
    i.GetDtcAmnt                             0x00005ff0   Section        0  can_user.o(i.GetDtcAmnt)
    i.GetDtcDispNum                          0x00005ffc   Section        0  can_user.o(i.GetDtcDispNum)
    i.Get_Bcm_Module                         0x0000600c   Section        0  can_user.o(i.Get_Bcm_Module)
    i.Get_CH0_BusOffStatus                   0x00006018   Section        0  can.o(i.Get_CH0_BusOffStatus)
    i.Get_CurFuelSetp                        0x00006030   Section        0  fuel.o(i.Get_CurFuelSetp)
    i.Get_Day_Or_Night                       0x0000603c   Section        0  bglinterface.o(i.Get_Day_Or_Night)
    i.Get_Fuel_Sensor_State                  0x00006048   Section        0  fuel.o(i.Get_Fuel_Sensor_State)
    i.Get_ID_01_Data                         0x00006054   Section        0  mcu_core_protocol.o(i.Get_ID_01_Data)
    i.Get_ID_02_Data                         0x000063e8   Section        0  mcu_core_protocol.o(i.Get_ID_02_Data)
    i.Get_ID_101_ECU_Engine_Temperature      0x00006430   Section        0  can_communication_matrix.o(i.Get_ID_101_ECU_Engine_Temperature)
    i.Get_ID_111_ISG_Ready                   0x0000644a   Section        0  can_communication_matrix.o(i.Get_ID_111_ISG_Ready)
    i.Get_ID_111_Sig_ISG_SideStand           0x0000645a   Section        0  can_communication_matrix.o(i.Get_ID_111_Sig_ISG_SideStand)
    i.Get_ID_125_Sig_TCS_WorkMode            0x0000646a   Section        0  can_communication_matrix.o(i.Get_ID_125_Sig_TCS_WorkMode)
    i.Get_ID_401_Sig_ECU_Battery_Voltage     0x0000647a   Section        0  can_communication_matrix.o(i.Get_ID_401_Sig_ECU_Battery_Voltage)
    i.Get_ID_402_ECU_DTC1Amnt                0x00006486   Section        0  can_communication_matrix.o(i.Get_ID_402_ECU_DTC1Amnt)
    i.Get_ID_402_ECU_DTCH1                   0x00006492   Section        0  can_communication_matrix.o(i.Get_ID_402_ECU_DTCH1)
    i.Get_ID_402_ECU_DTCH2                   0x0000649e   Section        0  can_communication_matrix.o(i.Get_ID_402_ECU_DTCH2)
    i.Get_ID_402_ECU_DTCL1                   0x000064aa   Section        0  can_communication_matrix.o(i.Get_ID_402_ECU_DTCL1)
    i.Get_ID_402_ECU_DTCL2                   0x000064b6   Section        0  can_communication_matrix.o(i.Get_ID_402_ECU_DTCL2)
    i.Get_ID_402_ECU_DTCM1                   0x000064c2   Section        0  can_communication_matrix.o(i.Get_ID_402_ECU_DTCM1)
    i.Get_ID_402_ECU_DTCM2                   0x000064ce   Section        0  can_communication_matrix.o(i.Get_ID_402_ECU_DTCM2)
    i.Get_ID_55C_Sig_ClearTrip               0x000064da   Section        0  can_communication_matrix.o(i.Get_ID_55C_Sig_ClearTrip)
    i.Get_ID_55C_Sig_ModifyODOSts            0x000064ea   Section        0  can_communication_matrix.o(i.Get_ID_55C_Sig_ModifyODOSts)
    i.Get_ID_55C_Sig_ModifyODOValue          0x000064f6   Section        0  can_communication_matrix.o(i.Get_ID_55C_Sig_ModifyODOValue)
    i.Get_Key1_Line_In_Sts                   0x0000651a   Section        0  key.o(i.Get_Key1_Line_In_Sts)
    i.Get_Key2_Line_In_Sts                   0x00006530   Section        0  key.o(i.Get_Key2_Line_In_Sts)
    i.Get_LED_ECU_Battery_VoltageFlag        0x00006548   Section        0  can_user.o(i.Get_LED_ECU_Battery_VoltageFlag)
    i.Get_RSCAN0Busoff_Status                0x00006554   Section        0  can_user.o(i.Get_RSCAN0Busoff_Status)
    i.Get_RTC_Time                           0x00006560   Section        0  rtc.o(i.Get_RTC_Time)
    i.Get_ReqSilentTimer                     0x00006590   Section        0  can_user.o(i.Get_ReqSilentTimer)
    i.Get_TCS_WorkModeFlash                  0x0000659c   Section        0  can_user.o(i.Get_TCS_WorkModeFlash)
    i.Get_UDS_01_MsgRecFlg                   0x000065a8   Section        0  u2_app_service.o(i.Get_UDS_01_MsgRecFlg)
    i.Get_UDS_59_MsgRecFlg                   0x000065b4   Section        0  u2_app_service.o(i.Get_UDS_59_MsgRecFlg)
    i.Get_UDS_62_MsgRecFlg                   0x000065c0   Section        0  u2_app_service.o(i.Get_UDS_62_MsgRecFlg)
    i.IIC20_Stop                             0x000065cc   Section        0  sci.o(i.IIC20_Stop)
    i.IIC20_StopCondition                    0x000065f0   Section        0  sci.o(i.IIC20_StopCondition)
    i.IIC21_Stop                             0x0000665c   Section        0  sci.o(i.IIC21_Stop)
    i.IIC21_StopCondition                    0x00006684   Section        0  sci.o(i.IIC21_StopCondition)
    i.IIC2_SDA_OUT                           0x000066e8   Section        0  aw93015.o(i.IIC2_SDA_OUT)
    i.IIC_SDA2_IN                            0x000066fe   Section        0  aw93015.o(i.IIC_SDA2_IN)
    i.IIC_SDAGet                             0x0000670c   Section        0  is31_iic_master.o(i.IIC_SDAGet)
    i.INTP_Init                              0x00006724   Section        0  intp.o(i.INTP_Init)
    i.INTP_Start                             0x00006c28   Section        0  intp.o(i.INTP_Start)
    i.IRQ00_Handler                          0x00006d20   Section        0  isr_bat32a239.o(i.IRQ00_Handler)
    i.IRQ01_Handler                          0x00006d4c   Section        0  isr_bat32a239.o(i.IRQ01_Handler)
    i.IRQ02_Handler                          0x00006d6c   Section        0  isr_bat32a239.o(i.IRQ02_Handler)
    i.IRQ03_Handler                          0x00006d8c   Section        0  isr_bat32a239.o(i.IRQ03_Handler)
    i.IRQ04_Handler                          0x00006dac   Section        0  isr_bat32a239.o(i.IRQ04_Handler)
    i.IRQ05_Handler                          0x00006dcc   Section        0  isr_bat32a239.o(i.IRQ05_Handler)
    i.IRQ06_Handler                          0x00006dec   Section        0  isr_bat32a239.o(i.IRQ06_Handler)
    i.IRQ07_Handler                          0x00006e0c   Section        0  isr_bat32a239.o(i.IRQ07_Handler)
    i.IRQ08_Handler                          0x00006e2c   Section        0  isr_bat32a239.o(i.IRQ08_Handler)
    i.IRQ09_Handler                          0x00006e4c   Section        0  isr_bat32a239.o(i.IRQ09_Handler)
    i.IRQ10_Handler                          0x00006e70   Section        0  isr_bat32a239.o(i.IRQ10_Handler)
    i.IRQ11_Handler                          0x00006e84   Section        0  isr_bat32a239.o(i.IRQ11_Handler)
    i.IRQ12_Handler                          0x00006e98   Section        0  isr_bat32a239.o(i.IRQ12_Handler)
    i.IRQ13_Handler                          0x00006ebc   Section        0  isr_bat32a239.o(i.IRQ13_Handler)
    i.IRQ14_Handler                          0x00006ed0   Section        0  isr_bat32a239.o(i.IRQ14_Handler)
    i.IRQ15_Handler                          0x00006ee4   Section        0  isr_bat32a239.o(i.IRQ15_Handler)
    i.IRQ16_Handler                          0x00006f08   Section        0  isr_bat32a239.o(i.IRQ16_Handler)
    i.IRQ17_Handler                          0x00006f34   Section        0  isr_bat32a239.o(i.IRQ17_Handler)
    i.IRQ18_Handler                          0x00006f64   Section        0  isr_bat32a239.o(i.IRQ18_Handler)
    i.IRQ19_Handler                          0x00006f94   Section        0  isr_bat32a239.o(i.IRQ19_Handler)
    i.IRQ20_Handler                          0x00006fc4   Section        0  isr_bat32a239.o(i.IRQ20_Handler)
    i.IRQ21_Handler                          0x00006ff4   Section        0  isr_bat32a239.o(i.IRQ21_Handler)
    i.IRQ22_Handler                          0x00007008   Section        0  isr_bat32a239.o(i.IRQ22_Handler)
    i.IRQ23_Handler                          0x0000702c   Section        0  isr_bat32a239.o(i.IRQ23_Handler)
    i.IRQ24_Handler                          0x00007050   Section        0  isr_bat32a239.o(i.IRQ24_Handler)
    i.IRQ25_Handler                          0x00007070   Section        0  isr_bat32a239.o(i.IRQ25_Handler)
    i.IRQ26_Handler                          0x00007094   Section        0  isr_bat32a239.o(i.IRQ26_Handler)
    i.IRQ27_Handler                          0x000070b8   Section        0  isr_bat32a239.o(i.IRQ27_Handler)
    i.IRQ28_Handler                          0x000070cc   Section        0  isr_bat32a239.o(i.IRQ28_Handler)
    i.IRQ29_Handler                          0x000070e0   Section        0  isr_bat32a239.o(i.IRQ29_Handler)
    i.IRQ30_Handler                          0x00007104   Section        0  isr_bat32a239.o(i.IRQ30_Handler)
    i.IRQ31_Handler                          0x00007128   Section        0  isr_bat32a239.o(i.IRQ31_Handler)
    i.IS31FL3236_Init                        0x0000714c   Section        0  is31fl3236.o(i.IS31FL3236_Init)
    i.IS31FL3236_Update                      0x000073b8   Section        0  is31fl3236.o(i.IS31FL3236_Update)
    i.IS31_IIC_ACK                           0x00007564   Section        0  is31_iic_master.o(i.IS31_IIC_ACK)
    i.IS31_IIC_ReadByte                      0x0000759c   Section        0  is31_iic_master.o(i.IS31_IIC_ReadByte)
    i.IS31_IIC_SCL_Dir_Out                   0x000075ec   Section        0  is31_iic_master.o(i.IS31_IIC_SCL_Dir_Out)
    i.IS31_IIC_SDA_Dir_In                    0x0000763c   Section        0  is31_iic_master.o(i.IS31_IIC_SDA_Dir_In)
    i.IS31_IIC_SDA_Dir_Out                   0x0000764a   Section        0  is31_iic_master.o(i.IS31_IIC_SDA_Dir_Out)
    i.IS31_IIC_SendByte                      0x00007658   Section        0  is31_iic_master.o(i.IS31_IIC_SendByte)
    i.IS31_IIC_Start                         0x000076ae   Section        0  is31_iic_master.o(i.IS31_IIC_Start)
    i.IS31_IIC_Stop                          0x000076e6   Section        0  is31_iic_master.o(i.IS31_IIC_Stop)
    i.IS31_IIC_WaitAck                       0x00007720   Section        0  is31_iic_master.o(i.IS31_IIC_WaitAck)
    i.IS31_IIC_delay                         0x000077c8   Section        0  is31_iic_master.o(i.IS31_IIC_delay)
    i.IS31_OFF_Wakeup                        0x000077de   Section        0  is31fl3236.o(i.IS31_OFF_Wakeup)
    i.IS31_Set_SDB_Pin                       0x000077e8   Section        0  is31fl3236.o(i.IS31_Set_SDB_Pin)
    i.IS31_Shutdown                          0x00007804   Section        0  is31fl3236.o(i.IS31_Shutdown)
    i.Init93015_IIC                          0x00007810   Section        0  aw93015.o(i.Init93015_IIC)
    i.Key_Status_Detect_Service              0x0000789c   Section        0  key.o(i.Key_Status_Detect_Service)
    i.Key_Status_Init                        0x00007c98   Section        0  key.o(i.Key_Status_Init)
    i.LED_ABS_Execution                      0x00007ccc   Section        0  telltales_user.o(i.LED_ABS_Execution)
    i.LED_ABS_Judgement                      0x00007cf4   Section        0  telltales_user.o(i.LED_ABS_Judgement)
    i.LED_AutoStarStop_Execution             0x00007d10   Section        0  telltales_user.o(i.LED_AutoStarStop_Execution)
    i.LED_AutoStarStop_Judgement             0x00007d38   Section        0  telltales_user.o(i.LED_AutoStarStop_Judgement)
    i.LED_Auto_HI_BEAM_Execution             0x00007d54   Section        0  telltales_user.o(i.LED_Auto_HI_BEAM_Execution)
    i.LED_Auto_HI_BEAM_Judgement             0x00007d68   Section        0  telltales_user.o(i.LED_Auto_HI_BEAM_Judgement)
    i.LED_Batterylow_Execution               0x00007d78   Section        0  telltales_user.o(i.LED_Batterylow_Execution)
    i.LED_Batterylow_Judgement               0x00007da0   Section        0  telltales_user.o(i.LED_Batterylow_Judgement)
    i.LED_ENGINE_OIL_LOW_Execution           0x00007dce   Section        0  telltales_user.o(i.LED_ENGINE_OIL_LOW_Execution)
    i.LED_ENGINE_OIL_LOW_Judgement           0x00007df6   Section        0  telltales_user.o(i.LED_ENGINE_OIL_LOW_Judgement)
    i.LED_Fuel_Execution                     0x00007e06   Section        0  telltales_user.o(i.LED_Fuel_Execution)
    i.LED_Fuel_Judgement                     0x00007e5c   Section        0  telltales_user.o(i.LED_Fuel_Judgement)
    i.LED_HI_BEAM_Execution                  0x00007e9c   Section        0  telltales_user.o(i.LED_HI_BEAM_Execution)
    i.LED_HI_BEAM_Judgement                  0x00007ec4   Section        0  telltales_user.o(i.LED_HI_BEAM_Judgement)
    i.LED_LEFT_Execution                     0x00007ee0   Section        0  telltales_user.o(i.LED_LEFT_Execution)
    i.LED_LEFT_Judgement                     0x00007f08   Section        0  telltales_user.o(i.LED_LEFT_Judgement)
    i.LED_MIL_Execution                      0x00007f24   Section        0  telltales_user.o(i.LED_MIL_Execution)
    i.LED_MIL_Judgement                      0x00007f4c   Section        0  telltales_user.o(i.LED_MIL_Judgement)
    i.LED_READY_Execution                    0x00007f68   Section        0  telltales_user.o(i.LED_READY_Execution)
    i.LED_READY_Judgement                    0x00007f90   Section        0  telltales_user.o(i.LED_READY_Judgement)
    i.LED_RIGHT_Execution                    0x00007faa   Section        0  telltales_user.o(i.LED_RIGHT_Execution)
    i.LED_RIGHT_Judgement                    0x00007fd2   Section        0  telltales_user.o(i.LED_RIGHT_Judgement)
    i.LED_Shore_Execution                    0x00007fee   Section        0  telltales_user.o(i.LED_Shore_Execution)
    i.LED_Shore_Judgement                    0x00008016   Section        0  telltales_user.o(i.LED_Shore_Judgement)
    i.LED_TPMS_Execution                     0x00008030   Section        0  telltales_user.o(i.LED_TPMS_Execution)
    i.LED_TPMS_Judgement                     0x00008058   Section        0  telltales_user.o(i.LED_TPMS_Judgement)
    i.LED_TSC_Execution                      0x00008068   Section        0  telltales_user.o(i.LED_TSC_Execution)
    i.LED_TSC_Judgement                      0x0000806a   Section        0  telltales_user.o(i.LED_TSC_Judgement)
    i.LED_Temp_Execution                     0x00008078   Section        0  telltales_user.o(i.LED_Temp_Execution)
    i.LED_Temp_Judgement                     0x000080cc   Section        0  telltales_user.o(i.LED_Temp_Judgement)
    i.LINE_IN_Get_ABS                        0x000080e4   Section        0  line_in.o(i.LINE_IN_Get_ABS)
    i.LINE_IN_Get_AutoStarStop               0x000080fa   Section        0  line_in.o(i.LINE_IN_Get_AutoStarStop)
    i.LINE_IN_Get_HighBeam                   0x00008110   Section        0  line_in.o(i.LINE_IN_Get_HighBeam)
    i.LINE_IN_Get_LeftTurn                   0x00008126   Section        0  line_in.o(i.LINE_IN_Get_LeftTurn)
    i.LINE_IN_Get_OBD                        0x0000813c   Section        0  line_in.o(i.LINE_IN_Get_OBD)
    i.LINE_IN_Get_OilPressure                0x00008152   Section        0  line_in.o(i.LINE_IN_Get_OilPressure)
    i.LINE_IN_Get_RightTurn                  0x00008168   Section        0  line_in.o(i.LINE_IN_Get_RightTurn)
    i.LINE_IN_Get_TirePressure               0x0000817e   Section        0  line_in.o(i.LINE_IN_Get_TirePressure)
    i.LK_FillMsg                             0x00008194   Section        0  link_layer.o(i.LK_FillMsg)
    i.LK_Link_main                           0x000081a8   Section        0  link_layer.o(i.LK_Link_main)
    i.Line_In_Debounce_Handle                0x000081f8   Section        0  line_in.o(i.Line_In_Debounce_Handle)
    Line_In_Debounce_Handle                  0x000081f9   Thumb Code   200  line_in.o(i.Line_In_Debounce_Handle)
    i.Line_In_Debounce_Service               0x000082c8   Section        0  line_in.o(i.Line_In_Debounce_Service)
    i.Line_In_Get_Status                     0x00008320   Section        0  line_in.o(i.Line_In_Get_Status)
    i.Line_In_KL15_OFF_Init                  0x00008330   Section        0  line_in.o(i.Line_In_KL15_OFF_Init)
    i.Line_In_KL15_ON_Init                   0x00008370   Section        0  line_in.o(i.Line_In_KL15_ON_Init)
    i.Line_In_KL30_Init                      0x000083b0   Section        0  line_in.o(i.Line_In_KL30_Init)
    i.Mileage_Delay_ms                       0x000083e8   Section        0  services_mileage_user.o(i.Mileage_Delay_ms)
    i.PD_IIC_ReadPage                        0x0000840c   Section        0  aw93015.o(i.PD_IIC_ReadPage)
    i.PD_IIC_ReadReg                         0x000084b8   Section        0  aw93015.o(i.PD_IIC_ReadReg)
    i.PD_IIC_WritePage                       0x000084ec   Section        0  aw93015.o(i.PD_IIC_WritePage)
    i.PD_IIC_WriteReg                        0x000085a0   Section        0  aw93015.o(i.PD_IIC_WriteReg)
    PD_IIC_WriteReg                          0x000085a1   Thumb Code    44  aw93015.o(i.PD_IIC_WriteReg)
    i.PORT_ClrBit                            0x000085cc   Section        0  gpio.o(i.PORT_ClrBit)
    i.PORT_GetBit                            0x000085f0   Section        0  gpio.o(i.PORT_GetBit)
    i.PORT_Init                              0x0000860c   Section        0  gpio.o(i.PORT_Init)
    i.PORT_SetBit                            0x000087a4   Section        0  gpio.o(i.PORT_SetBit)
    i.PowerMemInit                           0x000087c8   Section        0  powermanagement.o(i.PowerMemInit)
    i.Power_IG_LVP_Init                      0x00008808   Section        0  powermanagement_user.o(i.Power_IG_LVP_Init)
    i.Power_IG_OFF_Init                      0x0000880c   Section        0  powermanagement_user.o(i.Power_IG_OFF_Init)
    i.Power_IG_ON_Init                       0x00008874   Section        0  powermanagement_user.o(i.Power_IG_ON_Init)
    i.Power_IG_OVP_Init                      0x000088d6   Section        0  powermanagement_user.o(i.Power_IG_OVP_Init)
    i.Power_KL30_Init                        0x000088d8   Section        0  powermanagement_user.o(i.Power_KL30_Init)
    i.Power_Management_Init                  0x000088f0   Section        0  powermanagement.o(i.Power_Management_Init)
    i.Power_Management_Lib_Init              0x00008918   Section        0  powermanagement_user.o(i.Power_Management_Lib_Init)
    i.Power_Management_Service               0x00008980   Section        0  powermanagement.o(i.Power_Management_Service)
    i.Power_Management_Service_user          0x00008aa4   Section        0  powermanagement_user.o(i.Power_Management_Service_user)
    i.Power_Sleep_Init                       0x00008abc   Section        0  powermanagement_user.o(i.Power_Sleep_Init)
    i.Power_Stay_OFF                         0x00008c24   Section        0  powermanagement_user.o(i.Power_Stay_OFF)
    i.Power_Stay_ON                          0x00008c80   Section        0  powermanagement_user.o(i.Power_Stay_ON)
    i.Power_Stay_Protect                     0x00008cb0   Section        0  powermanagement_user.o(i.Power_Stay_Protect)
    i.Power_Stay_Sleep                       0x00008cb4   Section        0  powermanagement_user.o(i.Power_Stay_Sleep)
    i.Power_Wakeup_Init                      0x00008cc0   Section        0  powermanagement_user.o(i.Power_Wakeup_Init)
    i.Protocol_KL15_ON_Init                  0x00008cfc   Section        0  mcu_core_protocol.o(i.Protocol_KL15_ON_Init)
    i.RTC_Get_CounterValue                   0x00008d18   Section        0  rtc.o(i.RTC_Get_CounterValue)
    i.RTC_Init                               0x00008d7c   Section        0  rtc.o(i.RTC_Init)
    i.RTC_Service                            0x00008e18   Section        0  rtc.o(i.RTC_Service)
    i.RTC_Set_CounterValue                   0x00008e28   Section        0  rtc.o(i.RTC_Set_CounterValue)
    i.RTC_Start                              0x00008e80   Section        0  rtc.o(i.RTC_Start)
    i.RTE_ForceRead_KL30_Voltage             0x00008ef4   Section        0  rte_adc.o(i.RTE_ForceRead_KL30_Voltage)
    i.RTE_Read_KL15_Voltage                  0x00008f04   Section        0  rte_adc.o(i.RTE_Read_KL15_Voltage)
    i.RTE_Read_KL30_Valid                    0x00008f14   Section        0  rte_adc.o(i.RTE_Read_KL30_Valid)
    i.RTE_Read_KL30_Voltage                  0x00008f24   Section        0  rte_adc.o(i.RTE_Read_KL30_Voltage)
    i.ReqSilentTimer100mSService             0x00008f34   Section        0  can_user.o(i.ReqSilentTimer100mSService)
    i.Reset_Mil_Signal_Time                  0x00008f4c   Section        0  can_user.o(i.Reset_Mil_Signal_Time)
    i.SEG_Coolant_Temp_Display               0x00008f64   Section        0  seg_lcd.o(i.SEG_Coolant_Temp_Display)
    i.SEG_Fuel_Level_Display                 0x000091ac   Section        0  seg_lcd.o(i.SEG_Fuel_Level_Display)
    i.SEG_LCD_ABS                            0x000093a8   Section        0  seg_lcd.o(i.SEG_LCD_ABS)
    i.SEG_LCD_AutoStarStop                   0x000093c0   Section        0  seg_lcd.o(i.SEG_LCD_AutoStarStop)
    i.SEG_LCD_Battery_Voltage_Display        0x000093d8   Section        0  seg_lcd.o(i.SEG_LCD_Battery_Voltage_Display)
    i.SEG_LCD_Battery_Voltage_Selftest       0x00009a5c   Section        0  seg_lcd.o(i.SEG_LCD_Battery_Voltage_Selftest)
    i.SEG_LCD_Batterylow                     0x00009e70   Section        0  seg_lcd.o(i.SEG_LCD_Batterylow)
    i.SEG_LCD_Engine_Speed_Seg_Display       0x00009e8c   Section        0  seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Display)
    i.SEG_LCD_Engine_Speed_Seg_Selftest      0x0000a744   Section        0  seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Selftest)
    i.SEG_LCD_Fuel                           0x0000aca4   Section        0  seg_lcd.o(i.SEG_LCD_Fuel)
    i.SEG_LCD_Gear_Display                   0x0000acc0   Section        0  seg_lcd.o(i.SEG_LCD_Gear_Display)
    i.SEG_LCD_Gear_Selftest                  0x0000aef8   Section        0  seg_lcd.o(i.SEG_LCD_Gear_Selftest)
    i.SEG_LCD_HI_BEAM                        0x0000b050   Section        0  seg_lcd.o(i.SEG_LCD_HI_BEAM)
    i.SEG_LCD_HighBeam                       0x0000b06c   Section        0  seg_lcd.o(i.SEG_LCD_HighBeam)
    i.SEG_LCD_Init                           0x0000b084   Section        0  seg_lcd.o(i.SEG_LCD_Init)
    i.SEG_LCD_LeftTurn                       0x0000b0d0   Section        0  seg_lcd.o(i.SEG_LCD_LeftTurn)
    i.SEG_LCD_OBD                            0x0000b0e8   Section        0  seg_lcd.o(i.SEG_LCD_OBD)
    i.SEG_LCD_ODO_Trip_Display               0x0000b104   Section        0  seg_lcd.o(i.SEG_LCD_ODO_Trip_Display)
    i.SEG_LCD_ODO_Trip_FaultCode_Selftest    0x0000bc24   Section        0  seg_lcd.o(i.SEG_LCD_ODO_Trip_FaultCode_Selftest)
    i.SEG_LCD_OilPressure                    0x0000c374   Section        0  seg_lcd.o(i.SEG_LCD_OilPressure)
    i.SEG_LCD_READY                          0x0000c390   Section        0  seg_lcd.o(i.SEG_LCD_READY)
    i.SEG_LCD_RightTurn                      0x0000c3a8   Section        0  seg_lcd.o(i.SEG_LCD_RightTurn)
    i.SEG_LCD_Shore                          0x0000c3c0   Section        0  seg_lcd.o(i.SEG_LCD_Shore)
    i.SEG_LCD_Shutdown                       0x0000c3dc   Section        0  seg_lcd.o(i.SEG_LCD_Shutdown)
    i.SEG_LCD_Temp                           0x0000c3f4   Section        0  seg_lcd.o(i.SEG_LCD_Temp)
    i.SEG_LCD_TirePressure                   0x0000c40c   Section        0  seg_lcd.o(i.SEG_LCD_TirePressure)
    i.SEG_LCD_Vehicle_Speed_Num_Display      0x0000c428   Section        0  seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Display)
    i.SEG_LCD_Vehicle_Speed_Num_Selftest     0x0000c7e4   Section        0  seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Selftest)
    i.SET_LED_ECU_Battery_VoltageFlag        0x0000ca84   Section        0  can_user.o(i.SET_LED_ECU_Battery_VoltageFlag)
    i.Selfcheck_Display_Update_Service       0x0000ca90   Section        0  mcu_core_protocol.o(i.Selfcheck_Display_Update_Service)
    i.Send_01_01                             0x0000cdc4   Section        0  can_user.o(i.Send_01_01)
    i.Send_19_0209                           0x0000cdf8   Section        0  can_user.o(i.Send_19_0209)
    i.Send_22_ID0005                         0x0000ce2e   Section        0  can_user.o(i.Send_22_ID0005)
    i.SetBGLNTCVol                           0x0000ce64   Section        0  bglinterface.o(i.SetBGLNTCVol)
    i.SetBGLTheme                            0x0000ce70   Section        0  bglinterface.o(i.SetBGLTheme)
    i.SetBGLType                             0x0000ce7c   Section        0  bglinterface.o(i.SetBGLType)
    i.SetBackLightOutput                     0x0000ce88   Section        0  backgroundlight.o(i.SetBackLightOutput)
    i.SetBaudRadio                           0x0000ce98   Section        0  can.o(i.SetBaudRadio)
    i.SetDtcFault                            0x0000cef0   Section        0  can_user.o(i.SetDtcFault)
    i.SetSendUdsTimeCount_0101               0x0000cffc   Section        0  can_user.o(i.SetSendUdsTimeCount_0101)
    i.SetSendUdsTimeCount_190209             0x0000d008   Section        0  can_user.o(i.SetSendUdsTimeCount_190209)
    i.SetSendUdsTimeCount_220005             0x0000d014   Section        0  can_user.o(i.SetSendUdsTimeCount_220005)
    i.Set_CanSleepDelayTime                  0x0000d020   Section        0  can_user.o(i.Set_CanSleepDelayTime)
    i.Set_ReqSilentTimer                     0x0000d02c   Section        0  can_user.o(i.Set_ReqSilentTimer)
    i.Set_TCS_WorkModeFlsh                   0x0000d038   Section        0  can_user.o(i.Set_TCS_WorkModeFlsh)
    i.Set_UDS_01_MsgRecFlg                   0x0000d044   Section        0  u2_app_service.o(i.Set_UDS_01_MsgRecFlg)
    i.Set_UDS_59_MsgRecFlg                   0x0000d050   Section        0  u2_app_service.o(i.Set_UDS_59_MsgRecFlg)
    i.Set_UDS_62_MsgRecFlg                   0x0000d05c   Section        0  u2_app_service.o(i.Set_UDS_62_MsgRecFlg)
    i.Simulated_IIC_2_Init                   0x0000d068   Section        0  is31_iic_master.o(i.Simulated_IIC_2_Init)
    i.SysTick_Handler                        0x0000d078   Section        0  sys_tick.o(i.SysTick_Handler)
    i.Sys_BlockDelay                         0x0000d108   Section        0  system_monitor_user.o(i.Sys_BlockDelay)
    i.Sys_Enter_Sleep_Mode                   0x0000d124   Section        0  clk.o(i.Sys_Enter_Sleep_Mode)
    i.Sys_Exact_100ms_Tasks                  0x0000d174   Section        0  tasks.o(i.Sys_Exact_100ms_Tasks)
    i.Sys_Exact_50us_Tasks                   0x0000d176   Section        0  tasks.o(i.Sys_Exact_50us_Tasks)
    i.Sys_Force_Read_KL30_Voltage            0x0000d178   Section        0  system_monitor_user.o(i.Sys_Force_Read_KL30_Voltage)
    i.Sys_Init                               0x0000d184   Section        0  sys_scheduler.o(i.Sys_Init)
    i.Sys_KL30_Init                          0x0000d1c0   Section        0  system_monitor_user.o(i.Sys_KL30_Init)
    i.Sys_LogicProcess                       0x0000d1e8   Section        0  system_monitor_user.o(i.Sys_LogicProcess)
    i.Sys_Read_KL30_Valid                    0x0000d1ea   Section        0  system_monitor_user.o(i.Sys_Read_KL30_Valid)
    i.Sys_Read_KL30_Voltage                  0x0000d1f6   Section        0  system_monitor_user.o(i.Sys_Read_KL30_Voltage)
    i.Sys_Run_Mode_100ms_Tasks_Group1        0x0000d20e   Section        0  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group1)
    i.Sys_Run_Mode_100ms_Tasks_Group10       0x0000d216   Section        0  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group10)
    i.Sys_Run_Mode_100ms_Tasks_Group2        0x0000d218   Section        0  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group2)
    i.Sys_Run_Mode_100ms_Tasks_Group3        0x0000d222   Section        0  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group3)
    i.Sys_Run_Mode_100ms_Tasks_Group4        0x0000d224   Section        0  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group4)
    i.Sys_Run_Mode_100ms_Tasks_Group5        0x0000d230   Section        0  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group5)
    i.Sys_Run_Mode_100ms_Tasks_Group6        0x0000d232   Section        0  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group6)
    i.Sys_Run_Mode_100ms_Tasks_Group7        0x0000d23a   Section        0  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group7)
    i.Sys_Run_Mode_100ms_Tasks_Group8        0x0000d248   Section        0  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group8)
    i.Sys_Run_Mode_100ms_Tasks_Group9        0x0000d250   Section        0  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group9)
    i.Sys_Run_Mode_10ms_Tasks                0x0000d252   Section        0  tasks.o(i.Sys_Run_Mode_10ms_Tasks)
    i.Sys_Run_Mode_20ms_Tasks                0x0000d27c   Section        0  tasks.o(i.Sys_Run_Mode_20ms_Tasks)
    i.Sys_Run_Mode_2ms_Tasks                 0x0000d28e   Section        0  tasks.o(i.Sys_Run_Mode_2ms_Tasks)
    i.Sys_Run_Mode_50ms_Tasks                0x0000d2a2   Section        0  tasks.o(i.Sys_Run_Mode_50ms_Tasks)
    i.Sys_Run_Mode_5ms_Tasks                 0x0000d2b6   Section        0  tasks.o(i.Sys_Run_Mode_5ms_Tasks)
    i.Sys_Run_Mode_Pseudo_Real_Time_Tasks    0x0000d2c0   Section        0  tasks.o(i.Sys_Run_Mode_Pseudo_Real_Time_Tasks)
    i.Sys_Scheduling_Service                 0x0000d2d8   Section        0  sys_scheduler.o(i.Sys_Scheduling_Service)
    i.Sys_Scheduling_Tmr                     0x0000d404   Section        0  sys_scheduler.o(i.Sys_Scheduling_Tmr)
    i.Sys_Set_DebounceTimer                  0x0000d598   Section        0  system_monitor.o(i.Sys_Set_DebounceTimer)
    i.Sys_Set_VolRange                       0x0000d5bc   Section        0  system_monitor.o(i.Sys_Set_VolRange)
    i.Sys_Startup_Init                       0x0000d624   Section        0  init.o(i.Sys_Startup_Init)
    i.Sys_Status_Update_Service              0x0000d69e   Section        0  system_monitor.o(i.Sys_Status_Update_Service)
    i.Sys_Tick_Timer_Start                   0x0000d6b0   Section        0  sys_tick.o(i.Sys_Tick_Timer_Start)
    i.Sys_Tick_Timer_Stop                    0x0000d714   Section        0  sys_tick.o(i.Sys_Tick_Timer_Stop)
    i.Sys_WakeUp_Init                        0x0000d728   Section        0  system_monitor_user.o(i.Sys_WakeUp_Init)
    i.SystemCoreClockUpdate                  0x0000d754   Section        0  system_bat32a239.o(i.SystemCoreClockUpdate)
    i.SystemInit                             0x0000d764   Section        0  system_bat32a239.o(i.SystemInit)
    i.System_Calc_FunRange                   0x0000d7f8   Section        0  system_monitor.o(i.System_Calc_FunRange)
    System_Calc_FunRange                     0x0000d7f9   Thumb Code    30  system_monitor.o(i.System_Calc_FunRange)
    i.System_Calc_NMRange                    0x0000d81c   Section        0  system_monitor.o(i.System_Calc_NMRange)
    System_Calc_NMRange                      0x0000d81d   Thumb Code    30  system_monitor.o(i.System_Calc_NMRange)
    i.System_FUN_KL15_Status_Get             0x0000d840   Section        0  system_monitor.o(i.System_FUN_KL15_Status_Get)
    i.System_FUN_KL30_Status_Get             0x0000d84c   Section        0  system_monitor.o(i.System_FUN_KL30_Status_Get)
    i.System_Fast_WakeUp                     0x0000d858   Section        0  system_monitor.o(i.System_Fast_WakeUp)
    i.System_Fun_Process                     0x0000d904   Section        0  system_monitor.o(i.System_Fun_Process)
    System_Fun_Process                       0x0000d905   Thumb Code   364  system_monitor.o(i.System_Fun_Process)
    i.System_LINE_KL15                       0x0000da8c   Section        0  system_monitor_user.o(i.System_LINE_KL15)
    i.System_Monitor_KL30Init                0x0000daa4   Section        0  system_monitor.o(i.System_Monitor_KL30Init)
    i.System_Monitor_WakeupInit              0x0000dbe8   Section        0  system_monitor.o(i.System_Monitor_WakeupInit)
    i.System_NM_Process                      0x0000dd10   Section        0  system_monitor.o(i.System_NM_Process)
    System_NM_Process                        0x0000dd11   Thumb Code   314  system_monitor.o(i.System_NM_Process)
    i.TMB0_PWM_Pin33_Freq_Duty               0x0000de60   Section        0  timera_b_c.o(i.TMB0_PWM_Pin33_Freq_Duty)
    i.TMB0_PWM_Pin33_Init                    0x0000dea0   Section        0  timera_b_c.o(i.TMB0_PWM_Pin33_Init)
    i.TMB0_Start                             0x0000df5c   Section        0  timera_b_c.o(i.TMB0_Start)
    i.TP_AbnormalInReqFC_handle              0x0000df90   Section        0  tp_layer.o(i.TP_AbnormalInReqFC_handle)
    i.TP_AbnormalInReqFF_handle              0x0000dfbc   Section        0  tp_layer.o(i.TP_AbnormalInReqFF_handle)
    i.TP_AbnormalInResCF_handle              0x0000dff8   Section        0  tp_layer.o(i.TP_AbnormalInResCF_handle)
    i.TP_AbnormalInResFC_handle              0x0000e024   Section        0  tp_layer.o(i.TP_AbnormalInResFC_handle)
    i.TP_AbnormalInResSF_handle              0x0000e050   Section        0  tp_layer.o(i.TP_AbnormalInResSF_handle)
    i.TP_BsTimerOver                         0x0000e09c   Section        0  tp_layer.o(i.TP_BsTimerOver)
    i.TP_Buffer_handle                       0x0000e0c0   Section        0  tp_layer.o(i.TP_Buffer_handle)
    i.TP_CalMsgLen                           0x0000e120   Section        0  tp_layer.o(i.TP_CalMsgLen)
    i.TP_CrTimerOver                         0x0000e14c   Section        0  tp_layer.o(i.TP_CrTimerOver)
    i.TP_NormalRecFC_handle                  0x0000e170   Section        0  tp_layer.o(i.TP_NormalRecFC_handle)
    i.TP_NormalSendFC_Fun                    0x0000e240   Section        0  tp_layer.o(i.TP_NormalSendFC_Fun)
    i.TP_ReciveMultiF_handle                 0x0000e2c4   Section        0  tp_layer.o(i.TP_ReciveMultiF_handle)
    i.TP_ReciveSF_handle                     0x0000e464   Section        0  tp_layer.o(i.TP_ReciveSF_handle)
    i.TP_STminTimerOver                      0x0000e4e8   Section        0  tp_layer.o(i.TP_STminTimerOver)
    i.TP_SetBsTimer                          0x0000e50c   Section        0  tp_layer.o(i.TP_SetBsTimer)
    i.TP_SetCrTimer                          0x0000e51a   Section        0  tp_layer.o(i.TP_SetCrTimer)
    i.TP_SetSTminTimer                       0x0000e528   Section        0  tp_layer.o(i.TP_SetSTminTimer)
    i.TP_TooShortDLC_handle                  0x0000e538   Section        0  tp_layer.o(i.TP_TooShortDLC_handle)
    i.TP_TransmitNegatePDU                   0x0000e5c8   Section        0  tp_layer.o(i.TP_TransmitNegatePDU)
    i.TP_TransmitPDU                         0x0000e688   Section        0  tp_layer.o(i.TP_TransmitPDU)
    i.TP_UnknownlPDU_handle                  0x0000e8a4   Section        0  tp_layer.o(i.TP_UnknownlPDU_handle)
    i.Telltales_IG_OFF_Work                  0x0000e8f0   Section        0  telltales_lib.o(i.Telltales_IG_OFF_Work)
    Telltales_IG_OFF_Work                    0x0000e8f1   Thumb Code   240  telltales_lib.o(i.Telltales_IG_OFF_Work)
    i.Telltales_IG_ON_Work                   0x0000e9e4   Section        0  telltales_lib.o(i.Telltales_IG_ON_Work)
    Telltales_IG_ON_Work                     0x0000e9e5   Thumb Code   666  telltales_lib.o(i.Telltales_IG_ON_Work)
    i.Telltales_Init                         0x0000ec84   Section        0  telltales_user.o(i.Telltales_Init)
    i.Telltales_KL15_Init                    0x0000ecb8   Section        0  telltales_lib.o(i.Telltales_KL15_Init)
    i.Telltales_KL30_Wakeup_Init             0x0000ecc8   Section        0  telltales_lib.o(i.Telltales_KL30_Wakeup_Init)
    i.Telltales_Management                   0x0000ed28   Section        0  telltales_lib.o(i.Telltales_Management)
    i.U2_App_01_service                      0x0000edf4   Section        0  u2_app_service.o(i.U2_App_01_service)
    i.U2_App_11_Reset_handle                 0x0000ee30   Section        0  u2_app_serviceproc.o(i.U2_App_11_Reset_handle)
    i.U2_App_59_service                      0x0000ee34   Section        0  u2_app_service.o(i.U2_App_59_service)
    i.U2_App_62_service                      0x0000ee94   Section        0  u2_app_service.o(i.U2_App_62_service)
    i.U2_App_CopyRam                         0x0000eee4   Section        0  u2_app_serviceproc.o(i.U2_App_CopyRam)
    i.U2_App_DtcMsgTimerOver                 0x0000eefc   Section        0  u2_app_service.o(i.U2_App_DtcMsgTimerOver)
    i.U2_App_ErrorInfoInit                   0x0000ef20   Section        0  u2_app_serviceproc.o(i.U2_App_ErrorInfoInit)
    i.U2_App_Load_DID                        0x0000ef34   Section        0  u2_app_serviceproc.o(i.U2_App_Load_DID)
    i.U2_App_ReUnlockTimerOver               0x0000ef4a   Section        0  u2_app_service.o(i.U2_App_ReUnlockTimerOver)
    i.U2_App_SessionTimerOver                0x0000ef6e   Section        0  u2_app_service.o(i.U2_App_SessionTimerOver)
    i.U2_App_SetDtcMsgTimer                  0x0000ef92   Section        0  u2_app_service.o(i.U2_App_SetDtcMsgTimer)
    i.U2_Diagno_Tick                         0x0000efa0   Section        0  u2_app_serviceproc.o(i.U2_Diagno_Tick)
    i.U2_DiagnosisInit_main                  0x0000f0b0   Section        0  u2_app_service.o(i.U2_DiagnosisInit_main)
    i.U2_Diagnosis_main                      0x0000f13c   Section        0  u2_app_service.o(i.U2_Diagnosis_main)
    i.U2_LK_FillMsg                          0x0000f340   Section        0  u2_link_layer.o(i.U2_LK_FillMsg)
    i.U2_LK_Link_main                        0x0000f354   Section        0  u2_link_layer.o(i.U2_LK_Link_main)
    i.U2_TP_AbnormalInReqFC_handle           0x0000f3d4   Section        0  u2_tp_layer.o(i.U2_TP_AbnormalInReqFC_handle)
    i.U2_TP_AbnormalInReqFF_handle           0x0000f400   Section        0  u2_tp_layer.o(i.U2_TP_AbnormalInReqFF_handle)
    i.U2_TP_AbnormalInResCF_handle           0x0000f43c   Section        0  u2_tp_layer.o(i.U2_TP_AbnormalInResCF_handle)
    i.U2_TP_AbnormalInResFC_handle           0x0000f468   Section        0  u2_tp_layer.o(i.U2_TP_AbnormalInResFC_handle)
    i.U2_TP_AbnormalInResSF_handle           0x0000f494   Section        0  u2_tp_layer.o(i.U2_TP_AbnormalInResSF_handle)
    i.U2_TP_BsTimerOver                      0x0000f4e0   Section        0  u2_tp_layer.o(i.U2_TP_BsTimerOver)
    i.U2_TP_Buffer_handle                    0x0000f504   Section        0  u2_tp_layer.o(i.U2_TP_Buffer_handle)
    i.U2_TP_CalMsgLen                        0x0000f564   Section        0  u2_tp_layer.o(i.U2_TP_CalMsgLen)
    i.U2_TP_CrTimerOver                      0x0000f590   Section        0  u2_tp_layer.o(i.U2_TP_CrTimerOver)
    i.U2_TP_NormalRecFC_handle               0x0000f5b4   Section        0  u2_tp_layer.o(i.U2_TP_NormalRecFC_handle)
    i.U2_TP_NormalSendFC_Fun                 0x0000f684   Section        0  u2_tp_layer.o(i.U2_TP_NormalSendFC_Fun)
    i.U2_TP_ReciveMultiF_handle              0x0000f708   Section        0  u2_tp_layer.o(i.U2_TP_ReciveMultiF_handle)
    i.U2_TP_ReciveSF_handle                  0x0000f8a8   Section        0  u2_tp_layer.o(i.U2_TP_ReciveSF_handle)
    i.U2_TP_STminTimerOver                   0x0000f92c   Section        0  u2_tp_layer.o(i.U2_TP_STminTimerOver)
    i.U2_TP_SetBsTimer                       0x0000f950   Section        0  u2_tp_layer.o(i.U2_TP_SetBsTimer)
    i.U2_TP_SetCrTimer                       0x0000f95e   Section        0  u2_tp_layer.o(i.U2_TP_SetCrTimer)
    i.U2_TP_SetSTminTimer                    0x0000f96c   Section        0  u2_tp_layer.o(i.U2_TP_SetSTminTimer)
    i.U2_TP_TooShortDLC_handle               0x0000f97c   Section        0  u2_tp_layer.o(i.U2_TP_TooShortDLC_handle)
    i.U2_TP_TransmitNegatePDU                0x0000fa0c   Section        0  u2_tp_layer.o(i.U2_TP_TransmitNegatePDU)
    i.U2_TP_TransmitPDU                      0x0000facc   Section        0  u2_tp_layer.o(i.U2_TP_TransmitPDU)
    i.U2_TP_UnknownlPDU_handle               0x0000fce8   Section        0  u2_tp_layer.o(i.U2_TP_UnknownlPDU_handle)
    i.WDT_Restart                            0x0000fd34   Section        0  wdt.o(i.WDT_Restart)
    i.__ARM_common_switch8                   0x0000fd40   Section        0  gpio.o(i.__ARM_common_switch8)
    i.__NVIC_ClearPendingIRQ                 0x0000fd5c   Section        0  adc.o(i.__NVIC_ClearPendingIRQ)
    __NVIC_ClearPendingIRQ                   0x0000fd5d   Thumb Code    18  adc.o(i.__NVIC_ClearPendingIRQ)
    i.__NVIC_ClearPendingIRQ                 0x0000fd74   Section        0  tim4.o(i.__NVIC_ClearPendingIRQ)
    __NVIC_ClearPendingIRQ                   0x0000fd75   Thumb Code    18  tim4.o(i.__NVIC_ClearPendingIRQ)
    i.__NVIC_SetPriority                     0x0000fd8c   Section        0  sys_tick.o(i.__NVIC_SetPriority)
    __NVIC_SetPriority                       0x0000fd8d   Thumb Code   110  sys_tick.o(i.__NVIC_SetPriority)
    i.adc_interrupt                          0x0000fe04   Section        0  isr_bat32a239.o(i.adc_interrupt)
    i.bsp_CAN0_Rev_isr                       0x0000fe10   Section        0  can.o(i.bsp_CAN0_Rev_isr)
    i.bsp_CAN0_Tx_isr                        0x0000ff24   Section        0  can.o(i.bsp_CAN0_Tx_isr)
    i.bsp_CANSendFrame                       0x0000ff44   Section        0  can.o(i.bsp_CANSendFrame)
    i.bsp_CAN_BusOff_Recover                 0x0000ffd8   Section        0  can.o(i.bsp_CAN_BusOff_Recover)
    i.bsp_CAN_Init                           0x000100d4   Section        0  can.o(i.bsp_CAN_Init)
    i.bsp_CAN_MaskCheck                      0x0001023c   Section        0  can.o(i.bsp_CAN_MaskCheck)
    i.bsp_CAN_Sleep                          0x00010280   Section        0  can.o(i.bsp_CAN_Sleep)
    i.bsp_CAN_SleepRelease                   0x00010290   Section        0  can.o(i.bsp_CAN_SleepRelease)
    i.bsp_CanBuf_Clear                       0x0001029c   Section        0  can.o(i.bsp_CanBuf_Clear)
    i.bsp_CanBuf_Init                        0x000102cc   Section        0  can.o(i.bsp_CanBuf_Init)
    i.bsp_IIC2_ACK                           0x0001038c   Section        0  aw93015.o(i.bsp_IIC2_ACK)
    i.bsp_IIC2_ReadByte                      0x000103b4   Section        0  aw93015.o(i.bsp_IIC2_ReadByte)
    i.bsp_IIC2_SendByte                      0x000103fc   Section        0  aw93015.o(i.bsp_IIC2_SendByte)
    i.bsp_IIC2_Start                         0x00010442   Section        0  aw93015.o(i.bsp_IIC2_Start)
    i.bsp_IIC2_Stop                          0x0001046a   Section        0  aw93015.o(i.bsp_IIC2_Stop)
    i.bsp_IIC2_WaitAck                       0x00010492   Section        0  aw93015.o(i.bsp_IIC2_WaitAck)
    i.bsp_IIC_SCL_out                        0x000104d8   Section        0  is31_iic_master.o(i.bsp_IIC_SCL_out)
    i.bsp_IIC_SDA_out                        0x00010514   Section        0  is31_iic_master.o(i.bsp_IIC_SDA_out)
    i.bsp_Is_CAN_Sleep                       0x00010550   Section        0  can.o(i.bsp_Is_CAN_Sleep)
    i.bsp_rx_mask_init                       0x00010590   Section        0  can.o(i.bsp_rx_mask_init)
    i.bsp_rx_msgbuf_init                     0x000105ec   Section        0  can.o(i.bsp_rx_msgbuf_init)
    i.bsp_tim4_01_isr_Handler                0x00010680   Section        0  tim4.o(i.bsp_tim4_01_isr_Handler)
    i.bsp_tim4_02_isr_Handler                0x000106b8   Section        0  tim4.o(i.bsp_tim4_02_isr_Handler)
    i.bsp_tx_msgbuf_abort                    0x000106c4   Section        0  can.o(i.bsp_tx_msgbuf_abort)
    i.bsp_tx_msgbuf_init                     0x000106dc   Section        0  can.o(i.bsp_tx_msgbuf_init)
    i.cmp0_interrupt                         0x00010738   Section        0  isr_bat32a239.o(i.cmp0_interrupt)
    i.cmp1_interrupt                         0x00010744   Section        0  isr_bat32a239.o(i.cmp1_interrupt)
    i.div_interrupt                          0x00010750   Section        0  isr_bat32a239.o(i.div_interrupt)
    i.eeprom_StoreInfo_Init                  0x0001075c   Section        0  eemanager_interface.o(i.eeprom_StoreInfo_Init)
    i.eeprom_comm_DelayUs                    0x00010770   Section        0  eemanager_interface.o(i.eeprom_comm_DelayUs)
    i.extend_i2c_write_one_byte              0x00010790   Section        0  is31fl3236.o(i.extend_i2c_write_one_byte)
    i.flash_interrupt                        0x000107c8   Section        0  isr_bat32a239.o(i.flash_interrupt)
    i.get_CoolantTempVal                     0x000107d4   Section        0  can_user.o(i.get_CoolantTempVal)
    i.get_ECU_Battery_Voltage                0x000107e2   Section        0  can_user.o(i.get_ECU_Battery_Voltage)
    i.get_ECU_Temperature_WaterVal           0x000107f4   Section        0  can_user.o(i.get_ECU_Temperature_WaterVal)
    i.iic20_callback_master_error            0x0001081c   Section        0  sci_user.o(i.iic20_callback_master_error)
    iic20_callback_master_error              0x0001081d   Thumb Code     2  sci_user.o(i.iic20_callback_master_error)
    i.iic20_callback_master_receiveend       0x00010820   Section        0  sci_user.o(i.iic20_callback_master_receiveend)
    iic20_callback_master_receiveend         0x00010821   Thumb Code    14  sci_user.o(i.iic20_callback_master_receiveend)
    i.iic20_callback_master_sendend          0x00010834   Section        0  sci_user.o(i.iic20_callback_master_sendend)
    iic20_callback_master_sendend            0x00010835   Thumb Code    14  sci_user.o(i.iic20_callback_master_sendend)
    i.iic20_interrupt                        0x00010848   Section        0  sci_user.o(i.iic20_interrupt)
    i.iic21_callback_master_error            0x000109bc   Section        0  sci_user.o(i.iic21_callback_master_error)
    iic21_callback_master_error              0x000109bd   Thumb Code     2  sci_user.o(i.iic21_callback_master_error)
    i.iic21_callback_master_receiveend       0x000109c0   Section        0  sci_user.o(i.iic21_callback_master_receiveend)
    iic21_callback_master_receiveend         0x000109c1   Thumb Code    14  sci_user.o(i.iic21_callback_master_receiveend)
    i.iic21_callback_master_sendend          0x000109d4   Section        0  sci_user.o(i.iic21_callback_master_sendend)
    iic21_callback_master_sendend            0x000109d5   Thumb Code    14  sci_user.o(i.iic21_callback_master_sendend)
    i.iic21_interrupt                        0x000109e8   Section        0  sci_user.o(i.iic21_interrupt)
    i.iica0_interrupt                        0x00010b5c   Section        0  isr_bat32a239.o(i.iica0_interrupt)
    i.iica1_interrupt                        0x00010b68   Section        0  isr_bat32a239.o(i.iica1_interrupt)
    i.intp0_callback                         0x00010b74   Section        0  intp_user.o(i.intp0_callback)
    intp0_callback                           0x00010b75   Thumb Code    12  intp_user.o(i.intp0_callback)
    i.intp0_interrupt                        0x00010b84   Section        0  intp_user.o(i.intp0_interrupt)
    i.intp10_callback                        0x00010b98   Section        0  intp_user.o(i.intp10_callback)
    intp10_callback                          0x00010b99   Thumb Code    12  intp_user.o(i.intp10_callback)
    i.intp10_interrupt                       0x00010ba8   Section        0  intp_user.o(i.intp10_interrupt)
    i.intp11_callback                        0x00010bbc   Section        0  intp_user.o(i.intp11_callback)
    intp11_callback                          0x00010bbd   Thumb Code    12  intp_user.o(i.intp11_callback)
    i.intp11_interrupt                       0x00010bcc   Section        0  intp_user.o(i.intp11_interrupt)
    i.intp1_callback                         0x00010be0   Section        0  intp_user.o(i.intp1_callback)
    intp1_callback                           0x00010be1   Thumb Code    12  intp_user.o(i.intp1_callback)
    i.intp1_interrupt                        0x00010bf0   Section        0  intp_user.o(i.intp1_interrupt)
    i.intp2_callback                         0x00010c04   Section        0  intp_user.o(i.intp2_callback)
    intp2_callback                           0x00010c05   Thumb Code    12  intp_user.o(i.intp2_callback)
    i.intp2_interrupt                        0x00010c14   Section        0  intp_user.o(i.intp2_interrupt)
    i.intp3_callback                         0x00010c28   Section        0  intp_user.o(i.intp3_callback)
    intp3_callback                           0x00010c29   Thumb Code    12  intp_user.o(i.intp3_callback)
    i.intp3_interrupt                        0x00010c38   Section        0  intp_user.o(i.intp3_interrupt)
    i.intp4_callback                         0x00010c4c   Section        0  intp_user.o(i.intp4_callback)
    intp4_callback                           0x00010c4d   Thumb Code    12  intp_user.o(i.intp4_callback)
    i.intp4_interrupt                        0x00010c5c   Section        0  intp_user.o(i.intp4_interrupt)
    i.intp5_callback                         0x00010c70   Section        0  intp_user.o(i.intp5_callback)
    intp5_callback                           0x00010c71   Thumb Code    12  intp_user.o(i.intp5_callback)
    i.intp5_interrupt                        0x00010c80   Section        0  intp_user.o(i.intp5_interrupt)
    i.intp6_callback                         0x00010c94   Section        0  intp_user.o(i.intp6_callback)
    intp6_callback                           0x00010c95   Thumb Code    12  intp_user.o(i.intp6_callback)
    i.intp6_interrupt                        0x00010ca4   Section        0  intp_user.o(i.intp6_interrupt)
    i.intp7_callback                         0x00010cb8   Section        0  intp_user.o(i.intp7_callback)
    intp7_callback                           0x00010cb9   Thumb Code    12  intp_user.o(i.intp7_callback)
    i.intp7_interrupt                        0x00010cc8   Section        0  intp_user.o(i.intp7_interrupt)
    i.intp8_callback                         0x00010cdc   Section        0  intp_user.o(i.intp8_callback)
    intp8_callback                           0x00010cdd   Thumb Code    12  intp_user.o(i.intp8_callback)
    i.intp8_interrupt                        0x00010cec   Section        0  intp_user.o(i.intp8_interrupt)
    i.intp9_callback                         0x00010d00   Section        0  intp_user.o(i.intp9_callback)
    intp9_callback                           0x00010d01   Thumb Code    12  intp_user.o(i.intp9_callback)
    i.intp9_interrupt                        0x00010d10   Section        0  intp_user.o(i.intp9_interrupt)
    i.it_interrupt                           0x00010d24   Section        0  isr_bat32a239.o(i.it_interrupt)
    i.key_interrupt                          0x00010d30   Section        0  isr_bat32a239.o(i.key_interrupt)
    i.lvi_interrupt                          0x00010d3c   Section        0  isr_bat32a239.o(i.lvi_interrupt)
    i.main                                   0x00010d48   Section        0  main.o(i.main)
    i.memcpy1                                0x00010d58   Section        0  can.o(i.memcpy1)
    i.ocrv_interrupt                         0x00010d6c   Section        0  isr_bat32a239.o(i.ocrv_interrupt)
    i.osdc_interrupt                         0x00010d78   Section        0  isr_bat32a239.o(i.osdc_interrupt)
    i.rtc_interrupt                          0x00010d84   Section        0  isr_bat32a239.o(i.rtc_interrupt)
    i.sre0_interrupt                         0x00010d90   Section        0  isr_bat32a239.o(i.sre0_interrupt)
    i.sre1_interrupt                         0x00010d9c   Section        0  isr_bat32a239.o(i.sre1_interrupt)
    i.sre2_interrupt                         0x00010da8   Section        0  isr_bat32a239.o(i.sre2_interrupt)
    i.tm01h_interrupt                        0x00010db4   Section        0  isr_bat32a239.o(i.tm01h_interrupt)
    i.tm03h_interrupt                        0x00010dc0   Section        0  isr_bat32a239.o(i.tm03h_interrupt)
    i.tm40_channel0_interrupt                0x00010dcc   Section        0  isr_bat32a239.o(i.tm40_channel0_interrupt)
    i.tm40_channel1_interrupt                0x00010dd8   Section        0  isr_bat32a239.o(i.tm40_channel1_interrupt)
    i.tm40_channel2_interrupt                0x00010de0   Section        0  isr_bat32a239.o(i.tm40_channel2_interrupt)
    i.tm40_channel3_interrupt                0x00010de8   Section        0  isr_bat32a239.o(i.tm40_channel3_interrupt)
    i.tm81_channel10_interrupt               0x00010df4   Section        0  isr_bat32a239.o(i.tm81_channel10_interrupt)
    i.tm81_channel11_interrupt               0x00010e00   Section        0  isr_bat32a239.o(i.tm81_channel11_interrupt)
    i.tm81_channel12_interrupt               0x00010e0c   Section        0  isr_bat32a239.o(i.tm81_channel12_interrupt)
    i.tm81_channel13_interrupt               0x00010e18   Section        0  isr_bat32a239.o(i.tm81_channel13_interrupt)
    i.tm81_channel14_interrupt               0x00010e24   Section        0  isr_bat32a239.o(i.tm81_channel14_interrupt)
    i.tm81_channel15_interrupt               0x00010e30   Section        0  isr_bat32a239.o(i.tm81_channel15_interrupt)
    i.tm81_channel16_interrupt               0x00010e3c   Section        0  isr_bat32a239.o(i.tm81_channel16_interrupt)
    i.tm81_channel17_interrupt               0x00010e48   Section        0  isr_bat32a239.o(i.tm81_channel17_interrupt)
    i.tma0_interrupt                         0x00010e54   Section        0  isr_bat32a239.o(i.tma0_interrupt)
    i.tmb0_interrupt                         0x00010e60   Section        0  isr_bat32a239.o(i.tmb0_interrupt)
    i.tmc_interrupt                          0x00010e6c   Section        0  isr_bat32a239.o(i.tmc_interrupt)
    i.tmm0_interrupt                         0x00010e78   Section        0  isr_bat32a239.o(i.tmm0_interrupt)
    i.tmm1_interrupt                         0x00010e84   Section        0  isr_bat32a239.o(i.tmm1_interrupt)
    i.uart0_callback_sendend                 0x00010e90   Section        0  sci_user.o(i.uart0_callback_sendend)
    uart0_callback_sendend                   0x00010e91   Thumb Code     2  sci_user.o(i.uart0_callback_sendend)
    i.uart0_interrupt_receive                0x00010e94   Section        0  sci_user.o(i.uart0_interrupt_receive)
    i.uart0_interrupt_send                   0x00010eb8   Section        0  sci_user.o(i.uart0_interrupt_send)
    i.uart1_callback_error                   0x00010f00   Section        0  sci_user.o(i.uart1_callback_error)
    uart1_callback_error                     0x00010f01   Thumb Code     2  sci_user.o(i.uart1_callback_error)
    i.uart1_callback_receiveend              0x00010f02   Section        0  sci_user.o(i.uart1_callback_receiveend)
    uart1_callback_receiveend                0x00010f03   Thumb Code     2  sci_user.o(i.uart1_callback_receiveend)
    i.uart1_callback_sendend                 0x00010f04   Section        0  sci_user.o(i.uart1_callback_sendend)
    uart1_callback_sendend                   0x00010f05   Thumb Code     2  sci_user.o(i.uart1_callback_sendend)
    i.uart1_callback_softwareoverrun         0x00010f06   Section        0  sci_user.o(i.uart1_callback_softwareoverrun)
    uart1_callback_softwareoverrun           0x00010f07   Thumb Code     2  sci_user.o(i.uart1_callback_softwareoverrun)
    i.uart1_interrupt_receive                0x00010f08   Section        0  sci_user.o(i.uart1_interrupt_receive)
    i.uart1_interrupt_send                   0x00010f94   Section        0  sci_user.o(i.uart1_interrupt_send)
    i.uart2_User_KL15_Init                   0x00010fdc   Section        0  sci_user.o(i.uart2_User_KL15_Init)
    i.uart3_callback_error                   0x00010fe8   Section        0  sci_user.o(i.uart3_callback_error)
    uart3_callback_error                     0x00010fe9   Thumb Code     2  sci_user.o(i.uart3_callback_error)
    i.uart3_callback_receiveend              0x00010fea   Section        0  sci_user.o(i.uart3_callback_receiveend)
    uart3_callback_receiveend                0x00010feb   Thumb Code     2  sci_user.o(i.uart3_callback_receiveend)
    i.uart3_callback_sendend                 0x00010fec   Section        0  sci_user.o(i.uart3_callback_sendend)
    uart3_callback_sendend                   0x00010fed   Thumb Code     2  sci_user.o(i.uart3_callback_sendend)
    i.uart3_callback_softwareoverrun         0x00010fee   Section        0  sci_user.o(i.uart3_callback_softwareoverrun)
    uart3_callback_softwareoverrun           0x00010fef   Thumb Code     2  sci_user.o(i.uart3_callback_softwareoverrun)
    i.uart3_interrupt_receive                0x00010ff0   Section        0  sci_user.o(i.uart3_interrupt_receive)
    i.uart3_interrupt_send                   0x00011084   Section        0  sci_user.o(i.uart3_interrupt_send)
    ram_fetch_code                           0x000110d0   Section        0  flash.o(ram_fetch_code)
    sram_code                                0x000111b4   Section        0  clk.o(sram_code)
    .constdata                               0x00011208   Section      132  analog_signals.o(.constdata)
    .constdata                               0x0001128c   Section       36  seg_lcd.o(.constdata)
    .constdata                               0x000112b0   Section     1200  aw93015.o(.constdata)
    PD_IIC_DAC_Int                           0x000112b0   Data        1200  aw93015.o(.constdata)
    .constdata                               0x00011760   Section       96  line_in.o(.constdata)
    .constdata                               0x000117c0   Section       40  system_monitor_user.o(.constdata)
    SysFun_Range                             0x000117c0   Data          20  system_monitor_user.o(.constdata)
    SysNM_Range                              0x000117d4   Data          20  system_monitor_user.o(.constdata)
    .constdata                               0x000117e8   Section      380  telltales_user.o(.constdata)
    KeyAttrTable                             0x000117e8   Data          16  telltales_user.o(.constdata)
    KeyHoldThreshold                         0x000117f8   Data           4  telltales_user.o(.constdata)
    .constdata                               0x00011964   Section      100  flash_synchronizer.o(.constdata)
    .constdata                               0x000119c8   Section       77  bglinterface.o(.constdata)
    .constdata                               0x00011a18   Section       20  key.o(.constdata)
    KeyAttrTable                             0x00011a18   Data          16  key.o(.constdata)
    KeyHoldThreshold                         0x00011a28   Data           4  key.o(.constdata)
    .constdata                               0x00011a2c   Section      548  can_communication_matrix.o(.constdata)
    .constdata                               0x00011c50   Section       72  app_telltales.o(.constdata)
    .data                                    0x20000000   Section        4  sys_tick.o(.data)
    .data                                    0x20000004   Section       10  adc.o(.data)
    .data                                    0x2000000e   Section       14  analog_signals.o(.data)
    .data                                    0x2000001c   Section      368  sci.o(.data)
    dummy_sio00                              0x2000017c   Data           1  sci.o(.data)
    dummy_sio00                              0x2000017d   Data           1  sci.o(.data)
    dummy_sio01                              0x2000017e   Data           1  sci.o(.data)
    dummy_sio01                              0x2000017f   Data           1  sci.o(.data)
    dummy_sio10                              0x20000180   Data           1  sci.o(.data)
    dummy_sio10                              0x20000181   Data           1  sci.o(.data)
    dummy_sio11                              0x20000182   Data           1  sci.o(.data)
    dummy_sio11                              0x20000183   Data           1  sci.o(.data)
    dummy_sio20                              0x20000184   Data           1  sci.o(.data)
    dummy_sio20                              0x20000185   Data           1  sci.o(.data)
    dummy_sio21                              0x20000186   Data           1  sci.o(.data)
    dummy_sio21                              0x20000187   Data           1  sci.o(.data)
    dummy_sio20                              0x20000188   Data           1  sci.o(.data)
    dummy_sio30                              0x20000189   Data           1  sci.o(.data)
    dummy_sio31                              0x2000018a   Data           1  sci.o(.data)
    dummy_sio31                              0x2000018b   Data           1  sci.o(.data)
    .data                                    0x2000018c   Section       18  sci_user.o(.data)
    .data                                    0x200001a0   Section       48  intp_user.o(.data)
    .data                                    0x200001d0   Section        7  rtc.o(.data)
    .data                                    0x200001d8   Section       14  can.o(.data)
    .data                                    0x200001e6   Section        6  bu98r10.o(.data)
    .data                                    0x200001ec   Section       11  seg_lcd.o(.data)
    Gear                                     0x200001f5   Data           1  seg_lcd.o(.data)
    time                                     0x200001f6   Data           1  seg_lcd.o(.data)
    .data                                    0x200001f8   Section       12  is31fl3236.o(.data)
    .data                                    0x20000204   Section        9  aw93015.o(.data)
    .data                                    0x20000210   Section        8  is31_iic_master.o(.data)
    .data                                    0x20000218   Section        1  line_in.o(.data)
    .data                                    0x20000219   Section        1  powermanagement.o(.data)
    g_Power_St                               0x20000219   Data           1  powermanagement.o(.data)
    .data                                    0x2000021a   Section        2  powermanagement_user.o(.data)
    .data                                    0x2000021c   Section       58  system_monitor.o(.data)
    SetVolFlag                               0x2000021d   Data           1  system_monitor.o(.data)
    t_NM_KL30_Debounce                       0x2000021e   Data           2  system_monitor.o(.data)
    t_NM_KL15_Debounce                       0x20000220   Data           2  system_monitor.o(.data)
    t_FUN_KL30_Debounce                      0x20000222   Data           2  system_monitor.o(.data)
    t_FUN_KL15_Debounce                      0x20000224   Data           2  system_monitor.o(.data)
    FUNSysVol_Range                          0x20000226   Data          20  system_monitor.o(.data)
    NMSysVol_Range                           0x2000023a   Data          20  system_monitor.o(.data)
    DebpounceTimer                           0x20000252   Data           2  system_monitor.o(.data)
    DebpounceTimer                           0x20000254   Data           2  system_monitor.o(.data)
    .data                                    0x20000258   Section       44  common_interface.o(.data)
    PowerIgnOnTimeLine                       0x20000258   Data           4  common_interface.o(.data)
    PowerIgnOffTimeLine                      0x2000025c   Data           4  common_interface.o(.data)
    SelfcheckStart                           0x20000260   Data           1  common_interface.o(.data)
    g_Disp_Mode                              0x20000261   Data           1  common_interface.o(.data)
    g_Language                               0x20000262   Data           1  common_interface.o(.data)
    PowerSts                                 0x20000263   Data           1  common_interface.o(.data)
    Act_V_Speed                              0x20000264   Data           2  common_interface.o(.data)
    Act_E_Speed                              0x20000266   Data           2  common_interface.o(.data)
    Disp_V_Speed                             0x20000268   Data           2  common_interface.o(.data)
    Disp_E_Speed                             0x2000026a   Data           2  common_interface.o(.data)
    Disp_Gauges_E_Speed                      0x2000026c   Data           2  common_interface.o(.data)
    Disp_E_Speed_Test                        0x2000026e   Data           2  common_interface.o(.data)
    Disp_V_Speed_Test                        0x20000270   Data           2  common_interface.o(.data)
    Disp_Fuel_Test                           0x20000272   Data           2  common_interface.o(.data)
    Disp_Temp_Test                           0x20000274   Data           2  common_interface.o(.data)
    Act_RV_Speed                             0x20000276   Data           2  common_interface.o(.data)
    Disp_RV_Speed                            0x20000278   Data           2  common_interface.o(.data)
    Disp_RV_Speed_Test                       0x2000027a   Data           2  common_interface.o(.data)
    Act_V_Speed_Valid                        0x2000027c   Data           1  common_interface.o(.data)
    Act_E_Speed_Valid                        0x2000027d   Data           1  common_interface.o(.data)
    Act_RV_Speed_Valid                       0x2000027e   Data           1  common_interface.o(.data)
    Disp_V_Speed_Valid                       0x2000027f   Data           1  common_interface.o(.data)
    Disp_E_Speed_Valid                       0x20000280   Data           1  common_interface.o(.data)
    Disp_RV_Speed_Valid                      0x20000281   Data           1  common_interface.o(.data)
    SysRollingCounter                        0x20000282   Data           2  common_interface.o(.data)
    .data                                    0x20000284   Section       98  mcu_core_protocol.o(.data)
    Send_ID_01_00                            0x20000291   Data           2  mcu_core_protocol.o(.data)
    Send_ID_01_01                            0x20000293   Data           3  mcu_core_protocol.o(.data)
    Send_ID_01_03                            0x20000296   Data           6  mcu_core_protocol.o(.data)
    Receive_ID_12                            0x2000029c   Data           7  mcu_core_protocol.o(.data)
    Event_Msg_QueueFront                     0x200002a3   Data           1  mcu_core_protocol.o(.data)
    Event_Msg_QueueRear                      0x200002a4   Data           1  mcu_core_protocol.o(.data)
    Event_Msg_Count                          0x200002a5   Data           1  mcu_core_protocol.o(.data)
    DtcDispNum                               0x200002c2   Data           2  mcu_core_protocol.o(.data)
    SpeedStandTime                           0x200002c6   Data           2  mcu_core_protocol.o(.data)
    Animat_GEAR                              0x200002c8   Data           4  mcu_core_protocol.o(.data)
    Animat_Vspeed                            0x200002cc   Data           4  mcu_core_protocol.o(.data)
    Animat_Espeed                            0x200002d0   Data           4  mcu_core_protocol.o(.data)
    Animat_ODO                               0x200002d4   Data           4  mcu_core_protocol.o(.data)
    Animat_Temp                              0x200002d8   Data           4  mcu_core_protocol.o(.data)
    Animat_Fuel                              0x200002dc   Data           4  mcu_core_protocol.o(.data)
    Animat_Battery                           0x200002e0   Data           4  mcu_core_protocol.o(.data)
    Checktime                                0x200002e4   Data           2  mcu_core_protocol.o(.data)
    .data                                    0x200002e6   Section        6  flash_synchronizer.o(.data)
    .data                                    0x200002ec   Section       26  fuel.o(.data)
    FuelRBak                                 0x200002f0   Data           2  fuel.o(.data)
    timeCount                                0x20000302   Data           2  fuel.o(.data)
    time                                     0x20000304   Data           2  fuel.o(.data)
    .data                                    0x20000308   Section       16  services_mileage_user.o(.data)
    clearEnFlag                              0x20000316   Data           1  services_mileage_user.o(.data)
    TripClearCommandBak                      0x20000317   Data           1  services_mileage_user.o(.data)
    .data                                    0x20000318   Section        2  data_gear.o(.data)
    Gear_Number                              0x20000318   Data           1  data_gear.o(.data)
    timeCount                                0x20000319   Data           1  data_gear.o(.data)
    .data                                    0x2000031a   Section       27  backgroundlight.o(.data)
    BackLightLevelNTC                        0x20000321   Data           3  backgroundlight.o(.data)
    .data                                    0x20000338   Section       12  bglinterface.o(.data)
    time                                     0x20000342   Data           2  bglinterface.o(.data)
    .data                                    0x20000344   Section      104  can_user.o(.data)
    SendTempValue                            0x20000344   Data           2  can_user.o(.data)
    RSCAN0Busoff                             0x20000346   Data           4  can_user.o(.data)
    UDSSendStep                              0x20000350   Data           1  can_user.o(.data)
    CurFaultNum                              0x20000354   Data           1  can_user.o(.data)
    HisFaultNum                              0x20000355   Data           1  can_user.o(.data)
    BCM_Module                               0x20000357   Data           1  can_user.o(.data)
    BatteryClearnflag                        0x20000388   Data           2  can_user.o(.data)
    Oldget_ECU_Battery_Voltage               0x2000038a   Data           2  can_user.o(.data)
    FauleSendStep                            0x2000039c   Data           1  can_user.o(.data)
    CurFaultSendCount                        0x2000039d   Data           1  can_user.o(.data)
    HisFaultSendCount                        0x2000039e   Data           1  can_user.o(.data)
    DtcCurFault1                             0x200003a0   Data           4  can_user.o(.data)
    DtcCurFault2                             0x200003a4   Data           4  can_user.o(.data)
    CurrentDispPosition                      0x200003a8   Data           1  can_user.o(.data)
    FaultNumber                              0x200003a9   Data           1  can_user.o(.data)
    tmp                                      0x200003aa   Data           2  can_user.o(.data)
    .data                                    0x200003ac   Section       30  app_service.o(.data)
    .data                                    0x200003ca   Section        2  tp_layer.o(.data)
    .data                                    0x200003cc   Section       13  u2_app_service.o(.data)
    .data                                    0x200003da   Section        2  u2_tp_layer.o(.data)
    .data                                    0x200003dc   Section        4  system_bat32a239.o(.data)
    .data                                    0x200003e0   Section        1  can_signal_rx.o(.data)
    .data                                    0x200003e1   Section        1  can_signal_tx.o(.data)
    .bss                                     0x200003e4   Section       24  sys_tick.o(.bss)
    .bss                                     0x200003fc   Section       16  analog_signals.o(.bss)
    .bss                                     0x2000040c   Section      360  bu98r10.o(.bss)
    .bss                                     0x20000574   Section       32  seg_lcd.o(.bss)
    .bss                                     0x20000594   Section       36  is31fl3236.o(.bss)
    .bss                                     0x200005b8   Section      200  aw93015.o(.bss)
    .bss                                     0x20000680   Section       44  sys_scheduler.o(.bss)
    .bss                                     0x200006ac   Section       48  line_in.o(.bss)
    .bss                                     0x200006dc   Section       44  powermanagement.o(.bss)
    .bss                                     0x20000708   Section       48  system_monitor.o(.bss)
    .bss                                     0x20000738   Section      576  mcu_core_protocol.o(.bss)
    Send_ID_01_02                            0x20000800   Data          23  mcu_core_protocol.o(.bss)
    Send_ID_02                               0x20000817   Data          11  mcu_core_protocol.o(.bss)
    Event_Send_Queue                         0x20000822   Data         342  mcu_core_protocol.o(.bss)
    .bss                                     0x20000978   Section       46  telltales_user.o(.bss)
    .bss                                     0x200009a6   Section       40  fuel.o(.bss)
    .bss                                     0x200009d0   Section       30  services_mileage_user.o(.bss)
    .bss                                     0x200009ee   Section       60  backgroundlight.o(.bss)
    .bss                                     0x20000a2a   Section       76  bglinterface.o(.bss)
    .bss                                     0x20000a76   Section       16  key.o(.bss)
    .bss                                     0x20000a88   Section      676  can_user.o(.bss)
    CurFault                                 0x20000a88   Data         100  can_user.o(.bss)
    HisFault                                 0x20000aec   Data         100  can_user.o(.bss)
    pTXBuff                                  0x20000b50   Data         224  can_user.o(.bss)
    pRXBuff                                  0x20000c30   Data         192  can_user.o(.bss)
    .bss                                     0x20000d2c   Section      473  app_service.o(.bss)
    .bss                                     0x20000f06   Section       36  link_layer.o(.bss)
    .bss                                     0x20000f2c   Section      646  tp_layer.o(.bss)
    .bss                                     0x200011b4   Section      483  u2_app_service.o(.bss)
    .bss                                     0x20001398   Section       36  u2_link_layer.o(.bss)
    .bss                                     0x200013bc   Section      646  u2_tp_layer.o(.bss)
    .bss                                     0x20001644   Section       12  can_signal_rx.o(.bss)
    .bss                                     0x20001650   Section       16  can_signal_tx.o(.bss)
    .bss                                     0x20001660   Section       28  telltales_lib.o(.bss)
    .bss                                     0x2000167c   Section       96  libspace.o(.bss)
    [Anonymous Symbol]                       0x200016dc   Section        0  eeprommanage.o(.bss.IsReadOdoState)
    IsReadOdoState                           0x200016dc   Data           2  eeprommanage.o(.bss.IsReadOdoState)
    [Anonymous Symbol]                       0x200016de   Section        0  eeprommanage.o(.bss.MemoryConfig.0)
    MemoryConfig.0                           0x200016de   Data           1  eeprommanage.o(.bss.MemoryConfig.0)
    [Anonymous Symbol]                       0x200016df   Section        0  eeprommanage.o(.bss.MemoryConfig.1)
    MemoryConfig.1                           0x200016df   Data           1  eeprommanage.o(.bss.MemoryConfig.1)
    [Anonymous Symbol]                       0x200016e0   Section        0  eeprommanage.o(.bss.MemoryConfig.2)
    MemoryConfig.2                           0x200016e0   Data           4  eeprommanage.o(.bss.MemoryConfig.2)
    [Anonymous Symbol]                       0x200016e4   Section        0  eeprommanage.o(.bss.MemoryConfig.3)
    MemoryConfig.3                           0x200016e4   Data           2  eeprommanage.o(.bss.MemoryConfig.3)
    [Anonymous Symbol]                       0x200016e8   Section        0  eeprommanage.o(.bss.memIgnState)
    memIgnState                              0x200016e8   Data           1  eeprommanage.o(.bss.memIgnState)
    [Anonymous Symbol]                       0x200016ec   Section        0  eeprommanage.o(.bss.memoryOdo)
    memoryOdo                                0x200016ec   Data           4  eeprommanage.o(.bss.memoryOdo)
    [Anonymous Symbol]                       0x200016f0   Section        0  eeprommanage.o(.bss.readDebugState)
    readDebugState                           0x200016f0   Data           2  eeprommanage.o(.bss.readDebugState)
    [Anonymous Symbol]                       0x200016f2   Section        0  eeprommanage.o(.bss.readState)
    readState                                0x200016f2   Data           1  eeprommanage.o(.bss.readState)
    [Anonymous Symbol]                       0x200016f3   Section        0  eeprommanage.o(.bss.tWR_count)
    tWR_count                                0x200016f3   Data           1  eeprommanage.o(.bss.tWR_count)
    [Anonymous Symbol]                       0x200016f4   Section        0  eeprommanage.o(.bss.writeBakEnable)
    writeBakEnable                           0x200016f4   Data           1  eeprommanage.o(.bss.writeBakEnable)
    [Anonymous Symbol]                       0x200016f6   Section        0  eeprommanage.o(.bss.writeDebugState)
    writeDebugState                          0x200016f6   Data           2  eeprommanage.o(.bss.writeDebugState)
    [Anonymous Symbol]                       0x200016f8   Section        0  eeprommanage.o(.bss.writeState)
    writeState                               0x200016f8   Data           2  eeprommanage.o(.bss.writeState)
    [Anonymous Symbol]                       0x200016fc   Section        0  eeprommanage.o(.bss.writeWaitTime)
    writeWaitTime                            0x200016fc   Data           4  eeprommanage.o(.bss.writeWaitTime)
    [Anonymous Symbol]                       0x20001700   Section        0  eeprommanage.o(.bss.write_pos)
    write_pos                                0x20001700   Data           2  eeprommanage.o(.bss.write_pos)
    HEAP                                     0x20001708   Section      256  startup_bat32a239.o(HEAP)
    Heap_Mem                                 0x20001708   Data         256  startup_bat32a239.o(HEAP)
    STACK                                    0x20001808   Section     1536  startup_bat32a239.o(STACK)
    Stack_Mem                                0x20001808   Data        1536  startup_bat32a239.o(STACK)
    __initial_sp                             0x20001e08   Data           0  startup_bat32a239.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv3M$S$PE$A:L22$X:L11$S22$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OTIME$ROPI$EBA8$UX$STANDARDLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    __Vectors                                0x00000000   Data           4  startup_bat32a239.o(RESET)
    __ARM_exceptions_init                     - Undefined Weak Reference
    __alloca_initialize                       - Undefined Weak Reference
    __arm_fini_                               - Undefined Weak Reference
    __arm_preinit_                            - Undefined Weak Reference
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    __rt_locale                               - Undefined Weak Reference
    __sigvec_lookup                           - Undefined Weak Reference
    _atexit_init                              - Undefined Weak Reference
    _call_atexit_fns                          - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _fp_trap_init                             - Undefined Weak Reference
    _fp_trap_shutdown                         - Undefined Weak Reference
    _get_lc_collate                           - Undefined Weak Reference
    _get_lc_ctype                             - Undefined Weak Reference
    _get_lc_monetary                          - Undefined Weak Reference
    _get_lc_numeric                           - Undefined Weak Reference
    _get_lc_time                              - Undefined Weak Reference
    _getenv_init                              - Undefined Weak Reference
    _handle_redirection                       - Undefined Weak Reference
    _init_alloc                               - Undefined Weak Reference
    _init_user_alloc                          - Undefined Weak Reference
    _initio                                   - Undefined Weak Reference
    _rand_init                                - Undefined Weak Reference
    _signal_finish                            - Undefined Weak Reference
    _signal_init                              - Undefined Weak Reference
    _terminate_alloc                          - Undefined Weak Reference
    _terminate_user_alloc                     - Undefined Weak Reference
    _terminateio                              - Undefined Weak Reference
    __Vectors_End                            0x000000c0   Data           0  startup_bat32a239.o(RESET)
    __Vectors_Size                           0x000000c0   Number         0  startup_bat32a239.o ABSOLUTE
    user_opt_data                            0x000000c0   Data           4  system_bat32a239.o(.ARM.__AT_0x000000C0)
    __main                                   0x000000c5   Thumb Code     8  __main.o(!!!main)
    __scatterload                            0x000000cd   Thumb Code     0  __scatter.o(!!!scatter)
    __scatterload_rt2                        0x000000cd   Thumb Code    52  __scatter.o(!!!scatter)
    __scatterload_rt2_thumb_only             0x000000cd   Thumb Code     0  __scatter.o(!!!scatter)
    __scatterload_null                       0x000000dd   Thumb Code     0  __scatter.o(!!!scatter)
    __scatterload_zeroinit                   0x00000109   Thumb Code    28  __scatter_zi.o(!!handler_zi)
    __rt_lib_init                            0x00000125   Thumb Code     0  libinit.o(.ARM.Collect$$libinit$$00000000)
    __rt_lib_init_alloca_1                   0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$0000002E)
    __rt_lib_init_argv_1                     0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$0000002C)
    __rt_lib_init_atexit_1                   0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$0000001B)
    __rt_lib_init_clock_1                    0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000021)
    __rt_lib_init_cpp_1                      0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000032)
    __rt_lib_init_exceptions_1               0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000030)
    __rt_lib_init_fp_1                       0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000002)
    __rt_lib_init_fp_trap_1                  0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$0000001F)
    __rt_lib_init_getenv_1                   0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000023)
    __rt_lib_init_heap_1                     0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$0000000A)
    __rt_lib_init_lc_collate_1               0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000011)
    __rt_lib_init_lc_ctype_1                 0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000013)
    __rt_lib_init_lc_monetary_1              0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000015)
    __rt_lib_init_lc_numeric_1               0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000017)
    __rt_lib_init_lc_time_1                  0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000019)
    __rt_lib_init_preinit_1                  0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000004)
    __rt_lib_init_rand_1                     0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$0000000E)
    __rt_lib_init_return                     0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000033)
    __rt_lib_init_signal_1                   0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$0000001D)
    __rt_lib_init_stdio_1                    0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$00000025)
    __rt_lib_init_user_alloc_1               0x00000127   Thumb Code     0  libinit2.o(.ARM.Collect$$libinit$$0000000C)
    __rt_lib_shutdown                        0x00000129   Thumb Code     0  libshutdown.o(.ARM.Collect$$libshutdown$$00000000)
    __rt_lib_shutdown_cpp_1                  0x0000012b   Thumb Code     0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000004)
    __rt_lib_shutdown_fini_1                 0x0000012b   Thumb Code     0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000002)
    __rt_lib_shutdown_fp_trap_1              0x0000012b   Thumb Code     0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000009)
    __rt_lib_shutdown_heap_1                 0x0000012b   Thumb Code     0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000011)
    __rt_lib_shutdown_return                 0x0000012b   Thumb Code     0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000012)
    __rt_lib_shutdown_signal_1               0x0000012b   Thumb Code     0  libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C)
    __rt_lib_shutdown_stdio_1                0x0000012b   Thumb Code     0  libshutdown2.o(.ARM.Collect$$libshutdown$$00000006)
    __rt_lib_shutdown_user_alloc_1           0x0000012b   Thumb Code     0  libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E)
    __rt_entry                               0x0000012d   Thumb Code     0  __rtentry.o(.ARM.Collect$$rtentry$$00000000)
    __rt_entry_presh_1                       0x0000012d   Thumb Code     0  __rtentry2.o(.ARM.Collect$$rtentry$$00000002)
    __rt_entry_sh                            0x0000012d   Thumb Code     0  __rtentry4.o(.ARM.Collect$$rtentry$$00000004)
    __rt_entry_li                            0x00000133   Thumb Code     0  __rtentry2.o(.ARM.Collect$$rtentry$$0000000A)
    __rt_entry_postsh_1                      0x00000133   Thumb Code     0  __rtentry2.o(.ARM.Collect$$rtentry$$00000009)
    __rt_entry_main                          0x00000137   Thumb Code     0  __rtentry2.o(.ARM.Collect$$rtentry$$0000000D)
    __rt_entry_postli_1                      0x00000137   Thumb Code     0  __rtentry2.o(.ARM.Collect$$rtentry$$0000000C)
    __rt_exit                                0x0000013f   Thumb Code     0  rtexit.o(.ARM.Collect$$rtexit$$00000000)
    __rt_exit_ls                             0x00000141   Thumb Code     0  rtexit2.o(.ARM.Collect$$rtexit$$00000003)
    __rt_exit_prels_1                        0x00000141   Thumb Code     0  rtexit2.o(.ARM.Collect$$rtexit$$00000002)
    __rt_exit_exit                           0x00000145   Thumb Code     0  rtexit2.o(.ARM.Collect$$rtexit$$00000004)
    __aeabi_memcpy4                          0x0000014d   Thumb Code    56  rt_memcpy.o(.emb_text)
    __aeabi_memcpy8                          0x0000014d   Thumb Code     0  rt_memcpy.o(.emb_text)
    Reset_Handler                            0x00000185   Thumb Code     8  startup_bat32a239.o(.text)
    NMI_Handler                              0x0000018d   Thumb Code     2  startup_bat32a239.o(.text)
    HardFault_Handler                        0x0000018f   Thumb Code     2  startup_bat32a239.o(.text)
    MemManage_Handler                        0x00000191   Thumb Code     2  startup_bat32a239.o(.text)
    BusFault_Handler                         0x00000193   Thumb Code     2  startup_bat32a239.o(.text)
    UsageFault_Handler                       0x00000195   Thumb Code     2  startup_bat32a239.o(.text)
    SVC_Handler                              0x00000197   Thumb Code     2  startup_bat32a239.o(.text)
    DebugMon_Handler                         0x00000199   Thumb Code     2  startup_bat32a239.o(.text)
    PendSV_Handler                           0x0000019b   Thumb Code     2  startup_bat32a239.o(.text)
    __user_initial_stackheap                 0x000001e1   Thumb Code    10  startup_bat32a239.o(.text)
    __aeabi_lmul                             0x00000205   Thumb Code    48  llmul.o(.text)
    _ll_mul                                  0x00000205   Thumb Code     0  llmul.o(.text)
    __aeabi_uldivmod                         0x00000235   Thumb Code   258  lludiv.o(.text)
    _ll_udiv                                 0x00000235   Thumb Code     0  lludiv.o(.text)
    __aeabi_memcpy                           0x00000337   Thumb Code   130  rt_memcpy.o(.text)
    __rt_memcpy                              0x00000337   Thumb Code     0  rt_memcpy.o(.text)
    _memset_w                                0x000003b9   Thumb Code    26  rt_memclr.o(.text)
    _memset                                  0x000003d3   Thumb Code    30  rt_memclr.o(.text)
    __aeabi_memclr                           0x000003f1   Thumb Code     4  rt_memclr.o(.text)
    __rt_memclr                              0x000003f1   Thumb Code     0  rt_memclr.o(.text)
    __aeabi_memclr4                          0x000003f5   Thumb Code     0  rt_memclr.o(.text)
    __aeabi_memclr8                          0x000003f5   Thumb Code     0  rt_memclr.o(.text)
    __rt_memclr_w                            0x000003f5   Thumb Code     4  rt_memclr.o(.text)
    __aeabi_uidiv                            0x000003f9   Thumb Code     0  aeabi_sdivfast.o(.text)
    __aeabi_uidivmod                         0x000003f9   Thumb Code    28  aeabi_sdivfast.o(.text)
    __aeabi_idiv                             0x00000415   Thumb Code     0  aeabi_sdivfast.o(.text)
    __aeabi_idivmod                          0x00000415   Thumb Code   460  aeabi_sdivfast.o(.text)
    __use_two_region_memory                  0x000005e1   Thumb Code     2  heapauxi.o(.text)
    __rt_heap_escrow$2region                 0x000005e3   Thumb Code     2  heapauxi.o(.text)
    __rt_heap_expand$2region                 0x000005e5   Thumb Code     2  heapauxi.o(.text)
    __user_setup_stackheap                   0x000005e7   Thumb Code    62  sys_stackheap_outer.o(.text)
    exit                                     0x00000625   Thumb Code    16  exit.o(.text)
    __user_libspace                          0x00000635   Thumb Code     8  libspace.o(.text)
    __user_perproc_libspace                  0x00000635   Thumb Code     0  libspace.o(.text)
    __user_perthread_libspace                0x00000635   Thumb Code     0  libspace.o(.text)
    _sys_exit                                0x0000063d   Thumb Code     8  sys_exit.o(.text)
    __I$use$semihosting                      0x00000649   Thumb Code     0  use_no_semi.o(.text)
    __use_no_semihosting_swi                 0x00000649   Thumb Code     2  use_no_semi.o(.text)
    __decompress                             0x0000064b   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x0000064b   Thumb Code    86  __dczerorl2.o(.text)
    __semihosting_library_function           0x0000064b   Thumb Code     0  indicate_semi.o(.text)
    ee_IIC_ACK                               0x000006a1   Thumb Code    68  eeprommanage.o(.text.ee_IIC_ACK)
    ee_IIC_NACK                              0x000006e5   Thumb Code    54  eeprommanage.o(.text.ee_IIC_NACK)
    ee_IIC_Read_8bit                         0x0000071b   Thumb Code    78  eeprommanage.o(.text.ee_IIC_Read_8bit)
    ee_IIC_SendByte                          0x00000769   Thumb Code    86  eeprommanage.o(.text.ee_IIC_SendByte)
    ee_IIC_SequentialRead                    0x000007bf   Thumb Code   138  eeprommanage.o(.text.ee_IIC_SequentialRead)
    ee_IIC_SequentialWrite                   0x00000849   Thumb Code   104  eeprommanage.o(.text.ee_IIC_SequentialWrite)
    ee_IIC_Start                             0x000008b1   Thumb Code    68  eeprommanage.o(.text.ee_IIC_Start)
    ee_IIC_Stop                              0x000008f5   Thumb Code    68  eeprommanage.o(.text.ee_IIC_Stop)
    ee_IIC_WaitAck                           0x00000939   Thumb Code    72  eeprommanage.o(.text.ee_IIC_WaitAck)
    eeprom_1ms_timeCount                     0x00000985   Thumb Code    16  eeprommanage.o(.text.eeprom_1ms_timeCount)
    eeprom_ClearOdoSection                   0x00000999   Thumb Code    80  eeprommanage.o(.text.eeprom_ClearOdoSection)
    eeprom_CreateCRC_8_Num                   0x000009f1   Thumb Code    68  eeprommanage.o(.text.eeprom_CreateCRC_8_Num)
    eeprom_OdoDecryption                     0x00000a35   Thumb Code   286  eeprommanage.o(.text.eeprom_OdoDecryption)
    eeprom_OdoEncryption                     0x00000b53   Thumb Code   266  eeprommanage.o(.text.eeprom_OdoEncryption)
    eeprom_ReadODO                           0x00000c5d   Thumb Code   476  eeprommanage.o(.text.eeprom_ReadODO)
    eeprom_ReadRecord                        0x00000e51   Thumb Code   144  eeprommanage.o(.text.eeprom_ReadRecord)
    eeprom_SetParameter                      0x00000eed   Thumb Code    44  eeprommanage.o(.text.eeprom_SetParameter)
    eeprom_WriteODO                          0x00000f2d   Thumb Code   620  eeprommanage.o(.text.eeprom_WriteODO)
    eeprom_WriteRecord                       0x000011cd   Thumb Code   276  eeprommanage.o(.text.eeprom_WriteRecord)
    ADC_Conv_Single_Channel                  0x00001301   Thumb Code   342  analog_signals.o(i.ADC_Conv_Single_Channel)
    ADC_Data_Calibrate                       0x00001471   Thumb Code    48  analog_circuits.o(i.ADC_Data_Calibrate)
    ADC_Get_Conversion_Result                0x000014a5   Thumb Code    36  adc.o(i.ADC_Get_Conversion_Result)
    ADC_Get_Conversion_Status                0x000014d1   Thumb Code     6  adc.o(i.ADC_Get_Conversion_Status)
    ADC_Init                                 0x000014dd   Thumb Code   168  adc.o(i.ADC_Init)
    ADC_Input_Voltage_Calc                   0x00001599   Thumb Code    52  analog_circuits.o(i.ADC_Input_Voltage_Calc)
    ADC_Read_Signal                          0x000015cd   Thumb Code    20  analog_signals.o(i.ADC_Read_Signal)
    ADC_Read_Signal_Valid                    0x000015e5   Thumb Code    18  analog_signals.o(i.ADC_Read_Signal_Valid)
    ADC_Res_Calc_Circuit101                  0x000015fd   Thumb Code   166  analog_circuits.o(i.ADC_Res_Calc_Circuit101)
    ADC_Start                                0x000016a9   Thumb Code    44  adc.o(i.ADC_Start)
    ADC_Start_Conversion                     0x000016dd   Thumb Code    28  adc.o(i.ADC_Start_Conversion)
    ADC_Stop                                 0x00001705   Thumb Code    34  adc.o(i.ADC_Stop)
    ADC_Stop_Conversion                      0x00001735   Thumb Code     8  adc.o(i.ADC_Stop_Conversion)
    ADC_Voltage_Calc_Circuit101              0x0000173d   Thumb Code    22  analog_circuits.o(i.ADC_Voltage_Calc_Circuit101)
    ADC_Voltage_Calc_Circuit102              0x00001755   Thumb Code   132  analog_circuits.o(i.ADC_Voltage_Calc_Circuit102)
    APP_CAN_Init                             0x000017dd   Thumb Code    66  can_user.o(i.APP_CAN_Init)
    Analog_Signal_Conv_Init                  0x00001845   Thumb Code    72  analog_signals.o(i.Analog_Signal_Conv_Init)
    Analog_Signal_Conv_Real_Time_Run         0x000018a5   Thumb Code    82  adc.o(i.Analog_Signal_Conv_Real_Time_Run)
    Analog_Signal_Conv_Service               0x00001911   Thumb Code   568  analog_signals.o(i.Analog_Signal_Conv_Service)
    Analog_Signal_Conv_Stop                  0x00001b65   Thumb Code    44  analog_signals.o(i.Analog_Signal_Conv_Stop)
    App_10_service                           0x00001ba1   Thumb Code   622  app_service.o(i.App_10_service)
    App_11_Reset_handle                      0x00001e29   Thumb Code    66  app_serviceproc.o(i.App_11_Reset_handle)
    App_11_service                           0x00001e7d   Thumb Code   208  app_service.o(i.App_11_service)
    App_22_service                           0x00001f59   Thumb Code   566  app_service.o(i.App_22_service)
    App_27_service                           0x000021b5   Thumb Code   820  app_service.o(i.App_27_service)
    App_28_service                           0x00002501   Thumb Code   190  app_service.o(i.App_28_service)
    App_2E_service                           0x000025cd   Thumb Code   176  app_service.o(i.App_2E_service)
    App_3E_service                           0x00002689   Thumb Code   126  app_service.o(i.App_3E_service)
    App_85_service                           0x00002719   Thumb Code   188  app_service.o(i.App_85_service)
    App_CopyRam                              0x000027e1   Thumb Code    24  app_serviceproc.o(i.App_CopyRam)
    App_ErrorInfoInit                        0x000027f9   Thumb Code    16  app_serviceproc.o(i.App_ErrorInfoInit)
    App_Load_DID                             0x0000280d   Thumb Code    22  app_serviceproc.o(i.App_Load_DID)
    App_ReUnlockTimerOver                    0x00002823   Thumb Code    36  app_service.o(i.App_ReUnlockTimerOver)
    App_SessionTimerOver                     0x00002847   Thumb Code    36  app_service.o(i.App_SessionTimerOver)
    App_SetReUnlockTimer                     0x0000286b   Thumb Code    14  app_service.o(i.App_SetReUnlockTimer)
    App_SetSessionTimer                      0x00002879   Thumb Code    14  app_service.o(i.App_SetSessionTimer)
    App_Telltales_AllOFF                     0x00002887   Thumb Code    26  app_telltales.o(i.App_Telltales_AllOFF)
    App_Telltales_Ctrl                       0x000028a1   Thumb Code    38  app_telltales.o(i.App_Telltales_Ctrl)
    BGLPwm_Config                            0x000028d1   Thumb Code    24  bglinterface.o(i.BGLPwm_Config)
    BGTask                                   0x000028f1   Thumb Code    80  bglinterface.o(i.BGTask)
    BU98R10_All_Command_Write                0x00002941   Thumb Code   244  bu98r10.o(i.BU98R10_All_Command_Write)
    BU98R10_All_Data_Write                   0x00002a39   Thumb Code   260  bu98r10.o(i.BU98R10_All_Data_Write)
    BU98R10_Init                             0x00002b41   Thumb Code   266  bu98r10.o(i.BU98R10_Init)
    BU98R10_Shutdown                         0x00002c61   Thumb Code    10  bu98r10.o(i.BU98R10_Shutdown)
    BU98R10_Update_Request                   0x00002c6d   Thumb Code    18  bu98r10.o(i.BU98R10_Update_Request)
    BU98R10_Update_Service                   0x00002c89   Thumb Code   290  bu98r10.o(i.BU98R10_Update_Service)
    BackLightDamp                            0x00002dc1   Thumb Code   620  backgroundlight.o(i.BackLightDamp)
    BackLightSchedu                          0x00003059   Thumb Code    50  bglinterface.o(i.BackLightSchedu)
    BatteryVoltageDelayInit                  0x0000309d   Thumb Code    16  can_user.o(i.BatteryVoltageDelayInit)
    CAN0Err_Interrupt                        0x000030b5   Thumb Code     8  isr_bat32a239.o(i.CAN0Err_Interrupt)
    CAN0Rec_Interrupt                        0x000030c1   Thumb Code     8  isr_bat32a239.o(i.CAN0Rec_Interrupt)
    CAN0Trx_Interrupt                        0x000030c9   Thumb Code     8  isr_bat32a239.o(i.CAN0Trx_Interrupt)
    CAN0Wup_Interrupt                        0x000030d1   Thumb Code     8  isr_bat32a239.o(i.CAN0Wup_Interrupt)
    CAN1Err_Interrupt                        0x000030dd   Thumb Code     8  isr_bat32a239.o(i.CAN1Err_Interrupt)
    CAN1Rec_Interrupt                        0x000030e9   Thumb Code     8  isr_bat32a239.o(i.CAN1Rec_Interrupt)
    CAN1Trx_Interrupt                        0x000030f5   Thumb Code     8  isr_bat32a239.o(i.CAN1Trx_Interrupt)
    CAN1Wup_Interrupt                        0x00003101   Thumb Code     8  isr_bat32a239.o(i.CAN1Wup_Interrupt)
    CAN_LED_Check_50msTask                   0x0000310d   Thumb Code   160  can_user.o(i.CAN_LED_Check_50msTask)
    CAN_MSG_Read                             0x000031b5   Thumb Code    40  can_signal_rx.o(i.CAN_MSG_Read)
    CAN_MSG_Status                           0x000031e1   Thumb Code    28  can_signal_rx.o(i.CAN_MSG_Status)
    CAN_RX_SetEnable                         0x00003201   Thumb Code    18  can_signal_rx.o(i.CAN_RX_SetEnable)
    CAN_RX_Tick                              0x00003219   Thumb Code    10  can_user.o(i.CAN_RX_Tick)
    CAN_TX_SetEnable                         0x00003225   Thumb Code    18  can_signal_tx.o(i.CAN_TX_SetEnable)
    CAN_TX_Tick                              0x0000323d   Thumb Code    12  can_user.o(i.CAN_TX_Tick)
    CLK_GetCoreFreq                          0x00003249   Thumb Code   152  system_bat32a239.o(i.CLK_GetCoreFreq)
    CLK_GetfIHFreq                           0x000032ed   Thumb Code   124  system_bat32a239.o(i.CLK_GetfIHFreq)
    CLK_Osc_Setting                          0x0000339d   Thumb Code   128  clk.o(i.CLK_Osc_Setting)
    CLK_PLL_Setting                          0x00003421   Thumb Code    62  clk.o(i.CLK_PLL_Setting)
    CLK_PLL_Start                            0x00003465   Thumb Code    30  clk.o(i.CLK_PLL_Start)
    CalcODOKL15Init                          0x00003489   Thumb Code     8  services_mileage_user.o(i.CalcODOKL15Init)
    CalcODOKL30Init                          0x00003495   Thumb Code    98  services_mileage_user.o(i.CalcODOKL30Init)
    CalcODO_100ms_Services                   0x00003509   Thumb Code   442  services_mileage_user.o(i.CalcODO_100ms_Services)
    CalculateKey                             0x000036f1   Thumb Code   116  app_service.o(i.CalculateKey)
    CanMSg_XMS_Analysis                      0x0000376d   Thumb Code   446  can_signal_rx.o(i.CanMSg_XMS_Analysis)
    Can_BusOffRecover                        0x00003935   Thumb Code    18  can_user.o(i.Can_BusOffRecover)
    Can_BusOff_Fun                           0x00003951   Thumb Code   194  can_user.o(i.Can_BusOff_Fun)
    Can_RX_BuffInit                          0x00003a25   Thumb Code   162  can_signal_rx.o(i.Can_RX_BuffInit)
    Can_Receive_Msg                          0x00003ad1   Thumb Code    26  can_user.o(i.Can_Receive_Msg)
    Can_Set_Buff_105                         0x00003aed   Thumb Code    62  can_user.o(i.Can_Set_Buff_105)
    Can_Set_Buff_450                         0x00003b31   Thumb Code    24  can_user.o(i.Can_Set_Buff_450)
    Can_Set_Buff_510                         0x00003b49   Thumb Code    86  can_user.o(i.Can_Set_Buff_510)
    Can_Set_Buff_515                         0x00003ba9   Thumb Code   374  can_user.o(i.Can_Set_Buff_515)
    Can_Set_Buff_51C                         0x00003d4d   Thumb Code    30  can_user.o(i.Can_Set_Buff_51C)
    Can_Set_Buff_522                         0x00003d6d   Thumb Code   236  can_user.o(i.Can_Set_Buff_522)
    Can_Set_Buff_523                         0x00003e6d   Thumb Code   262  can_user.o(i.Can_Set_Buff_523)
    Can_TX_BuffInit                          0x00003f79   Thumb Code   432  can_signal_tx.o(i.Can_TX_BuffInit)
    Can_User_Time_Service                    0x00004131   Thumb Code   120  can_user.o(i.Can_User_Time_Service)
    Can_Write                                0x000041bd   Thumb Code   260  can_user.o(i.Can_Write)
    Can_Write_Fun                            0x000042cd   Thumb Code   898  can_signal_tx.o(i.Can_Write_Fun)
    Capture_Stop                             0x0000465d   Thumb Code   392  tim4.o(i.Capture_Stop)
    Clock_Init                               0x00004805   Thumb Code    52  clk.o(i.Clock_Init)
    Co_Can_Buff_Set                          0x00004845   Thumb Code   120  can_signal_rx.o(i.Co_Can_Buff_Set)
    Co_Can_ConvertSubID                      0x000048c1   Thumb Code    96  can_communication_matrix.o(i.Co_Can_ConvertSubID)
    Common_DataInit                          0x00004925   Thumb Code    76  common_interface.o(i.Common_DataInit)
    Common_GetIgnOffTime                     0x000049b1   Thumb Code     6  common_interface.o(i.Common_GetIgnOffTime)
    Common_GetIgnOnTime                      0x000049bd   Thumb Code     6  common_interface.o(i.Common_GetIgnOnTime)
    Common_Get_DispMode                      0x000049c9   Thumb Code     6  common_interface.o(i.Common_Get_DispMode)
    Common_Get_Disp_E_Speed                  0x000049d5   Thumb Code     6  common_interface.o(i.Common_Get_Disp_E_Speed)
    Common_Get_Disp_V_Speed                  0x000049e1   Thumb Code     6  common_interface.o(i.Common_Get_Disp_V_Speed)
    Common_Get_IG_Sts                        0x000049ed   Thumb Code     6  common_interface.o(i.Common_Get_IG_Sts)
    Common_Get_Language                      0x000049f9   Thumb Code     6  common_interface.o(i.Common_Get_Language)
    Common_Input_Para                        0x00004a05   Thumb Code    78  common_interface.o(i.Common_Input_Para)
    Common_SetSelfcheckStart                 0x00004a65   Thumb Code     6  common_interface.o(i.Common_SetSelfcheckStart)
    Common_Set_IG_Sts                        0x00004a71   Thumb Code     6  common_interface.o(i.Common_Set_IG_Sts)
    Data_Clear_Trip                          0x00004a7d   Thumb Code    38  services_mileage_user.o(i.Data_Clear_Trip)
    Data_Gear_KL15_Init                      0x00004aad   Thumb Code     8  data_gear.o(i.Data_Gear_KL15_Init)
    Data_Gear_KL30_Init                      0x00004ab9   Thumb Code     2  data_gear.o(i.Data_Gear_KL30_Init)
    Data_ODO_Read                            0x00004abd   Thumb Code     6  services_mileage_user.o(i.Data_ODO_Read)
    Data_Read_Trip                           0x00004ac9   Thumb Code    24  services_mileage_user.o(i.Data_Read_Trip)
    DelfuModuleIn                            0x00004ae5   Thumb Code     8  can_user.o(i.DelfuModuleIn)
    Diag_Req_Send                            0x00004af1   Thumb Code   348  can_user.o(i.Diag_Req_Send)
    Diagno_Tick                              0x00004c6d   Thumb Code   230  app_serviceproc.o(i.Diagno_Tick)
    DiagnosisInit_main                       0x00004d59   Thumb Code   102  app_service.o(i.DiagnosisInit_main)
    Diagnosis_main                           0x00004de5   Thumb Code   618  app_service.o(i.Diagnosis_main)
    Drive_Info_Display_Update_Service        0x00005081   Thumb Code   186  mcu_core_protocol.o(i.Drive_Info_Display_Update_Service)
    DtcFaultInit                             0x00005149   Thumb Code    16  can_user.o(i.DtcFaultInit)
    EE_FeedDog                               0x00005165   Thumb Code     8  eemanager_interface.o(i.EE_FeedDog)
    EE_NOP                                   0x0000516d   Thumb Code     4  eemanager_interface.o(i.EE_NOP)
    EE_SCL_OUT                               0x00005171   Thumb Code    28  eemanager_interface.o(i.EE_SCL_OUT)
    EE_SCL_OutConfig                         0x0000518d   Thumb Code    14  eemanager_interface.o(i.EE_SCL_OutConfig)
    EE_SDA_GetValue                          0x0000519b   Thumb Code    22  eemanager_interface.o(i.EE_SDA_GetValue)
    EE_SDA_InConfig                          0x000051b1   Thumb Code    14  eemanager_interface.o(i.EE_SDA_InConfig)
    EE_SDA_OUT                               0x000051bf   Thumb Code    28  eemanager_interface.o(i.EE_SDA_OUT)
    EE_SDA_OutConfig                         0x000051db   Thumb Code    14  eemanager_interface.o(i.EE_SDA_OutConfig)
    Enable_Cyc_Msg                           0x000051e9   Thumb Code    18  mcu_core_protocol.o(i.Enable_Cyc_Msg)
    Flash_Sync_Signal_Generation_Service     0x00005201   Thumb Code    94  flash_synchronizer.o(i.Flash_Sync_Signal_Generation_Service)
    Fuel_Cal_Sevice                          0x00005289   Thumb Code    24  fuel.o(i.Fuel_Cal_Sevice)
    Fuel_Gauges_Cal                          0x000052a1   Thumb Code   656  fuel.o(i.Fuel_Gauges_Cal)
    Fuel_KL15_Init                           0x0000555d   Thumb Code    58  fuel.o(i.Fuel_KL15_Init)
    Fuel_KL30_Init                           0x000055c1   Thumb Code    12  fuel.o(i.Fuel_KL30_Init)
    Fuel_R_Cal                               0x000055cd   Thumb Code   200  fuel.o(i.Fuel_R_Cal)
    Fuel_State_Check                         0x000056a9   Thumb Code   228  fuel.o(i.Fuel_State_Check)
    GET_Key_Prosess                          0x000057b9   Thumb Code    88  aw93015.o(i.GET_Key_Prosess)
    GPIO_Init                                0x00005819   Thumb Code  1464  gpio.o(i.GPIO_Init)
    GetAllDtcFault                           0x00005dd5   Thumb Code   540  can_user.o(i.GetAllDtcFault)
    GetDtcAmnt                               0x00005ff1   Thumb Code     6  can_user.o(i.GetDtcAmnt)
    GetDtcDispNum                            0x00005ffd   Thumb Code    10  can_user.o(i.GetDtcDispNum)
    Get_Bcm_Module                           0x0000600d   Thumb Code     6  can_user.o(i.Get_Bcm_Module)
    Get_CH0_BusOffStatus                     0x00006019   Thumb Code    20  can.o(i.Get_CH0_BusOffStatus)
    Get_CurFuelSetp                          0x00006031   Thumb Code     6  fuel.o(i.Get_CurFuelSetp)
    Get_Day_Or_Night                         0x0000603d   Thumb Code     6  bglinterface.o(i.Get_Day_Or_Night)
    Get_Fuel_Sensor_State                    0x00006049   Thumb Code     6  fuel.o(i.Get_Fuel_Sensor_State)
    Get_ID_01_Data                           0x00006055   Thumb Code   892  mcu_core_protocol.o(i.Get_ID_01_Data)
    Get_ID_02_Data                           0x000063e9   Thumb Code    66  mcu_core_protocol.o(i.Get_ID_02_Data)
    Get_ID_101_ECU_Engine_Temperature        0x00006431   Thumb Code    26  can_communication_matrix.o(i.Get_ID_101_ECU_Engine_Temperature)
    Get_ID_111_ISG_Ready                     0x0000644b   Thumb Code    16  can_communication_matrix.o(i.Get_ID_111_ISG_Ready)
    Get_ID_111_Sig_ISG_SideStand             0x0000645b   Thumb Code    16  can_communication_matrix.o(i.Get_ID_111_Sig_ISG_SideStand)
    Get_ID_125_Sig_TCS_WorkMode              0x0000646b   Thumb Code    16  can_communication_matrix.o(i.Get_ID_125_Sig_TCS_WorkMode)
    Get_ID_401_Sig_ECU_Battery_Voltage       0x0000647b   Thumb Code    12  can_communication_matrix.o(i.Get_ID_401_Sig_ECU_Battery_Voltage)
    Get_ID_402_ECU_DTC1Amnt                  0x00006487   Thumb Code    12  can_communication_matrix.o(i.Get_ID_402_ECU_DTC1Amnt)
    Get_ID_402_ECU_DTCH1                     0x00006493   Thumb Code    12  can_communication_matrix.o(i.Get_ID_402_ECU_DTCH1)
    Get_ID_402_ECU_DTCH2                     0x0000649f   Thumb Code    12  can_communication_matrix.o(i.Get_ID_402_ECU_DTCH2)
    Get_ID_402_ECU_DTCL1                     0x000064ab   Thumb Code    12  can_communication_matrix.o(i.Get_ID_402_ECU_DTCL1)
    Get_ID_402_ECU_DTCL2                     0x000064b7   Thumb Code    12  can_communication_matrix.o(i.Get_ID_402_ECU_DTCL2)
    Get_ID_402_ECU_DTCM1                     0x000064c3   Thumb Code    12  can_communication_matrix.o(i.Get_ID_402_ECU_DTCM1)
    Get_ID_402_ECU_DTCM2                     0x000064cf   Thumb Code    12  can_communication_matrix.o(i.Get_ID_402_ECU_DTCM2)
    Get_ID_55C_Sig_ClearTrip                 0x000064db   Thumb Code    16  can_communication_matrix.o(i.Get_ID_55C_Sig_ClearTrip)
    Get_ID_55C_Sig_ModifyODOSts              0x000064eb   Thumb Code    12  can_communication_matrix.o(i.Get_ID_55C_Sig_ModifyODOSts)
    Get_ID_55C_Sig_ModifyODOValue            0x000064f7   Thumb Code    36  can_communication_matrix.o(i.Get_ID_55C_Sig_ModifyODOValue)
    Get_Key1_Line_In_Sts                     0x0000651b   Thumb Code    22  key.o(i.Get_Key1_Line_In_Sts)
    Get_Key2_Line_In_Sts                     0x00006531   Thumb Code    24  key.o(i.Get_Key2_Line_In_Sts)
    Get_LED_ECU_Battery_VoltageFlag          0x00006549   Thumb Code     6  can_user.o(i.Get_LED_ECU_Battery_VoltageFlag)
    Get_RSCAN0Busoff_Status                  0x00006555   Thumb Code     6  can_user.o(i.Get_RSCAN0Busoff_Status)
    Get_RTC_Time                             0x00006561   Thumb Code    44  rtc.o(i.Get_RTC_Time)
    Get_ReqSilentTimer                       0x00006591   Thumb Code     6  can_user.o(i.Get_ReqSilentTimer)
    Get_TCS_WorkModeFlash                    0x0000659d   Thumb Code     6  can_user.o(i.Get_TCS_WorkModeFlash)
    Get_UDS_01_MsgRecFlg                     0x000065a9   Thumb Code     6  u2_app_service.o(i.Get_UDS_01_MsgRecFlg)
    Get_UDS_59_MsgRecFlg                     0x000065b5   Thumb Code     6  u2_app_service.o(i.Get_UDS_59_MsgRecFlg)
    Get_UDS_62_MsgRecFlg                     0x000065c1   Thumb Code     6  u2_app_service.o(i.Get_UDS_62_MsgRecFlg)
    IIC20_Stop                               0x000065cd   Thumb Code    24  sci.o(i.IIC20_Stop)
    IIC20_StopCondition                      0x000065f1   Thumb Code    96  sci.o(i.IIC20_StopCondition)
    IIC21_Stop                               0x0000665d   Thumb Code    26  sci.o(i.IIC21_Stop)
    IIC21_StopCondition                      0x00006685   Thumb Code    90  sci.o(i.IIC21_StopCondition)
    IIC2_SDA_OUT                             0x000066e9   Thumb Code    22  aw93015.o(i.IIC2_SDA_OUT)
    IIC_SDA2_IN                              0x000066ff   Thumb Code    14  aw93015.o(i.IIC_SDA2_IN)
    IIC_SDAGet                               0x0000670d   Thumb Code    22  is31_iic_master.o(i.IIC_SDAGet)
    INTP_Init                                0x00006725   Thumb Code  1264  intp.o(i.INTP_Init)
    INTP_Start                               0x00006c29   Thumb Code   238  intp.o(i.INTP_Start)
    IRQ00_Handler                            0x00006d21   Thumb Code    40  isr_bat32a239.o(i.IRQ00_Handler)
    IRQ01_Handler                            0x00006d4d   Thumb Code    28  isr_bat32a239.o(i.IRQ01_Handler)
    IRQ02_Handler                            0x00006d6d   Thumb Code    28  isr_bat32a239.o(i.IRQ02_Handler)
    IRQ03_Handler                            0x00006d8d   Thumb Code    28  isr_bat32a239.o(i.IRQ03_Handler)
    IRQ04_Handler                            0x00006dad   Thumb Code    28  isr_bat32a239.o(i.IRQ04_Handler)
    IRQ05_Handler                            0x00006dcd   Thumb Code    28  isr_bat32a239.o(i.IRQ05_Handler)
    IRQ06_Handler                            0x00006ded   Thumb Code    28  isr_bat32a239.o(i.IRQ06_Handler)
    IRQ07_Handler                            0x00006e0d   Thumb Code    28  isr_bat32a239.o(i.IRQ07_Handler)
    IRQ08_Handler                            0x00006e2d   Thumb Code    28  isr_bat32a239.o(i.IRQ08_Handler)
    IRQ09_Handler                            0x00006e4d   Thumb Code    30  isr_bat32a239.o(i.IRQ09_Handler)
    IRQ10_Handler                            0x00006e71   Thumb Code    16  isr_bat32a239.o(i.IRQ10_Handler)
    IRQ11_Handler                            0x00006e85   Thumb Code    16  isr_bat32a239.o(i.IRQ11_Handler)
    IRQ12_Handler                            0x00006e99   Thumb Code    30  isr_bat32a239.o(i.IRQ12_Handler)
    IRQ13_Handler                            0x00006ebd   Thumb Code    16  isr_bat32a239.o(i.IRQ13_Handler)
    IRQ14_Handler                            0x00006ed1   Thumb Code    16  isr_bat32a239.o(i.IRQ14_Handler)
    IRQ15_Handler                            0x00006ee5   Thumb Code    30  isr_bat32a239.o(i.IRQ15_Handler)
    IRQ16_Handler                            0x00006f09   Thumb Code    40  isr_bat32a239.o(i.IRQ16_Handler)
    IRQ17_Handler                            0x00006f35   Thumb Code    44  isr_bat32a239.o(i.IRQ17_Handler)
    IRQ18_Handler                            0x00006f65   Thumb Code    44  isr_bat32a239.o(i.IRQ18_Handler)
    IRQ19_Handler                            0x00006f95   Thumb Code    44  isr_bat32a239.o(i.IRQ19_Handler)
    IRQ20_Handler                            0x00006fc5   Thumb Code    44  isr_bat32a239.o(i.IRQ20_Handler)
    IRQ21_Handler                            0x00006ff5   Thumb Code    16  isr_bat32a239.o(i.IRQ21_Handler)
    IRQ22_Handler                            0x00007009   Thumb Code    30  isr_bat32a239.o(i.IRQ22_Handler)
    IRQ23_Handler                            0x0000702d   Thumb Code    30  isr_bat32a239.o(i.IRQ23_Handler)
    IRQ24_Handler                            0x00007051   Thumb Code    28  isr_bat32a239.o(i.IRQ24_Handler)
    IRQ25_Handler                            0x00007071   Thumb Code    30  isr_bat32a239.o(i.IRQ25_Handler)
    IRQ26_Handler                            0x00007095   Thumb Code    30  isr_bat32a239.o(i.IRQ26_Handler)
    IRQ27_Handler                            0x000070b9   Thumb Code    16  isr_bat32a239.o(i.IRQ27_Handler)
    IRQ28_Handler                            0x000070cd   Thumb Code    16  isr_bat32a239.o(i.IRQ28_Handler)
    IRQ29_Handler                            0x000070e1   Thumb Code    30  isr_bat32a239.o(i.IRQ29_Handler)
    IRQ30_Handler                            0x00007105   Thumb Code    30  isr_bat32a239.o(i.IRQ30_Handler)
    IRQ31_Handler                            0x00007129   Thumb Code    30  isr_bat32a239.o(i.IRQ31_Handler)
    IS31FL3236_Init                          0x0000714d   Thumb Code   594  is31fl3236.o(i.IS31FL3236_Init)
    IS31FL3236_Update                        0x000073b9   Thumb Code   392  is31fl3236.o(i.IS31FL3236_Update)
    IS31_IIC_ACK                             0x00007565   Thumb Code    56  is31_iic_master.o(i.IS31_IIC_ACK)
    IS31_IIC_ReadByte                        0x0000759d   Thumb Code    80  is31_iic_master.o(i.IS31_IIC_ReadByte)
    IS31_IIC_SCL_Dir_Out                     0x000075ed   Thumb Code    74  is31_iic_master.o(i.IS31_IIC_SCL_Dir_Out)
    IS31_IIC_SDA_Dir_In                      0x0000763d   Thumb Code    14  is31_iic_master.o(i.IS31_IIC_SDA_Dir_In)
    IS31_IIC_SDA_Dir_Out                     0x0000764b   Thumb Code    14  is31_iic_master.o(i.IS31_IIC_SDA_Dir_Out)
    IS31_IIC_SendByte                        0x00007659   Thumb Code    86  is31_iic_master.o(i.IS31_IIC_SendByte)
    IS31_IIC_Start                           0x000076af   Thumb Code    56  is31_iic_master.o(i.IS31_IIC_Start)
    IS31_IIC_Stop                            0x000076e7   Thumb Code    56  is31_iic_master.o(i.IS31_IIC_Stop)
    IS31_IIC_WaitAck                         0x00007721   Thumb Code   156  is31_iic_master.o(i.IS31_IIC_WaitAck)
    IS31_IIC_delay                           0x000077c9   Thumb Code    22  is31_iic_master.o(i.IS31_IIC_delay)
    IS31_OFF_Wakeup                          0x000077df   Thumb Code    10  is31fl3236.o(i.IS31_OFF_Wakeup)
    IS31_Set_SDB_Pin                         0x000077e9   Thumb Code    28  is31fl3236.o(i.IS31_Set_SDB_Pin)
    IS31_Shutdown                            0x00007805   Thumb Code    10  is31fl3236.o(i.IS31_Shutdown)
    Init93015_IIC                            0x00007811   Thumb Code   118  aw93015.o(i.Init93015_IIC)
    Key_Status_Detect_Service                0x0000789d   Thumb Code  1020  key.o(i.Key_Status_Detect_Service)
    Key_Status_Init                          0x00007c99   Thumb Code    48  key.o(i.Key_Status_Init)
    LED_ABS_Execution                        0x00007ccd   Thumb Code    40  telltales_user.o(i.LED_ABS_Execution)
    LED_ABS_Judgement                        0x00007cf5   Thumb Code    28  telltales_user.o(i.LED_ABS_Judgement)
    LED_AutoStarStop_Execution               0x00007d11   Thumb Code    40  telltales_user.o(i.LED_AutoStarStop_Execution)
    LED_AutoStarStop_Judgement               0x00007d39   Thumb Code    28  telltales_user.o(i.LED_AutoStarStop_Judgement)
    LED_Auto_HI_BEAM_Execution               0x00007d55   Thumb Code    20  telltales_user.o(i.LED_Auto_HI_BEAM_Execution)
    LED_Auto_HI_BEAM_Judgement               0x00007d69   Thumb Code    16  telltales_user.o(i.LED_Auto_HI_BEAM_Judgement)
    LED_Batterylow_Execution                 0x00007d79   Thumb Code    40  telltales_user.o(i.LED_Batterylow_Execution)
    LED_Batterylow_Judgement                 0x00007da1   Thumb Code    46  telltales_user.o(i.LED_Batterylow_Judgement)
    LED_ENGINE_OIL_LOW_Execution             0x00007dcf   Thumb Code    40  telltales_user.o(i.LED_ENGINE_OIL_LOW_Execution)
    LED_ENGINE_OIL_LOW_Judgement             0x00007df7   Thumb Code    16  telltales_user.o(i.LED_ENGINE_OIL_LOW_Judgement)
    LED_Fuel_Execution                       0x00007e07   Thumb Code    84  telltales_user.o(i.LED_Fuel_Execution)
    LED_Fuel_Judgement                       0x00007e5d   Thumb Code    58  telltales_user.o(i.LED_Fuel_Judgement)
    LED_HI_BEAM_Execution                    0x00007e9d   Thumb Code    40  telltales_user.o(i.LED_HI_BEAM_Execution)
    LED_HI_BEAM_Judgement                    0x00007ec5   Thumb Code    28  telltales_user.o(i.LED_HI_BEAM_Judgement)
    LED_LEFT_Execution                       0x00007ee1   Thumb Code    40  telltales_user.o(i.LED_LEFT_Execution)
    LED_LEFT_Judgement                       0x00007f09   Thumb Code    28  telltales_user.o(i.LED_LEFT_Judgement)
    LED_MIL_Execution                        0x00007f25   Thumb Code    40  telltales_user.o(i.LED_MIL_Execution)
    LED_MIL_Judgement                        0x00007f4d   Thumb Code    28  telltales_user.o(i.LED_MIL_Judgement)
    LED_READY_Execution                      0x00007f69   Thumb Code    40  telltales_user.o(i.LED_READY_Execution)
    LED_READY_Judgement                      0x00007f91   Thumb Code    26  telltales_user.o(i.LED_READY_Judgement)
    LED_RIGHT_Execution                      0x00007fab   Thumb Code    40  telltales_user.o(i.LED_RIGHT_Execution)
    LED_RIGHT_Judgement                      0x00007fd3   Thumb Code    28  telltales_user.o(i.LED_RIGHT_Judgement)
    LED_Shore_Execution                      0x00007fef   Thumb Code    40  telltales_user.o(i.LED_Shore_Execution)
    LED_Shore_Judgement                      0x00008017   Thumb Code    26  telltales_user.o(i.LED_Shore_Judgement)
    LED_TPMS_Execution                       0x00008031   Thumb Code    40  telltales_user.o(i.LED_TPMS_Execution)
    LED_TPMS_Judgement                       0x00008059   Thumb Code    16  telltales_user.o(i.LED_TPMS_Judgement)
    LED_TSC_Execution                        0x00008069   Thumb Code     2  telltales_user.o(i.LED_TSC_Execution)
    LED_TSC_Judgement                        0x0000806b   Thumb Code    14  telltales_user.o(i.LED_TSC_Judgement)
    LED_Temp_Execution                       0x00008079   Thumb Code    84  telltales_user.o(i.LED_Temp_Execution)
    LED_Temp_Judgement                       0x000080cd   Thumb Code    24  telltales_user.o(i.LED_Temp_Judgement)
    LINE_IN_Get_ABS                          0x000080e5   Thumb Code    22  line_in.o(i.LINE_IN_Get_ABS)
    LINE_IN_Get_AutoStarStop                 0x000080fb   Thumb Code    22  line_in.o(i.LINE_IN_Get_AutoStarStop)
    LINE_IN_Get_HighBeam                     0x00008111   Thumb Code    22  line_in.o(i.LINE_IN_Get_HighBeam)
    LINE_IN_Get_LeftTurn                     0x00008127   Thumb Code    22  line_in.o(i.LINE_IN_Get_LeftTurn)
    LINE_IN_Get_OBD                          0x0000813d   Thumb Code    22  line_in.o(i.LINE_IN_Get_OBD)
    LINE_IN_Get_OilPressure                  0x00008153   Thumb Code    22  line_in.o(i.LINE_IN_Get_OilPressure)
    LINE_IN_Get_RightTurn                    0x00008169   Thumb Code    22  line_in.o(i.LINE_IN_Get_RightTurn)
    LINE_IN_Get_TirePressure                 0x0000817f   Thumb Code    22  line_in.o(i.LINE_IN_Get_TirePressure)
    LK_FillMsg                               0x00008195   Thumb Code    20  link_layer.o(i.LK_FillMsg)
    LK_Link_main                             0x000081a9   Thumb Code    74  link_layer.o(i.LK_Link_main)
    Line_In_Debounce_Service                 0x000082c9   Thumb Code    78  line_in.o(i.Line_In_Debounce_Service)
    Line_In_Get_Status                       0x00008321   Thumb Code    12  line_in.o(i.Line_In_Get_Status)
    Line_In_KL15_OFF_Init                    0x00008331   Thumb Code    52  line_in.o(i.Line_In_KL15_OFF_Init)
    Line_In_KL15_ON_Init                     0x00008371   Thumb Code    52  line_in.o(i.Line_In_KL15_ON_Init)
    Line_In_KL30_Init                        0x000083b1   Thumb Code    48  line_in.o(i.Line_In_KL30_Init)
    Mileage_Delay_ms                         0x000083e9   Thumb Code    36  services_mileage_user.o(i.Mileage_Delay_ms)
    PD_IIC_ReadPage                          0x0000840d   Thumb Code   172  aw93015.o(i.PD_IIC_ReadPage)
    PD_IIC_ReadReg                           0x000084b9   Thumb Code    52  aw93015.o(i.PD_IIC_ReadReg)
    PD_IIC_WritePage                         0x000084ed   Thumb Code   170  aw93015.o(i.PD_IIC_WritePage)
    PORT_ClrBit                              0x000085cd   Thumb Code    32  gpio.o(i.PORT_ClrBit)
    PORT_GetBit                              0x000085f1   Thumb Code    24  gpio.o(i.PORT_GetBit)
    PORT_Init                                0x0000860d   Thumb Code   402  gpio.o(i.PORT_Init)
    PORT_SetBit                              0x000087a5   Thumb Code    32  gpio.o(i.PORT_SetBit)
    PowerMemInit                             0x000087c9   Thumb Code    54  powermanagement.o(i.PowerMemInit)
    Power_IG_LVP_Init                        0x00008809   Thumb Code     2  powermanagement_user.o(i.Power_IG_LVP_Init)
    Power_IG_OFF_Init                        0x0000880d   Thumb Code    98  powermanagement_user.o(i.Power_IG_OFF_Init)
    Power_IG_ON_Init                         0x00008875   Thumb Code    98  powermanagement_user.o(i.Power_IG_ON_Init)
    Power_IG_OVP_Init                        0x000088d7   Thumb Code     2  powermanagement_user.o(i.Power_IG_OVP_Init)
    Power_KL30_Init                          0x000088d9   Thumb Code    24  powermanagement_user.o(i.Power_KL30_Init)
    Power_Management_Init                    0x000088f1   Thumb Code    30  powermanagement.o(i.Power_Management_Init)
    Power_Management_Lib_Init                0x00008919   Thumb Code    58  powermanagement_user.o(i.Power_Management_Lib_Init)
    Power_Management_Service                 0x00008981   Thumb Code   282  powermanagement.o(i.Power_Management_Service)
    Power_Management_Service_user            0x00008aa5   Thumb Code    20  powermanagement_user.o(i.Power_Management_Service_user)
    Power_Sleep_Init                         0x00008abd   Thumb Code   346  powermanagement_user.o(i.Power_Sleep_Init)
    Power_Stay_OFF                           0x00008c25   Thumb Code    84  powermanagement_user.o(i.Power_Stay_OFF)
    Power_Stay_ON                            0x00008c81   Thumb Code    48  powermanagement_user.o(i.Power_Stay_ON)
    Power_Stay_Protect                       0x00008cb1   Thumb Code     4  powermanagement_user.o(i.Power_Stay_Protect)
    Power_Stay_Sleep                         0x00008cb5   Thumb Code    12  powermanagement_user.o(i.Power_Stay_Sleep)
    Power_Wakeup_Init                        0x00008cc1   Thumb Code    58  powermanagement_user.o(i.Power_Wakeup_Init)
    Protocol_KL15_ON_Init                    0x00008cfd   Thumb Code    16  mcu_core_protocol.o(i.Protocol_KL15_ON_Init)
    RTC_Get_CounterValue                     0x00008d19   Thumb Code    96  rtc.o(i.RTC_Get_CounterValue)
    RTC_Init                                 0x00008d7d   Thumb Code   144  rtc.o(i.RTC_Init)
    RTC_Service                              0x00008e19   Thumb Code    10  rtc.o(i.RTC_Service)
    RTC_Set_CounterValue                     0x00008e29   Thumb Code    82  rtc.o(i.RTC_Set_CounterValue)
    RTC_Start                                0x00008e81   Thumb Code    98  rtc.o(i.RTC_Start)
    RTE_ForceRead_KL30_Voltage               0x00008ef5   Thumb Code    16  rte_adc.o(i.RTE_ForceRead_KL30_Voltage)
    RTE_Read_KL15_Voltage                    0x00008f05   Thumb Code    16  rte_adc.o(i.RTE_Read_KL15_Voltage)
    RTE_Read_KL30_Valid                      0x00008f15   Thumb Code    16  rte_adc.o(i.RTE_Read_KL30_Valid)
    RTE_Read_KL30_Voltage                    0x00008f25   Thumb Code    16  rte_adc.o(i.RTE_Read_KL30_Voltage)
    ReqSilentTimer100mSService               0x00008f35   Thumb Code    20  can_user.o(i.ReqSilentTimer100mSService)
    Reset_Mil_Signal_Time                    0x00008f4d   Thumb Code    14  can_user.o(i.Reset_Mil_Signal_Time)
    SEG_Coolant_Temp_Display                 0x00008f65   Thumb Code   576  seg_lcd.o(i.SEG_Coolant_Temp_Display)
    SEG_Fuel_Level_Display                   0x000091ad   Thumb Code   498  seg_lcd.o(i.SEG_Fuel_Level_Display)
    SEG_LCD_ABS                              0x000093a9   Thumb Code    20  seg_lcd.o(i.SEG_LCD_ABS)
    SEG_LCD_AutoStarStop                     0x000093c1   Thumb Code    20  seg_lcd.o(i.SEG_LCD_AutoStarStop)
    SEG_LCD_Battery_Voltage_Display          0x000093d9   Thumb Code  1654  seg_lcd.o(i.SEG_LCD_Battery_Voltage_Display)
    SEG_LCD_Battery_Voltage_Selftest         0x00009a5d   Thumb Code  1038  seg_lcd.o(i.SEG_LCD_Battery_Voltage_Selftest)
    SEG_LCD_Batterylow                       0x00009e71   Thumb Code    22  seg_lcd.o(i.SEG_LCD_Batterylow)
    SEG_LCD_Engine_Speed_Seg_Display         0x00009e8d   Thumb Code  2222  seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Display)
    SEG_LCD_Engine_Speed_Seg_Selftest        0x0000a745   Thumb Code  1370  seg_lcd.o(i.SEG_LCD_Engine_Speed_Seg_Selftest)
    SEG_LCD_Fuel                             0x0000aca5   Thumb Code    22  seg_lcd.o(i.SEG_LCD_Fuel)
    SEG_LCD_Gear_Display                     0x0000acc1   Thumb Code   552  seg_lcd.o(i.SEG_LCD_Gear_Display)
    SEG_LCD_Gear_Selftest                    0x0000aef9   Thumb Code   332  seg_lcd.o(i.SEG_LCD_Gear_Selftest)
    SEG_LCD_HI_BEAM                          0x0000b051   Thumb Code    22  seg_lcd.o(i.SEG_LCD_HI_BEAM)
    SEG_LCD_HighBeam                         0x0000b06d   Thumb Code    20  seg_lcd.o(i.SEG_LCD_HighBeam)
    SEG_LCD_Init                             0x0000b085   Thumb Code    76  seg_lcd.o(i.SEG_LCD_Init)
    SEG_LCD_LeftTurn                         0x0000b0d1   Thumb Code    20  seg_lcd.o(i.SEG_LCD_LeftTurn)
    SEG_LCD_OBD                              0x0000b0e9   Thumb Code    22  seg_lcd.o(i.SEG_LCD_OBD)
    SEG_LCD_ODO_Trip_Display                 0x0000b105   Thumb Code  2840  seg_lcd.o(i.SEG_LCD_ODO_Trip_Display)
    SEG_LCD_ODO_Trip_FaultCode_Selftest      0x0000bc25   Thumb Code  1862  seg_lcd.o(i.SEG_LCD_ODO_Trip_FaultCode_Selftest)
    SEG_LCD_OilPressure                      0x0000c375   Thumb Code    22  seg_lcd.o(i.SEG_LCD_OilPressure)
    SEG_LCD_READY                            0x0000c391   Thumb Code    20  seg_lcd.o(i.SEG_LCD_READY)
    SEG_LCD_RightTurn                        0x0000c3a9   Thumb Code    20  seg_lcd.o(i.SEG_LCD_RightTurn)
    SEG_LCD_Shore                            0x0000c3c1   Thumb Code    22  seg_lcd.o(i.SEG_LCD_Shore)
    SEG_LCD_Shutdown                         0x0000c3dd   Thumb Code    20  seg_lcd.o(i.SEG_LCD_Shutdown)
    SEG_LCD_Temp                             0x0000c3f5   Thumb Code    20  seg_lcd.o(i.SEG_LCD_Temp)
    SEG_LCD_TirePressure                     0x0000c40d   Thumb Code    22  seg_lcd.o(i.SEG_LCD_TirePressure)
    SEG_LCD_Vehicle_Speed_Num_Display        0x0000c429   Thumb Code   934  seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Display)
    SEG_LCD_Vehicle_Speed_Num_Selftest       0x0000c7e5   Thumb Code   654  seg_lcd.o(i.SEG_LCD_Vehicle_Speed_Num_Selftest)
    SET_LED_ECU_Battery_VoltageFlag          0x0000ca85   Thumb Code     6  can_user.o(i.SET_LED_ECU_Battery_VoltageFlag)
    Selfcheck_Display_Update_Service         0x0000ca91   Thumb Code   786  mcu_core_protocol.o(i.Selfcheck_Display_Update_Service)
    Send_01_01                               0x0000cdc5   Thumb Code    48  can_user.o(i.Send_01_01)
    Send_19_0209                             0x0000cdf9   Thumb Code    54  can_user.o(i.Send_19_0209)
    Send_22_ID0005                           0x0000ce2f   Thumb Code    54  can_user.o(i.Send_22_ID0005)
    SetBGLNTCVol                             0x0000ce65   Thumb Code     6  bglinterface.o(i.SetBGLNTCVol)
    SetBGLTheme                              0x0000ce71   Thumb Code     6  bglinterface.o(i.SetBGLTheme)
    SetBGLType                               0x0000ce7d   Thumb Code     6  bglinterface.o(i.SetBGLType)
    SetBackLightOutput                       0x0000ce89   Thumb Code    16  backgroundlight.o(i.SetBackLightOutput)
    SetBaudRadio                             0x0000ce99   Thumb Code    80  can.o(i.SetBaudRadio)
    SetDtcFault                              0x0000cef1   Thumb Code   252  can_user.o(i.SetDtcFault)
    SetSendUdsTimeCount_0101                 0x0000cffd   Thumb Code     6  can_user.o(i.SetSendUdsTimeCount_0101)
    SetSendUdsTimeCount_190209               0x0000d009   Thumb Code     6  can_user.o(i.SetSendUdsTimeCount_190209)
    SetSendUdsTimeCount_220005               0x0000d015   Thumb Code     6  can_user.o(i.SetSendUdsTimeCount_220005)
    Set_CanSleepDelayTime                    0x0000d021   Thumb Code     6  can_user.o(i.Set_CanSleepDelayTime)
    Set_ReqSilentTimer                       0x0000d02d   Thumb Code     6  can_user.o(i.Set_ReqSilentTimer)
    Set_TCS_WorkModeFlsh                     0x0000d039   Thumb Code     6  can_user.o(i.Set_TCS_WorkModeFlsh)
    Set_UDS_01_MsgRecFlg                     0x0000d045   Thumb Code     6  u2_app_service.o(i.Set_UDS_01_MsgRecFlg)
    Set_UDS_59_MsgRecFlg                     0x0000d051   Thumb Code     6  u2_app_service.o(i.Set_UDS_59_MsgRecFlg)
    Set_UDS_62_MsgRecFlg                     0x0000d05d   Thumb Code     6  u2_app_service.o(i.Set_UDS_62_MsgRecFlg)
    Simulated_IIC_2_Init                     0x0000d069   Thumb Code    16  is31_iic_master.o(i.Simulated_IIC_2_Init)
    SysTick_Handler                          0x0000d079   Thumb Code   132  sys_tick.o(i.SysTick_Handler)
    Sys_BlockDelay                           0x0000d109   Thumb Code    28  system_monitor_user.o(i.Sys_BlockDelay)
    Sys_Enter_Sleep_Mode                     0x0000d125   Thumb Code    74  clk.o(i.Sys_Enter_Sleep_Mode)
    Sys_Exact_100ms_Tasks                    0x0000d175   Thumb Code     2  tasks.o(i.Sys_Exact_100ms_Tasks)
    Sys_Exact_50us_Tasks                     0x0000d177   Thumb Code     2  tasks.o(i.Sys_Exact_50us_Tasks)
    Sys_Force_Read_KL30_Voltage              0x0000d179   Thumb Code    12  system_monitor_user.o(i.Sys_Force_Read_KL30_Voltage)
    Sys_Init                                 0x0000d185   Thumb Code    56  sys_scheduler.o(i.Sys_Init)
    Sys_KL30_Init                            0x0000d1c1   Thumb Code    28  system_monitor_user.o(i.Sys_KL30_Init)
    Sys_LogicProcess                         0x0000d1e9   Thumb Code     2  system_monitor_user.o(i.Sys_LogicProcess)
    Sys_Read_KL30_Valid                      0x0000d1eb   Thumb Code    12  system_monitor_user.o(i.Sys_Read_KL30_Valid)
    Sys_Read_KL30_Voltage                    0x0000d1f7   Thumb Code    24  system_monitor_user.o(i.Sys_Read_KL30_Voltage)
    Sys_Run_Mode_100ms_Tasks_Group1          0x0000d20f   Thumb Code     8  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group1)
    Sys_Run_Mode_100ms_Tasks_Group10         0x0000d217   Thumb Code     2  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group10)
    Sys_Run_Mode_100ms_Tasks_Group2          0x0000d219   Thumb Code    10  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group2)
    Sys_Run_Mode_100ms_Tasks_Group3          0x0000d223   Thumb Code     2  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group3)
    Sys_Run_Mode_100ms_Tasks_Group4          0x0000d225   Thumb Code    12  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group4)
    Sys_Run_Mode_100ms_Tasks_Group5          0x0000d231   Thumb Code     2  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group5)
    Sys_Run_Mode_100ms_Tasks_Group6          0x0000d233   Thumb Code     8  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group6)
    Sys_Run_Mode_100ms_Tasks_Group7          0x0000d23b   Thumb Code    14  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group7)
    Sys_Run_Mode_100ms_Tasks_Group8          0x0000d249   Thumb Code     8  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group8)
    Sys_Run_Mode_100ms_Tasks_Group9          0x0000d251   Thumb Code     2  tasks.o(i.Sys_Run_Mode_100ms_Tasks_Group9)
    Sys_Run_Mode_10ms_Tasks                  0x0000d253   Thumb Code    42  tasks.o(i.Sys_Run_Mode_10ms_Tasks)
    Sys_Run_Mode_20ms_Tasks                  0x0000d27d   Thumb Code    18  tasks.o(i.Sys_Run_Mode_20ms_Tasks)
    Sys_Run_Mode_2ms_Tasks                   0x0000d28f   Thumb Code    20  tasks.o(i.Sys_Run_Mode_2ms_Tasks)
    Sys_Run_Mode_50ms_Tasks                  0x0000d2a3   Thumb Code    20  tasks.o(i.Sys_Run_Mode_50ms_Tasks)
    Sys_Run_Mode_5ms_Tasks                   0x0000d2b7   Thumb Code     8  tasks.o(i.Sys_Run_Mode_5ms_Tasks)
    Sys_Run_Mode_Pseudo_Real_Time_Tasks      0x0000d2c1   Thumb Code    20  tasks.o(i.Sys_Run_Mode_Pseudo_Real_Time_Tasks)
    Sys_Scheduling_Service                   0x0000d2d9   Thumb Code   296  sys_scheduler.o(i.Sys_Scheduling_Service)
    Sys_Scheduling_Tmr                       0x0000d405   Thumb Code   388  sys_scheduler.o(i.Sys_Scheduling_Tmr)
    Sys_Set_DebounceTimer                    0x0000d599   Thumb Code    20  system_monitor.o(i.Sys_Set_DebounceTimer)
    Sys_Set_VolRange                         0x0000d5bd   Thumb Code    92  system_monitor.o(i.Sys_Set_VolRange)
    Sys_Startup_Init                         0x0000d625   Thumb Code   122  init.o(i.Sys_Startup_Init)
    Sys_Status_Update_Service                0x0000d69f   Thumb Code    16  system_monitor.o(i.Sys_Status_Update_Service)
    Sys_Tick_Timer_Start                     0x0000d6b1   Thumb Code    74  sys_tick.o(i.Sys_Tick_Timer_Start)
    Sys_Tick_Timer_Stop                      0x0000d715   Thumb Code    14  sys_tick.o(i.Sys_Tick_Timer_Stop)
    Sys_WakeUp_Init                          0x0000d729   Thumb Code    32  system_monitor_user.o(i.Sys_WakeUp_Init)
    SystemCoreClockUpdate                    0x0000d755   Thumb Code    12  system_bat32a239.o(i.SystemCoreClockUpdate)
    SystemInit                               0x0000d765   Thumb Code   114  system_bat32a239.o(i.SystemInit)
    System_FUN_KL15_Status_Get               0x0000d841   Thumb Code     6  system_monitor.o(i.System_FUN_KL15_Status_Get)
    System_FUN_KL30_Status_Get               0x0000d84d   Thumb Code     6  system_monitor.o(i.System_FUN_KL30_Status_Get)
    System_Fast_WakeUp                       0x0000d859   Thumb Code   148  system_monitor.o(i.System_Fast_WakeUp)
    System_LINE_KL15                         0x0000da8d   Thumb Code    24  system_monitor_user.o(i.System_LINE_KL15)
    System_Monitor_KL30Init                  0x0000daa5   Thumb Code   248  system_monitor.o(i.System_Monitor_KL30Init)
    System_Monitor_WakeupInit                0x0000dbe9   Thumb Code   222  system_monitor.o(i.System_Monitor_WakeupInit)
    TMB0_PWM_Pin33_Freq_Duty                 0x0000de61   Thumb Code    54  timera_b_c.o(i.TMB0_PWM_Pin33_Freq_Duty)
    TMB0_PWM_Pin33_Init                      0x0000dea1   Thumb Code   156  timera_b_c.o(i.TMB0_PWM_Pin33_Init)
    TMB0_Start                               0x0000df5d   Thumb Code    38  timera_b_c.o(i.TMB0_Start)
    TP_AbnormalInReqFC_handle                0x0000df91   Thumb Code    36  tp_layer.o(i.TP_AbnormalInReqFC_handle)
    TP_AbnormalInReqFF_handle                0x0000dfbd   Thumb Code    48  tp_layer.o(i.TP_AbnormalInReqFF_handle)
    TP_AbnormalInResCF_handle                0x0000dff9   Thumb Code    36  tp_layer.o(i.TP_AbnormalInResCF_handle)
    TP_AbnormalInResFC_handle                0x0000e025   Thumb Code    36  tp_layer.o(i.TP_AbnormalInResFC_handle)
    TP_AbnormalInResSF_handle                0x0000e051   Thumb Code    64  tp_layer.o(i.TP_AbnormalInResSF_handle)
    TP_BsTimerOver                           0x0000e09d   Thumb Code    36  tp_layer.o(i.TP_BsTimerOver)
    TP_Buffer_handle                         0x0000e0c1   Thumb Code    86  tp_layer.o(i.TP_Buffer_handle)
    TP_CalMsgLen                             0x0000e121   Thumb Code    44  tp_layer.o(i.TP_CalMsgLen)
    TP_CrTimerOver                           0x0000e14d   Thumb Code    36  tp_layer.o(i.TP_CrTimerOver)
    TP_NormalRecFC_handle                    0x0000e171   Thumb Code   186  tp_layer.o(i.TP_NormalRecFC_handle)
    TP_NormalSendFC_Fun                      0x0000e241   Thumb Code   112  tp_layer.o(i.TP_NormalSendFC_Fun)
    TP_ReciveMultiF_handle                   0x0000e2c5   Thumb Code   386  tp_layer.o(i.TP_ReciveMultiF_handle)
    TP_ReciveSF_handle                       0x0000e465   Thumb Code   120  tp_layer.o(i.TP_ReciveSF_handle)
    TP_STminTimerOver                        0x0000e4e9   Thumb Code    36  tp_layer.o(i.TP_STminTimerOver)
    TP_SetBsTimer                            0x0000e50d   Thumb Code    14  tp_layer.o(i.TP_SetBsTimer)
    TP_SetCrTimer                            0x0000e51b   Thumb Code    14  tp_layer.o(i.TP_SetCrTimer)
    TP_SetSTminTimer                         0x0000e529   Thumb Code    14  tp_layer.o(i.TP_SetSTminTimer)
    TP_TooShortDLC_handle                    0x0000e539   Thumb Code   136  tp_layer.o(i.TP_TooShortDLC_handle)
    TP_TransmitNegatePDU                     0x0000e5c9   Thumb Code   178  tp_layer.o(i.TP_TransmitNegatePDU)
    TP_TransmitPDU                           0x0000e689   Thumb Code   504  tp_layer.o(i.TP_TransmitPDU)
    TP_UnknownlPDU_handle                    0x0000e8a5   Thumb Code    64  tp_layer.o(i.TP_UnknownlPDU_handle)
    Telltales_Init                           0x0000ec85   Thumb Code    30  telltales_user.o(i.Telltales_Init)
    Telltales_KL15_Init                      0x0000ecb9   Thumb Code    10  telltales_lib.o(i.Telltales_KL15_Init)
    Telltales_KL30_Wakeup_Init               0x0000ecc9   Thumb Code    92  telltales_lib.o(i.Telltales_KL30_Wakeup_Init)
    Telltales_Management                     0x0000ed29   Thumb Code   194  telltales_lib.o(i.Telltales_Management)
    U2_App_01_service                        0x0000edf5   Thumb Code    50  u2_app_service.o(i.U2_App_01_service)
    U2_App_11_Reset_handle                   0x0000ee31   Thumb Code     2  u2_app_serviceproc.o(i.U2_App_11_Reset_handle)
    U2_App_59_service                        0x0000ee35   Thumb Code    78  u2_app_service.o(i.U2_App_59_service)
    U2_App_62_service                        0x0000ee95   Thumb Code    70  u2_app_service.o(i.U2_App_62_service)
    U2_App_CopyRam                           0x0000eee5   Thumb Code    24  u2_app_serviceproc.o(i.U2_App_CopyRam)
    U2_App_DtcMsgTimerOver                   0x0000eefd   Thumb Code    36  u2_app_service.o(i.U2_App_DtcMsgTimerOver)
    U2_App_ErrorInfoInit                     0x0000ef21   Thumb Code    16  u2_app_serviceproc.o(i.U2_App_ErrorInfoInit)
    U2_App_Load_DID                          0x0000ef35   Thumb Code    22  u2_app_serviceproc.o(i.U2_App_Load_DID)
    U2_App_ReUnlockTimerOver                 0x0000ef4b   Thumb Code    36  u2_app_service.o(i.U2_App_ReUnlockTimerOver)
    U2_App_SessionTimerOver                  0x0000ef6f   Thumb Code    36  u2_app_service.o(i.U2_App_SessionTimerOver)
    U2_App_SetDtcMsgTimer                    0x0000ef93   Thumb Code    14  u2_app_service.o(i.U2_App_SetDtcMsgTimer)
    U2_Diagno_Tick                           0x0000efa1   Thumb Code   268  u2_app_serviceproc.o(i.U2_Diagno_Tick)
    U2_DiagnosisInit_main                    0x0000f0b1   Thumb Code   102  u2_app_service.o(i.U2_DiagnosisInit_main)
    U2_Diagnosis_main                        0x0000f13d   Thumb Code   468  u2_app_service.o(i.U2_Diagnosis_main)
    U2_LK_FillMsg                            0x0000f341   Thumb Code    20  u2_link_layer.o(i.U2_LK_FillMsg)
    U2_LK_Link_main                          0x0000f355   Thumb Code   122  u2_link_layer.o(i.U2_LK_Link_main)
    U2_TP_AbnormalInReqFC_handle             0x0000f3d5   Thumb Code    36  u2_tp_layer.o(i.U2_TP_AbnormalInReqFC_handle)
    U2_TP_AbnormalInReqFF_handle             0x0000f401   Thumb Code    48  u2_tp_layer.o(i.U2_TP_AbnormalInReqFF_handle)
    U2_TP_AbnormalInResCF_handle             0x0000f43d   Thumb Code    36  u2_tp_layer.o(i.U2_TP_AbnormalInResCF_handle)
    U2_TP_AbnormalInResFC_handle             0x0000f469   Thumb Code    36  u2_tp_layer.o(i.U2_TP_AbnormalInResFC_handle)
    U2_TP_AbnormalInResSF_handle             0x0000f495   Thumb Code    64  u2_tp_layer.o(i.U2_TP_AbnormalInResSF_handle)
    U2_TP_BsTimerOver                        0x0000f4e1   Thumb Code    36  u2_tp_layer.o(i.U2_TP_BsTimerOver)
    U2_TP_Buffer_handle                      0x0000f505   Thumb Code    86  u2_tp_layer.o(i.U2_TP_Buffer_handle)
    U2_TP_CalMsgLen                          0x0000f565   Thumb Code    44  u2_tp_layer.o(i.U2_TP_CalMsgLen)
    U2_TP_CrTimerOver                        0x0000f591   Thumb Code    36  u2_tp_layer.o(i.U2_TP_CrTimerOver)
    U2_TP_NormalRecFC_handle                 0x0000f5b5   Thumb Code   186  u2_tp_layer.o(i.U2_TP_NormalRecFC_handle)
    U2_TP_NormalSendFC_Fun                   0x0000f685   Thumb Code   112  u2_tp_layer.o(i.U2_TP_NormalSendFC_Fun)
    U2_TP_ReciveMultiF_handle                0x0000f709   Thumb Code   386  u2_tp_layer.o(i.U2_TP_ReciveMultiF_handle)
    U2_TP_ReciveSF_handle                    0x0000f8a9   Thumb Code   120  u2_tp_layer.o(i.U2_TP_ReciveSF_handle)
    U2_TP_STminTimerOver                     0x0000f92d   Thumb Code    36  u2_tp_layer.o(i.U2_TP_STminTimerOver)
    U2_TP_SetBsTimer                         0x0000f951   Thumb Code    14  u2_tp_layer.o(i.U2_TP_SetBsTimer)
    U2_TP_SetCrTimer                         0x0000f95f   Thumb Code    14  u2_tp_layer.o(i.U2_TP_SetCrTimer)
    U2_TP_SetSTminTimer                      0x0000f96d   Thumb Code    14  u2_tp_layer.o(i.U2_TP_SetSTminTimer)
    U2_TP_TooShortDLC_handle                 0x0000f97d   Thumb Code   136  u2_tp_layer.o(i.U2_TP_TooShortDLC_handle)
    U2_TP_TransmitNegatePDU                  0x0000fa0d   Thumb Code   178  u2_tp_layer.o(i.U2_TP_TransmitNegatePDU)
    U2_TP_TransmitPDU                        0x0000facd   Thumb Code   502  u2_tp_layer.o(i.U2_TP_TransmitPDU)
    U2_TP_UnknownlPDU_handle                 0x0000fce9   Thumb Code    64  u2_tp_layer.o(i.U2_TP_UnknownlPDU_handle)
    WDT_Restart                              0x0000fd35   Thumb Code     8  wdt.o(i.WDT_Restart)
    __ARM_common_switch8                     0x0000fd41   Thumb Code    28  gpio.o(i.__ARM_common_switch8)
    adc_interrupt                            0x0000fe05   Thumb Code     8  isr_bat32a239.o(i.adc_interrupt)
    bsp_CAN0_Rev_isr                         0x0000fe11   Thumb Code   252  can.o(i.bsp_CAN0_Rev_isr)
    bsp_CAN0_Tx_isr                          0x0000ff25   Thumb Code    20  can.o(i.bsp_CAN0_Tx_isr)
    bsp_CANSendFrame                         0x0000ff45   Thumb Code   142  can.o(i.bsp_CANSendFrame)
    bsp_CAN_BusOff_Recover                   0x0000ffd9   Thumb Code   218  can.o(i.bsp_CAN_BusOff_Recover)
    bsp_CAN_Init                             0x000100d5   Thumb Code   318  can.o(i.bsp_CAN_Init)
    bsp_CAN_MaskCheck                        0x0001023d   Thumb Code    60  can.o(i.bsp_CAN_MaskCheck)
    bsp_CAN_Sleep                            0x00010281   Thumb Code    10  can.o(i.bsp_CAN_Sleep)
    bsp_CAN_SleepRelease                     0x00010291   Thumb Code     8  can.o(i.bsp_CAN_SleepRelease)
    bsp_CanBuf_Clear                         0x0001029d   Thumb Code    44  can.o(i.bsp_CanBuf_Clear)
    bsp_CanBuf_Init                          0x000102cd   Thumb Code   176  can.o(i.bsp_CanBuf_Init)
    bsp_IIC2_ACK                             0x0001038d   Thumb Code    40  aw93015.o(i.bsp_IIC2_ACK)
    bsp_IIC2_ReadByte                        0x000103b5   Thumb Code    72  aw93015.o(i.bsp_IIC2_ReadByte)
    bsp_IIC2_SendByte                        0x000103fd   Thumb Code    70  aw93015.o(i.bsp_IIC2_SendByte)
    bsp_IIC2_Start                           0x00010443   Thumb Code    40  aw93015.o(i.bsp_IIC2_Start)
    bsp_IIC2_Stop                            0x0001046b   Thumb Code    40  aw93015.o(i.bsp_IIC2_Stop)
    bsp_IIC2_WaitAck                         0x00010493   Thumb Code    68  aw93015.o(i.bsp_IIC2_WaitAck)
    bsp_IIC_SCL_out                          0x000104d9   Thumb Code    56  is31_iic_master.o(i.bsp_IIC_SCL_out)
    bsp_IIC_SDA_out                          0x00010515   Thumb Code    56  is31_iic_master.o(i.bsp_IIC_SDA_out)
    bsp_Is_CAN_Sleep                         0x00010551   Thumb Code    60  can.o(i.bsp_Is_CAN_Sleep)
    bsp_rx_mask_init                         0x00010591   Thumb Code    88  can.o(i.bsp_rx_mask_init)
    bsp_rx_msgbuf_init                       0x000105ed   Thumb Code   138  can.o(i.bsp_rx_msgbuf_init)
    bsp_tim4_01_isr_Handler                  0x00010681   Thumb Code    42  tim4.o(i.bsp_tim4_01_isr_Handler)
    bsp_tim4_02_isr_Handler                  0x000106b9   Thumb Code     8  tim4.o(i.bsp_tim4_02_isr_Handler)
    bsp_tx_msgbuf_abort                      0x000106c5   Thumb Code    18  can.o(i.bsp_tx_msgbuf_abort)
    bsp_tx_msgbuf_init                       0x000106dd   Thumb Code    84  can.o(i.bsp_tx_msgbuf_init)
    cmp0_interrupt                           0x00010739   Thumb Code     8  isr_bat32a239.o(i.cmp0_interrupt)
    cmp1_interrupt                           0x00010745   Thumb Code     8  isr_bat32a239.o(i.cmp1_interrupt)
    div_interrupt                            0x00010751   Thumb Code     8  isr_bat32a239.o(i.div_interrupt)
    eeprom_StoreInfo_Init                    0x0001075d   Thumb Code    20  eemanager_interface.o(i.eeprom_StoreInfo_Init)
    eeprom_comm_DelayUs                      0x00010771   Thumb Code    32  eemanager_interface.o(i.eeprom_comm_DelayUs)
    extend_i2c_write_one_byte                0x00010791   Thumb Code    56  is31fl3236.o(i.extend_i2c_write_one_byte)
    flash_interrupt                          0x000107c9   Thumb Code     8  isr_bat32a239.o(i.flash_interrupt)
    get_CoolantTempVal                       0x000107d5   Thumb Code    14  can_user.o(i.get_CoolantTempVal)
    get_ECU_Battery_Voltage                  0x000107e3   Thumb Code    18  can_user.o(i.get_ECU_Battery_Voltage)
    get_ECU_Temperature_WaterVal             0x000107f5   Thumb Code    36  can_user.o(i.get_ECU_Temperature_WaterVal)
    iic20_interrupt                          0x00010849   Thumb Code   330  sci_user.o(i.iic20_interrupt)
    iic21_interrupt                          0x000109e9   Thumb Code   330  sci_user.o(i.iic21_interrupt)
    iica0_interrupt                          0x00010b5d   Thumb Code     8  isr_bat32a239.o(i.iica0_interrupt)
    iica1_interrupt                          0x00010b69   Thumb Code     8  isr_bat32a239.o(i.iica1_interrupt)
    intp0_interrupt                          0x00010b85   Thumb Code    14  intp_user.o(i.intp0_interrupt)
    intp10_interrupt                         0x00010ba9   Thumb Code    14  intp_user.o(i.intp10_interrupt)
    intp11_interrupt                         0x00010bcd   Thumb Code    14  intp_user.o(i.intp11_interrupt)
    intp1_interrupt                          0x00010bf1   Thumb Code    14  intp_user.o(i.intp1_interrupt)
    intp2_interrupt                          0x00010c15   Thumb Code    14  intp_user.o(i.intp2_interrupt)
    intp3_interrupt                          0x00010c39   Thumb Code    14  intp_user.o(i.intp3_interrupt)
    intp4_interrupt                          0x00010c5d   Thumb Code    14  intp_user.o(i.intp4_interrupt)
    intp5_interrupt                          0x00010c81   Thumb Code    14  intp_user.o(i.intp5_interrupt)
    intp6_interrupt                          0x00010ca5   Thumb Code    14  intp_user.o(i.intp6_interrupt)
    intp7_interrupt                          0x00010cc9   Thumb Code    14  intp_user.o(i.intp7_interrupt)
    intp8_interrupt                          0x00010ced   Thumb Code    14  intp_user.o(i.intp8_interrupt)
    intp9_interrupt                          0x00010d11   Thumb Code    14  intp_user.o(i.intp9_interrupt)
    it_interrupt                             0x00010d25   Thumb Code     8  isr_bat32a239.o(i.it_interrupt)
    key_interrupt                            0x00010d31   Thumb Code     8  isr_bat32a239.o(i.key_interrupt)
    lvi_interrupt                            0x00010d3d   Thumb Code     8  isr_bat32a239.o(i.lvi_interrupt)
    main                                     0x00010d49   Thumb Code    16  main.o(i.main)
    memcpy1                                  0x00010d59   Thumb Code    20  can.o(i.memcpy1)
    ocrv_interrupt                           0x00010d6d   Thumb Code     8  isr_bat32a239.o(i.ocrv_interrupt)
    osdc_interrupt                           0x00010d79   Thumb Code     8  isr_bat32a239.o(i.osdc_interrupt)
    rtc_interrupt                            0x00010d85   Thumb Code     8  isr_bat32a239.o(i.rtc_interrupt)
    sre0_interrupt                           0x00010d91   Thumb Code     8  isr_bat32a239.o(i.sre0_interrupt)
    sre1_interrupt                           0x00010d9d   Thumb Code     8  isr_bat32a239.o(i.sre1_interrupt)
    sre2_interrupt                           0x00010da9   Thumb Code     8  isr_bat32a239.o(i.sre2_interrupt)
    tm01h_interrupt                          0x00010db5   Thumb Code     8  isr_bat32a239.o(i.tm01h_interrupt)
    tm03h_interrupt                          0x00010dc1   Thumb Code     8  isr_bat32a239.o(i.tm03h_interrupt)
    tm40_channel0_interrupt                  0x00010dcd   Thumb Code     8  isr_bat32a239.o(i.tm40_channel0_interrupt)
    tm40_channel1_interrupt                  0x00010dd9   Thumb Code     8  isr_bat32a239.o(i.tm40_channel1_interrupt)
    tm40_channel2_interrupt                  0x00010de1   Thumb Code     8  isr_bat32a239.o(i.tm40_channel2_interrupt)
    tm40_channel3_interrupt                  0x00010de9   Thumb Code     8  isr_bat32a239.o(i.tm40_channel3_interrupt)
    tm81_channel10_interrupt                 0x00010df5   Thumb Code     8  isr_bat32a239.o(i.tm81_channel10_interrupt)
    tm81_channel11_interrupt                 0x00010e01   Thumb Code     8  isr_bat32a239.o(i.tm81_channel11_interrupt)
    tm81_channel12_interrupt                 0x00010e0d   Thumb Code     8  isr_bat32a239.o(i.tm81_channel12_interrupt)
    tm81_channel13_interrupt                 0x00010e19   Thumb Code     8  isr_bat32a239.o(i.tm81_channel13_interrupt)
    tm81_channel14_interrupt                 0x00010e25   Thumb Code     8  isr_bat32a239.o(i.tm81_channel14_interrupt)
    tm81_channel15_interrupt                 0x00010e31   Thumb Code     8  isr_bat32a239.o(i.tm81_channel15_interrupt)
    tm81_channel16_interrupt                 0x00010e3d   Thumb Code     8  isr_bat32a239.o(i.tm81_channel16_interrupt)
    tm81_channel17_interrupt                 0x00010e49   Thumb Code     8  isr_bat32a239.o(i.tm81_channel17_interrupt)
    tma0_interrupt                           0x00010e55   Thumb Code     8  isr_bat32a239.o(i.tma0_interrupt)
    tmb0_interrupt                           0x00010e61   Thumb Code     8  isr_bat32a239.o(i.tmb0_interrupt)
    tmc_interrupt                            0x00010e6d   Thumb Code     8  isr_bat32a239.o(i.tmc_interrupt)
    tmm0_interrupt                           0x00010e79   Thumb Code     8  isr_bat32a239.o(i.tmm0_interrupt)
    tmm1_interrupt                           0x00010e85   Thumb Code     8  isr_bat32a239.o(i.tmm1_interrupt)
    uart0_interrupt_receive                  0x00010e95   Thumb Code    28  sci_user.o(i.uart0_interrupt_receive)
    uart0_interrupt_send                     0x00010eb9   Thumb Code    54  sci_user.o(i.uart0_interrupt_send)
    uart1_interrupt_receive                  0x00010f09   Thumb Code   116  sci_user.o(i.uart1_interrupt_receive)
    uart1_interrupt_send                     0x00010f95   Thumb Code    54  sci_user.o(i.uart1_interrupt_send)
    uart2_User_KL15_Init                     0x00010fdd   Thumb Code     8  sci_user.o(i.uart2_User_KL15_Init)
    uart3_interrupt_receive                  0x00010ff1   Thumb Code   122  sci_user.o(i.uart3_interrupt_receive)
    uart3_interrupt_send                     0x00011085   Thumb Code    60  sci_user.o(i.uart3_interrupt_send)
    EraseChip                                0x000110d1   Thumb Code    62  flash.o(ram_fetch_code)
    EraseSector                              0x0001110f   Thumb Code    86  flash.o(ram_fetch_code)
    ProgramPage                              0x00011165   Thumb Code    74  flash.o(ram_fetch_code)
    CLK_Fclk_Select                          0x000111b5   Thumb Code    74  clk.o(sram_code)
    u8ADCChList                              0x00011208   Data           4  analog_signals.o(.constdata)
    stADCChCfg                               0x0001120c   Data          64  analog_signals.o(.constdata)
    stADCResList                             0x0001124c   Data          64  analog_signals.o(.constdata)
    SEG_DISPLAY_NUMBER0                      0x0001128c   Data          10  seg_lcd.o(.constdata)
    SEG_UNDISPLAY_NUMBER0                    0x00011296   Data          10  seg_lcd.o(.constdata)
    SEG_HEX_DISPLAY_NUMBER0                  0x000112a0   Data          16  seg_lcd.o(.constdata)
    g_stLineInAttribute                      0x00011760   Data          96  line_in.o(.constdata)
    LED_Attribute                            0x000117fc   Data         360  telltales_user.o(.constdata)
    FlashSync1HzTable                        0x00011964   Data          20  flash_synchronizer.o(.constdata)
    FlashSync2HzTable                        0x00011978   Data          20  flash_synchronizer.o(.constdata)
    FlashSync5HzTable                        0x0001198c   Data          20  flash_synchronizer.o(.constdata)
    FlashSync05HzTable                       0x000119a0   Data          40  flash_synchronizer.o(.constdata)
    BackLightValue_TFT_Default               0x000119c8   Data          72  bglinterface.o(.constdata)
    PwmChannel                               0x00011a10   Data           5  bglinterface.o(.constdata)
    st_CANSendAttr                           0x00011a2c   Data         196  can_communication_matrix.o(.constdata)
    CAN_MSG_CONST_ARRAY                      0x00011af0   Data         352  can_communication_matrix.o(.constdata)
    IS31FL3236_LED_Channel                   0x00011c50   Data          72  app_telltales.o(.constdata)
    Region$$Table$$Base                      0x00011c98   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x00011cb8   Number         0  anon$$obj.o(Region$$Table)
    g_u16SysRollingCounter50us               0x20000000   Data           2  sys_tick.o(.data)
    g_u16SysRollingCounter1ms                0x20000002   Data           2  sys_tick.o(.data)
    u8ADCSequenceRunningFlag                 0x20000004   Data           1  adc.o(.data)
    u8ADCChannelCount                        0x20000005   Data           1  adc.o(.data)
    u16ADCChannelResult                      0x20000006   Data           8  adc.o(.data)
    u16ADCRefVoltage                         0x2000000e   Data           2  analog_signals.o(.data)
    stADCCtrl                                0x20000010   Data           4  analog_signals.o(.data)
    u16ADCSample                             0x20000014   Data           8  analog_signals.o(.data)
    gp_uart0_tx_address                      0x2000001c   Data           4  sci.o(.data)
    g_uart0_tx_count                         0x20000020   Data           2  sci.o(.data)
    gp_uart0_rx_address                      0x20000024   Data           4  sci.o(.data)
    g_uart0_rx_count                         0x20000028   Data           2  sci.o(.data)
    g_uart0_rx_length                        0x2000002a   Data           2  sci.o(.data)
    gp_spi00_rx_address                      0x2000002c   Data           4  sci.o(.data)
    g_spi00_rx_length                        0x20000030   Data           2  sci.o(.data)
    g_spi00_rx_count                         0x20000032   Data           2  sci.o(.data)
    gp_spi00_tx_address                      0x20000034   Data           4  sci.o(.data)
    g_spi00_tx_length                        0x20000038   Data           2  sci.o(.data)
    g_spi00_tx_count                         0x2000003a   Data           2  sci.o(.data)
    gp_spi01_rx_address                      0x2000003c   Data           4  sci.o(.data)
    g_spi01_rx_length                        0x20000040   Data           2  sci.o(.data)
    g_spi01_rx_count                         0x20000042   Data           2  sci.o(.data)
    gp_spi01_tx_address                      0x20000044   Data           4  sci.o(.data)
    g_spi01_tx_length                        0x20000048   Data           2  sci.o(.data)
    g_spi01_tx_count                         0x2000004a   Data           2  sci.o(.data)
    g_iic00_master_status_flag               0x2000004c   Data           1  sci.o(.data)
    gp_iic00_tx_address                      0x20000050   Data           4  sci.o(.data)
    g_iic00_tx_count                         0x20000054   Data           2  sci.o(.data)
    gp_iic00_rx_address                      0x20000058   Data           4  sci.o(.data)
    g_iic00_rx_count                         0x2000005c   Data           2  sci.o(.data)
    g_iic00_rx_length                        0x2000005e   Data           2  sci.o(.data)
    g_iic01_master_status_flag               0x20000060   Data           1  sci.o(.data)
    gp_iic01_tx_address                      0x20000064   Data           4  sci.o(.data)
    g_iic01_tx_count                         0x20000068   Data           2  sci.o(.data)
    gp_iic01_rx_address                      0x2000006c   Data           4  sci.o(.data)
    g_iic01_rx_count                         0x20000070   Data           2  sci.o(.data)
    g_iic01_rx_length                        0x20000072   Data           2  sci.o(.data)
    gp_uart1_tx_address                      0x20000074   Data           4  sci.o(.data)
    g_uart1_tx_count                         0x20000078   Data           2  sci.o(.data)
    gp_uart1_rx_address                      0x2000007c   Data           4  sci.o(.data)
    g_uart1_rx_count                         0x20000080   Data           2  sci.o(.data)
    g_uart1_rx_length                        0x20000082   Data           2  sci.o(.data)
    gp_spi10_rx_address                      0x20000084   Data           4  sci.o(.data)
    g_spi10_rx_length                        0x20000088   Data           2  sci.o(.data)
    g_spi10_rx_count                         0x2000008a   Data           2  sci.o(.data)
    gp_spi10_tx_address                      0x2000008c   Data           4  sci.o(.data)
    g_spi10_tx_length                        0x20000090   Data           2  sci.o(.data)
    g_spi10_tx_count                         0x20000092   Data           2  sci.o(.data)
    gp_spi11_rx_address                      0x20000094   Data           4  sci.o(.data)
    g_spi11_rx_length                        0x20000098   Data           2  sci.o(.data)
    g_spi11_rx_count                         0x2000009a   Data           2  sci.o(.data)
    gp_spi11_tx_address                      0x2000009c   Data           4  sci.o(.data)
    g_spi11_tx_length                        0x200000a0   Data           2  sci.o(.data)
    g_spi11_tx_count                         0x200000a2   Data           2  sci.o(.data)
    g_iic10_master_status_flag               0x200000a4   Data           1  sci.o(.data)
    gp_iic10_tx_address                      0x200000a8   Data           4  sci.o(.data)
    g_iic10_tx_count                         0x200000ac   Data           2  sci.o(.data)
    gp_iic10_rx_address                      0x200000b0   Data           4  sci.o(.data)
    g_iic10_rx_count                         0x200000b4   Data           2  sci.o(.data)
    g_iic10_rx_length                        0x200000b6   Data           2  sci.o(.data)
    g_iic11_master_status_flag               0x200000b8   Data           1  sci.o(.data)
    gp_iic11_tx_address                      0x200000bc   Data           4  sci.o(.data)
    g_iic11_tx_count                         0x200000c0   Data           2  sci.o(.data)
    gp_iic11_rx_address                      0x200000c4   Data           4  sci.o(.data)
    g_iic11_rx_count                         0x200000c8   Data           2  sci.o(.data)
    g_iic11_rx_length                        0x200000ca   Data           2  sci.o(.data)
    gp_uart2_tx_address                      0x200000cc   Data           4  sci.o(.data)
    g_uart2_tx_count                         0x200000d0   Data           2  sci.o(.data)
    gp_uart2_rx_address                      0x200000d4   Data           4  sci.o(.data)
    g_uart2_rx_count                         0x200000d8   Data           2  sci.o(.data)
    g_uart2_rx_length                        0x200000da   Data           2  sci.o(.data)
    gp_spi20_rx_address                      0x200000dc   Data           4  sci.o(.data)
    g_spi20_rx_length                        0x200000e0   Data           2  sci.o(.data)
    g_spi20_rx_count                         0x200000e2   Data           2  sci.o(.data)
    gp_spi20_tx_address                      0x200000e4   Data           4  sci.o(.data)
    g_spi20_tx_length                        0x200000e8   Data           2  sci.o(.data)
    g_spi20_tx_count                         0x200000ea   Data           2  sci.o(.data)
    gp_spi21_rx_address                      0x200000ec   Data           4  sci.o(.data)
    g_spi21_rx_length                        0x200000f0   Data           2  sci.o(.data)
    g_spi21_rx_count                         0x200000f2   Data           2  sci.o(.data)
    gp_spi21_tx_address                      0x200000f4   Data           4  sci.o(.data)
    g_spi21_tx_length                        0x200000f8   Data           2  sci.o(.data)
    g_spi21_tx_count                         0x200000fa   Data           2  sci.o(.data)
    g_iic20_master_status_flag               0x200000fc   Data           1  sci.o(.data)
    gp_iic20_tx_address                      0x20000100   Data           4  sci.o(.data)
    g_iic20_tx_count                         0x20000104   Data           2  sci.o(.data)
    gp_iic20_rx_address                      0x20000108   Data           4  sci.o(.data)
    g_iic20_rx_count                         0x2000010c   Data           2  sci.o(.data)
    g_iic20_rx_length                        0x2000010e   Data           2  sci.o(.data)
    g_iic21_master_status_flag               0x20000110   Data           1  sci.o(.data)
    gp_iic21_tx_address                      0x20000114   Data           4  sci.o(.data)
    g_iic21_tx_count                         0x20000118   Data           2  sci.o(.data)
    gp_iic21_rx_address                      0x2000011c   Data           4  sci.o(.data)
    g_iic21_rx_count                         0x20000120   Data           2  sci.o(.data)
    g_iic21_rx_length                        0x20000122   Data           2  sci.o(.data)
    gp_uart3_tx_address                      0x20000124   Data           4  sci.o(.data)
    g_uart3_tx_count                         0x20000128   Data           2  sci.o(.data)
    gp_uart3_rx_address                      0x2000012c   Data           4  sci.o(.data)
    g_uart3_rx_count                         0x20000130   Data           2  sci.o(.data)
    g_uart3_rx_length                        0x20000132   Data           2  sci.o(.data)
    gp_spi30_rx_address                      0x20000134   Data           4  sci.o(.data)
    g_spi30_rx_length                        0x20000138   Data           2  sci.o(.data)
    g_spi30_rx_count                         0x2000013a   Data           2  sci.o(.data)
    gp_spi30_tx_address                      0x2000013c   Data           4  sci.o(.data)
    g_spi30_send_length                      0x20000140   Data           2  sci.o(.data)
    g_spi30_tx_count                         0x20000142   Data           2  sci.o(.data)
    gp_spi31_rx_address                      0x20000144   Data           4  sci.o(.data)
    g_spi31_rx_length                        0x20000148   Data           2  sci.o(.data)
    g_spi31_rx_count                         0x2000014a   Data           2  sci.o(.data)
    gp_spi31_tx_address                      0x2000014c   Data           4  sci.o(.data)
    g_spi31_send_length                      0x20000150   Data           2  sci.o(.data)
    g_spi31_tx_count                         0x20000152   Data           2  sci.o(.data)
    g_iic30_master_status_flag               0x20000154   Data           1  sci.o(.data)
    gp_iic30_tx_address                      0x20000158   Data           4  sci.o(.data)
    g_iic30_tx_count                         0x2000015c   Data           2  sci.o(.data)
    gp_iic30_rx_address                      0x20000160   Data           4  sci.o(.data)
    g_iic30_rx_count                         0x20000164   Data           2  sci.o(.data)
    g_iic30_rx_length                        0x20000166   Data           2  sci.o(.data)
    g_iic31_master_status_flag               0x20000168   Data           1  sci.o(.data)
    gp_iic31_tx_address                      0x2000016c   Data           4  sci.o(.data)
    g_iic31_tx_count                         0x20000170   Data           2  sci.o(.data)
    gp_iic31_rx_address                      0x20000174   Data           4  sci.o(.data)
    g_iic31_rx_count                         0x20000178   Data           2  sci.o(.data)
    g_iic31_rx_length                        0x2000017a   Data           2  sci.o(.data)
    g_iic00_tx_end                           0x2000018c   Data           1  sci_user.o(.data)
    g_iic00_rx_end                           0x2000018d   Data           1  sci_user.o(.data)
    g_iic01_tx_end                           0x2000018e   Data           1  sci_user.o(.data)
    g_iic01_rx_end                           0x2000018f   Data           1  sci_user.o(.data)
    g_iic10_tx_end                           0x20000190   Data           1  sci_user.o(.data)
    g_iic10_rx_end                           0x20000191   Data           1  sci_user.o(.data)
    g_iic11_tx_end                           0x20000192   Data           1  sci_user.o(.data)
    g_iic11_rx_end                           0x20000193   Data           1  sci_user.o(.data)
    g_iic20_tx_end                           0x20000194   Data           1  sci_user.o(.data)
    g_iic20_rx_end                           0x20000195   Data           1  sci_user.o(.data)
    g_iic21_tx_end                           0x20000196   Data           1  sci_user.o(.data)
    g_iic21_rx_end                           0x20000197   Data           1  sci_user.o(.data)
    g_iic30_tx_end                           0x20000198   Data           1  sci_user.o(.data)
    g_iic30_rx_end                           0x20000199   Data           1  sci_user.o(.data)
    g_iic31_tx_end                           0x2000019a   Data           1  sci_user.o(.data)
    g_iic31_rx_end                           0x2000019b   Data           1  sci_user.o(.data)
    g_uart2_tx_state                         0x2000019c   Data           1  sci_user.o(.data)
    uart_0x10_Rev_Flag                       0x2000019d   Data           1  sci_user.o(.data)
    g_intp0Taken                             0x200001a0   Data           4  intp_user.o(.data)
    g_intp1Taken                             0x200001a4   Data           4  intp_user.o(.data)
    g_intp2Taken                             0x200001a8   Data           4  intp_user.o(.data)
    g_intp3Taken                             0x200001ac   Data           4  intp_user.o(.data)
    g_intp4Taken                             0x200001b0   Data           4  intp_user.o(.data)
    g_intp5Taken                             0x200001b4   Data           4  intp_user.o(.data)
    g_intp6Taken                             0x200001b8   Data           4  intp_user.o(.data)
    g_intp7Taken                             0x200001bc   Data           4  intp_user.o(.data)
    g_intp8Taken                             0x200001c0   Data           4  intp_user.o(.data)
    g_intp9Taken                             0x200001c4   Data           4  intp_user.o(.data)
    g_intp10Taken                            0x200001c8   Data           4  intp_user.o(.data)
    g_intp11Taken                            0x200001cc   Data           4  intp_user.o(.data)
    calendar                                 0x200001d0   Data           7  rtc.o(.data)
    CanSendLock                              0x200001d8   Data           1  can.o(.data)
    g_bReturn                                0x200001d9   Data           1  can.o(.data)
    C0BTR_Reg                                0x200001da   Data           2  can.o(.data)
    C0IE_Reg                                 0x200001dc   Data           2  can.o(.data)
    cantemp16                                0x200001de   Data           8  can.o(.data)
    BU98R10Update                            0x200001e6   Data           5  bu98r10.o(.data)
    u8BU98R10CheckCount                      0x200001eb   Data           1  bu98r10.o(.data)
    DispText                                 0x200001ec   Data           6  seg_lcd.o(.data)
    DispSegNum                               0x200001f2   Data           2  seg_lcd.o(.data)
    OldSpeedStand                            0x200001f4   Data           1  seg_lcd.o(.data)
    IS31FLxxxx_Device_Addr                   0x200001f8   Data           1  is31fl3236.o(.data)
    IIC_3236_NACK_Time                       0x200001fc   Data           4  is31fl3236.o(.data)
    chipType                                 0x20000200   Data           1  is31fl3236.o(.data)
    LedUpdateStep                            0x20000201   Data           1  is31fl3236.o(.data)
    LedUpdateDevice                          0x20000202   Data           1  is31fl3236.o(.data)
    LedUpdateDeviceFlg                       0x20000203   Data           1  is31fl3236.o(.data)
    WR_CN                                    0x20000204   Data           2  aw93015.o(.data)
    test_read                                0x20000208   Data           4  aw93015.o(.data)
    IntKey                                   0x2000020c   Data           1  aw93015.o(.data)
    IIC_addr                                 0x20000210   Data           1  is31_iic_master.o(.data)
    IIC_8563_NACK_Time                       0x20000214   Data           4  is31_iic_master.o(.data)
    g_enLineInPowerStatus                    0x20000218   Data           1  line_in.o(.data)
    g_sleepDelay                             0x2000021a   Data           2  powermanagement_user.o(.data)
    SysWakeUpMode                            0x2000021c   Data           1  system_monitor.o(.data)
    liuKl30temp                              0x2000024e   Data           2  system_monitor.o(.data)
    liuKl30temp2                             0x20000250   Data           2  system_monitor.o(.data)
    PackageCnt                               0x20000284   Data           1  mcu_core_protocol.o(.data)
    Msg_12_Rec_Sta                           0x20000288   Data           8  mcu_core_protocol.o(.data)
    SendLength                               0x20000290   Data           1  mcu_core_protocol.o(.data)
    SendCtrl_Tbl                             0x200002a8   Data          24  mcu_core_protocol.o(.data)
    SEG_Check_ContrlTime                     0x200002c0   Data           2  mcu_core_protocol.o(.data)
    BatteryErrFlg                            0x200002c4   Data           1  mcu_core_protocol.o(.data)
    FlashSync1Hz                             0x200002e6   Data           1  flash_synchronizer.o(.data)
    FlashSync2Hz                             0x200002e7   Data           1  flash_synchronizer.o(.data)
    FlashSync5Hz                             0x200002e8   Data           1  flash_synchronizer.o(.data)
    FlashSync05Hz                            0x200002e9   Data           1  flash_synchronizer.o(.data)
    FlashTimer                               0x200002ea   Data           1  flash_synchronizer.o(.data)
    FlashTimer40                             0x200002eb   Data           1  flash_synchronizer.o(.data)
    FuelDataCount                            0x200002ec   Data           1  fuel.o(.data)
    FuelR                                    0x200002ee   Data           2  fuel.o(.data)
    DesFuelSetp                              0x200002f2   Data           1  fuel.o(.data)
    CurFuelSetp                              0x200002f3   Data           1  fuel.o(.data)
    FuelInitFlag                             0x200002f4   Data           1  fuel.o(.data)
    FuelStateInitFlag                        0x200002f5   Data           1  fuel.o(.data)
    FuelDir                                  0x200002f6   Data           1  fuel.o(.data)
    FuelSensorState                          0x200002f7   Data           1  fuel.o(.data)
    FuelSensorNormalTime                     0x200002f8   Data           2  fuel.o(.data)
    FuelSensorShortTime                      0x200002fa   Data           2  fuel.o(.data)
    FuelSensorOpenTime                       0x200002fc   Data           2  fuel.o(.data)
    FuelADCompleteFlg                        0x200002fe   Data           1  fuel.o(.data)
    TestFuelR                                0x20000300   Data           2  fuel.o(.data)
    TotalODOTemp                             0x20000308   Data           4  services_mileage_user.o(.data)
    ODORemainder                             0x2000030c   Data           2  services_mileage_user.o(.data)
    SaveODOValid                             0x2000030e   Data           1  services_mileage_user.o(.data)
    odoVaild                                 0x20000310   Data           2  services_mileage_user.o(.data)
    ModfyODORemainTimes                      0x20000312   Data           1  services_mileage_user.o(.data)
    ModfyODOTimeDelay_ms                     0x20000314   Data           2  services_mileage_user.o(.data)
    IgnOffKeepMs                             0x2000031a   Data           2  backgroundlight.o(.data)
    IgnOnKeepMs                              0x2000031c   Data           2  backgroundlight.o(.data)
    BGLCurIgnSt                              0x2000031e   Data           1  backgroundlight.o(.data)
    BGLWakeupSt                              0x2000031f   Data           1  backgroundlight.o(.data)
    CurBacklightLv                           0x20000320   Data           1  backgroundlight.o(.data)
    CurBackLightAdjustNum                    0x20000324   Data           1  backgroundlight.o(.data)
    BackLightDerating                        0x20000325   Data           1  backgroundlight.o(.data)
    CurBackLightAdjustValid                  0x20000326   Data           1  backgroundlight.o(.data)
    ThermistorIndex                          0x20000328   Data           2  backgroundlight.o(.data)
    ThermistorCurValue                       0x2000032a   Data           2  backgroundlight.o(.data)
    BLEffectFlag                             0x2000032c   Data           1  backgroundlight.o(.data)
    NTCUpdateTime                            0x2000032e   Data           2  backgroundlight.o(.data)
    PwmStopFlag                              0x20000330   Data           5  backgroundlight.o(.data)
    CurLcdBackLightCycle                     0x20000338   Data           2  bglinterface.o(.data)
    DayOrNight                               0x2000033a   Data           1  bglinterface.o(.data)
    Ave_LightValue                           0x2000033c   Data           4  bglinterface.o(.data)
    pLightValue                              0x20000340   Data           1  bglinterface.o(.data)
    BusOffEvent                              0x2000034a   Data           1  can_user.o(.data)
    BUS_OFF_FLAG                             0x2000034b   Data           1  can_user.o(.data)
    CanSleepDelayTime                        0x2000034c   Data           4  can_user.o(.data)
    ReqSilentTimer                           0x20000352   Data           2  can_user.o(.data)
    CanLibSendFlag                           0x20000356   Data           1  can_user.o(.data)
    LianDianModuleFlg                        0x20000358   Data           1  can_user.o(.data)
    DelfuModuleFlg                           0x20000359   Data           1  can_user.o(.data)
    CAN_Initflag                             0x2000035a   Data           1  can_user.o(.data)
    SendUdsTimeCount_190209                  0x2000035c   Data           4  can_user.o(.data)
    SendUdsTimeCount_220005                  0x20000360   Data           4  can_user.o(.data)
    SendUdsTimeCount_0101                    0x20000364   Data           4  can_user.o(.data)
    DTCCurFaultTimes                         0x20000368   Data           4  can_user.o(.data)
    DTCHisFaultTimes                         0x2000036c   Data           4  can_user.o(.data)
    Mil_Signal_Time                          0x20000370   Data           2  can_user.o(.data)
    Mil_Signal_Connect                       0x20000372   Data           1  can_user.o(.data)
    OldDtcAmnt                               0x20000374   Data           4  can_user.o(.data)
    Dtctotal                                 0x20000378   Data           1  can_user.o(.data)
    DtcCleanflag                             0x20000379   Data           1  can_user.o(.data)
    tempclk                                  0x2000037c   Data           4  can_user.o(.data)
    tempclk1                                 0x20000380   Data           4  can_user.o(.data)
    TCS_WorkModeFlsh                         0x20000384   Data           1  can_user.o(.data)
    ECU_Battery_VoltageFlag                  0x20000385   Data           1  can_user.o(.data)
    Sig_ECU_Temperature_Water                0x20000386   Data           2  can_user.o(.data)
    CANDTC                                   0x2000038c   Data           8  can_user.o(.data)
    DTCShowFaultVal                          0x20000394   Data           8  can_user.o(.data)
    Error                                    0x200003ac   Data           4  app_service.o(.data)
    CrcCheckSum                              0x200003b0   Data           4  app_service.o(.data)
    NormalCanSt                              0x200003b4   Data           1  app_service.o(.data)
    NMCanSt                                  0x200003b5   Data           1  app_service.o(.data)
    MCU_HWversion                            0x200003b6   Data           5  app_service.o(.data)
    MCU_SoftCode                             0x200003bb   Data           6  app_service.o(.data)
    MCU_FBLversion                           0x200003c1   Data           9  app_service.o(.data)
    N_RecLen                                 0x200003ca   Data           2  tp_layer.o(.data)
    U2_Error                                 0x200003cc   Data           4  u2_app_service.o(.data)
    U2_CrcCheckSum                           0x200003d0   Data           4  u2_app_service.o(.data)
    U2_NormalCanSt                           0x200003d4   Data           1  u2_app_service.o(.data)
    U2_NMCanSt                               0x200003d5   Data           1  u2_app_service.o(.data)
    UDS_59_MsgRecFlg                         0x200003d6   Data           1  u2_app_service.o(.data)
    UDS_62_MsgRecFlg                         0x200003d7   Data           1  u2_app_service.o(.data)
    UDS_01_MsgRecFlg                         0x200003d8   Data           1  u2_app_service.o(.data)
    U2_N_RecLen                              0x200003da   Data           2  u2_tp_layer.o(.data)
    SystemCoreClock                          0x200003dc   Data           4  system_bat32a239.o(.data)
    u8CAN_RX_ENABLE                          0x200003e0   Data           1  can_signal_rx.o(.data)
    u8CAN_TX_ENABLE                          0x200003e1   Data           1  can_signal_tx.o(.data)
    pfnSysTickCallBack                       0x200003e4   Data          12  sys_tick.o(.bss)
    g_stSysTickTimer                         0x200003f0   Data          12  sys_tick.o(.bss)
    stADCData                                0x200003fc   Data          16  analog_signals.o(.bss)
    BU98R10Chip0DDRAM                        0x2000040c   Data          90  bu98r10.o(.bss)
    BU98R10Chip0DDRAMBackup                  0x20000466   Data          90  bu98r10.o(.bss)
    BU98R10Chip1DDRAM                        0x200004c0   Data          90  bu98r10.o(.bss)
    BU98R10Chip1DDRAMBackup                  0x2000051a   Data          90  bu98r10.o(.bss)
    SEGLCDBackup                             0x20000574   Data          32  seg_lcd.o(.bss)
    u8IS31Data                               0x20000594   Data          36  is31fl3236.o(.bss)
    WR_REG                                   0x200005b8   Data         200  aw93015.o(.bss)
    SysScheduling                            0x20000680   Data          44  sys_scheduler.o(.bss)
    g_stLineInControl                        0x200006ac   Data          48  line_in.o(.bss)
    pFuncPower                               0x200006dc   Data          44  powermanagement.o(.bss)
    SysFun_KL30Monitor                       0x20000708   Data          12  system_monitor.o(.bss)
    SysFun_KL15Monitor                       0x20000714   Data          12  system_monitor.o(.bss)
    SysNM_KL30Monitor                        0x20000720   Data          12  system_monitor.o(.bss)
    SysNM_KL15Monitor                        0x2000072c   Data          12  system_monitor.o(.bss)
    Uart2_tx_buf                             0x20000738   Data         100  mcu_core_protocol.o(.bss)
    Uart2_rx_buf                             0x2000079c   Data         100  mcu_core_protocol.o(.bss)
    Tel_Mem                                  0x20000978   Data          46  telltales_user.o(.bss)
    FuelData                                 0x200009a6   Data          40  fuel.o(.bss)
    g_WriteMileage                           0x200009d0   Data          14  services_mileage_user.o(.bss)
    g_ReadMileage                            0x200009e0   Data          14  services_mileage_user.o(.bss)
    BackLightPara                            0x200009ee   Data          30  backgroundlight.o(.bss)
    BackLightModifyTimer                     0x20000a0c   Data          10  backgroundlight.o(.bss)
    ThermistorList                           0x20000a16   Data          10  backgroundlight.o(.bss)
    BackupsDuty                              0x20000a20   Data          10  backgroundlight.o(.bss)
    BLStatePara                              0x20000a2a   Data          14  bglinterface.o(.bss)
    BL_Tmp_PARA                              0x20000a38   Data          22  bglinterface.o(.bss)
    lightValue                               0x20000a4e   Data          40  bglinterface.o(.bss)
    KeyStatus                                0x20000a76   Data          16  key.o(.bss)
    CANTest                                  0x20000cf0   Data          60  can_user.o(.bss)
    DiagnoCtl                                0x20000d2c   Data          18  app_service.o(.bss)
    Exct_USData                              0x20000d3e   Data         276  app_service.o(.bss)
    DiagClock                                0x20000e54   Data          56  app_service.o(.bss)
    DiagReciveDTC                            0x20000e8c   Data         100  app_service.o(.bss)
    DiagReciveGaugePara                      0x20000ef0   Data          21  app_service.o(.bss)
    LinkDataBuf                              0x20000f06   Data          24  link_layer.o(.bss)
    LinkData                                 0x20000f1e   Data          12  link_layer.o(.bss)
    g_txCanMsg                               0x20000f2c   Data          16  tp_layer.o(.bss)
    N_US_R_MultiData                         0x20000f3c   Data         276  tp_layer.o(.bss)
    N_US_S_MultiData                         0x20001050   Data         276  tp_layer.o(.bss)
    N_RSPData                                0x20001164   Data          10  tp_layer.o(.bss)
    N_US_R_Data_FF                           0x2000116e   Data          16  tp_layer.o(.bss)
    N_US_S_Data_FF                           0x2000117e   Data          16  tp_layer.o(.bss)
    N_USSFData                               0x2000118e   Data          36  tp_layer.o(.bss)
    U2_DiagnoCtl                             0x200011b4   Data          18  u2_app_service.o(.bss)
    U2_Exct_USData                           0x200011c6   Data         276  u2_app_service.o(.bss)
    U2_DiagClock                             0x200012dc   Data          64  u2_app_service.o(.bss)
    U2_DiagReciveDTC                         0x2000131c   Data         100  u2_app_service.o(.bss)
    U2_DiagReciveGaugePara                   0x20001380   Data          23  u2_app_service.o(.bss)
    U2_LinkDataBuf                           0x20001398   Data          24  u2_link_layer.o(.bss)
    U2_LinkData                              0x200013b0   Data          12  u2_link_layer.o(.bss)
    U2_g_txCanMsg                            0x200013bc   Data          16  u2_tp_layer.o(.bss)
    U2_N_US_R_MultiData                      0x200013cc   Data         276  u2_tp_layer.o(.bss)
    U2_N_US_S_MultiData                      0x200014e0   Data         276  u2_tp_layer.o(.bss)
    U2_N_RSPData                             0x200015f4   Data          10  u2_tp_layer.o(.bss)
    U2_N_US_R_Data_FF                        0x200015fe   Data          16  u2_tp_layer.o(.bss)
    U2_N_US_S_Data_FF                        0x2000160e   Data          16  u2_tp_layer.o(.bss)
    U2_N_USSFData                            0x2000161e   Data          36  u2_tp_layer.o(.bss)
    CanRXMsgOp                               0x20001644   Data          12  can_signal_rx.o(.bss)
    CanMsgTxOp                               0x20001650   Data          16  can_signal_tx.o(.bss)
    LED_Operate                              0x20001660   Data          28  telltales_lib.o(.bss)
    __libspace_start                         0x2000167c   Data          96  libspace.o(.bss)
    __temporary_stack_top$libspace           0x200016dc   Data           0  libspace.o(.bss)
    OdoValidAddress                          0x200016e6   Data           2  eeprommanage.o(.bss.OdoValidAddress)



==============================================================================

Memory Map of the image

  Image Entry point : 0x000000c5

  Load Region LR_IROM1 (Base: 0x00000000, Size: 0x0001209c, Max: 0x00040000, ABSOLUTE, COMPRESSED[0x00011d14])

    Execution Region ER_IROM1 (Exec base: 0x00000000, Load base: 0x00000000, Size: 0x00011cb8, Max: 0x00040000, ABSOLUTE)

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00000000   0x00000000   0x000000c0   Data   RO         7493    RESET               startup_bat32a239.o
    0x000000c0   0x000000c0   0x00000004   Data   RO         7504    .ARM.__AT_0x000000C0  system_bat32a239.o
    0x000000c4   0x000000c4   0x00000008   Code   RO         7867  * !!!main             c_p.l(__main.o)
    0x000000cc   0x000000cc   0x0000003c   Code   RO         8044    !!!scatter          c_p.l(__scatter.o)
    0x00000108   0x00000108   0x0000001c   Code   RO         8046    !!handler_zi        c_p.l(__scatter_zi.o)
    0x00000124   0x00000124   0x00000002   Code   RO         7909    .ARM.Collect$$libinit$$00000000  c_p.l(libinit.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7923    .ARM.Collect$$libinit$$00000002  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7925    .ARM.Collect$$libinit$$00000004  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7928    .ARM.Collect$$libinit$$0000000A  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7930    .ARM.Collect$$libinit$$0000000C  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7932    .ARM.Collect$$libinit$$0000000E  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7935    .ARM.Collect$$libinit$$00000011  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7937    .ARM.Collect$$libinit$$00000013  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7939    .ARM.Collect$$libinit$$00000015  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7941    .ARM.Collect$$libinit$$00000017  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7943    .ARM.Collect$$libinit$$00000019  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7945    .ARM.Collect$$libinit$$0000001B  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7947    .ARM.Collect$$libinit$$0000001D  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7949    .ARM.Collect$$libinit$$0000001F  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7951    .ARM.Collect$$libinit$$00000021  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7953    .ARM.Collect$$libinit$$00000023  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7955    .ARM.Collect$$libinit$$00000025  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7959    .ARM.Collect$$libinit$$0000002C  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7961    .ARM.Collect$$libinit$$0000002E  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7963    .ARM.Collect$$libinit$$00000030  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000000   Code   RO         7965    .ARM.Collect$$libinit$$00000032  c_p.l(libinit2.o)
    0x00000126   0x00000126   0x00000002   Code   RO         7966    .ARM.Collect$$libinit$$00000033  c_p.l(libinit2.o)
    0x00000128   0x00000128   0x00000002   Code   RO         7997    .ARM.Collect$$libshutdown$$00000000  c_p.l(libshutdown.o)
    0x0000012a   0x0000012a   0x00000000   Code   RO         8023    .ARM.Collect$$libshutdown$$00000002  c_p.l(libshutdown2.o)
    0x0000012a   0x0000012a   0x00000000   Code   RO         8025    .ARM.Collect$$libshutdown$$00000004  c_p.l(libshutdown2.o)
    0x0000012a   0x0000012a   0x00000000   Code   RO         8027    .ARM.Collect$$libshutdown$$00000006  c_p.l(libshutdown2.o)
    0x0000012a   0x0000012a   0x00000000   Code   RO         8030    .ARM.Collect$$libshutdown$$00000009  c_p.l(libshutdown2.o)
    0x0000012a   0x0000012a   0x00000000   Code   RO         8033    .ARM.Collect$$libshutdown$$0000000C  c_p.l(libshutdown2.o)
    0x0000012a   0x0000012a   0x00000000   Code   RO         8035    .ARM.Collect$$libshutdown$$0000000E  c_p.l(libshutdown2.o)
    0x0000012a   0x0000012a   0x00000000   Code   RO         8038    .ARM.Collect$$libshutdown$$00000011  c_p.l(libshutdown2.o)
    0x0000012a   0x0000012a   0x00000002   Code   RO         8039    .ARM.Collect$$libshutdown$$00000012  c_p.l(libshutdown2.o)
    0x0000012c   0x0000012c   0x00000000   Code   RO         7869    .ARM.Collect$$rtentry$$00000000  c_p.l(__rtentry.o)
    0x0000012c   0x0000012c   0x00000000   Code   RO         7879    .ARM.Collect$$rtentry$$00000002  c_p.l(__rtentry2.o)
    0x0000012c   0x0000012c   0x00000006   Code   RO         7891    .ARM.Collect$$rtentry$$00000004  c_p.l(__rtentry4.o)
    0x00000132   0x00000132   0x00000000   Code   RO         7881    .ARM.Collect$$rtentry$$00000009  c_p.l(__rtentry2.o)
    0x00000132   0x00000132   0x00000004   Code   RO         7882    .ARM.Collect$$rtentry$$0000000A  c_p.l(__rtentry2.o)
    0x00000136   0x00000136   0x00000000   Code   RO         7884    .ARM.Collect$$rtentry$$0000000C  c_p.l(__rtentry2.o)
    0x00000136   0x00000136   0x00000008   Code   RO         7885    .ARM.Collect$$rtentry$$0000000D  c_p.l(__rtentry2.o)
    0x0000013e   0x0000013e   0x00000002   Code   RO         7914    .ARM.Collect$$rtexit$$00000000  c_p.l(rtexit.o)
    0x00000140   0x00000140   0x00000000   Code   RO         7970    .ARM.Collect$$rtexit$$00000002  c_p.l(rtexit2.o)
    0x00000140   0x00000140   0x00000004   Code   RO         7971    .ARM.Collect$$rtexit$$00000003  c_p.l(rtexit2.o)
    0x00000144   0x00000144   0x00000006   Code   RO         7972    .ARM.Collect$$rtexit$$00000004  c_p.l(rtexit2.o)
    0x0000014a   0x0000014a   0x00000002   PAD
    0x0000014c   0x0000014c   0x00000038   Code   RO         7855    .emb_text           c_p.l(rt_memcpy.o)
    0x00000184   0x00000184   0x00000080   Code   RO         7494    .text               startup_bat32a239.o
    0x00000204   0x00000204   0x00000030   Code   RO         7851    .text               c_p.l(llmul.o)
    0x00000234   0x00000234   0x00000102   Code   RO         7853    .text               c_p.l(lludiv.o)
    0x00000336   0x00000336   0x00000082   Code   RO         7856    .text               c_p.l(rt_memcpy.o)
    0x000003b8   0x000003b8   0x00000040   Code   RO         7859    .text               c_p.l(rt_memclr.o)
    0x000003f8   0x000003f8   0x000001e8   Code   RO         7861    .text               c_p.l(aeabi_sdivfast.o)
    0x000005e0   0x000005e0   0x00000006   Code   RO         7865    .text               c_p.l(heapauxi.o)
    0x000005e6   0x000005e6   0x0000003e   Code   RO         7895    .text               c_p.l(sys_stackheap_outer.o)
    0x00000624   0x00000624   0x00000010   Code   RO         7898    .text               c_p.l(exit.o)
    0x00000634   0x00000634   0x00000008   Code   RO         7910    .text               c_p.l(libspace.o)
    0x0000063c   0x0000063c   0x0000000c   Code   RO         7967    .text               c_p.l(sys_exit.o)
    0x00000648   0x00000648   0x00000002   Code   RO         7986    .text               c_p.l(use_no_semi.o)
    0x0000064a   0x0000064a   0x00000000   Code   RO         7988    .text               c_p.l(indicate_semi.o)
    0x0000064a   0x0000064a   0x00000056   Code   RO         8042    .text               c_p.l(__dczerorl2.o)
    0x000006a0   0x000006a0   0x00000044   Code   RO         7582    .text.ee_IIC_ACK    eepromManage.lib(eeprommanage.o)
    0x000006e4   0x000006e4   0x00000036   Code   RO         7584    .text.ee_IIC_NACK   eepromManage.lib(eeprommanage.o)
    0x0000071a   0x0000071a   0x0000004e   Code   RO         7592    .text.ee_IIC_Read_8bit  eepromManage.lib(eeprommanage.o)
    0x00000768   0x00000768   0x00000056   Code   RO         7588    .text.ee_IIC_SendByte  eepromManage.lib(eeprommanage.o)
    0x000007be   0x000007be   0x0000008a   Code   RO         7560    .text.ee_IIC_SequentialRead  eepromManage.lib(eeprommanage.o)
    0x00000848   0x00000848   0x00000068   Code   RO         7564    .text.ee_IIC_SequentialWrite  eepromManage.lib(eeprommanage.o)
    0x000008b0   0x000008b0   0x00000044   Code   RO         7578    .text.ee_IIC_Start  eepromManage.lib(eeprommanage.o)
    0x000008f4   0x000008f4   0x00000044   Code   RO         7580    .text.ee_IIC_Stop   eepromManage.lib(eeprommanage.o)
    0x00000938   0x00000938   0x0000004c   Code   RO         7586    .text.ee_IIC_WaitAck  eepromManage.lib(eeprommanage.o)
    0x00000984   0x00000984   0x00000014   Code   RO         7546    .text.eeprom_1ms_timeCount  eepromManage.lib(eeprommanage.o)
    0x00000998   0x00000998   0x00000058   Code   RO         7576    .text.eeprom_ClearOdoSection  eepromManage.lib(eeprommanage.o)
    0x000009f0   0x000009f0   0x00000044   Code   RO         7566    .text.eeprom_CreateCRC_8_Num  eepromManage.lib(eeprommanage.o)
    0x00000a34   0x00000a34   0x0000011e   Code   RO         7568    .text.eeprom_OdoDecryption  eepromManage.lib(eeprommanage.o)
    0x00000b52   0x00000b52   0x0000010a   Code   RO         7570    .text.eeprom_OdoEncryption  eepromManage.lib(eeprommanage.o)
    0x00000c5c   0x00000c5c   0x000001f4   Code   RO         7574    .text.eeprom_ReadODO  eepromManage.lib(eeprommanage.o)
    0x00000e50   0x00000e50   0x0000009c   Code   RO         7558    .text.eeprom_ReadRecord  eepromManage.lib(eeprommanage.o)
    0x00000eec   0x00000eec   0x00000040   Code   RO         7548    .text.eeprom_SetParameter  eepromManage.lib(eeprommanage.o)
    0x00000f2c   0x00000f2c   0x000002a0   Code   RO         7572    .text.eeprom_WriteODO  eepromManage.lib(eeprommanage.o)
    0x000011cc   0x000011cc   0x00000134   Code   RO         7562    .text.eeprom_WriteRecord  eepromManage.lib(eeprommanage.o)
    0x00001300   0x00001300   0x00000170   Code   RO          461    i.ADC_Conv_Single_Channel  analog_signals.o
    0x00001470   0x00001470   0x00000034   Code   RO          363    i.ADC_Data_Calibrate  analog_circuits.o
    0x000014a4   0x000014a4   0x0000002c   Code   RO          229    i.ADC_Get_Conversion_Result  adc.o
    0x000014d0   0x000014d0   0x0000000c   Code   RO          230    i.ADC_Get_Conversion_Status  adc.o
    0x000014dc   0x000014dc   0x000000bc   Code   RO          231    i.ADC_Init          adc.o
    0x00001598   0x00001598   0x00000034   Code   RO          364    i.ADC_Input_Voltage_Calc  analog_circuits.o
    0x000015cc   0x000015cc   0x00000018   Code   RO          462    i.ADC_Read_Signal   analog_signals.o
    0x000015e4   0x000015e4   0x00000018   Code   RO          463    i.ADC_Read_Signal_Valid  analog_signals.o
    0x000015fc   0x000015fc   0x000000ac   Code   RO          365    i.ADC_Res_Calc_Circuit101  analog_circuits.o
    0x000016a8   0x000016a8   0x00000034   Code   RO          239    i.ADC_Start         adc.o
    0x000016dc   0x000016dc   0x00000028   Code   RO          240    i.ADC_Start_Conversion  adc.o
    0x00001704   0x00001704   0x00000030   Code   RO          241    i.ADC_Stop          adc.o
    0x00001734   0x00001734   0x00000008   Code   RO          242    i.ADC_Stop_Conversion  adc.o
    0x0000173c   0x0000173c   0x00000016   Code   RO          375    i.ADC_Voltage_Calc_Circuit101  analog_circuits.o
    0x00001752   0x00001752   0x00000002   PAD
    0x00001754   0x00001754   0x00000088   Code   RO          376    i.ADC_Voltage_Calc_Circuit102  analog_circuits.o
    0x000017dc   0x000017dc   0x00000068   Code   RO         5391    i.APP_CAN_Init      can_user.o
    0x00001844   0x00001844   0x00000060   Code   RO          464    i.Analog_Signal_Conv_Init  analog_signals.o
    0x000018a4   0x000018a4   0x0000006c   Code   RO          243    i.Analog_Signal_Conv_Real_Time_Run  adc.o
    0x00001910   0x00001910   0x00000254   Code   RO          465    i.Analog_Signal_Conv_Service  analog_signals.o
    0x00001b64   0x00001b64   0x0000003c   Code   RO          466    i.Analog_Signal_Conv_Stop  analog_signals.o
    0x00001ba0   0x00001ba0   0x00000288   Code   RO         5817    i.App_10_service    app_service.o
    0x00001e28   0x00001e28   0x00000054   Code   RO         6026    i.App_11_Reset_handle  app_serviceproc.o
    0x00001e7c   0x00001e7c   0x000000dc   Code   RO         5818    i.App_11_service    app_service.o
    0x00001f58   0x00001f58   0x0000025c   Code   RO         5820    i.App_22_service    app_service.o
    0x000021b4   0x000021b4   0x0000034c   Code   RO         5821    i.App_27_service    app_service.o
    0x00002500   0x00002500   0x000000cc   Code   RO         5822    i.App_28_service    app_service.o
    0x000025cc   0x000025cc   0x000000bc   Code   RO         5823    i.App_2E_service    app_service.o
    0x00002688   0x00002688   0x00000090   Code   RO         5829    i.App_3E_service    app_service.o
    0x00002718   0x00002718   0x000000c8   Code   RO         5831    i.App_85_service    app_service.o
    0x000027e0   0x000027e0   0x00000018   Code   RO         6027    i.App_CopyRam       app_serviceproc.o
    0x000027f8   0x000027f8   0x00000014   Code   RO         6029    i.App_ErrorInfoInit  app_serviceproc.o
    0x0000280c   0x0000280c   0x00000016   Code   RO         6030    i.App_Load_DID      app_serviceproc.o
    0x00002822   0x00002822   0x00000024   Code   RO         5833    i.App_ReUnlockTimerOver  app_service.o
    0x00002846   0x00002846   0x00000024   Code   RO         5835    i.App_SessionTimerOver  app_service.o
    0x0000286a   0x0000286a   0x0000000e   Code   RO         5836    i.App_SetReUnlockTimer  app_service.o
    0x00002878   0x00002878   0x0000000e   Code   RO         5838    i.App_SetSessionTimer  app_service.o
    0x00002886   0x00002886   0x0000001a   Code   RO         5781    i.App_Telltales_AllOFF  app_telltales.o
    0x000028a0   0x000028a0   0x00000030   Code   RO         5783    i.App_Telltales_Ctrl  app_telltales.o
    0x000028d0   0x000028d0   0x00000020   Code   RO         5062    i.BGLPwm_Config     bglinterface.o
    0x000028f0   0x000028f0   0x00000050   Code   RO         5065    i.BGTask            bglinterface.o
    0x00002940   0x00002940   0x000000f8   Code   RO         2552    i.BU98R10_All_Command_Write  bu98r10.o
    0x00002a38   0x00002a38   0x00000108   Code   RO         2553    i.BU98R10_All_Data_Write  bu98r10.o
    0x00002b40   0x00002b40   0x00000120   Code   RO         2555    i.BU98R10_Init      bu98r10.o
    0x00002c60   0x00002c60   0x0000000a   Code   RO         2556    i.BU98R10_Shutdown  bu98r10.o
    0x00002c6a   0x00002c6a   0x00000002   PAD
    0x00002c6c   0x00002c6c   0x0000001c   Code   RO         2557    i.BU98R10_Update_Request  bu98r10.o
    0x00002c88   0x00002c88   0x00000138   Code   RO         2558    i.BU98R10_Update_Service  bu98r10.o
    0x00002dc0   0x00002dc0   0x00000298   Code   RO         4980    i.BackLightDamp     backgroundlight.o
    0x00003058   0x00003058   0x00000044   Code   RO         5066    i.BackLightSchedu   bglinterface.o
    0x0000309c   0x0000309c   0x00000018   Code   RO         5392    i.BatteryVoltageDelayInit  can_user.o
    0x000030b4   0x000030b4   0x0000000c   Code   RO         6806    i.CAN0Err_Interrupt  isr_bat32a239.o
    0x000030c0   0x000030c0   0x00000008   Code   RO         6807    i.CAN0Rec_Interrupt  isr_bat32a239.o
    0x000030c8   0x000030c8   0x00000008   Code   RO         6808    i.CAN0Trx_Interrupt  isr_bat32a239.o
    0x000030d0   0x000030d0   0x0000000c   Code   RO         6809    i.CAN0Wup_Interrupt  isr_bat32a239.o
    0x000030dc   0x000030dc   0x0000000c   Code   RO         6810    i.CAN1Err_Interrupt  isr_bat32a239.o
    0x000030e8   0x000030e8   0x0000000c   Code   RO         6811    i.CAN1Rec_Interrupt  isr_bat32a239.o
    0x000030f4   0x000030f4   0x0000000c   Code   RO         6812    i.CAN1Trx_Interrupt  isr_bat32a239.o
    0x00003100   0x00003100   0x0000000c   Code   RO         6813    i.CAN1Wup_Interrupt  isr_bat32a239.o
    0x0000310c   0x0000310c   0x000000a8   Code   RO         5395    i.CAN_LED_Check_50msTask  can_user.o
    0x000031b4   0x000031b4   0x0000002c   Code   RO         7617    i.CAN_MSG_Read      CAN_Lib.lib(can_signal_rx.o)
    0x000031e0   0x000031e0   0x00000020   Code   RO         7618    i.CAN_MSG_Status    CAN_Lib.lib(can_signal_rx.o)
    0x00003200   0x00003200   0x00000018   Code   RO         7622    i.CAN_RX_SetEnable  CAN_Lib.lib(can_signal_rx.o)
    0x00003218   0x00003218   0x0000000a   Code   RO         5396    i.CAN_RX_Tick       can_user.o
    0x00003222   0x00003222   0x00000002   PAD
    0x00003224   0x00003224   0x00000018   Code   RO         7706    i.CAN_TX_SetEnable  CAN_Lib.lib(can_signal_tx.o)
    0x0000323c   0x0000323c   0x0000000c   Code   RO         5398    i.CAN_TX_Tick       can_user.o
    0x00003248   0x00003248   0x000000a4   Code   RO         7500    i.CLK_GetCoreFreq   system_bat32a239.o
    0x000032ec   0x000032ec   0x000000b0   Code   RO         7501    i.CLK_GetfIHFreq    system_bat32a239.o
    0x0000339c   0x0000339c   0x00000084   Code   RO         1894    i.CLK_Osc_Setting   clk.o
    0x00003420   0x00003420   0x00000044   Code   RO         1895    i.CLK_PLL_Setting   clk.o
    0x00003464   0x00003464   0x00000024   Code   RO         1896    i.CLK_PLL_Start     clk.o
    0x00003488   0x00003488   0x0000000c   Code   RO         4848    i.CalcODOKL15Init   services_mileage_user.o
    0x00003494   0x00003494   0x00000074   Code   RO         4849    i.CalcODOKL30Init   services_mileage_user.o
    0x00003508   0x00003508   0x000001e8   Code   RO         4850    i.CalcODO_100ms_Services  services_mileage_user.o
    0x000036f0   0x000036f0   0x0000007c   Code   RO         5839    i.CalculateKey      app_service.o
    0x0000376c   0x0000376c   0x000001c8   Code   RO         7623    i.CanMSg_XMS_Analysis  CAN_Lib.lib(can_signal_rx.o)
    0x00003934   0x00003934   0x0000001c   Code   RO         5399    i.Can_BusOffRecover  can_user.o
    0x00003950   0x00003950   0x000000d4   Code   RO         5400    i.Can_BusOff_Fun    can_user.o
    0x00003a24   0x00003a24   0x000000ac   Code   RO         7624    i.Can_RX_BuffInit   CAN_Lib.lib(can_signal_rx.o)
    0x00003ad0   0x00003ad0   0x0000001a   Code   RO         5401    i.Can_Receive_Msg   can_user.o
    0x00003aea   0x00003aea   0x00000002   PAD
    0x00003aec   0x00003aec   0x00000044   Code   RO         5402    i.Can_Set_Buff_105  can_user.o
    0x00003b30   0x00003b30   0x00000018   Code   RO         5403    i.Can_Set_Buff_450  can_user.o
    0x00003b48   0x00003b48   0x00000060   Code   RO         5405    i.Can_Set_Buff_510  can_user.o
    0x00003ba8   0x00003ba8   0x000001a4   Code   RO         5406    i.Can_Set_Buff_515  can_user.o
    0x00003d4c   0x00003d4c   0x0000001e   Code   RO         5407    i.Can_Set_Buff_51C  can_user.o
    0x00003d6a   0x00003d6a   0x00000002   PAD
    0x00003d6c   0x00003d6c   0x00000100   Code   RO         5408    i.Can_Set_Buff_522  can_user.o
    0x00003e6c   0x00003e6c   0x0000010c   Code   RO         5409    i.Can_Set_Buff_523  can_user.o
    0x00003f78   0x00003f78   0x000001b8   Code   RO         7710    i.Can_TX_BuffInit   CAN_Lib.lib(can_signal_tx.o)
    0x00004130   0x00004130   0x0000008c   Code   RO         5410    i.Can_User_Time_Service  can_user.o
    0x000041bc   0x000041bc   0x00000110   Code   RO         5411    i.Can_Write         can_user.o
    0x000042cc   0x000042cc   0x00000390   Code   RO         7711    i.Can_Write_Fun     CAN_Lib.lib(can_signal_tx.o)
    0x0000465c   0x0000465c   0x000001a8   Code   RO         2188    i.Capture_Stop      tim4.o
    0x00004804   0x00004804   0x00000040   Code   RO         1901    i.Clock_Init        clk.o
    0x00004844   0x00004844   0x0000007c   Code   RO         7627    i.Co_Can_Buff_Set   CAN_Lib.lib(can_signal_rx.o)
    0x000048c0   0x000048c0   0x00000064   Code   RO         5214    i.Co_Can_ConvertSubID  can_communication_matrix.o
    0x00004924   0x00004924   0x0000008c   Code   RO         4076    i.Common_DataInit   common_interface.o
    0x000049b0   0x000049b0   0x0000000c   Code   RO         4077    i.Common_GetIgnOffTime  common_interface.o
    0x000049bc   0x000049bc   0x0000000c   Code   RO         4078    i.Common_GetIgnOnTime  common_interface.o
    0x000049c8   0x000049c8   0x0000000c   Code   RO         4084    i.Common_Get_DispMode  common_interface.o
    0x000049d4   0x000049d4   0x0000000c   Code   RO         4085    i.Common_Get_Disp_E_Speed  common_interface.o
    0x000049e0   0x000049e0   0x0000000c   Code   RO         4088    i.Common_Get_Disp_V_Speed  common_interface.o
    0x000049ec   0x000049ec   0x0000000c   Code   RO         4093    i.Common_Get_IG_Sts  common_interface.o
    0x000049f8   0x000049f8   0x0000000c   Code   RO         4094    i.Common_Get_Language  common_interface.o
    0x00004a04   0x00004a04   0x00000060   Code   RO         4097    i.Common_Input_Para  common_interface.o
    0x00004a64   0x00004a64   0x0000000c   Code   RO         4101    i.Common_SetSelfcheckStart  common_interface.o
    0x00004a70   0x00004a70   0x0000000c   Code   RO         4112    i.Common_Set_IG_Sts  common_interface.o
    0x00004a7c   0x00004a7c   0x00000030   Code   RO         4852    i.Data_Clear_Trip   services_mileage_user.o
    0x00004aac   0x00004aac   0x0000000c   Code   RO         4932    i.Data_Gear_KL15_Init  data_gear.o
    0x00004ab8   0x00004ab8   0x00000002   Code   RO         4933    i.Data_Gear_KL30_Init  data_gear.o
    0x00004aba   0x00004aba   0x00000002   PAD
    0x00004abc   0x00004abc   0x0000000c   Code   RO         4854    i.Data_ODO_Read     services_mileage_user.o
    0x00004ac8   0x00004ac8   0x0000001c   Code   RO         4855    i.Data_Read_Trip    services_mileage_user.o
    0x00004ae4   0x00004ae4   0x0000000c   Code   RO         5412    i.DelfuModuleIn     can_user.o
    0x00004af0   0x00004af0   0x0000017c   Code   RO         5413    i.Diag_Req_Send     can_user.o
    0x00004c6c   0x00004c6c   0x000000ec   Code   RO         6031    i.Diagno_Tick       app_serviceproc.o
    0x00004d58   0x00004d58   0x0000008c   Code   RO         5841    i.DiagnosisInit_main  app_service.o
    0x00004de4   0x00004de4   0x0000029c   Code   RO         5842    i.Diagnosis_main    app_service.o
    0x00005080   0x00005080   0x000000c8   Code   RO         4324    i.Drive_Info_Display_Update_Service  mcu_core_protocol.o
    0x00005148   0x00005148   0x0000001c   Code   RO         5414    i.DtcFaultInit      can_user.o
    0x00005164   0x00005164   0x00000008   Code   RO         4766    i.EE_FeedDog        eemanager_interface.o
    0x0000516c   0x0000516c   0x00000004   Code   RO         4767    i.EE_NOP            eemanager_interface.o
    0x00005170   0x00005170   0x0000001c   Code   RO         4768    i.EE_SCL_OUT        eemanager_interface.o
    0x0000518c   0x0000518c   0x0000000e   Code   RO         4769    i.EE_SCL_OutConfig  eemanager_interface.o
    0x0000519a   0x0000519a   0x00000016   Code   RO         4770    i.EE_SDA_GetValue   eemanager_interface.o
    0x000051b0   0x000051b0   0x0000000e   Code   RO         4771    i.EE_SDA_InConfig   eemanager_interface.o
    0x000051be   0x000051be   0x0000001c   Code   RO         4772    i.EE_SDA_OUT        eemanager_interface.o
    0x000051da   0x000051da   0x0000000e   Code   RO         4773    i.EE_SDA_OutConfig  eemanager_interface.o
    0x000051e8   0x000051e8   0x00000018   Code   RO         4325    i.Enable_Cyc_Msg    mcu_core_protocol.o
    0x00005200   0x00005200   0x00000088   Code   RO         4659    i.Flash_Sync_Signal_Generation_Service  flash_synchronizer.o
    0x00005288   0x00005288   0x00000018   Code   RO         4691    i.Fuel_Cal_Sevice   fuel.o
    0x000052a0   0x000052a0   0x000002bc   Code   RO         4692    i.Fuel_Gauges_Cal   fuel.o
    0x0000555c   0x0000555c   0x00000064   Code   RO         4693    i.Fuel_KL15_Init    fuel.o
    0x000055c0   0x000055c0   0x0000000c   Code   RO         4694    i.Fuel_KL30_Init    fuel.o
    0x000055cc   0x000055cc   0x000000dc   Code   RO         4695    i.Fuel_R_Cal        fuel.o
    0x000056a8   0x000056a8   0x00000110   Code   RO         4696    i.Fuel_State_Check  fuel.o
    0x000057b8   0x000057b8   0x00000060   Code   RO         2977    i.GET_Key_Prosess   aw93015.o
    0x00005818   0x00005818   0x000005bc   Code   RO            4    i.GPIO_Init         gpio.o
    0x00005dd4   0x00005dd4   0x0000021c   Code   RO         5416    i.GetAllDtcFault    can_user.o
    0x00005ff0   0x00005ff0   0x0000000c   Code   RO         5417    i.GetDtcAmnt        can_user.o
    0x00005ffc   0x00005ffc   0x00000010   Code   RO         5418    i.GetDtcDispNum     can_user.o
    0x0000600c   0x0000600c   0x0000000c   Code   RO         5420    i.Get_Bcm_Module    can_user.o
    0x00006018   0x00006018   0x00000018   Code   RO         2356    i.Get_CH0_BusOffStatus  can.o
    0x00006030   0x00006030   0x0000000c   Code   RO         4697    i.Get_CurFuelSetp   fuel.o
    0x0000603c   0x0000603c   0x0000000c   Code   RO         5067    i.Get_Day_Or_Night  bglinterface.o
    0x00006048   0x00006048   0x0000000c   Code   RO         4699    i.Get_Fuel_Sensor_State  fuel.o
    0x00006054   0x00006054   0x00000394   Code   RO         4328    i.Get_ID_01_Data    mcu_core_protocol.o
    0x000063e8   0x000063e8   0x00000048   Code   RO         4329    i.Get_ID_02_Data    mcu_core_protocol.o
    0x00006430   0x00006430   0x0000001a   Code   RO         5215    i.Get_ID_101_ECU_Engine_Temperature  can_communication_matrix.o
    0x0000644a   0x0000644a   0x00000010   Code   RO         5219    i.Get_ID_111_ISG_Ready  can_communication_matrix.o
    0x0000645a   0x0000645a   0x00000010   Code   RO         5220    i.Get_ID_111_Sig_ISG_SideStand  can_communication_matrix.o
    0x0000646a   0x0000646a   0x00000010   Code   RO         5225    i.Get_ID_125_Sig_TCS_WorkMode  can_communication_matrix.o
    0x0000647a   0x0000647a   0x0000000c   Code   RO         5228    i.Get_ID_401_Sig_ECU_Battery_Voltage  can_communication_matrix.o
    0x00006486   0x00006486   0x0000000c   Code   RO         5229    i.Get_ID_402_ECU_DTC1Amnt  can_communication_matrix.o
    0x00006492   0x00006492   0x0000000c   Code   RO         5230    i.Get_ID_402_ECU_DTCH1  can_communication_matrix.o
    0x0000649e   0x0000649e   0x0000000c   Code   RO         5231    i.Get_ID_402_ECU_DTCH2  can_communication_matrix.o
    0x000064aa   0x000064aa   0x0000000c   Code   RO         5232    i.Get_ID_402_ECU_DTCL1  can_communication_matrix.o
    0x000064b6   0x000064b6   0x0000000c   Code   RO         5233    i.Get_ID_402_ECU_DTCL2  can_communication_matrix.o
    0x000064c2   0x000064c2   0x0000000c   Code   RO         5234    i.Get_ID_402_ECU_DTCM1  can_communication_matrix.o
    0x000064ce   0x000064ce   0x0000000c   Code   RO         5235    i.Get_ID_402_ECU_DTCM2  can_communication_matrix.o
    0x000064da   0x000064da   0x00000010   Code   RO         5236    i.Get_ID_55C_Sig_ClearTrip  can_communication_matrix.o
    0x000064ea   0x000064ea   0x0000000c   Code   RO         5237    i.Get_ID_55C_Sig_ModifyODOSts  can_communication_matrix.o
    0x000064f6   0x000064f6   0x00000024   Code   RO         5238    i.Get_ID_55C_Sig_ModifyODOValue  can_communication_matrix.o
    0x0000651a   0x0000651a   0x00000016   Code   RO         5147    i.Get_Key1_Line_In_Sts  key.o
    0x00006530   0x00006530   0x00000018   Code   RO         5148    i.Get_Key2_Line_In_Sts  key.o
    0x00006548   0x00006548   0x0000000c   Code   RO         5422    i.Get_LED_ECU_Battery_VoltageFlag  can_user.o
    0x00006554   0x00006554   0x0000000c   Code   RO         5424    i.Get_RSCAN0Busoff_Status  can_user.o
    0x00006560   0x00006560   0x00000030   Code   RO         2239    i.Get_RTC_Time      rtc.o
    0x00006590   0x00006590   0x0000000c   Code   RO         5425    i.Get_ReqSilentTimer  can_user.o
    0x0000659c   0x0000659c   0x0000000c   Code   RO         5426    i.Get_TCS_WorkModeFlash  can_user.o
    0x000065a8   0x000065a8   0x0000000c   Code   RO         6301    i.Get_UDS_01_MsgRecFlg  u2_app_service.o
    0x000065b4   0x000065b4   0x0000000c   Code   RO         6302    i.Get_UDS_59_MsgRecFlg  u2_app_service.o
    0x000065c0   0x000065c0   0x0000000c   Code   RO         6303    i.Get_UDS_62_MsgRecFlg  u2_app_service.o
    0x000065cc   0x000065cc   0x00000024   Code   RO          551    i.IIC20_Stop        sci.o
    0x000065f0   0x000065f0   0x0000006c   Code   RO          552    i.IIC20_StopCondition  sci.o
    0x0000665c   0x0000665c   0x00000028   Code   RO          557    i.IIC21_Stop        sci.o
    0x00006684   0x00006684   0x00000064   Code   RO          558    i.IIC21_StopCondition  sci.o
    0x000066e8   0x000066e8   0x00000016   Code   RO         2978    i.IIC2_SDA_OUT      aw93015.o
    0x000066fe   0x000066fe   0x0000000e   Code   RO         2979    i.IIC_SDA2_IN       aw93015.o
    0x0000670c   0x0000670c   0x00000016   Code   RO         3099    i.IIC_SDAGet        is31_iic_master.o
    0x00006722   0x00006722   0x00000002   PAD
    0x00006724   0x00006724   0x00000504   Code   RO         2003    i.INTP_Init         intp.o
    0x00006c28   0x00006c28   0x000000f8   Code   RO         2004    i.INTP_Start        intp.o
    0x00006d20   0x00006d20   0x0000002c   Code   RO         6814    i.IRQ00_Handler     isr_bat32a239.o
    0x00006d4c   0x00006d4c   0x00000020   Code   RO         6815    i.IRQ01_Handler     isr_bat32a239.o
    0x00006d6c   0x00006d6c   0x00000020   Code   RO         6816    i.IRQ02_Handler     isr_bat32a239.o
    0x00006d8c   0x00006d8c   0x00000020   Code   RO         6817    i.IRQ03_Handler     isr_bat32a239.o
    0x00006dac   0x00006dac   0x00000020   Code   RO         6818    i.IRQ04_Handler     isr_bat32a239.o
    0x00006dcc   0x00006dcc   0x00000020   Code   RO         6819    i.IRQ05_Handler     isr_bat32a239.o
    0x00006dec   0x00006dec   0x00000020   Code   RO         6820    i.IRQ06_Handler     isr_bat32a239.o
    0x00006e0c   0x00006e0c   0x00000020   Code   RO         6821    i.IRQ07_Handler     isr_bat32a239.o
    0x00006e2c   0x00006e2c   0x00000020   Code   RO         6822    i.IRQ08_Handler     isr_bat32a239.o
    0x00006e4c   0x00006e4c   0x00000024   Code   RO         6823    i.IRQ09_Handler     isr_bat32a239.o
    0x00006e70   0x00006e70   0x00000014   Code   RO         6824    i.IRQ10_Handler     isr_bat32a239.o
    0x00006e84   0x00006e84   0x00000014   Code   RO         6825    i.IRQ11_Handler     isr_bat32a239.o
    0x00006e98   0x00006e98   0x00000024   Code   RO         6826    i.IRQ12_Handler     isr_bat32a239.o
    0x00006ebc   0x00006ebc   0x00000014   Code   RO         6827    i.IRQ13_Handler     isr_bat32a239.o
    0x00006ed0   0x00006ed0   0x00000014   Code   RO         6828    i.IRQ14_Handler     isr_bat32a239.o
    0x00006ee4   0x00006ee4   0x00000024   Code   RO         6829    i.IRQ15_Handler     isr_bat32a239.o
    0x00006f08   0x00006f08   0x0000002c   Code   RO         6830    i.IRQ16_Handler     isr_bat32a239.o
    0x00006f34   0x00006f34   0x00000030   Code   RO         6831    i.IRQ17_Handler     isr_bat32a239.o
    0x00006f64   0x00006f64   0x00000030   Code   RO         6832    i.IRQ18_Handler     isr_bat32a239.o
    0x00006f94   0x00006f94   0x00000030   Code   RO         6833    i.IRQ19_Handler     isr_bat32a239.o
    0x00006fc4   0x00006fc4   0x00000030   Code   RO         6834    i.IRQ20_Handler     isr_bat32a239.o
    0x00006ff4   0x00006ff4   0x00000014   Code   RO         6835    i.IRQ21_Handler     isr_bat32a239.o
    0x00007008   0x00007008   0x00000024   Code   RO         6836    i.IRQ22_Handler     isr_bat32a239.o
    0x0000702c   0x0000702c   0x00000024   Code   RO         6837    i.IRQ23_Handler     isr_bat32a239.o
    0x00007050   0x00007050   0x00000020   Code   RO         6838    i.IRQ24_Handler     isr_bat32a239.o
    0x00007070   0x00007070   0x00000024   Code   RO         6839    i.IRQ25_Handler     isr_bat32a239.o
    0x00007094   0x00007094   0x00000024   Code   RO         6840    i.IRQ26_Handler     isr_bat32a239.o
    0x000070b8   0x000070b8   0x00000014   Code   RO         6841    i.IRQ27_Handler     isr_bat32a239.o
    0x000070cc   0x000070cc   0x00000014   Code   RO         6842    i.IRQ28_Handler     isr_bat32a239.o
    0x000070e0   0x000070e0   0x00000024   Code   RO         6843    i.IRQ29_Handler     isr_bat32a239.o
    0x00007104   0x00007104   0x00000024   Code   RO         6844    i.IRQ30_Handler     isr_bat32a239.o
    0x00007128   0x00007128   0x00000024   Code   RO         6845    i.IRQ31_Handler     isr_bat32a239.o
    0x0000714c   0x0000714c   0x0000026c   Code   RO         2901    i.IS31FL3236_Init   is31fl3236.o
    0x000073b8   0x000073b8   0x000001ac   Code   RO         2902    i.IS31FL3236_Update  is31fl3236.o
    0x00007564   0x00007564   0x00000038   Code   RO         3100    i.IS31_IIC_ACK      is31_iic_master.o
    0x0000759c   0x0000759c   0x00000050   Code   RO         3102    i.IS31_IIC_ReadByte  is31_iic_master.o
    0x000075ec   0x000075ec   0x00000050   Code   RO         3104    i.IS31_IIC_SCL_Dir_Out  is31_iic_master.o
    0x0000763c   0x0000763c   0x0000000e   Code   RO         3105    i.IS31_IIC_SDA_Dir_In  is31_iic_master.o
    0x0000764a   0x0000764a   0x0000000e   Code   RO         3106    i.IS31_IIC_SDA_Dir_Out  is31_iic_master.o
    0x00007658   0x00007658   0x00000056   Code   RO         3107    i.IS31_IIC_SendByte  is31_iic_master.o
    0x000076ae   0x000076ae   0x00000038   Code   RO         3108    i.IS31_IIC_Start    is31_iic_master.o
    0x000076e6   0x000076e6   0x00000038   Code   RO         3109    i.IS31_IIC_Stop     is31_iic_master.o
    0x0000771e   0x0000771e   0x00000002   PAD
    0x00007720   0x00007720   0x000000a8   Code   RO         3110    i.IS31_IIC_WaitAck  is31_iic_master.o
    0x000077c8   0x000077c8   0x00000016   Code   RO         3111    i.IS31_IIC_delay    is31_iic_master.o
    0x000077de   0x000077de   0x0000000a   Code   RO         2903    i.IS31_OFF_Wakeup   is31fl3236.o
    0x000077e8   0x000077e8   0x0000001c   Code   RO         2904    i.IS31_Set_SDB_Pin  is31fl3236.o
    0x00007804   0x00007804   0x0000000a   Code   RO         2905    i.IS31_Shutdown     is31fl3236.o
    0x0000780e   0x0000780e   0x00000002   PAD
    0x00007810   0x00007810   0x0000008c   Code   RO         2980    i.Init93015_IIC     aw93015.o
    0x0000789c   0x0000789c   0x000003fc   Code   RO         5151    i.Key_Status_Detect_Service  key.o
    0x00007c98   0x00007c98   0x00000034   Code   RO         5152    i.Key_Status_Init   key.o
    0x00007ccc   0x00007ccc   0x00000028   Code   RO         4439    i.LED_ABS_Execution  telltales_user.o
    0x00007cf4   0x00007cf4   0x0000001c   Code   RO         4440    i.LED_ABS_Judgement  telltales_user.o
    0x00007d10   0x00007d10   0x00000028   Code   RO         4441    i.LED_AutoStarStop_Execution  telltales_user.o
    0x00007d38   0x00007d38   0x0000001c   Code   RO         4442    i.LED_AutoStarStop_Judgement  telltales_user.o
    0x00007d54   0x00007d54   0x00000014   Code   RO         4443    i.LED_Auto_HI_BEAM_Execution  telltales_user.o
    0x00007d68   0x00007d68   0x00000010   Code   RO         4444    i.LED_Auto_HI_BEAM_Judgement  telltales_user.o
    0x00007d78   0x00007d78   0x00000028   Code   RO         4445    i.LED_Batterylow_Execution  telltales_user.o
    0x00007da0   0x00007da0   0x0000002e   Code   RO         4446    i.LED_Batterylow_Judgement  telltales_user.o
    0x00007dce   0x00007dce   0x00000028   Code   RO         4447    i.LED_ENGINE_OIL_LOW_Execution  telltales_user.o
    0x00007df6   0x00007df6   0x00000010   Code   RO         4448    i.LED_ENGINE_OIL_LOW_Judgement  telltales_user.o
    0x00007e06   0x00007e06   0x00000054   Code   RO         4449    i.LED_Fuel_Execution  telltales_user.o
    0x00007e5a   0x00007e5a   0x00000002   PAD
    0x00007e5c   0x00007e5c   0x00000040   Code   RO         4450    i.LED_Fuel_Judgement  telltales_user.o
    0x00007e9c   0x00007e9c   0x00000028   Code   RO         4451    i.LED_HI_BEAM_Execution  telltales_user.o
    0x00007ec4   0x00007ec4   0x0000001c   Code   RO         4452    i.LED_HI_BEAM_Judgement  telltales_user.o
    0x00007ee0   0x00007ee0   0x00000028   Code   RO         4453    i.LED_LEFT_Execution  telltales_user.o
    0x00007f08   0x00007f08   0x0000001c   Code   RO         4454    i.LED_LEFT_Judgement  telltales_user.o
    0x00007f24   0x00007f24   0x00000028   Code   RO         4455    i.LED_MIL_Execution  telltales_user.o
    0x00007f4c   0x00007f4c   0x0000001c   Code   RO         4456    i.LED_MIL_Judgement  telltales_user.o
    0x00007f68   0x00007f68   0x00000028   Code   RO         4457    i.LED_READY_Execution  telltales_user.o
    0x00007f90   0x00007f90   0x0000001a   Code   RO         4458    i.LED_READY_Judgement  telltales_user.o
    0x00007faa   0x00007faa   0x00000028   Code   RO         4459    i.LED_RIGHT_Execution  telltales_user.o
    0x00007fd2   0x00007fd2   0x0000001c   Code   RO         4460    i.LED_RIGHT_Judgement  telltales_user.o
    0x00007fee   0x00007fee   0x00000028   Code   RO         4461    i.LED_Shore_Execution  telltales_user.o
    0x00008016   0x00008016   0x0000001a   Code   RO         4462    i.LED_Shore_Judgement  telltales_user.o
    0x00008030   0x00008030   0x00000028   Code   RO         4463    i.LED_TPMS_Execution  telltales_user.o
    0x00008058   0x00008058   0x00000010   Code   RO         4464    i.LED_TPMS_Judgement  telltales_user.o
    0x00008068   0x00008068   0x00000002   Code   RO         4465    i.LED_TSC_Execution  telltales_user.o
    0x0000806a   0x0000806a   0x0000000e   Code   RO         4466    i.LED_TSC_Judgement  telltales_user.o
    0x00008078   0x00008078   0x00000054   Code   RO         4467    i.LED_Temp_Execution  telltales_user.o
    0x000080cc   0x000080cc   0x00000018   Code   RO         4468    i.LED_Temp_Judgement  telltales_user.o
    0x000080e4   0x000080e4   0x00000016   Code   RO         3541    i.LINE_IN_Get_ABS   line_in.o
    0x000080fa   0x000080fa   0x00000016   Code   RO         3542    i.LINE_IN_Get_AutoStarStop  line_in.o
    0x00008110   0x00008110   0x00000016   Code   RO         3543    i.LINE_IN_Get_HighBeam  line_in.o
    0x00008126   0x00008126   0x00000016   Code   RO         3544    i.LINE_IN_Get_LeftTurn  line_in.o
    0x0000813c   0x0000813c   0x00000016   Code   RO         3545    i.LINE_IN_Get_OBD   line_in.o
    0x00008152   0x00008152   0x00000016   Code   RO         3546    i.LINE_IN_Get_OilPressure  line_in.o
    0x00008168   0x00008168   0x00000016   Code   RO         3547    i.LINE_IN_Get_RightTurn  line_in.o
    0x0000817e   0x0000817e   0x00000016   Code   RO         3548    i.LINE_IN_Get_TirePressure  line_in.o
    0x00008194   0x00008194   0x00000014   Code   RO         6101    i.LK_FillMsg        link_layer.o
    0x000081a8   0x000081a8   0x00000050   Code   RO         6102    i.LK_Link_main      link_layer.o
    0x000081f8   0x000081f8   0x000000d0   Code   RO         3549    i.Line_In_Debounce_Handle  line_in.o
    0x000082c8   0x000082c8   0x00000058   Code   RO         3550    i.Line_In_Debounce_Service  line_in.o
    0x00008320   0x00008320   0x00000010   Code   RO         3551    i.Line_In_Get_Status  line_in.o
    0x00008330   0x00008330   0x00000040   Code   RO         3552    i.Line_In_KL15_OFF_Init  line_in.o
    0x00008370   0x00008370   0x00000040   Code   RO         3553    i.Line_In_KL15_ON_Init  line_in.o
    0x000083b0   0x000083b0   0x00000038   Code   RO         3554    i.Line_In_KL30_Init  line_in.o
    0x000083e8   0x000083e8   0x00000024   Code   RO         4856    i.Mileage_Delay_ms  services_mileage_user.o
    0x0000840c   0x0000840c   0x000000ac   Code   RO         2981    i.PD_IIC_ReadPage   aw93015.o
    0x000084b8   0x000084b8   0x00000034   Code   RO         2982    i.PD_IIC_ReadReg    aw93015.o
    0x000084ec   0x000084ec   0x000000b4   Code   RO         2983    i.PD_IIC_WritePage  aw93015.o
    0x000085a0   0x000085a0   0x0000002c   Code   RO         2984    i.PD_IIC_WriteReg   aw93015.o
    0x000085cc   0x000085cc   0x00000024   Code   RO           12    i.PORT_ClrBit       gpio.o
    0x000085f0   0x000085f0   0x0000001c   Code   RO           13    i.PORT_GetBit       gpio.o
    0x0000860c   0x0000860c   0x00000198   Code   RO           14    i.PORT_Init         gpio.o
    0x000087a4   0x000087a4   0x00000024   Code   RO           15    i.PORT_SetBit       gpio.o
    0x000087c8   0x000087c8   0x00000040   Code   RO         3653    i.PowerMemInit      powermanagement.o
    0x00008808   0x00008808   0x00000002   Code   RO         3697    i.Power_IG_LVP_Init  powermanagement_user.o
    0x0000880a   0x0000880a   0x00000002   PAD
    0x0000880c   0x0000880c   0x00000068   Code   RO         3698    i.Power_IG_OFF_Init  powermanagement_user.o
    0x00008874   0x00008874   0x00000062   Code   RO         3699    i.Power_IG_ON_Init  powermanagement_user.o
    0x000088d6   0x000088d6   0x00000002   Code   RO         3700    i.Power_IG_OVP_Init  powermanagement_user.o
    0x000088d8   0x000088d8   0x00000018   Code   RO         3701    i.Power_KL30_Init   powermanagement_user.o
    0x000088f0   0x000088f0   0x00000028   Code   RO         3654    i.Power_Management_Init  powermanagement.o
    0x00008918   0x00008918   0x00000068   Code   RO         3702    i.Power_Management_Lib_Init  powermanagement_user.o
    0x00008980   0x00008980   0x00000124   Code   RO         3655    i.Power_Management_Service  powermanagement.o
    0x00008aa4   0x00008aa4   0x00000018   Code   RO         3703    i.Power_Management_Service_user  powermanagement_user.o
    0x00008abc   0x00008abc   0x00000168   Code   RO         3704    i.Power_Sleep_Init  powermanagement_user.o
    0x00008c24   0x00008c24   0x0000005c   Code   RO         3705    i.Power_Stay_OFF    powermanagement_user.o
    0x00008c80   0x00008c80   0x00000030   Code   RO         3706    i.Power_Stay_ON     powermanagement_user.o
    0x00008cb0   0x00008cb0   0x00000004   Code   RO         3707    i.Power_Stay_Protect  powermanagement_user.o
    0x00008cb4   0x00008cb4   0x0000000c   Code   RO         3708    i.Power_Stay_Sleep  powermanagement_user.o
    0x00008cc0   0x00008cc0   0x0000003a   Code   RO         3709    i.Power_Wakeup_Init  powermanagement_user.o
    0x00008cfa   0x00008cfa   0x00000002   PAD
    0x00008cfc   0x00008cfc   0x0000001c   Code   RO         4331    i.Protocol_KL15_ON_Init  mcu_core_protocol.o
    0x00008d18   0x00008d18   0x00000064   Code   RO         2240    i.RTC_Get_CounterValue  rtc.o
    0x00008d7c   0x00008d7c   0x0000009c   Code   RO         2241    i.RTC_Init          rtc.o
    0x00008e18   0x00008e18   0x00000010   Code   RO         2242    i.RTC_Service       rtc.o
    0x00008e28   0x00008e28   0x00000058   Code   RO         2243    i.RTC_Set_CounterValue  rtc.o
    0x00008e80   0x00008e80   0x00000074   Code   RO         2244    i.RTC_Start         rtc.o
    0x00008ef4   0x00008ef4   0x00000010   Code   RO         3995    i.RTE_ForceRead_KL30_Voltage  rte_adc.o
    0x00008f04   0x00008f04   0x00000010   Code   RO         4000    i.RTE_Read_KL15_Voltage  rte_adc.o
    0x00008f14   0x00008f14   0x00000010   Code   RO         4001    i.RTE_Read_KL30_Valid  rte_adc.o
    0x00008f24   0x00008f24   0x00000010   Code   RO         4002    i.RTE_Read_KL30_Voltage  rte_adc.o
    0x00008f34   0x00008f34   0x00000018   Code   RO         5428    i.ReqSilentTimer100mSService  can_user.o
    0x00008f4c   0x00008f4c   0x00000018   Code   RO         5429    i.Reset_Mil_Signal_Time  can_user.o
    0x00008f64   0x00008f64   0x00000248   Code   RO         2646    i.SEG_Coolant_Temp_Display  seg_lcd.o
    0x000091ac   0x000091ac   0x000001fc   Code   RO         2647    i.SEG_Fuel_Level_Display  seg_lcd.o
    0x000093a8   0x000093a8   0x00000018   Code   RO         2648    i.SEG_LCD_ABS       seg_lcd.o
    0x000093c0   0x000093c0   0x00000018   Code   RO         2649    i.SEG_LCD_AutoStarStop  seg_lcd.o
    0x000093d8   0x000093d8   0x00000684   Code   RO         2651    i.SEG_LCD_Battery_Voltage_Display  seg_lcd.o
    0x00009a5c   0x00009a5c   0x00000414   Code   RO         2652    i.SEG_LCD_Battery_Voltage_Selftest  seg_lcd.o
    0x00009e70   0x00009e70   0x0000001c   Code   RO         2653    i.SEG_LCD_Batterylow  seg_lcd.o
    0x00009e8c   0x00009e8c   0x000008b8   Code   RO         2654    i.SEG_LCD_Engine_Speed_Seg_Display  seg_lcd.o
    0x0000a744   0x0000a744   0x00000560   Code   RO         2655    i.SEG_LCD_Engine_Speed_Seg_Selftest  seg_lcd.o
    0x0000aca4   0x0000aca4   0x0000001c   Code   RO         2657    i.SEG_LCD_Fuel      seg_lcd.o
    0x0000acc0   0x0000acc0   0x00000238   Code   RO         2658    i.SEG_LCD_Gear_Display  seg_lcd.o
    0x0000aef8   0x0000aef8   0x00000158   Code   RO         2659    i.SEG_LCD_Gear_Selftest  seg_lcd.o
    0x0000b050   0x0000b050   0x0000001c   Code   RO         2660    i.SEG_LCD_HI_BEAM   seg_lcd.o
    0x0000b06c   0x0000b06c   0x00000018   Code   RO         2661    i.SEG_LCD_HighBeam  seg_lcd.o
    0x0000b084   0x0000b084   0x0000004c   Code   RO         2662    i.SEG_LCD_Init      seg_lcd.o
    0x0000b0d0   0x0000b0d0   0x00000018   Code   RO         2663    i.SEG_LCD_LeftTurn  seg_lcd.o
    0x0000b0e8   0x0000b0e8   0x0000001c   Code   RO         2664    i.SEG_LCD_OBD       seg_lcd.o
    0x0000b104   0x0000b104   0x00000b20   Code   RO         2665    i.SEG_LCD_ODO_Trip_Display  seg_lcd.o
    0x0000bc24   0x0000bc24   0x00000750   Code   RO         2666    i.SEG_LCD_ODO_Trip_FaultCode_Selftest  seg_lcd.o
    0x0000c374   0x0000c374   0x0000001c   Code   RO         2667    i.SEG_LCD_OilPressure  seg_lcd.o
    0x0000c390   0x0000c390   0x00000018   Code   RO         2668    i.SEG_LCD_READY     seg_lcd.o
    0x0000c3a8   0x0000c3a8   0x00000018   Code   RO         2669    i.SEG_LCD_RightTurn  seg_lcd.o
    0x0000c3c0   0x0000c3c0   0x0000001c   Code   RO         2670    i.SEG_LCD_Shore     seg_lcd.o
    0x0000c3dc   0x0000c3dc   0x00000018   Code   RO         2671    i.SEG_LCD_Shutdown  seg_lcd.o
    0x0000c3f4   0x0000c3f4   0x00000018   Code   RO         2673    i.SEG_LCD_Temp      seg_lcd.o
    0x0000c40c   0x0000c40c   0x0000001c   Code   RO         2674    i.SEG_LCD_TirePressure  seg_lcd.o
    0x0000c428   0x0000c428   0x000003bc   Code   RO         2675    i.SEG_LCD_Vehicle_Speed_Num_Display  seg_lcd.o
    0x0000c7e4   0x0000c7e4   0x000002a0   Code   RO         2676    i.SEG_LCD_Vehicle_Speed_Num_Selftest  seg_lcd.o
    0x0000ca84   0x0000ca84   0x0000000c   Code   RO         5430    i.SET_LED_ECU_Battery_VoltageFlag  can_user.o
    0x0000ca90   0x0000ca90   0x00000334   Code   RO         4332    i.Selfcheck_Display_Update_Service  mcu_core_protocol.o
    0x0000cdc4   0x0000cdc4   0x00000034   Code   RO         5431    i.Send_01_01        can_user.o
    0x0000cdf8   0x0000cdf8   0x00000036   Code   RO         5432    i.Send_19_0209      can_user.o
    0x0000ce2e   0x0000ce2e   0x00000036   Code   RO         5433    i.Send_22_ID0005    can_user.o
    0x0000ce64   0x0000ce64   0x0000000c   Code   RO         5070    i.SetBGLNTCVol      bglinterface.o
    0x0000ce70   0x0000ce70   0x0000000c   Code   RO         5071    i.SetBGLTheme       bglinterface.o
    0x0000ce7c   0x0000ce7c   0x0000000c   Code   RO         5072    i.SetBGLType        bglinterface.o
    0x0000ce88   0x0000ce88   0x00000010   Code   RO         4984    i.SetBackLightOutput  backgroundlight.o
    0x0000ce98   0x0000ce98   0x00000058   Code   RO         2357    i.SetBaudRadio      can.o
    0x0000cef0   0x0000cef0   0x0000010c   Code   RO         5434    i.SetDtcFault       can_user.o
    0x0000cffc   0x0000cffc   0x0000000c   Code   RO         5435    i.SetSendUdsTimeCount_0101  can_user.o
    0x0000d008   0x0000d008   0x0000000c   Code   RO         5436    i.SetSendUdsTimeCount_190209  can_user.o
    0x0000d014   0x0000d014   0x0000000c   Code   RO         5437    i.SetSendUdsTimeCount_220005  can_user.o
    0x0000d020   0x0000d020   0x0000000c   Code   RO         5438    i.Set_CanSleepDelayTime  can_user.o
    0x0000d02c   0x0000d02c   0x0000000c   Code   RO         5439    i.Set_ReqSilentTimer  can_user.o
    0x0000d038   0x0000d038   0x0000000c   Code   RO         5440    i.Set_TCS_WorkModeFlsh  can_user.o
    0x0000d044   0x0000d044   0x0000000c   Code   RO         6304    i.Set_UDS_01_MsgRecFlg  u2_app_service.o
    0x0000d050   0x0000d050   0x0000000c   Code   RO         6305    i.Set_UDS_59_MsgRecFlg  u2_app_service.o
    0x0000d05c   0x0000d05c   0x0000000c   Code   RO         6306    i.Set_UDS_62_MsgRecFlg  u2_app_service.o
    0x0000d068   0x0000d068   0x00000010   Code   RO         3112    i.Simulated_IIC_2_Init  is31_iic_master.o
    0x0000d078   0x0000d078   0x00000090   Code   RO          155    i.SysTick_Handler   sys_tick.o
    0x0000d108   0x0000d108   0x0000001c   Code   RO         3923    i.Sys_BlockDelay    system_monitor_user.o
    0x0000d124   0x0000d124   0x00000050   Code   RO         1902    i.Sys_Enter_Sleep_Mode  clk.o
    0x0000d174   0x0000d174   0x00000002   Code   RO         3274    i.Sys_Exact_100ms_Tasks  tasks.o
    0x0000d176   0x0000d176   0x00000002   Code   RO         3275    i.Sys_Exact_50us_Tasks  tasks.o
    0x0000d178   0x0000d178   0x0000000c   Code   RO         3924    i.Sys_Force_Read_KL30_Voltage  system_monitor_user.o
    0x0000d184   0x0000d184   0x0000003c   Code   RO         3453    i.Sys_Init          sys_scheduler.o
    0x0000d1c0   0x0000d1c0   0x00000028   Code   RO         3925    i.Sys_KL30_Init     system_monitor_user.o
    0x0000d1e8   0x0000d1e8   0x00000002   Code   RO         3926    i.Sys_LogicProcess  system_monitor_user.o
    0x0000d1ea   0x0000d1ea   0x0000000c   Code   RO         3927    i.Sys_Read_KL30_Valid  system_monitor_user.o
    0x0000d1f6   0x0000d1f6   0x00000018   Code   RO         3928    i.Sys_Read_KL30_Voltage  system_monitor_user.o
    0x0000d20e   0x0000d20e   0x00000008   Code   RO         3276    i.Sys_Run_Mode_100ms_Tasks_Group1  tasks.o
    0x0000d216   0x0000d216   0x00000002   Code   RO         3277    i.Sys_Run_Mode_100ms_Tasks_Group10  tasks.o
    0x0000d218   0x0000d218   0x0000000a   Code   RO         3278    i.Sys_Run_Mode_100ms_Tasks_Group2  tasks.o
    0x0000d222   0x0000d222   0x00000002   Code   RO         3279    i.Sys_Run_Mode_100ms_Tasks_Group3  tasks.o
    0x0000d224   0x0000d224   0x0000000c   Code   RO         3280    i.Sys_Run_Mode_100ms_Tasks_Group4  tasks.o
    0x0000d230   0x0000d230   0x00000002   Code   RO         3281    i.Sys_Run_Mode_100ms_Tasks_Group5  tasks.o
    0x0000d232   0x0000d232   0x00000008   Code   RO         3282    i.Sys_Run_Mode_100ms_Tasks_Group6  tasks.o
    0x0000d23a   0x0000d23a   0x0000000e   Code   RO         3283    i.Sys_Run_Mode_100ms_Tasks_Group7  tasks.o
    0x0000d248   0x0000d248   0x00000008   Code   RO         3284    i.Sys_Run_Mode_100ms_Tasks_Group8  tasks.o
    0x0000d250   0x0000d250   0x00000002   Code   RO         3285    i.Sys_Run_Mode_100ms_Tasks_Group9  tasks.o
    0x0000d252   0x0000d252   0x0000002a   Code   RO         3286    i.Sys_Run_Mode_10ms_Tasks  tasks.o
    0x0000d27c   0x0000d27c   0x00000012   Code   RO         3287    i.Sys_Run_Mode_20ms_Tasks  tasks.o
    0x0000d28e   0x0000d28e   0x00000014   Code   RO         3288    i.Sys_Run_Mode_2ms_Tasks  tasks.o
    0x0000d2a2   0x0000d2a2   0x00000014   Code   RO         3289    i.Sys_Run_Mode_50ms_Tasks  tasks.o
    0x0000d2b6   0x0000d2b6   0x00000008   Code   RO         3290    i.Sys_Run_Mode_5ms_Tasks  tasks.o
    0x0000d2be   0x0000d2be   0x00000002   PAD
    0x0000d2c0   0x0000d2c0   0x00000018   Code   RO         3291    i.Sys_Run_Mode_Pseudo_Real_Time_Tasks  tasks.o
    0x0000d2d8   0x0000d2d8   0x0000012c   Code   RO         3454    i.Sys_Scheduling_Service  sys_scheduler.o
    0x0000d404   0x0000d404   0x00000194   Code   RO         3455    i.Sys_Scheduling_Tmr  sys_scheduler.o
    0x0000d598   0x0000d598   0x00000024   Code   RO         3820    i.Sys_Set_DebounceTimer  system_monitor.o
    0x0000d5bc   0x0000d5bc   0x00000068   Code   RO         3821    i.Sys_Set_VolRange  system_monitor.o
    0x0000d624   0x0000d624   0x0000007a   Code   RO         3497    i.Sys_Startup_Init  init.o
    0x0000d69e   0x0000d69e   0x00000010   Code   RO         3822    i.Sys_Status_Update_Service  system_monitor.o
    0x0000d6ae   0x0000d6ae   0x00000002   PAD
    0x0000d6b0   0x0000d6b0   0x00000064   Code   RO          157    i.Sys_Tick_Timer_Start  sys_tick.o
    0x0000d714   0x0000d714   0x00000014   Code   RO          158    i.Sys_Tick_Timer_Stop  sys_tick.o
    0x0000d728   0x0000d728   0x0000002c   Code   RO         3929    i.Sys_WakeUp_Init   system_monitor_user.o
    0x0000d754   0x0000d754   0x00000010   Code   RO         7502    i.SystemCoreClockUpdate  system_bat32a239.o
    0x0000d764   0x0000d764   0x00000094   Code   RO         7503    i.SystemInit        system_bat32a239.o
    0x0000d7f8   0x0000d7f8   0x00000024   Code   RO         3823    i.System_Calc_FunRange  system_monitor.o
    0x0000d81c   0x0000d81c   0x00000024   Code   RO         3824    i.System_Calc_NMRange  system_monitor.o
    0x0000d840   0x0000d840   0x0000000c   Code   RO         3825    i.System_FUN_KL15_Status_Get  system_monitor.o
    0x0000d84c   0x0000d84c   0x0000000c   Code   RO         3826    i.System_FUN_KL30_Status_Get  system_monitor.o
    0x0000d858   0x0000d858   0x000000ac   Code   RO         3827    i.System_Fast_WakeUp  system_monitor.o
    0x0000d904   0x0000d904   0x00000188   Code   RO         3828    i.System_Fun_Process  system_monitor.o
    0x0000da8c   0x0000da8c   0x00000018   Code   RO         3930    i.System_LINE_KL15  system_monitor_user.o
    0x0000daa4   0x0000daa4   0x00000144   Code   RO         3829    i.System_Monitor_KL30Init  system_monitor.o
    0x0000dbe8   0x0000dbe8   0x00000128   Code   RO         3830    i.System_Monitor_WakeupInit  system_monitor.o
    0x0000dd10   0x0000dd10   0x00000150   Code   RO         3833    i.System_NM_Process  system_monitor.o
    0x0000de60   0x0000de60   0x00000040   Code   RO         2297    i.TMB0_PWM_Pin33_Freq_Duty  timera_b_c.o
    0x0000dea0   0x0000dea0   0x000000bc   Code   RO         2298    i.TMB0_PWM_Pin33_Init  timera_b_c.o
    0x0000df5c   0x0000df5c   0x00000034   Code   RO         2299    i.TMB0_Start        timera_b_c.o
    0x0000df90   0x0000df90   0x0000002c   Code   RO         6144    i.TP_AbnormalInReqFC_handle  tp_layer.o
    0x0000dfbc   0x0000dfbc   0x0000003c   Code   RO         6145    i.TP_AbnormalInReqFF_handle  tp_layer.o
    0x0000dff8   0x0000dff8   0x0000002c   Code   RO         6146    i.TP_AbnormalInResCF_handle  tp_layer.o
    0x0000e024   0x0000e024   0x0000002c   Code   RO         6147    i.TP_AbnormalInResFC_handle  tp_layer.o
    0x0000e050   0x0000e050   0x0000004c   Code   RO         6148    i.TP_AbnormalInResSF_handle  tp_layer.o
    0x0000e09c   0x0000e09c   0x00000024   Code   RO         6149    i.TP_BsTimerOver    tp_layer.o
    0x0000e0c0   0x0000e0c0   0x00000060   Code   RO         6150    i.TP_Buffer_handle  tp_layer.o
    0x0000e120   0x0000e120   0x0000002c   Code   RO         6151    i.TP_CalMsgLen      tp_layer.o
    0x0000e14c   0x0000e14c   0x00000024   Code   RO         6152    i.TP_CrTimerOver    tp_layer.o
    0x0000e170   0x0000e170   0x000000d0   Code   RO         6153    i.TP_NormalRecFC_handle  tp_layer.o
    0x0000e240   0x0000e240   0x00000084   Code   RO         6154    i.TP_NormalSendFC_Fun  tp_layer.o
    0x0000e2c4   0x0000e2c4   0x000001a0   Code   RO         6155    i.TP_ReciveMultiF_handle  tp_layer.o
    0x0000e464   0x0000e464   0x00000084   Code   RO         6156    i.TP_ReciveSF_handle  tp_layer.o
    0x0000e4e8   0x0000e4e8   0x00000024   Code   RO         6157    i.TP_STminTimerOver  tp_layer.o
    0x0000e50c   0x0000e50c   0x0000000e   Code   RO         6158    i.TP_SetBsTimer     tp_layer.o
    0x0000e51a   0x0000e51a   0x0000000e   Code   RO         6159    i.TP_SetCrTimer     tp_layer.o
    0x0000e528   0x0000e528   0x0000000e   Code   RO         6160    i.TP_SetSTminTimer  tp_layer.o
    0x0000e536   0x0000e536   0x00000002   PAD
    0x0000e538   0x0000e538   0x00000090   Code   RO         6161    i.TP_TooShortDLC_handle  tp_layer.o
    0x0000e5c8   0x0000e5c8   0x000000c0   Code   RO         6162    i.TP_TransmitNegatePDU  tp_layer.o
    0x0000e688   0x0000e688   0x0000021c   Code   RO         6163    i.TP_TransmitPDU    tp_layer.o
    0x0000e8a4   0x0000e8a4   0x0000004c   Code   RO         6164    i.TP_UnknownlPDU_handle  tp_layer.o
    0x0000e8f0   0x0000e8f0   0x000000f4   Code   RO         7777    i.Telltales_IG_OFF_Work  Telltales.lib(telltales_lib.o)
    0x0000e9e4   0x0000e9e4   0x000002a0   Code   RO         7778    i.Telltales_IG_ON_Work  Telltales.lib(telltales_lib.o)
    0x0000ec84   0x0000ec84   0x00000034   Code   RO         4469    i.Telltales_Init    telltales_user.o
    0x0000ecb8   0x0000ecb8   0x00000010   Code   RO         7779    i.Telltales_KL15_Init  Telltales.lib(telltales_lib.o)
    0x0000ecc8   0x0000ecc8   0x00000060   Code   RO         7780    i.Telltales_KL30_Wakeup_Init  Telltales.lib(telltales_lib.o)
    0x0000ed28   0x0000ed28   0x000000cc   Code   RO         7781    i.Telltales_Management  Telltales.lib(telltales_lib.o)
    0x0000edf4   0x0000edf4   0x0000003c   Code   RO         6307    i.U2_App_01_service  u2_app_service.o
    0x0000ee30   0x0000ee30   0x00000002   Code   RO         6537    i.U2_App_11_Reset_handle  u2_app_serviceproc.o
    0x0000ee32   0x0000ee32   0x00000002   PAD
    0x0000ee34   0x0000ee34   0x00000060   Code   RO         6320    i.U2_App_59_service  u2_app_service.o
    0x0000ee94   0x0000ee94   0x00000050   Code   RO         6321    i.U2_App_62_service  u2_app_service.o
    0x0000eee4   0x0000eee4   0x00000018   Code   RO         6538    i.U2_App_CopyRam    u2_app_serviceproc.o
    0x0000eefc   0x0000eefc   0x00000024   Code   RO         6323    i.U2_App_DtcMsgTimerOver  u2_app_service.o
    0x0000ef20   0x0000ef20   0x00000014   Code   RO         6540    i.U2_App_ErrorInfoInit  u2_app_serviceproc.o
    0x0000ef34   0x0000ef34   0x00000016   Code   RO         6541    i.U2_App_Load_DID   u2_app_serviceproc.o
    0x0000ef4a   0x0000ef4a   0x00000024   Code   RO         6325    i.U2_App_ReUnlockTimerOver  u2_app_service.o
    0x0000ef6e   0x0000ef6e   0x00000024   Code   RO         6327    i.U2_App_SessionTimerOver  u2_app_service.o
    0x0000ef92   0x0000ef92   0x0000000e   Code   RO         6328    i.U2_App_SetDtcMsgTimer  u2_app_service.o
    0x0000efa0   0x0000efa0   0x00000110   Code   RO         6542    i.U2_Diagno_Tick    u2_app_serviceproc.o
    0x0000f0b0   0x0000f0b0   0x0000008c   Code   RO         6332    i.U2_DiagnosisInit_main  u2_app_service.o
    0x0000f13c   0x0000f13c   0x00000204   Code   RO         6333    i.U2_Diagnosis_main  u2_app_service.o
    0x0000f340   0x0000f340   0x00000014   Code   RO         6606    i.U2_LK_FillMsg     u2_link_layer.o
    0x0000f354   0x0000f354   0x00000080   Code   RO         6607    i.U2_LK_Link_main   u2_link_layer.o
    0x0000f3d4   0x0000f3d4   0x0000002c   Code   RO         6649    i.U2_TP_AbnormalInReqFC_handle  u2_tp_layer.o
    0x0000f400   0x0000f400   0x0000003c   Code   RO         6650    i.U2_TP_AbnormalInReqFF_handle  u2_tp_layer.o
    0x0000f43c   0x0000f43c   0x0000002c   Code   RO         6651    i.U2_TP_AbnormalInResCF_handle  u2_tp_layer.o
    0x0000f468   0x0000f468   0x0000002c   Code   RO         6652    i.U2_TP_AbnormalInResFC_handle  u2_tp_layer.o
    0x0000f494   0x0000f494   0x0000004c   Code   RO         6653    i.U2_TP_AbnormalInResSF_handle  u2_tp_layer.o
    0x0000f4e0   0x0000f4e0   0x00000024   Code   RO         6654    i.U2_TP_BsTimerOver  u2_tp_layer.o
    0x0000f504   0x0000f504   0x00000060   Code   RO         6655    i.U2_TP_Buffer_handle  u2_tp_layer.o
    0x0000f564   0x0000f564   0x0000002c   Code   RO         6656    i.U2_TP_CalMsgLen   u2_tp_layer.o
    0x0000f590   0x0000f590   0x00000024   Code   RO         6657    i.U2_TP_CrTimerOver  u2_tp_layer.o
    0x0000f5b4   0x0000f5b4   0x000000d0   Code   RO         6658    i.U2_TP_NormalRecFC_handle  u2_tp_layer.o
    0x0000f684   0x0000f684   0x00000084   Code   RO         6659    i.U2_TP_NormalSendFC_Fun  u2_tp_layer.o
    0x0000f708   0x0000f708   0x000001a0   Code   RO         6660    i.U2_TP_ReciveMultiF_handle  u2_tp_layer.o
    0x0000f8a8   0x0000f8a8   0x00000084   Code   RO         6661    i.U2_TP_ReciveSF_handle  u2_tp_layer.o
    0x0000f92c   0x0000f92c   0x00000024   Code   RO         6662    i.U2_TP_STminTimerOver  u2_tp_layer.o
    0x0000f950   0x0000f950   0x0000000e   Code   RO         6663    i.U2_TP_SetBsTimer  u2_tp_layer.o
    0x0000f95e   0x0000f95e   0x0000000e   Code   RO         6664    i.U2_TP_SetCrTimer  u2_tp_layer.o
    0x0000f96c   0x0000f96c   0x0000000e   Code   RO         6665    i.U2_TP_SetSTminTimer  u2_tp_layer.o
    0x0000f97a   0x0000f97a   0x00000002   PAD
    0x0000f97c   0x0000f97c   0x00000090   Code   RO         6666    i.U2_TP_TooShortDLC_handle  u2_tp_layer.o
    0x0000fa0c   0x0000fa0c   0x000000c0   Code   RO         6667    i.U2_TP_TransmitNegatePDU  u2_tp_layer.o
    0x0000facc   0x0000facc   0x0000021c   Code   RO         6668    i.U2_TP_TransmitPDU  u2_tp_layer.o
    0x0000fce8   0x0000fce8   0x0000004c   Code   RO         6669    i.U2_TP_UnknownlPDU_handle  u2_tp_layer.o
    0x0000fd34   0x0000fd34   0x0000000c   Code   RO          131    i.WDT_Restart       wdt.o
    0x0000fd40   0x0000fd40   0x0000001c   Code   RO           97    i.__ARM_common_switch8  gpio.o
    0x0000fd5c   0x0000fd5c   0x00000018   Code   RO          244    i.__NVIC_ClearPendingIRQ  adc.o
    0x0000fd74   0x0000fd74   0x00000018   Code   RO         2190    i.__NVIC_ClearPendingIRQ  tim4.o
    0x0000fd8c   0x0000fd8c   0x00000078   Code   RO          159    i.__NVIC_SetPriority  sys_tick.o
    0x0000fe04   0x0000fe04   0x0000000c   Code   RO         6846    i.adc_interrupt     isr_bat32a239.o
    0x0000fe10   0x0000fe10   0x00000114   Code   RO         2358    i.bsp_CAN0_Rev_isr  can.o
    0x0000ff24   0x0000ff24   0x00000020   Code   RO         2359    i.bsp_CAN0_Tx_isr   can.o
    0x0000ff44   0x0000ff44   0x00000094   Code   RO         2360    i.bsp_CANSendFrame  can.o
    0x0000ffd8   0x0000ffd8   0x000000fc   Code   RO         2361    i.bsp_CAN_BusOff_Recover  can.o
    0x000100d4   0x000100d4   0x00000168   Code   RO         2362    i.bsp_CAN_Init      can.o
    0x0001023c   0x0001023c   0x00000044   Code   RO         2363    i.bsp_CAN_MaskCheck  can.o
    0x00010280   0x00010280   0x00000010   Code   RO         2364    i.bsp_CAN_Sleep     can.o
    0x00010290   0x00010290   0x0000000c   Code   RO         2365    i.bsp_CAN_SleepRelease  can.o
    0x0001029c   0x0001029c   0x00000030   Code   RO         2366    i.bsp_CanBuf_Clear  can.o
    0x000102cc   0x000102cc   0x000000c0   Code   RO         2367    i.bsp_CanBuf_Init   can.o
    0x0001038c   0x0001038c   0x00000028   Code   RO         2985    i.bsp_IIC2_ACK      aw93015.o
    0x000103b4   0x000103b4   0x00000048   Code   RO         2987    i.bsp_IIC2_ReadByte  aw93015.o
    0x000103fc   0x000103fc   0x00000046   Code   RO         2988    i.bsp_IIC2_SendByte  aw93015.o
    0x00010442   0x00010442   0x00000028   Code   RO         2989    i.bsp_IIC2_Start    aw93015.o
    0x0001046a   0x0001046a   0x00000028   Code   RO         2990    i.bsp_IIC2_Stop     aw93015.o
    0x00010492   0x00010492   0x00000044   Code   RO         2991    i.bsp_IIC2_WaitAck  aw93015.o
    0x000104d6   0x000104d6   0x00000002   PAD
    0x000104d8   0x000104d8   0x0000003c   Code   RO         3114    i.bsp_IIC_SCL_out   is31_iic_master.o
    0x00010514   0x00010514   0x0000003c   Code   RO         3115    i.bsp_IIC_SDA_out   is31_iic_master.o
    0x00010550   0x00010550   0x00000040   Code   RO         2368    i.bsp_Is_CAN_Sleep  can.o
    0x00010590   0x00010590   0x0000005c   Code   RO         2369    i.bsp_rx_mask_init  can.o
    0x000105ec   0x000105ec   0x00000094   Code   RO         2370    i.bsp_rx_msgbuf_init  can.o
    0x00010680   0x00010680   0x00000038   Code   RO         2191    i.bsp_tim4_01_isr_Handler  tim4.o
    0x000106b8   0x000106b8   0x0000000c   Code   RO         2192    i.bsp_tim4_02_isr_Handler  tim4.o
    0x000106c4   0x000106c4   0x00000018   Code   RO         2371    i.bsp_tx_msgbuf_abort  can.o
    0x000106dc   0x000106dc   0x0000005c   Code   RO         2372    i.bsp_tx_msgbuf_init  can.o
    0x00010738   0x00010738   0x0000000c   Code   RO         6847    i.cmp0_interrupt    isr_bat32a239.o
    0x00010744   0x00010744   0x0000000c   Code   RO         6848    i.cmp1_interrupt    isr_bat32a239.o
    0x00010750   0x00010750   0x0000000c   Code   RO         6849    i.div_interrupt     isr_bat32a239.o
    0x0001075c   0x0001075c   0x00000014   Code   RO         4774    i.eeprom_StoreInfo_Init  eemanager_interface.o
    0x00010770   0x00010770   0x00000020   Code   RO         4775    i.eeprom_comm_DelayUs  eemanager_interface.o
    0x00010790   0x00010790   0x00000038   Code   RO         2907    i.extend_i2c_write_one_byte  is31fl3236.o
    0x000107c8   0x000107c8   0x0000000c   Code   RO         6850    i.flash_interrupt   isr_bat32a239.o
    0x000107d4   0x000107d4   0x0000000e   Code   RO         5444    i.get_CoolantTempVal  can_user.o
    0x000107e2   0x000107e2   0x00000012   Code   RO         5446    i.get_ECU_Battery_Voltage  can_user.o
    0x000107f4   0x000107f4   0x00000028   Code   RO         5447    i.get_ECU_Temperature_WaterVal  can_user.o
    0x0001081c   0x0001081c   0x00000002   Code   RO         1429    i.iic20_callback_master_error  sci_user.o
    0x0001081e   0x0001081e   0x00000002   PAD
    0x00010820   0x00010820   0x00000014   Code   RO         1430    i.iic20_callback_master_receiveend  sci_user.o
    0x00010834   0x00010834   0x00000014   Code   RO         1431    i.iic20_callback_master_sendend  sci_user.o
    0x00010848   0x00010848   0x00000174   Code   RO         1432    i.iic20_interrupt   sci_user.o
    0x000109bc   0x000109bc   0x00000002   Code   RO         1433    i.iic21_callback_master_error  sci_user.o
    0x000109be   0x000109be   0x00000002   PAD
    0x000109c0   0x000109c0   0x00000014   Code   RO         1434    i.iic21_callback_master_receiveend  sci_user.o
    0x000109d4   0x000109d4   0x00000014   Code   RO         1435    i.iic21_callback_master_sendend  sci_user.o
    0x000109e8   0x000109e8   0x00000174   Code   RO         1436    i.iic21_interrupt   sci_user.o
    0x00010b5c   0x00010b5c   0x0000000c   Code   RO         6859    i.iica0_interrupt   isr_bat32a239.o
    0x00010b68   0x00010b68   0x0000000c   Code   RO         6860    i.iica1_interrupt   isr_bat32a239.o
    0x00010b74   0x00010b74   0x00000010   Code   RO         2035    i.intp0_callback    intp_user.o
    0x00010b84   0x00010b84   0x00000014   Code   RO         2036    i.intp0_interrupt   intp_user.o
    0x00010b98   0x00010b98   0x00000010   Code   RO         2037    i.intp10_callback   intp_user.o
    0x00010ba8   0x00010ba8   0x00000014   Code   RO         2038    i.intp10_interrupt  intp_user.o
    0x00010bbc   0x00010bbc   0x00000010   Code   RO         2039    i.intp11_callback   intp_user.o
    0x00010bcc   0x00010bcc   0x00000014   Code   RO         2040    i.intp11_interrupt  intp_user.o
    0x00010be0   0x00010be0   0x00000010   Code   RO         2041    i.intp1_callback    intp_user.o
    0x00010bf0   0x00010bf0   0x00000014   Code   RO         2042    i.intp1_interrupt   intp_user.o
    0x00010c04   0x00010c04   0x00000010   Code   RO         2043    i.intp2_callback    intp_user.o
    0x00010c14   0x00010c14   0x00000014   Code   RO         2044    i.intp2_interrupt   intp_user.o
    0x00010c28   0x00010c28   0x00000010   Code   RO         2045    i.intp3_callback    intp_user.o
    0x00010c38   0x00010c38   0x00000014   Code   RO         2046    i.intp3_interrupt   intp_user.o
    0x00010c4c   0x00010c4c   0x00000010   Code   RO         2047    i.intp4_callback    intp_user.o
    0x00010c5c   0x00010c5c   0x00000014   Code   RO         2048    i.intp4_interrupt   intp_user.o
    0x00010c70   0x00010c70   0x00000010   Code   RO         2049    i.intp5_callback    intp_user.o
    0x00010c80   0x00010c80   0x00000014   Code   RO         2050    i.intp5_interrupt   intp_user.o
    0x00010c94   0x00010c94   0x00000010   Code   RO         2051    i.intp6_callback    intp_user.o
    0x00010ca4   0x00010ca4   0x00000014   Code   RO         2052    i.intp6_interrupt   intp_user.o
    0x00010cb8   0x00010cb8   0x00000010   Code   RO         2053    i.intp7_callback    intp_user.o
    0x00010cc8   0x00010cc8   0x00000014   Code   RO         2054    i.intp7_interrupt   intp_user.o
    0x00010cdc   0x00010cdc   0x00000010   Code   RO         2055    i.intp8_callback    intp_user.o
    0x00010cec   0x00010cec   0x00000014   Code   RO         2056    i.intp8_interrupt   intp_user.o
    0x00010d00   0x00010d00   0x00000010   Code   RO         2057    i.intp9_callback    intp_user.o
    0x00010d10   0x00010d10   0x00000014   Code   RO         2058    i.intp9_interrupt   intp_user.o
    0x00010d24   0x00010d24   0x0000000c   Code   RO         6873    i.it_interrupt      isr_bat32a239.o
    0x00010d30   0x00010d30   0x0000000c   Code   RO         6874    i.key_interrupt     isr_bat32a239.o
    0x00010d3c   0x00010d3c   0x0000000c   Code   RO         6875    i.lvi_interrupt     isr_bat32a239.o
    0x00010d48   0x00010d48   0x00000010   Code   RO         3229    i.main              main.o
    0x00010d58   0x00010d58   0x00000014   Code   RO         2373    i.memcpy1           can.o
    0x00010d6c   0x00010d6c   0x0000000c   Code   RO         6876    i.ocrv_interrupt    isr_bat32a239.o
    0x00010d78   0x00010d78   0x0000000c   Code   RO         6877    i.osdc_interrupt    isr_bat32a239.o
    0x00010d84   0x00010d84   0x0000000c   Code   RO         6878    i.rtc_interrupt     isr_bat32a239.o
    0x00010d90   0x00010d90   0x0000000c   Code   RO         6887    i.sre0_interrupt    isr_bat32a239.o
    0x00010d9c   0x00010d9c   0x0000000c   Code   RO         6888    i.sre1_interrupt    isr_bat32a239.o
    0x00010da8   0x00010da8   0x0000000c   Code   RO         6889    i.sre2_interrupt    isr_bat32a239.o
    0x00010db4   0x00010db4   0x0000000c   Code   RO         6890    i.tm01h_interrupt   isr_bat32a239.o
    0x00010dc0   0x00010dc0   0x0000000c   Code   RO         6891    i.tm03h_interrupt   isr_bat32a239.o
    0x00010dcc   0x00010dcc   0x0000000c   Code   RO         6892    i.tm40_channel0_interrupt  isr_bat32a239.o
    0x00010dd8   0x00010dd8   0x00000008   Code   RO         6893    i.tm40_channel1_interrupt  isr_bat32a239.o
    0x00010de0   0x00010de0   0x00000008   Code   RO         6894    i.tm40_channel2_interrupt  isr_bat32a239.o
    0x00010de8   0x00010de8   0x0000000c   Code   RO         6895    i.tm40_channel3_interrupt  isr_bat32a239.o
    0x00010df4   0x00010df4   0x0000000c   Code   RO         6896    i.tm81_channel10_interrupt  isr_bat32a239.o
    0x00010e00   0x00010e00   0x0000000c   Code   RO         6897    i.tm81_channel11_interrupt  isr_bat32a239.o
    0x00010e0c   0x00010e0c   0x0000000c   Code   RO         6898    i.tm81_channel12_interrupt  isr_bat32a239.o
    0x00010e18   0x00010e18   0x0000000c   Code   RO         6899    i.tm81_channel13_interrupt  isr_bat32a239.o
    0x00010e24   0x00010e24   0x0000000c   Code   RO         6900    i.tm81_channel14_interrupt  isr_bat32a239.o
    0x00010e30   0x00010e30   0x0000000c   Code   RO         6901    i.tm81_channel15_interrupt  isr_bat32a239.o
    0x00010e3c   0x00010e3c   0x0000000c   Code   RO         6902    i.tm81_channel16_interrupt  isr_bat32a239.o
    0x00010e48   0x00010e48   0x0000000c   Code   RO         6903    i.tm81_channel17_interrupt  isr_bat32a239.o
    0x00010e54   0x00010e54   0x0000000c   Code   RO         6904    i.tma0_interrupt    isr_bat32a239.o
    0x00010e60   0x00010e60   0x0000000c   Code   RO         6905    i.tmb0_interrupt    isr_bat32a239.o
    0x00010e6c   0x00010e6c   0x0000000c   Code   RO         6906    i.tmc_interrupt     isr_bat32a239.o
    0x00010e78   0x00010e78   0x0000000c   Code   RO         6907    i.tmm0_interrupt    isr_bat32a239.o
    0x00010e84   0x00010e84   0x0000000c   Code   RO         6908    i.tmm1_interrupt    isr_bat32a239.o
    0x00010e90   0x00010e90   0x00000002   Code   RO         1479    i.uart0_callback_sendend  sci_user.o
    0x00010e92   0x00010e92   0x00000002   PAD
    0x00010e94   0x00010e94   0x00000024   Code   RO         1481    i.uart0_interrupt_receive  sci_user.o
    0x00010eb8   0x00010eb8   0x00000048   Code   RO         1482    i.uart0_interrupt_send  sci_user.o
    0x00010f00   0x00010f00   0x00000002   Code   RO         1483    i.uart1_callback_error  sci_user.o
    0x00010f02   0x00010f02   0x00000002   Code   RO         1484    i.uart1_callback_receiveend  sci_user.o
    0x00010f04   0x00010f04   0x00000002   Code   RO         1485    i.uart1_callback_sendend  sci_user.o
    0x00010f06   0x00010f06   0x00000002   Code   RO         1486    i.uart1_callback_softwareoverrun  sci_user.o
    0x00010f08   0x00010f08   0x0000008c   Code   RO         1487    i.uart1_interrupt_receive  sci_user.o
    0x00010f94   0x00010f94   0x00000048   Code   RO         1488    i.uart1_interrupt_send  sci_user.o
    0x00010fdc   0x00010fdc   0x0000000c   Code   RO         1490    i.uart2_User_KL15_Init  sci_user.o
    0x00010fe8   0x00010fe8   0x00000002   Code   RO         1497    i.uart3_callback_error  sci_user.o
    0x00010fea   0x00010fea   0x00000002   Code   RO         1498    i.uart3_callback_receiveend  sci_user.o
    0x00010fec   0x00010fec   0x00000002   Code   RO         1499    i.uart3_callback_sendend  sci_user.o
    0x00010fee   0x00010fee   0x00000002   Code   RO         1500    i.uart3_callback_softwareoverrun  sci_user.o
    0x00010ff0   0x00010ff0   0x00000094   Code   RO         1501    i.uart3_interrupt_receive  sci_user.o
    0x00011084   0x00011084   0x0000004c   Code   RO         1502    i.uart3_interrupt_send  sci_user.o
    0x000110d0   0x000110d0   0x000000e4   Code   RO         2877    ram_fetch_code      flash.o
    0x000111b4   0x000111b4   0x00000054   Code   RO         1903    sram_code           clk.o
    0x00011208   0x00011208   0x00000084   Data   RO          468    .constdata          analog_signals.o
    0x0001128c   0x0001128c   0x00000024   Data   RO         2678    .constdata          seg_lcd.o
    0x000112b0   0x000112b0   0x000004b0   Data   RO         2994    .constdata          aw93015.o
    0x00011760   0x00011760   0x00000060   Data   RO         3557    .constdata          line_in.o
    0x000117c0   0x000117c0   0x00000028   Data   RO         3931    .constdata          system_monitor_user.o
    0x000117e8   0x000117e8   0x0000017c   Data   RO         4471    .constdata          telltales_user.o
    0x00011964   0x00011964   0x00000064   Data   RO         4660    .constdata          flash_synchronizer.o
    0x000119c8   0x000119c8   0x0000004d   Data   RO         5074    .constdata          bglinterface.o
    0x00011a15   0x00011a15   0x00000003   PAD
    0x00011a18   0x00011a18   0x00000014   Data   RO         5155    .constdata          key.o
    0x00011a2c   0x00011a2c   0x00000224   Data   RO         5239    .constdata          can_communication_matrix.o
    0x00011c50   0x00011c50   0x00000048   Data   RO         5784    .constdata          app_telltales.o
    0x00011c98   0x00011c98   0x00000020   Data   RO         8040    Region$$Table       anon$$obj.o


    Execution Region RW_IRAM1 (Exec base: 0x20000000, Load base: 0x00011cb8, Size: 0x00001e08, Max: 0x00008000, ABSOLUTE, COMPRESSED[0x0000005c])

    Exec Addr    Load Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x20000000   COMPRESSED   0x00000004   Data   RW          161    .data               sys_tick.o
    0x20000004   COMPRESSED   0x0000000a   Data   RW          245    .data               adc.o
    0x2000000e   COMPRESSED   0x0000000e   Data   RW          469    .data               analog_signals.o
    0x2000001c   COMPRESSED   0x00000170   Data   RW          669    .data               sci.o
    0x2000018c   COMPRESSED   0x00000012   Data   RW         1503    .data               sci_user.o
    0x2000019e   COMPRESSED   0x00000002   PAD
    0x200001a0   COMPRESSED   0x00000030   Data   RW         2059    .data               intp_user.o
    0x200001d0   COMPRESSED   0x00000007   Data   RW         2245    .data               rtc.o
    0x200001d7   COMPRESSED   0x00000001   PAD
    0x200001d8   COMPRESSED   0x0000000e   Data   RW         2374    .data               can.o
    0x200001e6   COMPRESSED   0x00000006   Data   RW         2560    .data               bu98r10.o
    0x200001ec   COMPRESSED   0x0000000b   Data   RW         2679    .data               seg_lcd.o
    0x200001f7   COMPRESSED   0x00000001   PAD
    0x200001f8   COMPRESSED   0x0000000c   Data   RW         2909    .data               is31fl3236.o
    0x20000204   COMPRESSED   0x00000009   Data   RW         2995    .data               aw93015.o
    0x2000020d   COMPRESSED   0x00000003   PAD
    0x20000210   COMPRESSED   0x00000008   Data   RW         3116    .data               is31_iic_master.o
    0x20000218   COMPRESSED   0x00000001   Data   RW         3558    .data               line_in.o
    0x20000219   COMPRESSED   0x00000001   Data   RW         3657    .data               powermanagement.o
    0x2000021a   COMPRESSED   0x00000002   Data   RW         3711    .data               powermanagement_user.o
    0x2000021c   COMPRESSED   0x0000003a   Data   RW         3835    .data               system_monitor.o
    0x20000256   COMPRESSED   0x00000002   PAD
    0x20000258   COMPRESSED   0x0000002c   Data   RW         4113    .data               common_interface.o
    0x20000284   COMPRESSED   0x00000062   Data   RW         4339    .data               mcu_core_protocol.o
    0x200002e6   COMPRESSED   0x00000006   Data   RW         4661    .data               flash_synchronizer.o
    0x200002ec   COMPRESSED   0x0000001a   Data   RW         4701    .data               fuel.o
    0x20000306   COMPRESSED   0x00000002   PAD
    0x20000308   COMPRESSED   0x00000010   Data   RW         4858    .data               services_mileage_user.o
    0x20000318   COMPRESSED   0x00000002   Data   RW         4938    .data               data_gear.o
    0x2000031a   COMPRESSED   0x0000001b   Data   RW         4989    .data               backgroundlight.o
    0x20000335   COMPRESSED   0x00000003   PAD
    0x20000338   COMPRESSED   0x0000000c   Data   RW         5075    .data               bglinterface.o
    0x20000344   COMPRESSED   0x00000068   Data   RW         5452    .data               can_user.o
    0x200003ac   COMPRESSED   0x0000001e   Data   RW         5846    .data               app_service.o
    0x200003ca   COMPRESSED   0x00000002   Data   RW         6166    .data               tp_layer.o
    0x200003cc   COMPRESSED   0x0000000d   Data   RW         6335    .data               u2_app_service.o
    0x200003d9   COMPRESSED   0x00000001   PAD
    0x200003da   COMPRESSED   0x00000002   Data   RW         6671    .data               u2_tp_layer.o
    0x200003dc   COMPRESSED   0x00000004   Data   RW         7505    .data               system_bat32a239.o
    0x200003e0   COMPRESSED   0x00000001   Data   RW         7631    .data               CAN_Lib.lib(can_signal_rx.o)
    0x200003e1   COMPRESSED   0x00000001   Data   RW         7714    .data               CAN_Lib.lib(can_signal_tx.o)
    0x200003e2   COMPRESSED   0x00000002   PAD
    0x200003e4        -       0x00000018   Zero   RW          160    .bss                sys_tick.o
    0x200003fc        -       0x00000010   Zero   RW          467    .bss                analog_signals.o
    0x2000040c        -       0x00000168   Zero   RW         2559    .bss                bu98r10.o
    0x20000574        -       0x00000020   Zero   RW         2677    .bss                seg_lcd.o
    0x20000594        -       0x00000024   Zero   RW         2908    .bss                is31fl3236.o
    0x200005b8        -       0x000000c8   Zero   RW         2993    .bss                aw93015.o
    0x20000680        -       0x0000002c   Zero   RW         3456    .bss                sys_scheduler.o
    0x200006ac        -       0x00000030   Zero   RW         3556    .bss                line_in.o
    0x200006dc        -       0x0000002c   Zero   RW         3656    .bss                powermanagement.o
    0x20000708        -       0x00000030   Zero   RW         3834    .bss                system_monitor.o
    0x20000738        -       0x00000240   Zero   RW         4337    .bss                mcu_core_protocol.o
    0x20000978        -       0x0000002e   Zero   RW         4470    .bss                telltales_user.o
    0x200009a6        -       0x00000028   Zero   RW         4700    .bss                fuel.o
    0x200009ce   COMPRESSED   0x00000002   PAD
    0x200009d0        -       0x0000001e   Zero   RW         4857    .bss                services_mileage_user.o
    0x200009ee        -       0x0000003c   Zero   RW         4988    .bss                backgroundlight.o
    0x20000a2a        -       0x0000004c   Zero   RW         5073    .bss                bglinterface.o
    0x20000a76        -       0x00000010   Zero   RW         5154    .bss                key.o
    0x20000a86   COMPRESSED   0x00000002   PAD
    0x20000a88        -       0x000002a4   Zero   RW         5451    .bss                can_user.o
    0x20000d2c        -       0x000001d9   Zero   RW         5844    .bss                app_service.o
    0x20000f05   COMPRESSED   0x00000001   PAD
    0x20000f06        -       0x00000024   Zero   RW         6103    .bss                link_layer.o
    0x20000f2a   COMPRESSED   0x00000002   PAD
    0x20000f2c        -       0x00000286   Zero   RW         6165    .bss                tp_layer.o
    0x200011b2   COMPRESSED   0x00000002   PAD
    0x200011b4        -       0x000001e3   Zero   RW         6334    .bss                u2_app_service.o
    0x20001397   COMPRESSED   0x00000001   PAD
    0x20001398        -       0x00000024   Zero   RW         6608    .bss                u2_link_layer.o
    0x200013bc        -       0x00000286   Zero   RW         6670    .bss                u2_tp_layer.o
    0x20001642   COMPRESSED   0x00000002   PAD
    0x20001644        -       0x0000000c   Zero   RW         7629    .bss                CAN_Lib.lib(can_signal_rx.o)
    0x20001650        -       0x00000010   Zero   RW         7713    .bss                CAN_Lib.lib(can_signal_tx.o)
    0x20001660        -       0x0000001c   Zero   RW         7784    .bss                Telltales.lib(telltales_lib.o)
    0x2000167c        -       0x00000060   Zero   RW         7911    .bss                c_p.l(libspace.o)
    0x200016dc        -       0x00000002   Zero   RW         7603    .bss.IsReadOdoState  eepromManage.lib(eeprommanage.o)
    0x200016de        -       0x00000001   Zero   RW         7606    .bss.MemoryConfig.0  eepromManage.lib(eeprommanage.o)
    0x200016df        -       0x00000001   Zero   RW         7607    .bss.MemoryConfig.1  eepromManage.lib(eeprommanage.o)
    0x200016e0        -       0x00000004   Zero   RW         7608    .bss.MemoryConfig.2  eepromManage.lib(eeprommanage.o)
    0x200016e4        -       0x00000002   Zero   RW         7609    .bss.MemoryConfig.3  eepromManage.lib(eeprommanage.o)
    0x200016e6        -       0x00000002   Zero   RW         7596    .bss.OdoValidAddress  eepromManage.lib(eeprommanage.o)
    0x200016e8        -       0x00000001   Zero   RW         7605    .bss.memIgnState    eepromManage.lib(eeprommanage.o)
    0x200016e9   COMPRESSED   0x00000003   PAD
    0x200016ec        -       0x00000004   Zero   RW         7595    .bss.memoryOdo      eepromManage.lib(eeprommanage.o)
    0x200016f0        -       0x00000002   Zero   RW         7599    .bss.readDebugState  eepromManage.lib(eeprommanage.o)
    0x200016f2        -       0x00000001   Zero   RW         7598    .bss.readState      eepromManage.lib(eeprommanage.o)
    0x200016f3        -       0x00000001   Zero   RW         7594    .bss.tWR_count      eepromManage.lib(eeprommanage.o)
    0x200016f4        -       0x00000001   Zero   RW         7604    .bss.writeBakEnable  eepromManage.lib(eeprommanage.o)
    0x200016f5   COMPRESSED   0x00000001   PAD
    0x200016f6        -       0x00000002   Zero   RW         7600    .bss.writeDebugState  eepromManage.lib(eeprommanage.o)
    0x200016f8        -       0x00000002   Zero   RW         7597    .bss.writeState     eepromManage.lib(eeprommanage.o)
    0x200016fa   COMPRESSED   0x00000002   PAD
    0x200016fc        -       0x00000004   Zero   RW         7601    .bss.writeWaitTime  eepromManage.lib(eeprommanage.o)
    0x20001700        -       0x00000002   Zero   RW         7602    .bss.write_pos      eepromManage.lib(eeprommanage.o)
    0x20001702   COMPRESSED   0x00000006   PAD
    0x20001708        -       0x00000100   Zero   RW         7492    HEAP                startup_bat32a239.o
    0x20001808        -       0x00000600   Zero   RW         7491    STACK               startup_bat32a239.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

       524        100          0         10          0      36257   adc.o
       434         14          0          0          0       4132   analog_circuits.o
      1168        112        132         14         16       5901   analog_signals.o
      4084        252          0         30        473      14606   app_service.o
       386         28          0          0          0      13773   app_serviceproc.o
        74         10         72          0          0       1957   app_telltales.o
      1050         40       1200          9        200       9508   aw93015.o
       680         44          0         27         60       5267   backgroundlight.o
       228         50         77         12         76       5338   bglinterface.o
      1150         70          0          6        360      28917   bu98r10.o
      1956        208          0         14          0      14863   can.o
       334          4        548          0          0      11225   can_communication_matrix.o
      3838        392          0        104        676      30516   can_user.o
       464         44          0          0          0       6834   clk.o
       344        136          0         44          0       6278   common_interface.o
        14          4          0          2          0       3679   data_gear.o
       184          0          0          0          0       5802   eemanager_interface.o
       228          6          0          0          0       1576   flash.o
       136         42        100          6          0       1751   flash_synchronizer.o
      1352        162          0         26         40       6870   fuel.o
      2004         30          0          0          0      77970   gpio.o
       122          0          0          0          0        515   init.o
      1532         50          0          0          0       2133   intp.o
       432        120          0         48          0      11102   intp_user.o
       790         26          0          8          0       8552   is31_iic_master.o
      1152         62          0         12         36       5235   is31fl3236.o
      1568        304          0          0          0      34928   isr_bat32a239.o
      1118         32         20          0         16       4581   key.o
       672         54         96          1         48       9223   line_in.o
       100          6          0          0         36       1811   link_layer.o
        16          0          0          0          0        423   main.o
      2060         96          0         98        576      11002   mcu_core_protocol.o
       396         42          0          1         44       4051   powermanagement.o
       932         78          0          2          0       8936   powermanagement_user.o
       524         50          0          7          0       4201   rtc.o
        64          0          0          0          0       2059   rte_adc.o
       284         48          0        368          0      26691   sci.o
      1402        222          0         18          0      25182   sci_user.o
     15136        420         36         11         32      23945   seg_lcd.o
       740         88          0         16         30       6305   services_mileage_user.o
       128         28        192          0       1792       2112   startup_bat32a239.o
       764         24          0          0         44       3524   sys_scheduler.o
       384         54          0          4         24      14150   sys_tick.o
       504        114          4          4          0       3456   system_bat32a239.o
      1772        276          0         58         48       9615   system_monitor.o
       186         24         40          0          0       5588   system_monitor_user.o
       204          4          0          0          0       9343   tasks.o
      1098         28        380          0         46      21371   telltales_user.o
       516         56          0          0          0       2291   tim4.o
       304         56          0          0          0       1746   timera_b_c.o
      2398        212          0          2        646      13306   tp_layer.o
      1086        160          0         13        483      12172   u2_app_service.o
       340          8          0          0          0       5954   u2_app_serviceproc.o
       148          6          0          0         36       1915   u2_link_layer.o
      2398        214          0          2        646      13737   u2_tp_layer.o
        12          4          0          0          0        394   wdt.o

    ----------------------------------------------------------------------
     61956       4714       2932        992       6496     604569   Object Totals
         0          0         32          0          0          0   (incl. Generated)
        42          0          3         15         12          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

       852         38          0          1         12       6406   can_signal_rx.o
      1376         28          0          1         16       3434   can_signal_tx.o
      1232         30          0          0         28       5788   telltales_lib.o
        86          0          0          0          0          0   __dczerorl2.o
         8          0          0          0          0         68   __main.o
         0          0          0          0          0          0   __rtentry.o
        12          0          0          0          0          0   __rtentry2.o
         6          0          0          0          0          0   __rtentry4.o
        60          8          0          0          0          0   __scatter.o
        28          0          0          0          0          0   __scatter_zi.o
       488          0          0          0          0         92   aeabi_sdivfast.o
        16          0          0          0          0         68   exit.o
         6          0          0          0          0        136   heapauxi.o
         0          0          0          0          0          0   indicate_semi.o
         2          0          0          0          0          0   libinit.o
         2          0          0          0          0          0   libinit2.o
         2          0          0          0          0          0   libshutdown.o
         2          0          0          0          0          0   libshutdown2.o
         8          4          0          0         96         68   libspace.o
        48          0          0          0          0         72   llmul.o
       258          0          0          0          0         88   lludiv.o
        64          0          0          0          0        108   rt_memclr.o
       186          0          0          0          0        144   rt_memcpy.o
         2          0          0          0          0          0   rtexit.o
        10          0          0          0          0          0   rtexit2.o
        12          4          0          0          0         60   sys_exit.o
        62          0          0          0          0         80   sys_stackheap_outer.o
         2          0          0          0          0         68   use_no_semi.o
      3168        156          0          0         32      12643   eeprommanage.o

    ----------------------------------------------------------------------
      8000        268          0          4        196      29323   Library Totals
         2          0          0          2         12          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

      2228         66          0          2         28       9840   CAN_Lib.lib
      1232         30          0          0         28       5788   Telltales.lib
      1370         16          0          0         96       1052   c_p.l
      3168        156          0          0         32      12643   eepromManage.lib

    ----------------------------------------------------------------------
      8000        268          0          4        196      29323   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     69956       4982       2932        996       6692     607388   Grand Totals
     69956       4982       2932         92       6692     607388   ELF Image Totals (compressed)
     69956       4982       2932         92          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                72888 (  71.18kB)
    Total RW  Size (RW Data + ZI Data)              7688 (   7.51kB)
    Total ROM Size (Code + RO Data + RW Data)      72980 (  71.27kB)

==============================================================================

