{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["软件自测用例"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"软件自测用例","index":0,"n_rows":7,"n_cols":8,"rows_kept":7,"cut":false,"hidden":false,"merged":[[64,7,81,7],[83,7,101,7],[103,7,109,7],[111,7,117,7],[8,7,15,7],[19,7,26,7],[30,7,37,7],[39,7,41,7],[1,1,1,7],[2,1,2,3],[2,6,2,7],[3,1,3,3],[3,6,3,7]]}
[]
[null,"仪表功能测试报告"]
[null,"供应商名称：黑龙江天有为电子有限责任公司",null,null,"ECU硬件版本：HV1.0","ECU软件版本：SV1.0"]
[null,"测试时间：2024.2.28",null,null,"测试地点：黑龙江天有为",null,"测试执行人：时昊"]
[null,"编号","测试用例名称","类型","步骤描述",null,"测试结果","数据log区"]
[null,1,"EBD,驻车制动,手刹逻辑共用手刹指示灯显示","指示灯","1.上30电,上15电\n2.手刹和驻车制动硬线悬空,且报文0x0a18a006掉线时,手刹指示灯点亮\n3.手刹和驻车制动硬线悬空,且报文0x0a18a006在线时,手刹指示灯点亮\n4.手刹硬线悬空,驻车制动硬线接地,且0x0a18a006报文掉线时,手刹指示灯闪烁,此时将0x0a18a006报文在线,手刹指示灯熄灭,此时将0x0a18a006报文在线,并发送信号EBDFail = 1时,手刹指示灯点亮\n5.手刹硬线接电源,驻车制动硬线接地,且0x0a18a006报文掉线时,手刹指示灯闪烁,此时将驻车制动硬线悬空,手刹指示灯点亮,",null,"通过"]
[null,2,"增加ABS指示灯功能","指示灯","1.上30电,上15电\n2.报文0x0a18a006掉线时,ABS指示灯闪烁\n3.报文0x0a18a006在线时,发送信号ABSFail = 1时,指示灯常亮\n4.报文0x0a18a006在线时,发送信号ABSFail = 0时,指示灯熄灭\n5.报文0x0a18a006在线时,发送信号ABSFail = 1时,下15电,指示灯熄灭",null,"通过"]