{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["软件自测用例"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"软件自测用例","index":0,"n_rows":8,"n_cols":8,"rows_kept":8,"cut":false,"hidden":false,"merged":[[1,1,1,7],[2,1,2,3],[2,6,2,7],[3,1,3,3],[3,6,3,7],[76,7,93,7],[95,7,113,7],[115,7,121,7],[123,7,129,7],[5,7,6,7],[20,7,27,7],[31,7,38,7],[42,7,49,7],[51,7,53,7]]}
[]
[null,"仪表功能测试报告"]
[null,"供应商名称：黑龙江天有为电子有限责任公司",null,null,"ECU硬件版本：001.001","ECU软件版本：001.003"]
[null,"测试时间：2024.9.2",null,null,"测试地点：黑龙江天有为",null,"测试执行人：时昊"]
[null,"编号","测试用例名称","类型","步骤描述",null,"测试结果","数据log区"]
[null,1,"45877 【依维柯NS216】燃油开路判定时间与规范要求不一致，规范要求20秒，实际仅10秒","燃油表","1.上15和30电,不接电阻箱\n2.等待弹窗报警,燃油传感器故障,\n3.接上电阻箱,计时20s后,弹窗报警消失\n4.不接电阻箱,计时20s后,弹窗报警显示",null,"通过"]
[null,2,"45879 【依维柯NS216】瞬时油耗单位显示，车速大于50km/h，才能按照L/100km显示","瞬时油耗","1.上15和30电,发送油耗信号10L/H，使瞬时油耗有数值显示10L/H\n2.发送车速信号，实际车速为0,瞬时油耗单位为10L/H\n3.车速发送100km/h,瞬时油耗单位显示为10L/100km\n4.车速发送4km/h,瞬时油耗单位显示为10L/H\n5.车速发送5km/h,瞬时油耗单位显示为19.9L/100km",null,"通过"]
[null,3,"45880 【依维柯NS216】平均油耗，车速为1km/h（无限小），喷油量3000L/h（无限大），平均油耗维持上一数值不动","燃油表","1.上15和30电,车速发送100km/h,发送油耗信号12L/H\n2.平均油耗从默认13.0降到12.0L/100km\n3.将喷油量信号发送30L/H,\n4.平均油耗从12.0升到19.9L/100km\n5.重新上30电,车速发送100km/h,喷油量19L/h，\n6.平均油耗会涨到19.0L/100km\n",null,"通过"]