{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["软件自测用例"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"软件自测用例","index":0,"n_rows":19,"n_cols":8,"rows_kept":19,"cut":false,"hidden":false,"merged":[[128,7,134,7],[47,7,54,7],[56,7,58,7],[81,7,98,7],[100,7,118,7],[120,7,126,7],[10,5,12,5],[10,6,12,6],[6,7,9,7],[25,7,32,7],[36,7,43,7],[10,0,11,0],[10,1,12,1],[10,2,12,2],[10,3,12,3],[10,4,12,4],[1,1,1,7],[2,1,2,3],[2,6,2,7],[3,1,3,3],[3,6,3,7]]}
[]
[null,"仪表功能测试报告"]
[null,"供应商名称：黑龙江天有为电子有限责任公司",null,null,"ECU硬件版本：001.001","ECU软件版本：001.003"]
[null,"测试时间：2024.3.28",null,null,"测试地点：黑龙江天有为",null,"测试执行人：时昊"]
[null,"编号","测试用例名称","类型","步骤描述",null,"测试结果","数据log区"]
[null,1,"配置为F102，非倒挡也报警","报警","1.上30、15电，连接诊断工具\n2.配置F102 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 52 00 00\n3.断开诊断工具\n4.发送报文0x18FAB027 信号VCU_GearPositionInd=0xFC（D档）；报文0xCFF1ADA 信号PDC_VirtualDisplaySts=0x1；报文0xCFF1ADA 信号PDC_Warning_Frq=0x1（雷达持续1HZ报警条件）\n5.雷达不报警\n6.连接诊断工具\n7.发送报文0x18FAB027 信号VCU_GearPositionInd=0xDF（R档）；报文0xCFF1ADA 信号PDC_VirtualDisplaySts=0x1；报文0xCFF1ADA 信号PDC_Warning_Frq=0x1（雷达持续1HZ报警条件）\n8.雷达报警",null,"通过"]
[null,2,"负功率计算错误","功率表","1.上30、15电\n2.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=12（车速>7km/h）\n3.车速表显示车速12km/h\n4.发送报文0X18FAB027 信号VCU_PTModeInd=0x1；报文0x18FA40F4 信号BMS_BattCurr=0x84D0（物理值101）\n5.功率表显示-100% 2格\n6.发送报文0x18FA40F4 信号BMS_BattCurr=0x84D0（物理值100）\n7.功率表显示-50% 1格\n8.发送报文0x18FA40F4 信号BMS_BattCurr=0x84BC（物理值99）\n9.功率表显示-50% 1格\n10.发送报文0x18FA40F4 信号BMS_BattCurr=0x7D00（物理值0）\n11.功率表显示0% 0格",null,"通过"]
[null,3,"时间信号掉线，重上电后不应显示时间","时间显示","1.上30、15电\n2.将报文0x18FEE69F在线\n3.显示时间\n4.重上大电\n5.显示时间\n6.掉线报文0x18FEE69F\n7.重上大电\n8.不显示时间",null,"通过"]
[null,4,"超速报警配置为无速度限制时，车速为2就开始报警","报警","1.上30、15电，连接诊断工具\n2.配置F102 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 A0 00 00\n3.断开诊断工具\n4.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=9\n5.车速表显示车速9km/h，无报警音\n6.连接诊断工具\n7.配置F102  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 F0 00 00\n8.断开诊断工具\n9.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=20\n10.车速表显示车速20km/h，无报警音",null,"通过"]
[null,5,"F102报警音取消或切换频率后有杂音","报警","1.上30、15电，连接诊断工具\n2.配置F102 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 52 00 00\n3.断开诊断工具\n4.发送报文0xCFF1ADA 信号PDC_VirtualDisplaySts=0x1；报文0xCFF1ADA 信号PDC_Warning_Frq=0x5\n5.报警声长鸣\n6.送报文0xCFF1ADA 信号PDC_VirtualDisplaySts=0x1；报文0xCFF1ADA 信号PDC_Warning_Frq=0x0\n7.报警声消除且没有杂音\n8.送报文0xCFF1ADA 信号PDC_VirtualDisplaySts=0x1；报文0xCFF1ADA 信号PDC_Warning_Frq=0x5\n9.报警声长鸣\n10.送报文0xCFF1ADA 信号PDC_VirtualDisplaySts=0x1；报文0xCFF1ADA 信号PDC_Warning_Frq=0x0\n11.报警声消除且没有杂音",null,"通过"]
[null,6,"超速报警解报点错误","超速报警","1.上30、15电，连接诊断工具\n2.配置F102 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 12 00 00 断开诊断工具\n3.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=60\n4.车速表显示车速61km/h，车速表闪烁，有报警音\n5.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=56\n6.车速表显示车速57km/h，车速表停止闪烁，连接诊断工具\n7.配置F102 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 22 00 00 断开诊断工具\n8.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=65\n9.车速表显示车速66km/h，车速表闪烁，有报警音\n10.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=61\n11.车速表显示车速62km/h，车速表停止闪烁，连接诊断工具\n12.配置F102 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 32 00 00 断开诊断工具\n13.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=69\n14.车速表显示车速71km/h，车速表闪烁，有报警音\n15.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=66\n16.车速表显示车速67km/h，车速表停止闪烁，连接诊断工具\n17.配置F102 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 42 00 00 断开诊断工具\n18.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=74\n19.车速表显示车速76km/h，车速表闪烁，有报警音\n20.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=70\n21.车速表显示车速72km/h，车速表停止闪烁，连接诊断工具\n22.配置F102 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 52 00 00 断开诊断工具\n23.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=79\n24.车速表显示车速81km/h，车速表闪烁，有报警音\n25.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=75\n26.车速表显示车速77km/h，车速表停止闪烁，连接诊断工具\n27.配置F102 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 62 00 00 断开诊断工具\n28.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=84\n29.车速表显示车速86km/h，车速表闪烁，有报警音\n30.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=80\n31.车速表显示车速82km/h，车速表停止闪烁，连接诊断工具\n32.配置F102 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 72 00 00 断开诊断工具\n33.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=89\n34.车速表显示车速91km/h，车速表闪烁，有报警音\n35.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=85\n36.车速表显示车速87km/h，车速表停止闪烁，连接诊断工具\n37.配置F102 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 82 00 00 断开诊断工具\n38.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=94\n39.车速表显示车速96km/h，车速表闪烁，有报警音\n40.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=90\n41.车速表显示车速92km/h，车速表停止闪烁，连接诊断工具\n42.配置F102 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 92 00 00 断开诊断工具\n43.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=99\n44.车速表显示车速101km/h，车速表闪烁，有报警音\n45.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=95\n46.车速表显示车速97km/h，车速表停止闪烁",null,"通过"]
[]
[]
[null,7,"声音报警优先级","报警","1.上30、15电\n2.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=79\n3.车速表显示车速81km/h，车速表闪烁，提示超速报警音\n4.发送报文0x18FAB027 信号VCU_VehicleSysErrorLevel=2\n5.掉线报文0x18FEBF0B\n6.响起动力系统故障报警音10声\n\n",null,"通过"]
[null,8,"休眠唤醒后，时间显示错误","时间显示","1.上30，15电\n2.发送报文0x18FEE69F 信号TBOX_Hour=12 信号TBOX_Minute=2\n3.时间显示12：02\n4.下15电，断开CAN信号\n5.四分钟后上15电，发时间信号\n6.时间显示12：02",null,"通过"]
[null,9,"修改时间发送无效值,显示00.00","时间显示","1.上30，15电\n2.发送报文0x18FEE69F 信号TBOX_Hour=12 信号TBOX_Minute=2\n3.时间显示12：02\n4.下15电，发送报文0x18FEE69F 信号TBOX_Hour=42 信号TBOX_Minute=2\n5.上15电,显示00:00\n6.发送报文0x18FEE69F 信号TBOX_Hour=12 信号TBOX_Minute=2\n7.时间显示12：02\n8.发送报文0x18FEE69F 信号TBOX_Hour=12 信号TBOX_Minute=62\n9.显示00:00",null,"通过"]
[null,10,"修改声音报警","声音报警","1.上30，15电\n2.发送18fa41f4,触发热失控报警,持续播放热失控报警音\n3.发送18febf0b,触发超速报警,此时播放热失控报警音\n4.此时取消热失控报警,\n5.超速报警不播放\n6.发送18febf0b,触发超速报警,播放超速报警音,\n7.发送18fab027,触发动力系统故障,此时播放超速报警音\n8.当取消超速报警音,\n9.动力系统报警不播放\n10.发送0cff1ada,触发雷达长鸣报警音,播放雷达长鸣声音\n11.发送18fa41f4,触发热失控报警,此时持续播放热失控报警音\n12,此时取消热失控报警音\n13.雷达长鸣不再播放\n14.发送18febf0b,触发超速报警,播放超速报警音,\n15.发送18fa41f4,触发热失控报警,此时持续播放热失控报警音\n16.此时取消热失控报警音\n17.超速报警音不再播放\n",null,"通过"]
[null,11,"功率表发送无效值显示不正确","功率表","1.上30，15电\n2.发送18febf0b,将车速显示10km/h\n3.发送0x18FAB027-VCU_PTModeInd=0x1\n&&0x18FA40F4-BMS_BattCurr=0xFB00~0xFFFF\n4.功率表显示--%\n5.0x18FA40F4-BMS_BattCurr=0\n6.功率表显示0%\n7.0x18FA40F4-BMS_BattCurr=0.1\n8.功率表显示-50%",null,"通过"]
[null,12,"雷达报警取消后,有杂音","雷达报警","1.上15电和30电\n2.报文0xCFF1ADA 信号PDC_VirtualDisplaySts=0x1；报文0xCFF1ADA 信号PDC_Warning_Frq=0x1（雷达持续1HZ报警条件）\n3.然后立刻取消,没有听到杂音",null,"通过"]