{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["软件自测用例"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"软件自测用例","index":0,"n_rows":10,"n_cols":8,"rows_kept":10,"cut":false,"hidden":false,"merged":[[1,1,1,7],[2,1,2,3],[2,6,2,7],[3,1,3,3],[3,6,3,7],[80,7,97,7],[99,7,117,7],[119,7,125,7],[127,7,133,7],[6,7,9,7],[24,7,31,7],[35,7,42,7],[46,7,53,7],[55,7,57,7]]}
[]
[null,"仪表功能测试报告"]
[null,"供应商名称：黑龙江天有为电子有限责任公司",null,null,"ECU硬件版本：001.001","ECU软件版本：001.003"]
[null,"测试时间：2024.3.25",null,null,"测试地点：黑龙江天有为",null,"测试执行人：时昊"]
[null,"编号","测试用例名称","类型","步骤描述",null,"测试结果","数据log区"]
[null,1,"配置为CAN雷达，非倒挡也报警","报警","1.上30、15电，连接诊断工具\n2.配置CAN雷达 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 52 00 00\n3.断开诊断工具\n4.发送报文0x18FAB027 信号VCU_GearPositionInd=0xFC（D档）；报文0xCFF1ADA 信号PDC_VirtualDisplaySts=0x1；报文0xCFF1ADA 信号PDC_Warning_Frq=0x1（雷达持续1HZ报警条件）\n5.雷达不报警\n6.连接诊断工具\n7.发送报文0x18FAB027 信号VCU_GearPositionInd=0xDF（R档）；报文0xCFF1ADA 信号PDC_VirtualDisplaySts=0x1；报文0xCFF1ADA 信号PDC_Warning_Frq=0x1（雷达持续1HZ报警条件）\n8.雷达报警",null,"通过"]
[null,2,"负功率计算错误","功率表","1.上30、15电\n2.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=12（车速>7km/h）\n3.车速表显示车速12km/h\n4.发送报文0X18FAB027 信号VCU_PTModeInd=0x1；报文0x18FA40F4 信号BMS_BattCurr=0x84D0（物理值101）\n5.功率表显示-100% 2格\n6.发送报文0x18FA40F4 信号BMS_BattCurr=0x84D0（物理值100）\n7.功率表显示-50% 1格\n8.发送报文0x18FA40F4 信号BMS_BattCurr=0x84BC（物理值99）\n9.功率表显示-50% 1格\n10.发送报文0x18FA40F4 信号BMS_BattCurr=0x7D00（物理值0）\n11.功率表显示0% 0格",null,"通过"]
[null,3,"时间信号掉线，重上电后不应显示时间","时间显示","1.上30、15电\n2.将报文0x18FEE69F在线\n3.显示时间\n4.重上大电\n5.显示时间\n6.掉线报文0x18FEE69F\n7.重上大电\n8.不显示时间",null,"通过"]
[null,4,"超速报警配置为无速度限制时，车速为2就开始报警","报警","1.上30、15电，连接诊断工具\n2.配置CAN雷达 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 A0 00 00\n3.断开诊断工具\n4.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=9\n5.车速表显示车速9km/h，雷达不报警\n6.连接诊断工具\n7.配置CAN雷达  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 F0 00 00\n8.断开诊断工具\n9.发送报文0x18FEBF0B 信号ABSFrontAxleSpeed=20\n10.车速表显示车速20km/h，雷达不报警",null,"通过"]
[null,5,"CAN雷达报警音取消或切换频率后有杂音","报警","1.上30、15电，连接诊断工具\n2.配置CAN雷达 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 52 00 00\n3.断开诊断工具\n4.发送报文0xCFF1ADA 信号PDC_VirtualDisplaySts=0x1；报文0xCFF1ADA 信号PDC_Warning_Frq=0x5\n5.报警声长鸣\n6.送报文0xCFF1ADA 信号PDC_VirtualDisplaySts=0x1；报文0xCFF1ADA 信号PDC_Warning_Frq=0x0\n7.报警声消除且没有杂音\n8.送报文0xCFF1ADA 信号PDC_VirtualDisplaySts=0x1；报文0xCFF1ADA 信号PDC_Warning_Frq=0x5\n9.报警声长鸣\n10.送报文0xCFF1ADA 信号PDC_VirtualDisplaySts=0x1；报文0xCFF1ADA 信号PDC_Warning_Frq=0x0\n11.报警声消除且没有杂音",null,"通过"]