# ESP32 supports SIGNED_APPS_RSA_SCHEME only in ECO3
CONFIG_ESP32_REV_MIN_3=y
CONFIG_ESP32_REV_MIN=3

CONFIG_EXAMPLE_FIRMWARE_UPGRADE_URL="FROM_STDIN"
CONFIG_EXAMPLE_SKIP_COMMON_NAME_CHECK=y

CONFIG_PARTITION_TABLE_OFFSET=0xC000

CONFIG_SECURE_SIGNED_APPS_NO_SECURE_BOOT=y
CONFIG_SECURE_SIGNED_ON_UPDATE_NO_SECURE_BOOT=y
CONFIG_SECURE_SIGNED_APPS_RSA_SCHEME=y
CONFIG_SECURE_BOOT_SIGNING_KEY="test/secure_boot_signing_key.pem"

CONFIG_EXAMPLE_CONNECT_ETHERNET=y
CONFIG_EXAMPLE_CONNECT_WIFI=n
CONFIG_EXAMPLE_USE_INTERNAL_ETHERNET=y
CONFIG_EXAMPLE_ETH_PHY_IP101=y
CONFIG_EXAMPLE_ETH_MDC_GPIO=23
CONFIG_EXAMPLE_ETH_MDIO_GPIO=18
CONFIG_EXAMPLE_ETH_PHY_RST_GPIO=5
CONFIG_EXAMPLE_ETH_PHY_ADDR=1

CONFIG_MBEDTLS_TLS_CLIENT_ONLY=y
CONFIG_COMPILER_OPTIMIZATION_SIZE=y
CONFIG_EXAMPLE_CONNECT_IPV6=n
