#!gbuild
primaryTarget=v800_standalone.tgt
[Program]
	
	-object_dir=./obj
	-map
	-gsize
	-preprocess_assembly_files
	-e _RESET
	-list
	-list_dir=./list
	-Mx
	-bsp generic
	-callgraph
	{optgroup=GhsCommonOptions} -o output/project.out
	:postexec='gmemfile output/project.out -o output/project.mem'
	:postexec='gsrec  -e 0 -hex386 output/project.out -o output/project.hex'
	:postexec='gsrec  -e 0 -noS5 output/project.out -o output/C211-L-APP.rec'
	--no_additional_output
	-dwarf2
	-D__GHS__
	{optgroup=GhsCompilerOptions} -cpu=rh850g3kh
	-DPlatform_RH850
	-DPlatform_32Bit
	-nothreshold
	-passsource
	-I..\source\Driver\Clock
	-I..\source\Driver\RH850F1KM_S1
	-I..\source\Driver\Timer
	-I..\source\Driver\TimerB
	-I..\source\Driver\Analog_Signals
	-I..\source\Driver\CAN
	-I..\source\Driver\GPIO
	-I..\source\System
	-I..\source\Appliciation
	-I..\source\FCL
	-I../source/EEL
	-I../source/eel_user
	-I../source/fdl_user
	-I../source/FDL
	-I../source/EEL/lib
	-I../source/FDL/lib
	-pack=4
	--diag_suppress 1
	#--diag_suppress 9
	#--diag_suppress 177
	#--diag_suppress 550
	#--diag_suppress 188
	-fsingle
	-Onone
	-O0
	-G
.\group\Application.gpj
.\group\Driver.gpj
.\group\System.gpj
.\group\FCL.gpj
.\group\Fdl.gpj
.\group\EEL.gpj
output\project.map
