{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["基本信息","电源配置","时序要求","仪表硬件测试需求","BAT32G137GH64FB 配置"],"not_rendered":{"images":7,"comments":5},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"基本信息","index":0,"n_rows":355,"n_cols":40,"rows_kept":355,"merged":[[1,2,1,7],[4,2,4,4],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,2,10,3],[11,2,11,3],[12,2,12,3],[13,2,13,3],[15,2,15,8],[24,2,24,8],[25,2,25,4],[25,5,25,8],[26,2,26,4],[26,5,26,8],[27,2,27,4],[27,5,27,8],[28,3,28,4],[29,3,29,4],[30,3,30,4],[31,3,31,4],[32,3,32,4],[33,3,33,4],[34,3,34,4],[35,3,35,4],[36,3,36,4],[37,3,37,4],[38,3,38,4],[39,3,39,4],[40,2,40,4],[40,5,40,8],[51,2,51,7],[66,2,66,7],[67,2,70,7],[72,2,72,7],[73,2,76,7],[342,25,342,31],[352,25,352,33],[353,26,353,33],[354,26,354,33]],"flags":["formulas_cached_only"]}
[]
[null,null,"天鹰项目软硬件交互文档"]
[]
[]
[null,null,"基本信息"]
[null,null,"项目代号",null,"天鹰TY100-ICU-M-C-V100-B00"]
[null,null,"目标客户",null,"天鹰摩托"]
[null,null,"硬件工程师",null,"李昊"]
[null,null,"MCU平台",null,"BAT32A239KK64FB"]
[null,null,"SOC平台"]
[null,null,"文档编号",null,"-"]
[null,null,"文档序号",null,"-"]
[null,null,"模板版本",null,"V2.1"]
[null,null,"保密级别",null,"商业秘密"]
[]
[null,null,"修改记录信息"]
[null,null,"序号","修订日期","文档版本","修订内容","修订人","审核人","适用硬件版本",null,"版本填写说明",{"$nulls":28},"未确认"]
[null,null,1,"2024-04-22","V1.0.0","初版","李昊","张轩","天鹰TY100-ICU-M-C-V100-B00",{"$nulls":30},"满足"]
[null,null,2,{"$nulls":36},"不满足"]
[null,null,3,{"$nulls":36},"不涉及"]
[null,null,4]
[null,null,5]
[]
[]
[null,null,"《软硬件交互文档》评审报告"]
[null,null,"评审文档版本"]
[null,null,"评审日期"]
[null,null,"文档制作人"]
[null,null,"序号","评审项",null,"评审内容","评审意见","确认人","备注"]
[null,null,1,"电源配置评审",null,"电源配置表格描述准确","未确认"]
[null,null,2,"IO分配评审",null,"GPIO使用合理","未确认"]
[null,null,3,"IO分配评审",null,"ADC使用专用IO，设计合理","未确认"]
[null,null,4,"IO分配评审",null,"SPI,UART必须使用专用IO,RX/TX数据传输方向设计正确","未确认"]
[null,null,5,"IO分配评审",null,"PWM输出使用正确的IO、设计正确","未确认"]
[null,null,6,"IO分配评审",null,"PWM输入使用正确的IO、设计正确","未确认"]
[null,null,7,"硬件测试需求评审",null,"评审所提需求是否合理正确，功能是否匹配","未确认"]
[null,null,8,"单板上下电时序评审",null,"整板上电时序设计合理，整板下电时序设计合理。","未确认"]
[null,null,9,"模块1上下电时序评审",null,"上电时序设计合理，下电时序设计合理。","未确认",{"$nulls":3},"填写说明"]
[null,null,10,"模块2上下电时序评审",null,"上电时序设计合理，下电时序设计合理。","未确认"]
[null,null,"N","......上下电时序评审",null,"上电时序设计合理，下电时序设计合理。","未确认"]
[null,null,"评审结论",null,null,"未确认"]
{"$rows_empty":10}
[null,null,"模板修订信息"]
[null,null,"序号","修订日期","模板修订版本","修订内容","修订人","审核人"]
[null,null,1,"2019-06-30","V1.0","初始版本","宋鑫鑫","徐剑"]
[null,null,2,"2020-03-14","V1.1","优化了电源配置，上电时序增加了总时序图模板","宋鑫鑫","徐剑"]
[null,null,3,"2020-07-02","V1.2","324和336页增加了“输入模式”和“实际电流配置”列","宋鑫鑫","徐剑"]
[null,null,4,"2021-07-02","V1.3","增加了AC7811 IO配置、ATSAMC21J17 IO配置、SKEAZN64M IO配置","李兴伟","宋鑫鑫"]
[null,null,5,"2021-07-13","V1.4","增加了RH850D1M1A IO配置","李兴伟","宋鑫鑫"]
[null,null,6,"2022-06-27","V1.5","更新上下电时序模板","徐剑","徐剑"]
[null,null,7,"2022-07-18","V1.6","增加了R7F701401、R5F10TPJJFB、KF32A156MQV、KF32A146LQT、BAT32G137GH64FBIO、R7F7016843AFP配置，修改原有部分内容,增加支持硬件单板测试的软件功能要求","张洁、徐剑","徐剑"]
[null,null,8,"2022-08-24","V1.7","增加完善Sleep Mode IO状态可选择项","张洁、徐剑","徐剑"]
[null,null,9,"2023-03-08","V1.8","增加BS9000AM28-TBBX配置，增加“仪表硬件测试需求”sheet，增加“导航显示板硬件测试需求”sheet。首页基本信息增加“SOC平台”首页增加对PWM频率的要求参考","张洁、宋鑫鑫、徐剑","徐剑"]
[null,null,10,"2023-05-19","V1.9","增加时序测试点","王洪强，宋鑫鑫","徐剑"]
[null,null,11,"2023-10-30","V2.0","修改三极管调光频率要求、将调光频率要求移动到MCU IO配置页、隐藏MCU IO mode等参考信息（防止产生争议）,修改部分MCU配置页内容，将列项统一。","徐剑","徐剑"]
[null,null,12,"2023-11-06","V2.1","增加此文档的评审报告相关内容、修改基本信息页部分描述","徐剑，宋鑫鑫","徐剑"]
[]
[null,null,"模板使用说明"]
[null,null,"1 实际使用模板时，只需保留项目对应的MCU，其他MCU配置sheet页全部删除\n2 要求MCU IO配置页信息必须严格准确，否则可能造成软件工程师错误编程\n3 需包含单板冷启动、休眠唤醒后所有软件控制的电源及其他重要功能性IO的时序需要（例如部分功能的使能、解复位IO等）,以及休眠时的下电时序要求，模板只是给出了格式，具体内容根据实际项目合理调整。\n4 硬件开发工程师必须在“测试需求”页将对应功能勾选好，否则无法指导软件如何编程才能尽快支撑硬件测试。"]
[]
[]
[]
[]
[null,null,"补充说明"]
[null,null,"产品上有PWM调光类应用必须按照如下要求执行：\n1 MPQ3367   400Hz±20%\n2 AW9967/TPS61161  20kHz±5%\n3 三极管调光 370~420Hz\n4 LP8867C 2.6kHz±5%\n5 RT8577A 1kHz±5%"]
{"$rows_empty":265}
[{"$nulls":25},"填写举例："]
[]
[]
[{"$nulls":25},"修改记录信息"]
[{"$nulls":25},"序号","修订日期","文档版本","修订内容","修订人","审核人","适用硬件版本"]
[{"$nulls":25},1,"2022-01-01","US4-ICU-M-C-V100-B00","首版","魏弘洋","孔繁宇","US4-ICU-M-C-V100-B00"]
[{"$nulls":25},2,"2022-02-01","US4-ICU-M-C-V100-B01","与上一版本内容一致、无变化","魏弘洋","孔繁宇","US4-ICU-M-C-V100-B00\nUS4-ICU-M-C-V100-B01"]
[{"$nulls":25},3,"2022-03-01","US4-ICU-M-C-V110-B00","修改LP8867C使能pin控制IO","魏弘洋","孔繁宇","US4-ICU-M-C-V110-B00"]
[{"$nulls":25},4,"2022-05-01","US4-ICU-M-C-V200-B00","MCU平台从324更换为RH850","魏弘洋","孔繁宇","US4-ICU-M-C-V200-B00"]
[{"$nulls":25},5]
[{"$nulls":25},6]
[{"$nulls":25},7]
[]
[{"$nulls":25},"填写说明"]
[{"$nulls":25},1,"每次研究院归档必须包含“《软硬件交互文档》”归档，并且文档版本同“《硬件图纸》”版本必须完全相同"]
[{"$nulls":25},2,"经常可能出现前后两次研究院归档的“《软硬件交互文档》”实际内容完全一样，此时文档版本号正常升级，但是修订内容里填“与上一版本内容一致、无变化”"]

{"sheet":"电源配置","index":1,"n_rows":28,"n_cols":14,"rows_kept":28,"merged":[[1,1,1,6],[2,1,2,2],[3,1,35,1],[3,2,25,2],[3,3,25,3],[3,4,12,4],[3,5,3,6],[4,5,4,6],[5,5,5,6],[6,5,6,6],[7,5,7,6],[8,5,10,6],[11,5,12,6],[13,4,15,4],[13,5,15,6],[16,5,16,6],[17,4,17,6],[18,4,18,6],[19,4,19,6],[20,4,20,6],[21,4,21,6],[22,4,22,6],[23,4,23,6],[24,4,24,6],[25,4,25,6],[26,3,26,6],[27,2,35,2],[27,3,35,6],[36,1,36,6]],"flags":["formulas_cached_only"]}
[]
[null,"电源MAP"]
[null,"一级电源",null,"二级电源","三级电源","四级电源","用途"]
[null,"最低电压--\n最高电压\n\n\n~B+\n~IGN+\n","VCC9V6\n_SYS","VCC5V_SYS\n\n\n","可切5V"]
[]
[]
[]
[{"$nulls":5},"断码屏"]
[{"$nulls":5},21036]
[]
[]
[{"$nulls":5},"报警灯"]
[]
[]
[]
[]
[{"$nulls":4},"VCC5V_LED_BL","断码背光"]
[{"$nulls":4},"BAT32A239KK64FB"]
[{"$nulls":4},"24G16"]
[{"$nulls":4},"TCAN1044"]
[{"$nulls":4},"燃油"]
[{"$nulls":4},"RSTX"]
[{"$nulls":4},"编程",{"$nulls":8},"，"]
[{"$nulls":4},"EEPROM存储器"]
[{"$nulls":4},"油位信号"]
[]
[null,null,"B+","KL30 Sampling"]
[null,null,"VCC12V_KL15_上拉","负控上拉"]

{"sheet":"时序要求","index":2,"n_rows":154,"n_cols":15,"rows_kept":154,"merged":[[0,1,0,9],[2,6,2,9],[3,6,3,9],[6,6,6,9],[14,1,14,4],[14,11,14,14],[16,1,16,4],[16,11,16,14],[18,11,18,14],[20,11,20,14],[22,1,22,4],[22,6,22,9],[22,11,22,14],[25,1,25,4],[27,1,27,4],[29,1,29,4],[31,1,31,4],[37,6,37,9],[38,6,38,9],[42,6,42,9],[45,6,45,9],[47,6,47,9],[50,6,50,9],[52,6,52,9],[54,6,54,9],[59,1,59,14],[61,1,61,4],[61,6,61,9],[61,11,61,14],[62,11,62,14]],"flags":["formulas_cached_only"]}
[null,"时序要求制定说明：\n\n1 需包含单板冷启动、休眠唤醒后所有软件控制的电源及其他重要功能性IO的时序需要（例如部分功能的使能、解复位IO等）,以及休眠时的下电时序要求，模板只是给出了格式，具体内容根据实际项目合理调整。\n\n2 上电时序要求制定时，尽量实现一条主线的上电时序要求，如某些产品系统复杂（包含多个时序要求的芯片或负载，则根据实际情况制定支线上电时序要求），否则会过度限制软件编程灵活性并可能会导致上电时间过长，开机速度慢。\n\n3 下电时序要求制定时，采用一条主线方式，下电时序不同于上电时序，大部分操作都是关闭负载的电源等，尽量采用一条主线的方式制定下电时序要求。"]
[]
[{"$nulls":6},"单板上电时序要求"]
[{"$nulls":6},"单板上电时序（冷启动及休眠唤醒）"]
[{"$nulls":6},"信号类型","控制方式","控制IO","软件控制方式"]
[{"$nulls":6},"VCC5V_SYS开电","hardware","-","-"]
[{"$nulls":6},"Delay≥0ms"]
[{"$nulls":6},"VCC3V3_SYS开电","hardware","-","-"]
[{"$nulls":8},"｜"]
[{"$nulls":8},"｜"]
[{"$nulls":3},"｜",{"$nulls":4},"↓",{"$nulls":4},"｜"]
[{"$nulls":3},"｜",{"$nulls":9},"｜"]
[{"$nulls":3},"↓",{"$nulls":9},"↓"]
[null,"信号类型","控制方式","控制IO","软件控制方式",{"$nulls":6},"信号类型","控制方式","控制IO","软件控制方式"]
[null,"Delay≥0ms",{"$nulls":9},"Delay≥0ms"]
[null,"630H的1.2v开电","software","Pin46(16843)","高有效",{"$nulls":6},"屏3.3v开电","software","Pin6(16843)","高有效"]
[null,"Delay≥30ms",{"$nulls":9},"Delay≥10ms"]
[null,"630H的3.3v开电","software","Pin49(16843)","高有效",{"$nulls":6},"1530芯片开电","software","Pin50(16843)","高有效"]
[{"$nulls":11},"Delay≥50ms"]
[{"$nulls":3},"｜",{"$nulls":4},"｜",null,null,"屏解复位","software","Pin20(16843)","高有效"]
[{"$nulls":3},"｜",{"$nulls":4},"｜",null,null,"300ms≥Delay≥1ms"]
[{"$nulls":3},"↓",{"$nulls":4},"↓",null,null,"630H的LVDS信号输出","software","Pin86~Pin95(630H)","高有效"]
[null,"Delay≥0ms",{"$nulls":4},"Delay≥5ms",{"$nulls":4},"Delay≥350ms"]
[null,"切电5V开电","software","Pin71(16843)","高有效",null,"MCU向630H发消息（TX）","software","Pin86(16843)","-",null,"液晶屏背光开","software","Pin87(16843)","PWM"]
[null,"AW88298的5V开电","software","Pin80(16843)","高有效"]
[null,"Delay≥1ms"]
[null,"AW88298的1.8v开电","software","Pin70(16843)","高有效"]
[null,"Delay≥5ms"]
[null,"AW88298解复位","software","Pin97(630H)","高有效"]
[null,"Delay≥1ms"]
[null,"AW88298的I2C配置","software","SCL:Pin8(630H)\nSDA:Pin9(630H)","-"]
[null,"Delay≥0ms"]
[null,"630H的I2S信号输出","software","BCLK：Pin99(630H)\nWCLK：Pin100(630H)\nDIN：Pin98(630H)","-"]
[]
[]
[]
[]
[{"$nulls":6},"单板下电时序要求"]
[{"$nulls":6},"（进入休眠）"]
[{"$nulls":6},"信号类型","控制方式","控制IO","软件控制方式"]
[{"$nulls":6},"液晶屏背光关","software","Pin87(16843)","低有效"]
[{"$nulls":6},"MCU与630H通信停止","software","TX:Pin86(16843)","-"]
[{"$nulls":6},"Delay≥10ms"]
[{"$nulls":6},"630H的3.3v关电","software","Pin49(16843)","低有效"]
[{"$nulls":6},"630H的1.2v关电","software","Pin46(16843)","低有效"]
[{"$nulls":6},"Delay≥10ms"]
[{"$nulls":6},"AW88298的1.8v关电","software","Pin70(16843)","低有效"]
[{"$nulls":6},"Delay≥1ms"]
[{"$nulls":6},"切电5V关电","software","Pin71(16843)","低有效"]
[{"$nulls":6},"AW88298的5V关电","software","Pin80(16843)","低有效"]
[{"$nulls":6},"Delay≥0ms"]
[{"$nulls":6},"1530芯片关电","software","Pin50(16843)","低有效"]
[{"$nulls":6},"Delay≥10ms"]
[{"$nulls":6},"屏复位","software","Pin20(16843)","低有效"]
[{"$nulls":6},"Delay≥50ms"]
[{"$nulls":6},"屏3.3v关电","software","Pin6(16843)","低有效"]
[]
[]
[]
[null,"注：硬件工程师需在下方将各类负载的时序要求附上截图或附上文字描述"]
[]
[null,"液晶屏 datasheet时序要求",{"$nulls":4},"AW88298 datasheet时序要求",{"$nulls":4},"AMT630H datasheet时序要求"]
[{"$nulls":11},"1.2V比3.3V提前上电至少10ms"]
{"$rows_empty":46}
[null,"测试位置"]
{"$rows_empty":31}
[null,"测点1：切电5V开/关电--Pin71(16843)"]
[null,"测点2：AW88298的5V开/关电--Pin80(16843)"]
[null,"测点3：AW88298的1.8v开/关电--Pin70(16843)"]
[null,"测点4：AW88298解复位--Pin97(630H)"]
[null,"测点5：AW88298的I2C配置--SCL:Pin8(630H)"]
[null,"测点6：630H的I2S信号输出--BCLK：Pin99(630H)"]
[null,"测点7：MCU向630H发消息（TX）--Pin86(16843)"]
[null,"测点8：630H的1.2v开/关电--Pin46(16843)"]
[null,"测点9：630H的3.3v开/关电--Pin49(16843)"]
[null,"测点10：屏3.3v开/关电--Pin6(16843)"]
[null,"测点11：1530芯片开/关电--Pin50(16843)"]
[null,"测点12：屏解复位--Pin20(16843)"]
[null,"测点13：液晶屏背光开/关--Pin87(16843)"]

{"sheet":"仪表硬件测试需求","index":3,"n_rows":120,"n_cols":36,"rows_kept":120,"merged":[[0,0,0,5],[1,0,1,1],[1,2,1,3],[1,4,1,5],[2,0,2,1],[2,2,2,3],[2,4,2,5],[3,0,3,1],[3,2,3,3],[3,4,3,5],[4,0,4,1],[4,2,4,5],[5,0,5,5],[6,0,6,1],[6,5,7,5],[7,0,7,2],[45,1,45,5]],"flags":["formulas_cached_only"]}
["板卡硬件测试需求功能"]
["优先级1版本测试软件需求时间",null,"2024-05-07",null,"此时间点由硬件工程师填写"]
["优先级2版本测试软件需求时间",null,"x年x月x日",null,"此时间点由硬件工程师填写，包含优先级1、2的所有功能，如果功能有冲突以优先级低的为准"]
["优先级3版本测试软件需求时间",null,"x年x月x日",null,"此时间点由硬件工程师填写，包含优先级1、2、3的所有功能，如果功能有冲突以优先级低的为准"]
["软件版本",null,"此处由软件工程师填写提供给硬件测试的对应软件版本号"]
[]
["项目功能",null,"优先级","调试情况","功能备注","备注"]
["此2列由硬件工程师选择",null,null,"此列由软件工程师选择","此列由软件工程师填写"]
[null,"彩屏--需要点亮","优先级1","功能暂未实现","如果有特殊说明，则填写","屏点亮并显示主界面即可,其他显示功能的完善性不做要求。",{"$nulls":29},false]
[null,"单色屏--需要点亮","优先级1","功能暂未实现","如果有特殊说明，则填写","屏点亮并显示主界面即可,其他显示功能的完善性不做要求。",{"$nulls":29},false]
[null,"段码屏--需要点亮","优先级1","功能暂未实现","如果有特殊说明，则填写","如果是复合屏，TFT屏需要点亮并显示主界面即可,对应段码部分需要开窗。\n段码背光、氛围灯、车速、转速、水温功能需要实现，指示灯不做要求。",{"$nulls":29},true]
[null,"屏背光亮度为用户可操作的最高亮度等级","优先级1","功能暂未实现","如果有特殊说明，则填写","只需把背光亮度设置成这款产品的最高亮度等级，不需要实现各级调光。（包括段码屏、单色屏、彩屏的背光）",{"$nulls":29},false]
[null,"实现所有等级调光功能","优先级2","功能暂未实现","如果有特殊说明，则填写","实现用户可操作的所有等级调光功能（包括段码屏、单色屏、彩屏的背光）",{"$nulls":28},2,true]
[null,"实现15电休眠唤醒功能","优先级1","功能暂未实现","如果有特殊说明，则填写","休眠时所有IO口状态要满足休眠状态要求。",{"$nulls":29},true]
[null,"实现CAN休眠唤醒功能","优先级1","功能暂未实现","如果有特殊说明，则填写","休眠时所有IO口状态要满足休眠状态要求。",{"$nulls":28},2,false]
[null,"实现CANFD休眠唤醒功能","优先级1","功能暂未实现","如果有特殊说明，则填写","休眠时所有IO口状态要满足休眠状态要求。",{"$nulls":28},2,false]
[null,"实现车速显示功能","优先级1","功能暂未实现","如果有特殊说明，则填写","通过CAN通讯，实现车速变化和显示功能",{"$nulls":29},true]
[null,"实现CANFD通讯功能","优先级1","功能暂未实现","如果有特殊说明，则填写","通过CANFD完成哪个功能，请软件工程师在“功能备注”中注明",{"$nulls":29},false]
[null,"实现LIN功能","优先级1","功能暂未实现","如果有特殊说明，则填写","至少实现一个跟LIN相关的功能，具体实现哪个功能不做具体要求，反馈硬件工程师实现了啥就行，实现了啥功能，硬件就测啥功能。",{"$nulls":29},false]
[null,"实现K线功能","优先级1","功能暂未实现","如果有特殊说明，则填写","至少实现一个跟K相关的功能，具体实现哪个功能不做具体要求，反馈硬件工程师实现了啥就行，实现了啥功能，硬件就测啥功能。",{"$nulls":29},false]
[null,"实现扬声器播放音源（报警音）","优先级1","功能暂未实现","如果有特殊说明，则填写","实现安全带报警，左转向，超速报警这三个报警音功能。",{"$nulls":29},false]
[null,"实现蜂鸣器播放音源（报警音）","优先级1","功能暂未实现","如果有特殊说明，则填写","实现安全带报警，左转向，超速报警这三个报警音功能。",{"$nulls":29},false]
[null,"实现车身扬声器播放音乐（手机蓝牙音乐）","优先级2","功能暂未实现","如果有特殊说明，则填写","-",{"$nulls":29},false]
[null,"实现车身扬声器播放音乐（USB音乐）","优先级2","功能暂未实现","如果有特殊说明，则填写","-",{"$nulls":29},false]
[null,"实现双屏互动功能","优先级3","功能暂未实现","如果有特殊说明，则填写","只针对有解串器投屏地图导航的产品",{"$nulls":28},2,false]
[null,"实现全部步进电机正常工作","优先级1","功能暂未实现","如果有特殊说明，则填写","所有步进电机所执行的功能正常",{"$nulls":29},false]
[null,"实现倒车硬线硬线功能","优先级2","功能暂未实现","如果有特殊说明，则填写","每种类型硬线电路对应的功能需要调通一个。此项需硬件工程师根据实际项目硬件填写",{"$nulls":29},false]
[null,"实现回零杆硬线功能","优先级2","功能暂未实现","如果有特殊说明，则填写","每种类型硬线电路对应的功能需要调通一个。此项需硬件工程师根据实际项目硬件填写",{"$nulls":29},false]
[null,"实现左右转硬线功能","优先级2","功能暂未实现","如果有特殊说明，则填写","每种类型硬线电路对应的功能需要调通一个。此项需硬件工程师根据实际项目硬件填写",{"$nulls":29},true]
[null,"实现机油压力硬线功能","优先级2","功能暂未实现","如果有特殊说明，则填写","每种类型硬线电路对应的功能需要调通一个。此项需硬件工程师根据实际项目硬件填写",{"$nulls":29},true]
[null,"实现发动机转速硬线功能","优先级2","功能暂未实现","如果有特殊说明，则填写","每种类型硬线电路对应的功能需要调通一个。此项需硬件工程师根据实际项目硬件填写",{"$nulls":29},true]
[null,"实现确认按键硬线功能","优先级2","功能暂未实现","如果有特殊说明，则填写","每种类型硬线电路对应的功能需要调通一个。此项需硬件工程师根据实际项目硬件填写",{"$nulls":29},true]
[null,"实现远光硬线功能","优先级2","功能暂未实现","如果有特殊说明，则填写","每种类型硬线电路对应的功能需要调通一个。此项需硬件工程师根据实际项目硬件填写",{"$nulls":29},true]
[null,"实现以太网通讯功能","优先级3","功能暂未实现","如果有特殊说明，则填写","-",{"$nulls":28},2,false]
[null,"实现手机互联功能","优先级3","功能暂未实现","如果有特殊说明，则填写","-",{"$nulls":28},2,false]
[null,"实现蓝牙接打电话功能","优先级3","功能暂未实现","如果有特殊说明，则填写","-",{"$nulls":28},2,false]
[null,"实现收音机收听一个台功能","优先级3","功能暂未实现","如果有特殊说明，则填写","功能完善性不做要求，至少能收到一个FM和一个AM电台",{"$nulls":28},2,false]
[null,"实现收音机全部功能","优先级3","功能暂未实现","如果有特殊说明，则填写","-",{"$nulls":29},false]
[null,"实现倒车影像功能","优先级2","功能暂未实现","如果有特殊说明，则填写","-",{"$nulls":28},2,false]
[null,"实现给手机进行USB充电功能","优先级2","功能暂未实现","如果有特殊说明，则填写","-",{"$nulls":28},2,false]
[null,"实现语音控制功能","优先级3","功能暂未实现","如果有特殊说明，则填写","实现一个词条即可。",{"$nulls":28},2,false]
[null,"实现U盘升级仪表程序功能","优先级3","功能暂未实现","如果有特殊说明，则填写","-",{"$nulls":29},false]
[null,"实现环境光传感器功能","优先级2","功能暂未实现","如果有特殊说明，则填写","-",{"$nulls":28},2,false]
[null,"实现胎压模块功能","优先级2","功能暂未实现","如果有特殊说明，则填写","-",{"$nulls":28},2,false]
[null,"实现“时序要求”sheet页的上下电时序要求","优先级1","功能暂未实现","如果有特殊说明，则填写","-",{"$nulls":29},true]
["说明","硬件开发工程师：\n1 根据产品实际情况勾选对应匹配的功能\n2 硬线功能每类选择一个并补充完整功能需求描述\n\n软件开发工程师：\n1 请优先开发此页勾选的功能以尽快支撑硬件测试，没有勾选的功能忽略即可。\n2 软件功能状态一般情况下无法在短期内全部完成本页中需求的功能，请优先开发优先级高的功能，分阶段提供软件\n3 请软件工程师在第一次给硬件开发人员提供首版测试程序时尽量完成优先级1所对应的功能\n4 每次提供硬件测试版本软件的同时，请在表格中填好此版软件对应已经完成的功能或备注并将表格回传给硬件开发工程师"]
{"$rows_empty":70}
[{"$nulls":19},"功能暂未实现"]
[{"$nulls":18},"优先级1","已完成"]
[{"$nulls":18},"优先级2","未完成"]
[{"$nulls":18},"优先级3"]

{"sheet":"BAT32G137GH64FB 配置","index":4,"n_rows":63,"n_cols":20,"rows_kept":63,"merged":[[6,4,7,4],[9,4,10,4],[12,4,13,4],[14,4,15,4],[22,4,24,4],[28,4,29,4],[39,4,40,4],[53,4,55,4],[62,1,62,9]],"flags":["formulas_cached_only"]}
["Pin","IO口","Power \nDomain","网络名","说明","I/O","有效","Sleep Mode\nIO状态","实际配置电流要求mA","最大输出电流能力mA","输入模式","输出模式","Mode1","Mode2","Mode3","Mode4","Mode5","Mode6","Mode7","Mode8"]
[1,"P120","EVDD","L_BiasBitSW_POW","GPIO：5V切电使能（PIN1）","O","H","L","/",40,"/","/","ANI14","VCOUT0"]
[2,"P43","EVDD","按键信号输入-N-IN-MCU","按键信号输入-N-IN-MCU","I","L","L","/",40,"/","/","(INTP9)"]
[3,"P42","EVDD","悬空","悬空","/","/","L","/",40,"/","/","(INTP8)"]
[4,"P41","EVDD","悬空","悬空","/","/","L","/",40,"/","/","(TAIO)"]
[5,"P40","EVDD","SEDIO-编程","烧写","/","/","L","/",40,"/","/","SWDIO"]
[7,"P124","VDD","XT2",32.768,"/","/","/","/","/","/","/","XT2","EXCLKS"]
[8,"P123","VDD","XT1",null,"/","/","/","/","/","/","/","XT1"]
[9,"P137","VDD","SWCLK-编程","烧写","/","/","L","/",40,"/","/","SWCLK"]
[10,"P122","VDD","X2","8M","/","/","/","/","/","/","/","X2","EXCLK"]
[11,"P121","VDD","X1",null,"/","/","/","/","/","/","/","X1"]
[16,"P136","EVDD","悬空","悬空","/","/","L","/",40,"/","/","INTP0"]
[17,"P60","EVDD","存储SCL","I2C：EEPROM（PIN17、PIN18）","/","/","H","/",40,"/","/","SCLA0"]
[18,"P61","EVDD","存储SDA",null,"/","/","H","/",40,"/","/","SDAA0"]
[19,"P62","EVDD","SCL_MCU","I2C：光感、LED Driver、Touch（PIN19\\PIN20）","/","/","L","/",40,"/","/","SS00"]
[20,"P63","EVDD","SDA_MCU",null,"/","/","L","/",40,"/","/","—"]
[21,"P31","EVDD","SDB_LED_DRIVER",21036,"O","H","L","/",40,"/","/","TI03","TO03","INTP4","(CLKBUZ0)","(TAIO)","VCOUT1"]
[22,"P77","EVDD","ABS故障信号输入-N-IN-MCU","ABS故障信号输入-N-IN-MCU","I","L","/","/",40,"/","/","KR7","INTP11","(TxD2)"]
[23,"P76","EVDD","机油压力信号输入-N-IN-MCU","机油压力信号输入-N-IN-MCU","I","L","/","/",40,"/","/","KR6","INTP10","(RxD2)"]
[24,"P75","EVDD","故障诊断信号输入-N-IN-MCU","故障诊断信号输入-N-IN-MCU","I","L","/","/",40,"/","/","KR5","INTP9","SCLK01","SCL01"]
[25,"P74","EVDD","电池电压低信号输入-N-IN-MCU","电池电压低信号输入-N-IN-MCU","I","L","/","/",40,"/","/","KR4","INTP8","SDI01","SDA01"]
[26,"P73","EVDD","自动启停信号输入-N-IN-MCU","自动启停信号输入-N-IN-MCU","I","L","/","/",40,"/","/","KR3","SDO01"]
[27,"P72","EVDD","SD-2","段码2：SPI20（PIN27/PIN28/PIN29）","/","/","L","/",40,"/","/","KR2","SDO21"]
[28,"P71","EVDD","CSB-2",null,"/","/","L","/",40,"/","/","KR1","SDI21","SDA21","(VCOUT0)"]
[29,"P70","EVDD","SCL-2",null,"/","/","L","/",40,"/","/","KR0","SCLK21","SCL21","(VCOUT1)"]
[30,"P06","EVDD","远光信号输入_P_IN_MCU","远光信号输入_P_IN_MCU","I","H","L","/",40,"/","/","(INTP11)","(TAIO)"]
[31,"P05","EVDD","位置灯信号输入_P_IN_MCU","位置灯信号输入_P_IN_MCU","I","H","L","/",40,"/","/","(INTP10)"]
[32,"P30","EVDD","悬空",null,"/","/","L","/",40,"/","/","INTP3","RTC1HZ","SCLK00","SCL00","TAO"]
[33,"P50","EVDD","CAN_MCU_RXD","CAN总线（PIN33、PIN34）","/","/","L","/",40,"/","/","INTP1","SDI00","RXD0","SDA00","TBIO0","(TAO)","(TMIOC1)","(CRxD0)"]
[34,"P51","EVDD","CAN_MCU_TXD",null,"/","/","L","/",40,"/","/","INTP2","SDO00","TXD0","TBIO1","(TMIOD1)","(CTxD0)"]
[35,"P52","EVDD","CAN_STB_MCU","CAN总线：STB（PIN35）","O","/","H","/",40,"/","/","(INTP1)"]
[36,"P53","EVDD","左转向信号输入_P_IN_MCU","左转向信号输入_P_IN_MCU","I","H","L","/",40,"/","/","(INTP2)"]
[37,"P54","EVDD","右转向信号输入_P_IN_MCU","右转向信号输入_P_IN_MCU","I","H","L","/",40,"/","/","(INTP3)"]
[38,"P55","EVDD","L_BiasBitSW_里程千位","里程千位背光灯","O","H","L","/",40,"/","/","(INTP4)","(CLKBUZ1)","(SCLK00)"]
[39,"P17","EVDD","L_BiasBitSW_里程万位","里程万位背光灯","O","H","L","/",40,"/","/","TI02","TO02","TMIOA0","TMCLK0","(SDO00)","(TXD0)","(TMIOD0)"]
[40,"P16","EVDD","L_BiasBitSW_百位","车速万百位背光灯","O","H","L","/",40,"/","/","TI01","TO01","INTP5","TMIOC0","(SDI00)","(RXD0)","(TMIOA1)"]
[41,"P15","EVDD","L_BiasBitSW_十位","车速千百位背光灯","O","H","L","/",40,"/","/","SCLK20","SCL20","TMIOD0","(SDAA0)"]
[42,"P14","EVDD","悬空",null,"/","/","L","/",40,"/","/","RXD2","SDI20","SDA20","TMIOB0","(TMIOC1)","(SCLA0)","IrRxd"]
[43,"P13","EVDD","悬空",null,"/","/","L","/",40,"/","/","TXD2","SDO20","TMIOC1","(TMIOD1)","IrTxd"]
[44,"P12","EVDD","TXD--ESP-IN-MCU","ESP32","/","/","L","/",40,"/","/","(TxD0)","SDO11","TMIOA1","(TMIOB0)","(INTP5)"]
[45,"P11","EVDD","RXD--ESP-IN-MCU",null,"/","/","L","/",40,"/","/","(RxD0)","SDI11","SDA11","TMIOD1","(TMIOA1)","ANI8"]
[46,"P10","EVDD","表盘背光-MCU-PWM","PWM：背光PWM输出（PIN46）","O","/","L","/",40,"/","/","SCLK11","SCL11","TMIOB1","ANI9"]
[47,"P146","EVDD","A_Version","硬件版本号识别","ADC","/","L","/",40,"/","/","ANI15"]
[48,"P147","EVDD","悬空",null,"/","/","L","/",40,"/","/","ANI12","VREF0"]
[49,"P27","VDD","BiasBitSW_燃油_AD_IN_MCU","ADC：燃油基准电压采集（PIN49）","ADC","/","L","/",3,"/","/","ANI7"]
[50,"P26","VDD","悬空",null,"/","/","L","/",3,"/","/","ANI6"]
[51,"P25","VDD","燃油信号输入_AD_IN_MCU","油位信号-AD-MCU-IN","ADC","/","/","/",3,"/","/","ANI5","PGA1GND"]
[52,"P24","VDD","悬空",null,"/","/","L","/",3,"/","/","ANI4","PGA1IN"]
[53,"P23","VDD","KL15-AD-MCU-IN","ADC：IGN+采集（PIN53）","ADC","H","/","/",3,"/","/","ANI3","ANO1","PGA0GND"]
[54,"P22","VDD","KL30-AD-MCU-IN","ADC：B+采集（PIN54）","ADC","H","/","/",3,"/","/","ANI2","ANO0","PGA0IN","VCIN0"]
[55,"P21","VDD","GND",null,"/","/","/","/",3,"/","/","ANI1","AVREFM","VCIN13"]
[56,"P20","VDD","AVDD",null,"/","/","/","/",3,"/","/","ANI0","AVREFP","VCIN12","(INTP11)"]
[57,"P130","EVDD","悬空",null,"/","/","L","/",40,"/","/","—"]
[58,"P04","EVDD","SCL","段码1：SPI10（PIN58/PIN59/PIN60）","/","/","L","/",40,"/","/","ANI13","SCLK10","SCL10"]
[59,"P03","EVDD","CSB",null,"/","/","L","/",40,"/","/","ANI10","SDI10","RXD1","SDA10","VCIN11","CRxD0"]
[60,"P02","EVDD","SD",null,"/","/","L","/",40,"/","/","ANI11","SDO10","TXD1","VCIN10","CTxD0"]
[61,"P01","EVDD","KL15-AD-IN","唤醒：IGN唤醒采集（PIN61）","ADC","H","/","/",40,"/","/","TO00","TBCLK1","TAIO","(INTP10)"]
[62,"P00","EVDD","悬空",null,"/","/","L","/",40,"/","/","TI00","TBCLK0","(TAO)","(INTP8)"]
[63,"P141","EVDD","L_BiasBitSW_燃油_OUT","油位信号-电源切_MCU-OUT","O","H","L","/",40,"/","/","CLKBUZ1","INTP7"]
[64,"P140","EVDD","L_BD433Ctrl_OUT","3.3V电源使能，各功能模块3.3V切电使能（PIN64）","O","H","L","/",40,"/","/","CLKBUZ0","INTP6"]
[{"$nulls":4}," "]
[]
[null,"软件工程师注意：\n1 所有标注“/”的地方表示此项硬件对软件编程无强制要求、软件自行决定如何设计。\n2 产品上有PWM调光类应用必须按照如下要求执行。\n  ① MPQ3367   400Hz±10%\n  ② AW9967/TPS61161  20kHz±5%\n  ③ 三极管调光 370~420Hz\n  ④ LP8867C 2.6kHz±5%\n  ⑤ RT8577A 1kHz±5%\n\n硬件工程师注意：\n1 对于一个IO驱动多个负载的应用(如一个PWM信号控制多个背光IC等类似应用),如果对驱动电流有要求，要给软件明确驱动电流配置要求，无要求的默认填“/”\n2 输入、输出模式默认填“/”，如有特殊要求可按照实际需求填写。\n3 所有使用了的IO在“网络名”、“说明”、“I/O”、“有效”、“Sleep Mode IO状态”列必须填写对应信息、未使用的IO可以保持模板默认状态"]