#include "int_enabled.h"
#pragma ghs startnomisra
-- Becasue MISR does not recognise -- as comment, and complains about the #include
-- we place it on top of this file 
-------------------------------------------------------------------------------
-- Module       = Startup_V850E2M_PF3.850
-- Version      = E1.00l
--                extracted from device file V850E2M_PF3.800 by DeFiX E2.13e
-------------------------------------------------------------------------------
--                                  COPYRIGHT
-------------------------------------------------------------------------------
-- Copyright (c) 2014 by Renesas Electronics Europe GmbH,
--               a company of the Renesas Electronics Corporation
-------------------------------------------------------------------------------
-- Purpose:      Startup Code
--
-------------------------------------------------------------------------------
--
-- Warranty Disclaimer
--
-- Because the Product(s) is licensed free of charge, there is no warranty
-- of any kind whatsoever and expressly disclaimed and excluded by Renesas,
-- either expressed or implied, including but not limited to those for
-- non-infringement of intellectual property, merchantability and/or
-- fitness for the particular purpose.
-- Renesas shall not have any obligation to maintain, service or provide bug
-- fixes for the supplied Product(s) and/or the Application.
--
-- Each User is solely responsible for determining the appropriateness of
-- using the Product(s) and assumes all risks associated with its exercise
-- of rights under this Agreement, including, but not limited to the risks
-- and costs of program errors, compliance with applicable laws, damage to
-- or loss of data, programs or equipment, and unavailability or
-- interruption of operations.
--
-- Limitation of Liability
--
-- In no event shall Renesas be liable to the User for any incidental,
-- consequential, indirect, or punitive damage (including but not limited
-- to lost profits) regardless of whether such liability is based on breach
-- of contract, tort, strict liability, breach of warranties, failure of
-- essential purpose or otherwise and even if advised of the possibility of
-- such damages. Renesas shall not be liable for any services or products
-- provided by third party vendors, developers or consultants identified or
-- referred to the User by Renesas in connection with the Product(s) and/or
-- the Application.
--
-------------------------------------------------------------------------------
-- Environment:
--              Device:           
--              IDE:            GHS Multi for V800
-------------------------------------------------------------------------------

-------------------------------------------------------------------------------
-------------  Selection of external interrupt service handler
-------------  User modifiable section
-------------  Please uncomment the required interrupt service handler
-------------------------------------------------------------------------------

#define IRQ_TABLE_START                 0x00000200u


-------------------------------------------------------------------------------
-------------  Basic Initialisation of the controller
-------------  User modifiable section
-------------------------------------------------------------------------------
.weak	___lowinit
.text
_RESET:
  -- Initialisation of the global pointer
  mov    __gp, gp

  -- Initialisation of the text pointer
  mov    __tp, tp
  
  -- Initialisation of the stack pointer
  movhi	hi(___ghsend_stack-4),zero,sp
  movea	lo(___ghsend_stack-4),sp,sp
  mov -4,r1
  and r1,sp

  -- Initialization of the interrupt base pointer
  mov IRQ_TABLE_START,r1
  ldsr r1,intbp,1

-- Either disable ECC ...
-- mov 0xFFC65400, r6
-- mov 0x4001, r7 
-- st.w   r7, 0[r6]   

-- ... or Clear all SelfRAM
  mov ___ghs_ramstart, r6  -- start of lram
  mov ___ghs_ramend, r7    -- end of lram
  mov r0, r1
1:
  st.dw   r0, 0[r6]
  addi    8, r6, r6
  cmp r7, r6
  bl 1b

-- enable coprocessor (required by sdram init) 
    mov 0x00010000, r6 
-- store PSW to r7 
    stsr 5, r7  
-- set bit 16 
    or  r6, r7
-- write PSW
    ldsr r7, 5
--


#ifndef R_DBG_PRINT_DEV_REGS
-- Define to skip Low Init 
#ifndef APP_SKIP_LOW_INIT
  -- Jump to the low level (e.g. DDR initialization) routines
  jarl  _R_BSP_LowInit, lp
#endif
#endif

 
  -- Jump to the HW Initialisation function
  jarl	___lowinit, lp
  -- Jump to the Initialisation functions of the library,
  -- from there to main()
  jr __start
-------------------------------------------------------------------------------

-------------------------------------------------------------------------------
-------------  Interrupt service routine of unused interrupts
  .global  __unused_isr
__unused_isr:
  br	__unused_isr
-------------------------------------------------------------------------------

-------------------------------------------------------------------------------
-------------  Add section ".intvect" to your linker command file
-------------  at address 0x0000
-------------
-------------	i.e.	.intvect    0x0000:
-------------------------------------------------------------------------------
.section".intvect",.text

-------------------------------------------------------------------------------
-------------  Initializing of interrupt vector table
-------------  Please don't modify this section
-------------------------------------------------------------------------------

  .global _RESET
  .offset 0x0000
  #if (RESET_ENABLE > 0x00000000)
    .extern _RESET
    jr _RESET
  #else
    jr __unused_isr
  #endif

#ifdef __OS_HANDLES__      

/* OS interrupt code can be added here */

#else /* __OS_HANDLES__ */ 

  .offset 0x0010
    /* SYSERR exception */
    jr __unused_isr

  .offset 0x0020
    /* Reserved <Unknown> exception */
    jr __unused_isr

  .offset 0x0030
    /* FETRAP exception */
    jr __unused_isr

  .offset 0x0040
  #if (TRAP0_ENABLE > 0x00000000)
    .extern _TRAP0
    jr _TRAP0
  #else
    jr __unused_isr
  #endif

  .offset 0x0050
  #if (TRAP1_ENABLE > 0x00000000)
    .extern _TRAP1
    jr _TRAP1
  #else
    jr __unused_isr
  #endif

  .offset 0x0060
    /* RIE exception */
    jr __unused_isr

  .offset 0x0070
    /* FPP and FPI exception */
    jr __unused_isr

  .offset 0x0080
    /* UCPOP exception */
    jr __unused_isr

  .offset 0x0090
    /* MIP and MDP exception */
    jr __unused_isr

  .offset 0x00a0
  #if (PIE_ENABLE > 0x00000000)
    .extern _PIE
    jr _PIE
  #else
    jr __unused_isr
  #endif

  .offset 0x00b0
    /* DEBUG exception */
    jr __unused_isr

  .offset 0x00c0
    /* MAE Misalignment exception */
    jr __unused_isr

  .offset 0x00d0
    /* Reserved <Unknown> exception */
    jr __unused_isr

  .offset 0x00e0
  #if (FENMI_ENABLE > 0x00000000)
    .extern _FENMI
    syncp /* G3M workaround */
    jr _FENMI
  #else
    jr __unused_isr
  #endif

  .offset 0x00f0
  #if (FEINT_ENABLE > 0x00000000)
    .extern _FEINT
    syncp /* G3M workaround */
    jr _FEINT
  #else
    jr __unused_isr
  #endif

  .offset 0x0100
  #if (PRIO_0_ENABLE > 0x00000000)
    .extern _EINTPRIO_0
    syncp /* G3M workaround */
    jr _EINTPRIO_0
  #else
    jr __unused_isr
  #endif

  .offset 0x0110
  #if (EINTPRIO_1_ENABLE > 0x00000000)
    .extern _EINTPRIO_1
    syncp /* G3M workaround */
    jr _EINTPRIO_1
  #else
    jr __unused_isr
  #endif

  .offset 0x0120
  #if (EINTPRIO_2_ENABLE > 0x00000000)
    .extern _EINTPRIO_2
    syncp /* G3M workaround */
    jr _EINTPRIO_2
  #else
    jr __unused_isr
  #endif

  .offset 0x0130
  #if (EINTPRIO_3_ENABLE > 0x00000000)
    .extern _EINTPRIO_3
    syncp /* G3M workaround */
    jr _EINTPRIO_3
  #else
    jr __unused_isr
  #endif

  .offset 0x0140
  #if (EINTPRIO_4_ENABLE > 0x00000000)
    .extern _EINTPRIO_4
    syncp /* G3M workaround */
    jr _EINTPRIO_4
  #else
    jr __unused_isr
  #endif

  .offset 0x0150
  #if (EINTPRIO_5_ENABLE > 0x00000000)
    .extern _EINTPRIO_5
    syncp /* G3M workaround */
    jr _EINTPRIO_5
  #else
    jr __unused_isr
  #endif

  .offset 0x0160
  #if (EINTPRIO_6_ENABLE > 0x00000000)
    .extern _EINTPRIO_6
    syncp /* G3M workaround */
    jr _EINTPRIO_6
  #else
    jr __unused_isr
  #endif

  .offset 0x0170
  #if (EINTPRIO_7_ENABLE > 0x00000000)
    .extern _EINTPRIO_7
    syncp /* G3M workaround */
    jr _EINTPRIO_7
  #else
    jr __unused_isr
  #endif

  .offset 0x0180
  #if (EINTPRIO_8_ENABLE > 0x00000000)
    .extern _EINTPRIO_8
    syncp /* G3M workaround */
    jr _EINTPRIO_8
  #else
    jr __unused_isr
  #endif

  .offset 0x0190
  #if (EINTPRIO_9_ENABLE > 0x00000000)
    .extern _EINTPRIO_9
    syncp /* G3M workaround */
    jr _EINTPRIO_9
  #else
    jr __unused_isr
  #endif

  .offset 0x01a0
  #if (EINTPRIO_10_ENABLE > 0x00000000)
    .extern _EINTPRIO_10
    syncp /* G3M workaround */
    jr _EINTPRIO_10
  #else
    jr __unused_isr
  #endif

  .offset 0x01b0
  #if (EINTPRIO_11_ENABLE > 0x00000000)
    .extern _EINTPRIO_11
    syncp /* G3M workaround */
    jr _EINTPRIO_11
  #else
    jr __unused_isr
  #endif

  .offset 0x01c0
  #if (EINTPRIO_12_ENABLE > 0x00000000)
    .extern _EINTPRIO_12
    syncp /* G3M workaround */
    jr _EINTPRIO_12
  #else
    jr __unused_isr
  #endif

  .offset 0x01d0
  #if (EINTPRIO_13_ENABLE > 0x00000000)
    .extern _EINTPRIO_13
    syncp /* G3M workaround */
    jr _EINTPRIO_13
  #else
    jr __unused_isr
  #endif

  .offset 0x01e0
  #if (EINTPRIO_14_ENABLE > 0x00000000)
    .extern _EINTPRIO_14
    syncp /* G3M workaround */
    jr _EINTPRIO_14
  #else
    jr __unused_isr
  #endif

  .offset 0x01f0
  #if (EINTPRIO_15_ENABLE > 0x00000000)
    .extern _EINTPRIO_15
    syncp /* G3M workaround */
    jr _EINTPRIO_15
  #else
    jr __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0000)
  #if (INTWDTA0_ENABLE > 0x00000000)
    .extern _INTWDTA0
    .word _INTWDTA0
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0004)
  #if (INTWDTA1_ENABLE > 0x00000000)
    .extern _INTWDTA1
    .word _INTWDTA1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0008)
  #if (INTRTCA01S_ENABLE > 0x00000000)
    .extern _INTRTCA01S
    .word _INTRTCA01S
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x000c)
  #if (INTRTCA0AL_ENABLE > 0x00000000)
    .extern _INTRTCA0AL
    .word _INTRTCA0AL
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0010)
  #if (INTRTCA0R_ENABLE > 0x00000000)
    .extern _INTRTCA0R
    .word _INTRTCA0R
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0014)
  #if (INTAWOT_ENABLE > 0x00000000)
    .extern _INTAWOT
    .word _INTAWOT
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0018)
  #if (INTP0_ENABLE > 0x00000000)
    .extern _INTP0
    .word _INTP0
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x001c)
  #if (INTP1_ENABLE > 0x00000000)
    .extern _INTP1
    .word _INTP1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0020)
  #if (INTP2_ENABLE > 0x00000000)
    .extern _INTP2
    .word _INTP2
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0024)
  #if (INTP3_ENABLE > 0x00000000)
    .extern _INTP3
    .word _INTP3
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0028)
  #if (INTP4_ENABLE > 0x00000000)
    .extern _INTP4
    .word _INTP4
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x002c)
  #if (INTP5_ENABLE > 0x00000000)
    .extern _INTP5
    .word _INTP5
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0030)
  #if (INTP6_ENABLE > 0x00000000)
    .extern _INTP6
    .word _INTP6
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0034)
  #if (INTP7_ENABLE > 0x00000000)
    .extern _INTP7
    .word _INTP7
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0038)
  #if (INTP8_ENABLE > 0x00000000)
    .extern _INTP8
    .word _INTP8
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x003c)
  #if (INTP9_ENABLE > 0x00000000)
    .extern _INTP9
    .word _INTP9
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0040)
  #if (INTP10_ENABLE > 0x00000000)
    .extern _INTP10
    .word _INTP10
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0044)
  #if (INTTAUB0I0_ENABLE > 0x00000000)
    .extern _INTTAUB0I0
    .word _INTTAUB0I0
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0048)
  #if (INTTAUB0I1_ENABLE > 0x00000000)
    .extern _INTTAUB0I1
    .word _INTTAUB0I1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x004c)
  #if (INTTAUB0I2_ENABLE > 0x00000000)
    .extern _INTTAUB0I2
    .word _INTTAUB0I2
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0050)
  #if (INTTAUB0I3_ENABLE > 0x00000000)
    .extern _INTTAUB0I3
    .word _INTTAUB0I3
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0054)
  #if (INTTAUB0I4_ENABLE > 0x00000000)
    .extern _INTTAUB0I4
    .word _INTTAUB0I4
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0058)
  #if (INTTAUB0I5_ENABLE > 0x00000000)
    .extern _INTTAUB0I5
    .word _INTTAUB0I5
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x005c)
  #if (INTTAUB0I6_ENABLE > 0x00000000)
    .extern _INTTAUB0I6
    .word _INTTAUB0I6
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0060)
  #if (INTTAUB0I7_ENABLE > 0x00000000)
    .extern _INTTAUB0I7
    .word _INTTAUB0I7
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0064)
  #if (INTTAUB0I8_ENABLE > 0x00000000)
    .extern _INTTAUB0I8
    .word _INTTAUB0I8
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0068)
  #if (INTTAUB0I9_ENABLE > 0x00000000)
    .extern _INTTAUB0I9
    .word _INTTAUB0I9
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x006c)
  #if (INTTAUB0I10_ENABLE > 0x00000000)
    .extern _INTTAUB0I10
    .word _INTTAUB0I10
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0070)
  #if (INTTAUB0I11_ENABLE > 0x00000000)
    .extern _INTTAUB0I11
    .word _INTTAUB0I11
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0074)
  #if (INTTAUB0I12_ENABLE > 0x00000000)
    .extern _INTTAUB0I12
    .word _INTTAUB0I12
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0078)
  #if (INTTAUB0I13_ENABLE > 0x00000000)
    .extern _INTTAUB0I13
    .word _INTTAUB0I13
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x007c)
  #if (INTTAUB0I14_ENABLE > 0x00000000)
    .extern _INTTAUB0I14
    .word _INTTAUB0I14
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0080)
  #if (INTTAUB0I15_ENABLE > 0x00000000)
    .extern _INTTAUB0I15
    .word _INTTAUB0I15
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0084)
  #if (INTTAUB1I0_ENABLE > 0x00000000)
    .extern _INTTAUB1I0
    .word _INTTAUB1I0
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0088)
  #if (INTTAUB1I1_ENABLE > 0x00000000)
    .extern _INTTAUB1I1
    .word _INTTAUB1I1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x008c)
  #if (INTTAUB1I2_ENABLE > 0x00000000)
    .extern _INTTAUB1I2
    .word _INTTAUB1I2
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0090)
  #if (INTTAUB1I3_ENABLE > 0x00000000)
    .extern _INTTAUB1I3
    .word _INTTAUB1I3
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0094)
  #if (INTTAUB1I4_ENABLE > 0x00000000)
    .extern _INTTAUB1I4
    .word _INTTAUB1I4
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0098)
  #if (INTTAUB1I5_ENABLE > 0x00000000)
    .extern _INTTAUB1I5
    .word _INTTAUB1I5
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x009c)
  #if (INTTAUB1I6_ENABLE > 0x00000000)
    .extern _INTTAUB1I6
    .word _INTTAUB1I6
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00a0)
  #if (INTTAUB1I7_ENABLE > 0x00000000)
    .extern _INTTAUB1I7
    .word _INTTAUB1I7
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00a4)
  #if (INTTAUB1I8_ENABLE > 0x00000000)
    .extern _INTTAUB1I8
    .word _INTTAUB1I8
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00a8)
  #if (INTTAUB1I9_ENABLE > 0x00000000)
    .extern _INTTAUB1I9
    .word _INTTAUB1I9
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00ac)
  #if (INTTAUB1I10_ENABLE > 0x00000000)
    .extern _INTTAUB1I10
    .word _INTTAUB1I10
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00b0)
  #if (INTTAUB1I11_ENABLE > 0x00000000)
    .extern _INTTAUB1I11
    .word _INTTAUB1I11
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00b4)
  #if (INTTAUB1I12_ENABLE > 0x00000000)
    .extern _INTTAUB1I12
    .word _INTTAUB1I12
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00b8)
  #if (INTTAUB1I13_ENABLE > 0x00000000)
    .extern _INTTAUB1I13
    .word _INTTAUB1I13
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00bc)
  #if (INTTAUB1I14_ENABLE > 0x00000000)
    .extern _INTTAUB1I14
    .word _INTTAUB1I14
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00c0)
  #if (INTTAUB1I15_ENABLE > 0x00000000)
    .extern _INTTAUB1I15
    .word _INTTAUB1I15
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00c4)
  #if (INTTAUB2I0_ENABLE > 0x00000000)
    .extern _INTTAUB2I0
    .word _INTTAUB2I0
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00c8)
  #if (INTTAUB2I1_ENABLE > 0x00000000)
    .extern _INTTAUB2I1
    .word _INTTAUB2I1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00cc)
  #if (INTTAUB2I2_ENABLE > 0x00000000)
    .extern _INTTAUB2I2
    .word _INTTAUB2I2
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00d0)
  #if (INTTAUB2I3_ENABLE > 0x00000000)
    .extern _INTTAUB2I3
    .word _INTTAUB2I3
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00d4)
  #if (INTTAUB2I4_ENABLE > 0x00000000)
    .extern _INTTAUB2I4
    .word _INTTAUB2I4
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00d8)
  #if (INTTAUB2I5_ENABLE > 0x00000000)
    .extern _INTTAUB2I5
    .word _INTTAUB2I5
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00dc)
  #if (INTTAUB2I6_ENABLE > 0x00000000)
    .extern _INTTAUB2I6
    .word _INTTAUB2I6
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00e0)
  #if (INTTAUB2I7_ENABLE > 0x00000000)
    .extern _INTTAUB2I7
    .word _INTTAUB2I7
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00e4)
  #if (INTTAUB2I8_ENABLE > 0x00000000)
    .extern _INTTAUB2I8
    .word _INTTAUB2I8
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00e8)
  #if (INTTAUB2I9_ENABLE > 0x00000000)
    .extern _INTTAUB2I9
    .word _INTTAUB2I9
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00ec)
  #if (INTTAUB2I10_ENABLE > 0x00000000)
    .extern _INTTAUB2I10
    .word _INTTAUB2I10
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00f0)
  #if (INTTAUB2I11_ENABLE > 0x00000000)
    .extern _INTTAUB2I11
    .word _INTTAUB2I11
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00f4)
  #if (INTTAUB2I12_ENABLE > 0x00000000)
    .extern _INTTAUB2I12
    .word _INTTAUB2I12
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00f8)
  #if (INTTAUB2I13_ENABLE > 0x00000000)
    .extern _INTTAUB2I13
    .word _INTTAUB2I13
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x00fc)
  #if (INTTAUB2I14_ENABLE > 0x00000000)
    .extern _INTTAUB2I14
    .word _INTTAUB2I14
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0100)
  #if (INTTAUB2I15_ENABLE > 0x00000000)
    .extern _INTTAUB2I15
    .word _INTTAUB2I15
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0104)
  #if (INTADCE0TSN_ENABLE > 0x00000000)
    .extern _INTADCE0TSN
    .word _INTADCE0TSN
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0108)
  #if (INTADCE0I1_ENABLE > 0x00000000)
    .extern _INTADCE0I1
    .word _INTADCE0I1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x010c)
  #if (INTADCE0I2_ENABLE > 0x00000000)
    .extern _INTADCE0I2
    .word _INTADCE0I2
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0110)
  #if (INTADCE0I3_ENABLE > 0x00000000)
    .extern _INTADCE0I3
    .word _INTADCE0I3
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0114)
  #if (INTRCANGERR_ENABLE > 0x00000000)
    .extern _INTRCANGERR
    .word _INTRCANGERR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0118)
  #if (INTRCANGRECC_ENABLE > 0x00000000)
    .extern _INTRCANGRECC
    .word _INTRCANGRECC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x011c)
  #if (INTRCAN0ERR_ENABLE > 0x00000000)
    .extern _INTRCAN0ERR
    .word _INTRCAN0ERR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0120)
  #if (INTRCAN0REC_ENABLE > 0x00000000)
    .extern _INTRCAN0REC
    .word _INTRCAN0REC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0124)
  #if (INTRCAN0TRX_ENABLE > 0x00000000)
    .extern _INTRCAN0TRX
    .word _INTRCAN0TRX
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0128)
  #if (INTCSIG0IRE_ENABLE > 0x00000000)
    .extern _INTCSIG0IRE
    .word _INTCSIG0IRE
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x012c)
  #if (INTCSIG0IR_ENABLE > 0x00000000)
    .extern _INTCSIG0IR
    .word _INTCSIG0IR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0130)
  #if (INTCSIG0IC_ENABLE > 0x00000000)
    .extern _INTCSIG0IC
    .word _INTCSIG0IC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0134)
  #if (INTCSIH0IRE_ENABLE > 0x00000000)
    .extern _INTCSIH0IRE
    .word _INTCSIH0IRE
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0138)
  #if (INTCSIH0IR_ENABLE > 0x00000000)
    .extern _INTCSIH0IR
    .word _INTCSIH0IR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x013c)
  #if (INTCSIH0IC_ENABLE > 0x00000000)
    .extern _INTCSIH0IC
    .word _INTCSIH0IC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0140)
  #if (INTCSIH0IJC_ENABLE > 0x00000000)
    .extern _INTCSIH0IJC
    .word _INTCSIH0IJC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0144)
  #if (INTRLIN30UR2_ENABLE > 0x00000000)
    .extern _INTRLIN30UR2
    .word _INTRLIN30UR2
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0148)
  #if (INTRLIN30UR1_ENABLE > 0x00000000)
    .extern _INTRLIN30UR1
    .word _INTRLIN30UR1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x014c)
  #if (INTRLIN30UR0_ENABLE > 0x00000000)
    .extern _INTRLIN30UR0
    .word _INTRLIN30UR0
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0150)
  #if (INTRLIN31UR2_ENABLE > 0x00000000)
    .extern _INTRLIN31UR2
    .word _INTRLIN31UR2
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0154)
  #if (INTRLIN31UR1_ENABLE > 0x00000000)
    .extern _INTRLIN31UR1
    .word _INTRLIN31UR1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0158)
  #if (INTRLIN31UR0_ENABLE > 0x00000000)
    .extern _INTRLIN31UR0
    .word _INTRLIN31UR0
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x015c)
  #if (INTSG0TI_ENABLE > 0x00000000)
    .extern _INTSG0TI
    .word _INTSG0TI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0160)
  #if (INTSG1TI_ENABLE > 0x00000000)
    .extern _INTSG1TI
    .word _INTSG1TI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0164)
  #if (INTSG2TI_ENABLE > 0x00000000)
    .extern _INTSG2TI
    .word _INTSG2TI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0168)
  #if (INTSG3TI_ENABLE > 0x00000000)
    .extern _INTSG3TI
    .word _INTSG3TI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x016c)
  #if (INTSG4TI_ENABLE > 0x00000000)
    .extern _INTSG4TI
    .word _INTSG4TI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0170)
  #if (INTDCUTDI_ENABLE > 0x00000000)
    .extern _INTDCUTDI
    .word _INTDCUTDI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0174)
  #if (INTDMAERR_ENABLE > 0x00000000)
    .extern _INTDMAERR
    .word _INTDMAERR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0178)
  #if (INTDMA0_ENABLE > 0x00000000)
    .extern _INTDMA0
    .word _INTDMA0
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x017c)
  #if (INTDMA1_ENABLE > 0x00000000)
    .extern _INTDMA1
    .word _INTDMA1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0180)
  #if (INTDMA2_ENABLE > 0x00000000)
    .extern _INTDMA2
    .word _INTDMA2
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0184)
  #if (INTDMA3_ENABLE > 0x00000000)
    .extern _INTDMA3
    .word _INTDMA3
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0188)
  #if (INTDMA4_ENABLE > 0x00000000)
    .extern _INTDMA4
    .word _INTDMA4
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x018c)
  #if (INTDMA5_ENABLE > 0x00000000)
    .extern _INTDMA5
    .word _INTDMA5
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0190)
  #if (INTDMA6_ENABLE > 0x00000000)
    .extern _INTDMA6
    .word _INTDMA6
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0194)
  #if (INTDMA7_ENABLE > 0x00000000)
    .extern _INTDMA7
    .word _INTDMA7
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0198)
  #if (INTDMA8_ENABLE > 0x00000000)
    .extern _INTDMA8
    .word _INTDMA8
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x019c)
  #if (INTDMA9_ENABLE > 0x00000000)
    .extern _INTDMA9
    .word _INTDMA9
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01a0)
  #if (INTDMA10_ENABLE > 0x00000000)
    .extern _INTDMA10
    .word _INTDMA10
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01a4)
  #if (INTDMA11_ENABLE > 0x00000000)
    .extern _INTDMA11
    .word _INTDMA11
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01a8)
  #if (INTDMA12_ENABLE > 0x00000000)
    .extern _INTDMA12
    .word _INTDMA12
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01ac)
  #if (INTDMA13_ENABLE > 0x00000000)
    .extern _INTDMA13
    .word _INTDMA13
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01b0)
  #if (INTDMA14_ENABLE > 0x00000000)
    .extern _INTDMA14
    .word _INTDMA14
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01b4)
  #if (INTDMA15_ENABLE > 0x00000000)
    .extern _INTDMA15
    .word _INTDMA15
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01b8)
  #if (INTRIIC0LEE_ENABLE > 0x00000000)
    .extern _INTRIIC0LEE
    .word _INTRIIC0LEE
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01bc)
  #if (INTRIIC0RI_ENABLE > 0x00000000)
    .extern _INTRIIC0RI
    .word _INTRIIC0RI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01c0)
  #if (INTRIIC0TI_ENABLE > 0x00000000)
    .extern _INTRIIC0TI
    .word _INTRIIC0TI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01c4)
  #if (INTRIIC0TEI_ENABLE > 0x00000000)
    .extern _INTRIIC0TEI
    .word _INTRIIC0TEI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01c8)
  #if (INTRIIC1LEE_ENABLE > 0x00000000)
    .extern _INTRIIC1LEE
    .word _INTRIIC1LEE
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01cc)
  #if (INTRIIC1RI_ENABLE > 0x00000000)
    .extern _INTRIIC1RI
    .word _INTRIIC1RI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01d0)
  #if (INTRIIC1TI_ENABLE > 0x00000000)
    .extern _INTRIIC1TI
    .word _INTRIIC1TI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01d4)
  #if (INTRIIC1TEI_ENABLE > 0x00000000)
    .extern _INTRIIC1TEI
    .word _INTRIIC1TEI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01d8)
  #if (INTRCAN1ERR_ENABLE > 0x00000000)
    .extern _INTRCAN1ERR
    .word _INTRCAN1ERR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01dc)
  #if (INTRCAN1REC_ENABLE > 0x00000000)
    .extern _INTRCAN1REC
    .word _INTRCAN1REC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01e0)
  #if (INTRCAN1TRX_ENABLE > 0x00000000)
    .extern _INTRCAN1TRX
    .word _INTRCAN1TRX
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01e4)
  #if (INTTAUJ0I0_ENABLE > 0x00000000)
    .extern _INTTAUJ0I0
    .word _INTTAUJ0I0
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01e8)
  #if (INTTAUJ0I1_ENABLE > 0x00000000)
    .extern _INTTAUJ0I1
    .word _INTTAUJ0I1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01ec)
  #if (INTTAUJ0I2_ENABLE > 0x00000000)
    .extern _INTTAUJ0I2
    .word _INTTAUJ0I2
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01f0)
  #if (INTTAUJ0I3_ENABLE > 0x00000000)
    .extern _INTTAUJ0I3
    .word _INTTAUJ0I3
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01f4)
  #if (INTOSTM0_ENABLE > 0x00000000)
    .extern _INTOSTM0
    .word _INTOSTM0
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01f8)
  #if (INTOSTM1_ENABLE > 0x00000000)
    .extern _INTOSTM1
    .word _INTOSTM1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x01fc)
  #if (INTCSIGT1IRE_ENABLE > 0x00000000)
    .extern _INTCSIGT1IRE
    .word _INTCSIGT1IRE
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0200)
  #if (INTCSIG1IR_ENABLE > 0x00000000)
    .extern _INTCSIG1IR
    .word _INTCSIG1IR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0204)
  #if (INTCSIG1IC_ENABLE > 0x00000000)
    .extern _INTCSIG1IC
    .word _INTCSIG1IC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0208)
  #if (INTCSIGT2IRE_ENABLE > 0x00000000)
    .extern _INTCSIGT2IRE
    .word _INTCSIGT2IRE
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x020c)
  #if (INTCSIG2IR_ENABLE > 0x00000000)
    .extern _INTCSIG2IR
    .word _INTCSIG2IR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0210)
  #if (INTCSIG2IC_ENABLE > 0x00000000)
    .extern _INTCSIG2IC
    .word _INTCSIG2IC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0214)
  #if (INTCSIGT3IRE_ENABLE > 0x00000000)
    .extern _INTCSIGT3IRE
    .word _INTCSIGT3IRE
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0218)
  #if (INTCSIG3IR_ENABLE > 0x00000000)
    .extern _INTCSIG3IR
    .word _INTCSIG3IR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x021c)
  #if (INTCSIG3IC_ENABLE > 0x00000000)
    .extern _INTCSIG3IC
    .word _INTCSIG3IC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0220)
  #if (INTCSIH1IRE_ENABLE > 0x00000000)
    .extern _INTCSIH1IRE
    .word _INTCSIH1IRE
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0224)
  #if (INTCSIH1IR_ENABLE > 0x00000000)
    .extern _INTCSIH1IR
    .word _INTCSIH1IR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0228)
  #if (INTCSIH1IC_ENABLE > 0x00000000)
    .extern _INTCSIH1IC
    .word _INTCSIH1IC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x022c)
  #if (INTCSIH1IJC_ENABLE > 0x00000000)
    .extern _INTCSIH1IJC
    .word _INTCSIH1IJC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0230)
  #if (INTQFULL_ENABLE > 0x00000000)
    .extern _INTQFULL
    .word _INTQFULL
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0234)
  #if (INTPWGA0_ENABLE > 0x00000000)
    .extern _INTPWGA0
    .word _INTPWGA0
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0238)
  #if (INTPWGA1_ENABLE > 0x00000000)
    .extern _INTPWGA1
    .word _INTPWGA1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x023c)
  #if (INTPWGA2_ENABLE > 0x00000000)
    .extern _INTPWGA2
    .word _INTPWGA2
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0240)
  #if (INTPWGA3_ENABLE > 0x00000000)
    .extern _INTPWGA3
    .word _INTPWGA3
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0244)
  #if (INTPWGA4_ENABLE > 0x00000000)
    .extern _INTPWGA4
    .word _INTPWGA4
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0248)
  #if (INTPWGA5_ENABLE > 0x00000000)
    .extern _INTPWGA5
    .word _INTPWGA5
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x024c)
  #if (INTPWGA6_ENABLE > 0x00000000)
    .extern _INTPWGA6
    .word _INTPWGA6
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0250)
  #if (INTPWGA7_ENABLE > 0x00000000)
    .extern _INTPWGA7
    .word _INTPWGA7
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0254)
  #if (INTPWGA8_ENABLE > 0x00000000)
    .extern _INTPWGA8
    .word _INTPWGA8
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0258)
  #if (INTPWGA9_ENABLE > 0x00000000)
    .extern _INTPWGA9
    .word _INTPWGA9
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x025c)
  #if (INTPWGA10_ENABLE > 0x00000000)
    .extern _INTPWGA10
    .word _INTPWGA10
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0260)
  #if (INTPWGA11_ENABLE > 0x00000000)
    .extern _INTPWGA11
    .word _INTPWGA11
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0264)
  #if (INTPWGA12_ENABLE > 0x00000000)
    .extern _INTPWGA12
    .word _INTPWGA12
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0268)
  #if (INTPWGA13_ENABLE > 0x00000000)
    .extern _INTPWGA13
    .word _INTPWGA13
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x026c)
  #if (INTPWGA14_ENABLE > 0x00000000)
    .extern _INTPWGA14
    .word _INTPWGA14
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0270)
  #if (INTPWGA15_ENABLE > 0x00000000)
    .extern _INTPWGA15
    .word _INTPWGA15
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0274)
  #if (INTPWGA16_ENABLE > 0x00000000)
    .extern _INTPWGA16
    .word _INTPWGA16
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0278)
  #if (INTPWGA17_ENABLE > 0x00000000)
    .extern _INTPWGA17
    .word _INTPWGA17
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x027c)
  #if (INTPWGA18_ENABLE > 0x00000000)
    .extern _INTPWGA18
    .word _INTPWGA18
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0280)
  #if (INTPWGA19_ENABLE > 0x00000000)
    .extern _INTPWGA19
    .word _INTPWGA19
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0284)
  #if (INTPWGA20_ENABLE > 0x00000000)
    .extern _INTPWGA20
    .word _INTPWGA20
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0288)
  #if (INTPWGA21_ENABLE > 0x00000000)
    .extern _INTPWGA21
    .word _INTPWGA21
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x028c)
  #if (INTPWGA22_ENABLE > 0x00000000)
    .extern _INTPWGA22
    .word _INTPWGA22
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0290)
  #if (INTPWGA23_ENABLE > 0x00000000)
    .extern _INTPWGA23
    .word _INTPWGA23
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0294)
  #if (INTICUSTWRDY_ENABLE > 0x00000000)
    .extern _INTICUSTWRDY
    .word _INTICUSTWRDY
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0298)
  #if (INTICUSTRRDY_ENABLE > 0x00000000)
    .extern _INTICUSTRRDY
    .word _INTICUSTRRDY
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02a0)
  #if (INTSCI30RXI_ENABLE > 0x00000000)
    .extern _INTSCI30RXI
    .word _INTSCI30RXI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02a4)
  #if (INTSCI30TXI_ENABLE > 0x00000000)
    .extern _INTSCI30TXI
    .word _INTSCI30TXI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02a8)
  #if (INTSCI30TEI_ENABLE > 0x00000000)
    .extern _INTSCI30TEI
    .word _INTSCI30TEI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02ac)
  #if (INTFLERR_ENABLE > 0x00000000)
    .extern _INTFLERR
    .word _INTFLERR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02b0)
  #if (INTFLENDNM_ENABLE > 0x00000000)
    .extern _INTFLENDNM
    .word _INTFLENDNM
  #else
    .word __unused_isr
  #endif


  .offset (IRQ_TABLE_START+0x02b4)
  #if (INTNFMA0_ENABLE > 0x00000000)
    .extern _INTNFMA0
    .word _INTNFMA0
  #else
    .word __unused_isr
  #endif


  .offset (IRQ_TABLE_START+0x02b8)
  #if (INTLCBI0RDY_ENABLE > 0x00000000)
    .extern _INTLCBI0RDY
    .word _INTLCBI0RDY
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02bc)
  #if (INTLCBI0EMPTY_ENABLE > 0x00000000)
    .extern _INTLCBI0EMPTY
    .word _INTLCBI0EMPTY
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02c0)
  #if (INTLCBI0HALF_ENABLE > 0x00000000)
    .extern _INTLCBI0HALF
    .word _INTLCBI0HALF
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02c4)
  #if (INTLCBI0FULL_ENABLE > 0x00000000)
    .extern _INTLCBI0FULL
    .word _INTLCBI0FULL
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02c8)
  #if (INTLCBI0QTR_ENABLE > 0x00000000)
    .extern _INTLCBI0QTR
    .word _INTLCBI0QTR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02cc)
  #if (INTLCBI03QTR_ENABLE > 0x00000000)
    .extern _INTLCBI03QTR
    .word _INTLCBI03QTR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02d0)
  #if (INTRCAN2ERR_ENABLE > 0x00000000)
    .extern _INTRCAN2ERR
    .word _INTRCAN2ERR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02d4)
  #if (INTRCAN2REC_ENABLE > 0x00000000)
    .extern _INTRCAN2REC
    .word _INTRCAN2REC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02d8)
  #if (INTRCAN2TRX_ENABLE > 0x00000000)
    .extern _INTRCAN2TRX
    .word _INTRCAN2TRX
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02dc)
  #if (INTPCMP0FFIL_ENABLE > 0x00000000)
    .extern _INTPCMP0FFIL
    .word _INTPCMP0FFIL
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02e0)
  #if (INTPCMP0FERR_ENABLE > 0x00000000)
    .extern _INTPCMP0FERR
    .word _INTPCMP0FERR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02e4)
  #if (INTISM0REACHED_ENABLE > 0x00000000)
    .extern _INTISM0REACHED
    .word _INTISM0REACHED
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02e8)
  #if (INTISM0DONE_ENABLE > 0x00000000)
    .extern _INTISM0DONE
    .word _INTISM0DONE
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02ec)
  #if (INTISM0ZPDAD_ENABLE > 0x00000000)
    .extern _INTISM0ZPDAD
    .word _INTISM0ZPDAD
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02f4)
  #if (INTSSIF0_ENABLE > 0x00000000)
    .extern _INTSSIF0
    .word _INTSSIF0
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02f8)
  #if (INTSSIF0RX_ENABLE > 0x00000000)
    .extern _INTSSIF0RX
    .word _INTSSIF0RX
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x02fc)
  #if (INTSSIF0TX_ENABLE > 0x00000000)
    .extern _INTSSIF0TX
    .word _INTSSIF0TX
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0300)
  #if (INTSSIF1_ENABLE > 0x00000000)
    .extern _INTSSIF1
    .word _INTSSIF1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0304)
  #if (INTSSIF1RX_ENABLE > 0x00000000)
    .extern _INTSSIF1RX
    .word _INTSSIF1RX
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0308)
  #if (INTSSIF1TX_ENABLE > 0x00000000)
    .extern _INTSSIF1TX
    .word _INTSSIF1TX
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x030c)
  #if (INTSDRB0_ENABLE > 0x00000000)
    .extern _INTSDRB0
    .word _INTSDRB0
  #else
    .word __unused_isr
  #endif
  .offset (IRQ_TABLE_START+0x0310)
  #if (INTGPU2D0PAUSE_ENABLE > 0x00000000)
    .extern _INTGPU2D0PAUSE
    .word _INTGPU2D0PAUSE
  #else
    #if (INTDHD_ENABLE > 0x00000000)
       .extern _INTDHD_PAUSE
       .word _INTDHD_PAUSE
    #else
        .word __unused_isr
    #endif
  #endif

  .offset (IRQ_TABLE_START+0x0314)
  #if (INTGPU2D0SYNC_ENABLE > 0x00000000)
    .extern _INTGPU2D0SYNC
    .word _INTGPU2D0SYNC
  #else
    #if (INTDHD_ENABLE > 0x00000000)
       .extern _INTDHD_SYNC
       .word _INTDHD_SYNC
    #else
        .word __unused_isr
    #endif
  #endif

  .offset (IRQ_TABLE_START+0x0318)
  #if (INTGPU2D0SP_ENABLE > 0x00000000)
    .extern _INTGPU2D0SP
    .word _INTGPU2D0SP
  #else
    #if (INTDHD_ENABLE > 0x00000000)
       .extern _INTDHD_SPECIAL
       .word _INTDHD_SPECIAL
    #else
        .word __unused_isr
    #endif
  #endif

  .offset (IRQ_TABLE_START+0x031c)
  #if (INTVDCE0ERR_ENABLE > 0x00000000)
    .extern _INTVDCE0ERR
    .word _INTVDCE0ERR
  #else
    #if (INTVDCE_ENABLE > 0x00000000)
        .extern _INTVDCE_CH0_ERR
        .word _INTVDCE_CH0_ERR
    #elif (INTVDCO_ENABLE > 0x00000000)
        .extern _INTVDCO_CH0_INT0
        .word _INTVDCO_CH0_INT0
    #else
        .word __unused_isr
    #endif
  #endif

  .offset (IRQ_TABLE_START+0x0320)
  #if (INTVDCE0GR3VBLANK_ENABLE > 0x00000000)
    .extern _INTVDCE0GR3VBLANK
    .word _INTVDCE0GR3VBLANK
  #else
    #if (INTVDCE_ENABLE > 0x00000000)
        .extern _INTVDCE_CH0_GR3VBLANK
        .word _INTVDCE_CH0_GR3VBLANK
    #elif (INTVDCO_ENABLE > 0x00000000)
        .extern _INTVDCO_CH0_INT1
        .word _INTVDCO_CH0_INT1
    #else
        .word __unused_isr
    #endif
  #endif

  .offset (IRQ_TABLE_START+0x0324)
  #if (INTVDCE0S0VIVSYNC_ENABLE > 0x00000000)
    .extern _INTVDCE0S0VIVSYNC
    .word _INTVDCE0S0VIVSYNC
  #else
    #if (INTVDCE_ENABLE > 0x00000000)
        .extern _INTVDCE_CH0_S0VIVSYNC
        .word _INTVDCE_CH0_S0VIVSYNC
    #elif (INTVDCO_ENABLE > 0x00000000)
        .extern _INTVDCO_CH0_INT2
        .word _INTVDCO_CH0_INT2
    #else
        .word __unused_isr
    #endif
  #endif

  .offset (IRQ_TABLE_START+0x0328)
  #if (INTVDCE0S0LOVSYNC_ENABLE > 0x00000000)
    .extern _INTVDCE0S0LOVSYNC
    .word _INTVDCE0S0LOVSYNC
  #elif (INTVDCE_ENABLE > 0x00000000)
    .extern _INTVDCE_CH0_S0LOVSYNC
    .word _INTVDCE_CH0_S0LOVSYNC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x032c)
  #if (INTVDCE0GR3VLINE_ENABLE > 0x00000000)
    .extern _INTVDCE0GR3VLINE
    .word _INTVDCE0GR3VLINE
  #elif (INTVDCE_ENABLE > 0x00000000)
    .extern _INTVDCE_CH0_GR3VLINE
    .word _INTVDCE_CH0_GR3VLINE
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0330)
  #if (INTVDCE0S0VFIELD_ENABLE > 0x00000000)
    .extern _INTVDCE0S0VFIELD
    .word _INTVDCE0S0VFIELD
  #elif (INTVDCE_ENABLE > 0x00000000)
    .extern _INTVDCE_CH0_S0VFIELD
    .word _INTVDCE_CH0_S0VFIELD
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0334)
    jr __unused_isr

  .offset (IRQ_TABLE_START+0x0338)
  #if (INTVDCE0S1LOVSYNC_ENABLE > 0x00000000)
    .extern _INTVDCE0S1LOVSYNC
    .word _INTVDCE0S1LOVSYNC
  #elif (INTVDCE_ENABLE > 0x00000000)
    .extern _INTVDCE_CH0_S1LOVSYNC
    .word _INTVDCE_CH0_S1LOVSYNC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x033C)
    jr __unused_isr

  .offset (IRQ_TABLE_START+0x0340)
  #if (INTVDCE0OIRVIVSYNC_ENABLE > 0x00000000)
    .extern _INTVDCE0OIRVIVSYNC
    .word _INTVDCE0OIRVIVSYNC
  #elif (INTVDCE_ENABLE > 0x00000000)
    .extern _INTVDCE_CH0_OIRVIVSYNC
    .word _INTVDCE_CH0_OIRVIVSYNC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0344)
  #if (INTVDCE0OIRLOVSYNC_ENABLE > 0x00000000)
    .extern _INTVDCE0OIRLOVSYNC
    .word _INTVDCE0OIRLOVSYNC
  #elif (INTVDCE_ENABLE > 0x00000000)
    .extern _INTVDCE_CH0_OIRLOVSYNC
    .word _INTVDCE_CH0_OIRLOVSYNC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0348)
  #if (INTVDCE0OIRVLINE_ENABLE > 0x00000000)
    .extern _INTVDCE0OIRVLINE
    .word _INTVDCE0OIRVLINE
  #elif (INTVDCE_ENABLE > 0x00000000)
    .extern _INTVDCE_CH0_OIRVLINE
    .word _INTVDCE_CH0_OIRVLINE
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x033C)
    jr __unused_isr

  .offset (IRQ_TABLE_START+0x0350)
    jr __unused_isr

  .offset (IRQ_TABLE_START+0x0354)
    jr __unused_isr

  .offset (IRQ_TABLE_START+0x0358)
    jr __unused_isr

  .offset (IRQ_TABLE_START+0x035c)
  #if (INTRLIN32UR2_ENABLE > 0x00000000)
    .extern _INTRLIN32UR2
    .word _INTRLIN32UR2
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0360)
  #if (INTRLIN32UR1_ENABLE > 0x00000000)
    .extern _INTRLIN32UR1
    .word _INTRLIN32UR1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0364)
  #if (INTRLIN32UR0_ENABLE > 0x00000000)
    .extern _INTRLIN32UR0
    .word _INTRLIN32UR0
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0368)
  #if (INTRLIN33UR2_ENABLE > 0x00000000)
    .extern _INTRLIN33UR2
    .word _INTRLIN33UR2
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x036c)
  #if (INTRLIN33UR1_ENABLE > 0x00000000)
    .extern _INTRLIN33UR1
    .word _INTRLIN33UR1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0370)
  #if (INTRLIN33UR0_ENABLE > 0x00000000)
    .extern _INTRLIN33UR0
    .word _INTRLIN33UR0
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0374)
  #if (INTVDCE1ERR_ENABLE > 0x00000000)
    .extern _INTVDCE1ERR
    .word _INTVDCE1ERR
  #else
    #if (INTVDCE_ENABLE > 0x00000000)
        .extern _INTVDCE_CH1_ERR
        .word _INTVDCE_CH1_ERR
    #elif (INTVDCO_ENABLE > 0x00000000)
        .extern _INTVDCO_CH1_INT0
        .word _INTVDCO_CH1_INT0
    #else
        .word __unused_isr
    #endif
  #endif

  .offset (IRQ_TABLE_START+0x0378)
  #if (INTVDCE1GR3VBLANK_ENABLE > 0x00000000)
    .extern _INTVDCE1GR3VBLANK
    .word _INTVDCE1GR3VBLANK
  #else
    #if (INTVDCE_ENABLE > 0x00000000)
        .extern _INTVDCE_CH1_GR3VBLANK
        .word _INTVDCE_CH1_GR3VBLANK
    #elif (INTVDCO_ENABLE > 0x00000000)
        .extern _INTVDCO_CH1_INT1
        .word _INTVDCO_CH1_INT1
    #else
        .word __unused_isr
    #endif
  #endif

  .offset (IRQ_TABLE_START+0x037c)
  #if (INTVDCE1S0VIVSYNC_ENABLE > 0x00000000)
    .extern _INTVDCE1S0VIVSYNC
    .word _INTVDCE1S0VIVSYNC
  #else
    #if (INTVDCE_ENABLE > 0x00000000)
        .extern _INTVDCE_CH1_S0VIVSYNC
        .word _INTVDCE_CH1_S0VIVSYNC
    #elif (INTVDCO_ENABLE > 0x00000000)
        .extern _INTVDCO_CH1_INT2
        .word _INTVDCO_CH1_INT2
    #else
        .word __unused_isr
    #endif
  #endif

  .offset (IRQ_TABLE_START+0x0380)
  #if (INTVDCE1S0LOVSYNC_ENABLE > 0x00000000)
    .extern _INTVDCE1S0LOVSYNC
    .word _INTVDCE1S0LOVSYNC
  #elif (INTVDCE_ENABLE > 0x00000000)
    .extern _INTVDCE_CH1_S0LOVSYNC
    .word _INTVDCE_CH1_S0LOVSYNC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0384)
  #if (INTVDCE1GR3VLINE_ENABLE > 0x00000000)
    .extern _INTVDCE1GR3VLINE
    .word _INTVDCE1GR3VLINE
  #elif (INTVDCE_ENABLE > 0x00000000)
    .extern _INTVDCE_CH1_GR3VLINE
    .word _INTVDCE_CH1_GR3VLINE
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0388)
  #if (INTVDCE1S0VFIELD_ENABLE > 0x00000000)
    .extern _INTVDCE1S0VFIELD
    .word _INTVDCE1S0VFIELD
  #elif (INTVDCE_ENABLE > 0x00000000)
    .extern _INTVDCE_CH1_S0VFIELD
    .word _INTVDCE_CH1_S0VFIELD
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x038C)
    jr __unused_isr

  .offset (IRQ_TABLE_START+0x0390)
  #if (INTVDCE1S1LOVSYNC_ENABLE > 0x00000000)
    .extern _INTVDCE1S1LOVSYNC
    .word _INTVDCE1S1LOVSYNC
  #elif (INTVDCE_ENABLE > 0x00000000)
    .extern _INTVDCE_CH1_S1LOVSYNC
    .word _INTVDCE_CH1_S1LOVSYNC
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x0394)
    jr __unused_isr

  .offset (IRQ_TABLE_START+0x0398)
    jr __unused_isr

  .offset (IRQ_TABLE_START+0x039C)
    jr __unused_isr

  .offset (IRQ_TABLE_START+0x03A0)
    jr __unused_isr

  .offset (IRQ_TABLE_START+0x03A4)
    jr __unused_isr

  .offset (IRQ_TABLE_START+0x03a8)
  #if (INTMLBB0STA0_ENABLE > 0x00000000)
    .extern _INTMLBB0STA0
    .word _INTMLBB0STA0
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03ac)
  #if (INTMLBB0STA1_ENABLE > 0x00000000)
    .extern _INTMLBB0STA1
    .word _INTMLBB0STA1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03b0)
  #if (INTMLBB0SYS_ENABLE > 0x00000000)
    .extern _INTMLBB0SYS
    .word _INTMLBB0SYS
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03b4)
  #if (INTMLBB0HBI_ENABLE > 0x00000000)
    .extern _INTMLBB0HBI
    .word _INTMLBB0HBI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03b8)
  #if (INTMIPI0OVF_ENABLE > 0x00000000)
    .extern _INTMIPI0OVF
    .word _INTMIPI0OVF
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03bc)
  #if (INTMIPI0CTL_ENABLE > 0x00000000)
    .extern _INTMIPI0CTL
    .word _INTMIPI0CTL
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03c0)
  #if (INTVOWE0_ENABLE > 0x00000000)
    .extern _INTVOWE0
    .word _INTVOWE0
  #elif (INTVOWE_ENABLE > 0x00000000)
    .extern _INTVOWE
    .word _INTVOWE
  #else
       .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03c4)
    jr __unused_isr

  .offset (IRQ_TABLE_START+0x03c8)
  #if (INTJCU0EDI_ENABLE > 0x00000000)
    .extern _INTJCU0EDI
    .word _INTJCU0EDI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03cc)
  #if (INTJCU0DTI_ENABLE > 0x00000000)
    .extern _INTJCU0DTI
    .word _INTJCU0DTI
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03d0)
  #if (INTETNB0LINE0_ENABLE > 0x00000000)
    .extern _INTETNB0LINE0
    .word _INTETNB0LINE0
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03d4)
  #if (INTETNB0LINE1_ENABLE > 0x00000000)
    .extern _INTETNB0LINE1
    .word _INTETNB0LINE1
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03d8)
  #if (INTETNB0LINE2_ENABLE > 0x00000000)
    .extern _INTETNB0LINE2
    .word _INTETNB0LINE2
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03dc)
  #if (INTETNB0LINE3_ENABLE > 0x00000000)
    .extern _INTETNB0LINE3
    .word _INTETNB0LINE3
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03e0)
  #if (INTMISRERR_ENABLE > 0x00000000)
    .extern _INTMISRERR
    .word _INTMISRERR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03e4)
  #if (INTVPISG1OVFERR_ENABLE > 0x00000000)
    .extern _INTVPISG1OVFERR
    .word _INTVPISG1OVFERR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03e8)
  #if (INTVPISG2OVFERR_ENABLE > 0x00000000)
    .extern _INTVPISG2OVFERR
    .word _INTVPISG2OVFERR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03ec)
  #if (INTVPISG3OVFERR_ENABLE > 0x00000000)
    .extern _INTVPISG3OVFERR
    .word _INTVPISG3OVFERR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03f0)
    jr __unused_isr

  .offset (IRQ_TABLE_START+0x03f4)
  #if (INTVPISG5OVFERR_ENABLE > 0x00000000)
    .extern _INTVPISG5OVFERR
    .word _INTVPISG5OVFERR
  #else
    .word __unused_isr
  #endif

  .offset (IRQ_TABLE_START+0x03f8)
    jr __unused_isr

  .offset (IRQ_TABLE_START+0x03fc)
  #if (INTBUSERR_ENABLE > 0x00000000)
    .extern _INTBUSERR
    .word _INTBUSERR
  #else
    .word __unused_isr
  #endif


#endif   /* __OS_HANDLES__ */  

#pragma ghs endnomisra

