{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["软件自测用例"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"软件自测用例","index":0,"n_rows":6,"n_cols":8,"rows_kept":6,"cut":false,"hidden":false,"merged":[[63,7,80,7],[82,7,100,7],[102,7,108,7],[110,7,116,7],[7,7,14,7],[18,7,25,7],[29,7,36,7],[38,7,40,7],[1,1,1,7],[2,1,2,3],[2,6,2,7],[3,1,3,3],[3,6,3,7]]}
[]
[null,"仪表功能测试报告"]
[null,"供应商名称：黑龙江天有为电子有限责任公司",null,null,"ECU硬件版本：HV1.0","ECU软件版本：SV1.0"]
[null,"测试时间：2024.3.7",null,null,"测试地点：黑龙江天有为",null,"测试执行人：时昊"]
[null,"编号","测试用例名称","类型","步骤描述",null,"测试结果","数据log区"]
[null,1,"LDWS外发功能","外发模块","1.上30电和15电,默认配置有ldws功能\n2.在ldws菜单界面,显示ldws打开状态,观察0x18A97121报文外发信号LaneDepWarnEnaCmd为1;\n3.按右键,显示ldws关闭状态,观察0x18A97121报文外发信号LaneDepWarnEnaCmd为0;\n4.配置取消ldws功能,诊断读取22f010,  00 00 00 00 00 00 00 00无LDWS功能,观察0x18A97121报文外发信号LaneDepWarnEnaCmd为0;\n5.ldws显示关闭状态,重上15电后,观察0x18A97121报文外发信号LaneDepWarnEnaCmd为0;\n6.重上30电,ldws显示开启状态,观察0x18A97121报文外发信号LaneDepWarnEnaCmd为1;",null,"通过"]