{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["软件自测用例"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"软件自测用例","index":0,"n_rows":6,"n_cols":8,"rows_kept":6,"cut":false,"hidden":false,"merged":[[1,1,1,7],[2,1,2,3],[2,6,2,7],[3,1,3,3],[3,6,3,7],[76,7,93,7],[95,7,113,7],[115,7,121,7],[123,7,129,7],[5,7,6,7],[20,7,27,7],[31,7,38,7],[42,7,49,7],[51,7,53,7]]}
[]
[null,"仪表功能测试报告"]
[null,"供应商名称：黑龙江天有为电子有限责任公司",null,null,"ECU硬件版本：001.001","ECU软件版本：001.003"]
[null,"测试时间：2024.7.10",null,null,"测试地点：黑龙江天有为",null,"测试执行人：时昊"]
[null,"编号","测试用例名称","类型","步骤描述",null,"测试结果","数据log区"]
[null,1,"诊断读取软硬件版本号","软硬件版本号","1.上30电,15电,连接诊断工具\n2.诊断工具发送22f189,回复软件版本号30 30 31 2E 30 30 33 20 20 20\n3.诊断工具发送22f191,回复硬件版本号30 30 31 2E 30 30 31 20 20 20\n4.诊断工具发送22f195,回复53 56 30 30 31 2E 30 30 33 20 20 20 20 20 20 20 \n5.诊断工具发送22f193,回复48 56 30 30 31 2E 30 30 31 20 20 20 20 20 20 20 ",null,"通过"]