/*===========================================================================*/
/* Module       = App_Common_Sample.ld                                       */
/* SW-VERSION   = 1.4.0                                                      */
/*===========================================================================*/
/*                                  COPYRIGHT                                */
/*===========================================================================*/
/* (c) 2018-2021 Renesas Electronics Corporation. All rights reserved.       */
/*===========================================================================*/
/* Purpose:     Template of common linker directive file                     */
/*                                                                           */
/*===========================================================================*/
/*                                                                           */
/* Warranty Disclaimer                                                       */
/*                                                                           */
/* Because the Product(s) is licensed free of charge, there is no warranty   */
/* of any kind whatsoever and expressly disclaimed and excluded by Renesas,  */
/* either expressed or implied, including but not limited to those for       */
/* non-infringement of intellectual property, merchantability and/or         */
/* fitness for the particular purpose.                                       */
/* Renesas shall not have any obligation to maintain, service or provide bug */
/* fixes for the supplied Product(s) and/or the Application.                 */
/*                                                                           */
/* Each User is solely responsible for determining the appropriateness of    */
/* using the Product(s) and assumes all risks associated with its exercise   */
/* of rights under this Agreement, including, but not limited to the risks   */
/* and costs of program errors, compliance with applicable laws, damage to   */
/* or loss of data, programs or equipment, and unavailability or             */
/* interruption of operations.                                               */
/*                                                                           */
/* Limitation of Liability                                                   */
/*                                                                           */
/* In no event shall Renesas be liable to the User for any incidental,       */
/* consequential, indirect, or punitive damage (including but not limited    */
/* to lost profits) regardless of whether such liability is based on breach  */
/* of contract, tort, strict liability, breach of warranties, failure of     */
/* essential purpose or otherwise and even if advised of the possibility of  */
/* such damages. Renesas shall not be liable for any services or products    */
/* provided by third party vendors, developers or consultants identified or  */
/* referred to the User by Renesas in connection with the Product(s) and/or  */
/* the Application.                                                          */
/*                                                                           */
/*===========================================================================*/
/* Environment:                                                              */
/*              Device:         U2A                                          */
/*              IDE:            GHS Multi V7.1.4 or later                    */
/*===========================================================================*/
/* Revision Control History:                                                 */
/*  1.3.2:  06/09/2021    : Updated section memory to support module multi   */
/*                          for Adc.                                         */
/*          28/08/2021    : Updated section memory to support module multi.  */
/*  1.3.1:  28/07/2021    : Move .INIT_RAM_PTR from iRAM_0 to cRAM_0         */
/*          19/07/2021    : Add .INIT_RAM_PTR section                        */
/*          01/04/2021    : Remove vendor ID from API names and parameters   */
/*                          for ETH according to BSW00347 requirement        */
/*  1.1.0:  19/06/2020    : Beta Release                                     */
/*  1.0.3:  14/01/2020    : Added section for pointers as per AR 4.3.1       */
/*  1.0.2:  09/07/2019    : Added section .mev_address in cRAM_0 for         */
/*                           Sync flags between multi core                   */
/*  1.0.1:  24/06/2019    : Added section for multi core sample for WDG.     */
/*  1.0.0:  14/02/2018    : Initial Version                                  */
/*===========================================================================*/

//Sky add start line
CONSTANTS
{
  zero_start = 0xffff8000
}

MEMORY
 {
  iROM_0     : ORIGIN = 0x00000000,  LENGTH = 3584k  /* Code flash User area */
  dBaseROM   : ORIGIN = 0x00380000,  LENGTH = 64k  /* MCAL Driver Database area */
  iROM_1     : ORIGIN = 0x00400000,  LENGTH = 32k  /* Code flash of PE1 */
  iROM_1_TOP : ORIGIN = .         ,  LENGTH = 0

  iRAM_1     : ORIGIN = 0xFDA00000,  LENGTH = 64k  /* Local RAM of PE1 */
  iRAM_1_TOP : ORIGIN = .         ,  LENGTH = 0
  iRAM_0     : ORIGIN = 0xFDC00000,  LENGTH = 64k  /* Local RAM of PE0 */
  iRAM_0_TOP : ORIGIN = .         ,  LENGTH = 0
  iRAM       : ORIGIN = 0xFDE00000,  LENGTH = 64k  /* Local RAM of Self */
  iRAM_TOP   : ORIGIN = .         ,  LENGTH = 0

  cRAM_SF_0  : ORIGIN = 0xFE000000,  LENGTH = 2k   /* Stack Frame for PE0 (in Cluster RAM) */
  cRAM_SF_1  : ORIGIN = 0xFE000800,  LENGTH = 2k   /* Stack Frame for PE1 (in Cluster RAM) */
  cRAM_SF_2  : ORIGIN = 0xFE001000,  LENGTH = 2k   /* Stack Frame for PE2 (in Cluster RAM) */
  cRAM_SF_3  : ORIGIN = 0xFE001800,  LENGTH = 2k   /* Stack Frame for PE3 (in Cluster RAM) */
  cRAM_HEAP  : ORIGIN = 0xFE008000,  LENGTH = 32k  /* Heap Area */

  cRAM_0     : ORIGIN = 0xFE010000,  LENGTH = 444k /* Cluster RAM 0 (512k) - 64k(for stack) */
  cRAM_0_TOP : ORIGIN = .         ,  LENGTH = 0
  cRAM_1     : ORIGIN = 0xFE100000,  LENGTH = 512k /* Cluster RAM 1 (512k) */
  cRAM_1_TOP : ORIGIN = .         ,  LENGTH = 0
  cRAM_2     : ORIGIN = 0xFE400000,  LENGTH = 512k /* Cluster RAM 2 (512k) */
  cRAM_2_TOP : ORIGIN = .         ,  LENGTH = 0
  iRAM_R     : ORIGIN = 0xFE800000,  LENGTH = 128k
  iRAM_R_TOP : ORIGIN = .         ,  LENGTH = 0
 }
//Sky add end line

SECTIONS
 {
  .stack1_PE1   align(4) pad(0x0800)     :>iRAM_1   /* this section is used for stack pointer of CPU1 */

  /* Start of internal ROM area (iROM_0) */

  .intvect_PE0 0x0000          align(16)        :> iROM_0   /* start of interrupt vector. This section contains RESET and exception table for PE0 */
  .inttable_PE0                align(0x200)     :>.
  .inttable_PE0_end                             :>.

  .intvect_PE1 0x2000          align(16)        :>.   /* start of interrupt vector. This section contains exception table for PE1 */
  .inttable_PE1                align(0x200)     :>.
  .inttable_PE1_end                             :>.

  .intvect_PE2 0x4000          align(16)        :>.   /* start of interrupt vector. This section contains exception table for PE2 */
  .inttable_PE2                align(0x200)     :>.
  .inttable_PE2_end                             :>.

  .intvect_PE3 0x6000          align(16)        :>.   /* start of interrupt vector. This section contains exception table for PE3 */
  .inttable_PE3                align(0x200)     :>.
  .inttable_PE3_end                             :>.

  .rozdata                                      :>.         /* constant datas in ZDA area */
  .robase                      align(4)         :>.         /* initialize textpointer TP for SDA addressing */
  .rosdata                     align(4)         :>.         /* constant datas in SDA area */
  .rodata                      align(4)         :>.         /* constant datas in normal area */

  .CONST_ROM_1BIT                               :>.  /* Single core */
  .CONST_ROM_8BIT                               :>.
  .CONST_ROM_16BIT                              :>.
  .CONST_ROM_32BIT                              :>.
  .CONST_ROM_UNSPECIFIED                        :>.
  .CONST_ROM_PTR                                :>.

  .CONST_ROM_1BIT_0                             :>.  /* Instance 0 */
  .CONST_ROM_8BIT_0                             :>.
  .CONST_ROM_16BIT_0                            :>.
  .CONST_ROM_32BIT_0                            :>.
  .CONST_ROM_UNSPECIFIED_0                      :>.
  .CONST_ROM_PTR_0                              :>.

  .CONST_ROM_1BIT_1                             :>.  /* Instance 1 */
  .CONST_ROM_8BIT_1                             :>.
  .CONST_ROM_16BIT_1                            :>.
  .CONST_ROM_32BIT_1                            :>.
  .CONST_ROM_UNSPECIFIED_1                      :>.
  .CONST_ROM_PTR_1                              :>.

  .CONST_ROM_1BIT_2                             :>.  /* Instance 2 */
  .CONST_ROM_8BIT_2                             :>.
  .CONST_ROM_16BIT_2                            :>.
  .CONST_ROM_32BIT_2                            :>.
  .CONST_ROM_UNSPECIFIED_2                      :>.
  .CONST_ROM_PTR_2                              :>.

  .CONST_ROM_1BIT_3                             :>.  /* Instance 3 */
  .CONST_ROM_8BIT_3                             :>.
  .CONST_ROM_16BIT_3                            :>.
  .CONST_ROM_32BIT_3                            :>.
  .CONST_ROM_UNSPECIFIED_3                      :>.
  .CONST_ROM_PTR_3                              :>.

  .CONST_ROM_1BIT_4                             :>.  /* Instance 4 */
  .CONST_ROM_8BIT_4                             :>.
  .CONST_ROM_16BIT_4                            :>.
  .CONST_ROM_32BIT_4                            :>.
  .CONST_ROM_UNSPECIFIED_4                      :>.
  .CONST_ROM_PTR_4                              :>.

  .CONST_ROM_1BIT_5                             :>.  /* Instance 5 */
  .CONST_ROM_8BIT_5                             :>.
  .CONST_ROM_16BIT_5                            :>.
  .CONST_ROM_32BIT_5                            :>.
  .CONST_ROM_UNSPECIFIED_5                      :>.
  .CONST_ROM_PTR_5                              :>.

  .CONST_ROM_1BIT_6                             :>.  /* Instance 6 */
  .CONST_ROM_8BIT_6                             :>.
  .CONST_ROM_16BIT_6                            :>.
  .CONST_ROM_32BIT_6                            :>.
  .CONST_ROM_UNSPECIFIED_6                      :>.
  .CONST_ROM_PTR_6                              :>.

  .CONST_ROM_1BIT_7                             :>.  /* Instance 7 */
  .CONST_ROM_8BIT_7                             :>.
  .CONST_ROM_16BIT_7                            :>.
  .CONST_ROM_32BIT_7                            :>.
  .CONST_ROM_UNSPECIFIED_7                      :>.
  .CONST_ROM_PTR_7                              :>.

  .CONST_FAR_ROM_1BIT                           :>.  /* Single core */
  .CONST_FAR_ROM_8BIT                           :>.
  .CONST_FAR_ROM_16BIT                          :>.
  .CONST_FAR_ROM_32BIT                          :>.
  .CONST_FAR_ROM_UNSPECIFIED                    :>.

  .CONST_FAR_ROM_1BIT_0                         :>.  /* Instance 0 */
  .CONST_FAR_ROM_8BIT_0                         :>.
  .CONST_FAR_ROM_16BIT_0                        :>.
  .CONST_FAR_ROM_32BIT_0                        :>.
  .CONST_FAR_ROM_UNSPECIFIED_0                  :>.

  .CONST_FAR_ROM_1BIT_1                         :>.  /* Instance 1 */
  .CONST_FAR_ROM_8BIT_1                         :>.
  .CONST_FAR_ROM_16BIT_1                        :>.
  .CONST_FAR_ROM_32BIT_1                        :>.
  .CONST_FAR_ROM_UNSPECIFIED_1                  :>.

  .CONST_FAR_ROM_1BIT_2                         :>.  /* Instance 2 */
  .CONST_FAR_ROM_8BIT_2                         :>.
  .CONST_FAR_ROM_16BIT_2                        :>.
  .CONST_FAR_ROM_32BIT_2                        :>.
  .CONST_FAR_ROM_UNSPECIFIED_2                  :>.

  .CONST_FAR_ROM_1BIT_3                         :>.  /* Instance 3 */
  .CONST_FAR_ROM_8BIT_3                         :>.
  .CONST_FAR_ROM_16BIT_3                        :>.
  .CONST_FAR_ROM_32BIT_3                        :>.
  .CONST_FAR_ROM_UNSPECIFIED_3                  :>.

  .CONST_FAR_ROM_1BIT_4                         :>.  /* Instance 4 */
  .CONST_FAR_ROM_8BIT_4                         :>.
  .CONST_FAR_ROM_16BIT_4                        :>.
  .CONST_FAR_ROM_32BIT_4                        :>.
  .CONST_FAR_ROM_UNSPECIFIED_4                  :>.

  .CONST_FAR_ROM_1BIT_5                         :>.  /* Instance 5 */
  .CONST_FAR_ROM_8BIT_5                         :>.
  .CONST_FAR_ROM_16BIT_5                        :>.
  .CONST_FAR_ROM_32BIT_5                        :>.
  .CONST_FAR_ROM_UNSPECIFIED_5                  :>.

  .CONST_FAR_ROM_1BIT_6                         :>.  /* Instance 6 */
  .CONST_FAR_ROM_8BIT_6                         :>.
  .CONST_FAR_ROM_16BIT_6                        :>.
  .CONST_FAR_ROM_32BIT_6                        :>.
  .CONST_FAR_ROM_UNSPECIFIED_6                  :>.

  .CONST_FAR_ROM_1BIT_7                         :>.  /* Instance 7 */
  .CONST_FAR_ROM_8BIT_7                         :>.
  .CONST_FAR_ROM_16BIT_7                        :>.
  .CONST_FAR_ROM_32BIT_7                        :>.
  .CONST_FAR_ROM_UNSPECIFIED_7                  :>.

  /* program code area */
  .text     align(4)                            :>.

  /* MCAL Driver code area *****/
  .DIO_PUBLIC_CODE_ROM                          :>.
  .DIO_PRIVATE_CODE_ROM                         :>.
  .DIO_APPL_CODE_ROM                            :>.

  .GPT_PUBLIC_CODE_ROM                          :>.  /* Single core */
  .GPT_PRIVATE_CODE_ROM                         :>.
  .GPT_APPL_CODE_ROM                            :>.
  .GPT_FAST_CODE_ROM                            :>.

  .GPT_59_INST0_PUBLIC_CODE_ROM                 :>.  /* Instance 0 */
  .GPT_59_INST0_PRIVATE_CODE_ROM                :>.
  .GPT_59_INST0_APPL_CODE_ROM                   :>.
  .GPT_59_INST0_FAST_CODE_ROM                   :>.

  .GPT_59_INST1_PUBLIC_CODE_ROM                 :>.  /* Instance 1 */
  .GPT_59_INST1_PRIVATE_CODE_ROM                :>.
  .GPT_59_INST1_APPL_CODE_ROM                   :>.
  .GPT_59_INST1_FAST_CODE_ROM                   :>.

  .GPT_59_INST2_PUBLIC_CODE_ROM                 :>.  /* Instance 2 */
  .GPT_59_INST2_PRIVATE_CODE_ROM                :>.
  .GPT_59_INST2_APPL_CODE_ROM                   :>.
  .GPT_59_INST2_FAST_CODE_ROM                   :>.

  .GPT_59_INST3_PUBLIC_CODE_ROM                 :>.  /* Instance 3 */
  .GPT_59_INST3_PRIVATE_CODE_ROM                :>.
  .GPT_59_INST3_APPL_CODE_ROM                   :>.
  .GPT_59_INST3_FAST_CODE_ROM                   :>.

  .GPT_59_INST4_PUBLIC_CODE_ROM                 :>.  /* Instance 4 */
  .GPT_59_INST4_PRIVATE_CODE_ROM                :>.
  .GPT_59_INST4_APPL_CODE_ROM                   :>.
  .GPT_59_INST4_FAST_CODE_ROM                   :>.

  .GPT_59_INST5_PUBLIC_CODE_ROM                 :>.  /* Instance 5 */
  .GPT_59_INST5_PRIVATE_CODE_ROM                :>.
  .GPT_59_INST5_APPL_CODE_ROM                   :>.
  .GPT_59_INST5_FAST_CODE_ROM                   :>.

  .GPT_59_INST6_PUBLIC_CODE_ROM                 :>.  /* Instance 6 */
  .GPT_59_INST6_PRIVATE_CODE_ROM                :>.
  .GPT_59_INST6_APPL_CODE_ROM                   :>.
  .GPT_59_INST6_FAST_CODE_ROM                   :>.

  .GPT_59_INST7_PUBLIC_CODE_ROM                 :>.  /* Instance 7 */
  .GPT_59_INST7_PRIVATE_CODE_ROM                :>.
  .GPT_59_INST7_APPL_CODE_ROM                   :>.
  .GPT_59_INST7_FAST_CODE_ROM                   :>.   

  .ICU_PUBLIC_CODE_ROM                          :>. /* Single core */
  .ICU_PRIVATE_CODE_ROM                         :>.
  .ICU_APPL_CODE_ROM                            :>.
  .ICU_FAST_CODE_ROM                            :>.

  .ICU_59_INST0_PUBLIC_CODE_ROM                 :>. /* Instance 0 */
  .ICU_59_INST0_PRIVATE_CODE_ROM                :>.
  .ICU_59_INST0_APPL_CODE_ROM                   :>.
  .ICU_59_INST0_FAST_CODE_ROM                   :>.

  .ICU_59_INST1_PUBLIC_CODE_ROM                 :>. /* Instance 1 */
  .ICU_59_INST1_PRIVATE_CODE_ROM                :>.
  .ICU_59_INST1_APPL_CODE_ROM                   :>.
  .ICU_59_INST1_FAST_CODE_ROM                   :>.

  .ICU_59_INST2_PUBLIC_CODE_ROM                 :>. /* Instance 2 */
  .ICU_59_INST2_PRIVATE_CODE_ROM                :>.
  .ICU_59_INST2_APPL_CODE_ROM                   :>.
  .ICU_59_INST2_FAST_CODE_ROM                   :>.

  .ICU_59_INST3_PUBLIC_CODE_ROM                 :>. /* Instance 3 */
  .ICU_59_INST3_PRIVATE_CODE_ROM                :>.
  .ICU_59_INST3_APPL_CODE_ROM                   :>.
  .ICU_59_INST3_FAST_CODE_ROM                   :>.

  .ICU_59_INST4_PUBLIC_CODE_ROM                 :>. /* Instance 4 */
  .ICU_59_INST4_PRIVATE_CODE_ROM                :>.
  .ICU_59_INST4_APPL_CODE_ROM                   :>.
  .ICU_59_INST4_FAST_CODE_ROM                   :>.

  .ICU_59_INST5_PUBLIC_CODE_ROM                 :>. /* Instance 5 */
  .ICU_59_INST5_PRIVATE_CODE_ROM                :>.
  .ICU_59_INST5_APPL_CODE_ROM                   :>.
  .ICU_59_INST5_FAST_CODE_ROM                   :>.

  .ICU_59_INST6_PUBLIC_CODE_ROM                 :>. /* Instance 6 */
  .ICU_59_INST6_PRIVATE_CODE_ROM                :>.
  .ICU_59_INST6_APPL_CODE_ROM                   :>.
  .ICU_59_INST6_FAST_CODE_ROM                   :>.

  .ICU_59_INST7_PUBLIC_CODE_ROM                 :>. /* Instance 7 */
  .ICU_59_INST7_PRIVATE_CODE_ROM                :>.
  .ICU_59_INST7_APPL_CODE_ROM                   :>.
  .ICU_59_INST7_FAST_CODE_ROM                   :>.

  .PORT_PUBLIC_CODE_ROM                         :>.
  .PORT_PRIVATE_CODE_ROM                        :>.
  .PORT_APPL_CODE_ROM                           :>.

  .PWM_PUBLIC_CODE_ROM                          :>. /* Single core */
  .PWM_PRIVATE_CODE_ROM                         :>.
  .PWM_APPL_CODE_ROM                            :>.
  .PWM_FAST_CODE_ROM                            :>.
  
  .PWM_59_INST0_PUBLIC_CODE_ROM                 :>. /* Instance 0 */
  .PWM_59_INST0_PRIVATE_CODE_ROM                :>.
  .PWM_59_INST0_APPL_CODE_ROM                   :>.
  .PWM_59_INST0_FAST_CODE_ROM                   :>.
                         
  .PWM_59_INST1_PUBLIC_CODE_ROM                 :>. /* Instance 1 */
  .PWM_59_INST1_PRIVATE_CODE_ROM                :>.
  .PWM_59_INST1_APPL_CODE_ROM                   :>.
  .PWM_59_INST1_FAST_CODE_ROM                   :>.

  .PWM_59_INST2_PUBLIC_CODE_ROM                 :>. /* Instance 2 */
  .PWM_59_INST2_PRIVATE_CODE_ROM                :>.
  .PWM_59_INST2_APPL_CODE_ROM                   :>.
  .PWM_59_INST2_FAST_CODE_ROM                   :>.
                         
  .PWM_59_INST3_PUBLIC_CODE_ROM                 :>. /* Instance 3 */
  .PWM_59_INST3_PRIVATE_CODE_ROM                :>.
  .PWM_59_INST3_APPL_CODE_ROM                   :>.
  .PWM_59_INST3_FAST_CODE_ROM                   :>.

  .PWM_59_INST4_PUBLIC_CODE_ROM                 :>. /* Instance 4 */
  .PWM_59_INST4_PRIVATE_CODE_ROM                :>.
  .PWM_59_INST4_APPL_CODE_ROM                   :>.
  .PWM_59_INST4_FAST_CODE_ROM                   :>.
                         
  .PWM_59_INST5_PUBLIC_CODE_ROM                 :>. /* Instance 5 */
  .PWM_59_INST5_PRIVATE_CODE_ROM                :>.
  .PWM_59_INST5_APPL_CODE_ROM                   :>.
  .PWM_59_INST5_FAST_CODE_ROM                   :>.

  .PWM_59_INST6_PUBLIC_CODE_ROM                 :>. /* Instance 6 */
  .PWM_59_INST6_PRIVATE_CODE_ROM                :>.
  .PWM_59_INST6_APPL_CODE_ROM                   :>.
  .PWM_59_INST6_FAST_CODE_ROM                   :>.
                         
  .PWM_59_INST7_PUBLIC_CODE_ROM                 :>. /* Instance 7 */
  .PWM_59_INST7_PRIVATE_CODE_ROM                :>.
  .PWM_59_INST7_APPL_CODE_ROM                   :>.
  .PWM_59_INST7_FAST_CODE_ROM                   :>.
  
  .SPI_PUBLIC_CODE_ROM                          :>. /* Single core */
  .SPI_PRIVATE_CODE_ROM                         :>.
  .SPI_APPL_CODE_ROM                            :>.
  .SPI_FAST_CODE_ROM                            :>.

  .SPI_59_INST0_PUBLIC_CODE_ROM                 :>. /* Instance 0 */
  .SPI_59_INST0_PRIVATE_CODE_ROM                :>.
  .SPI_59_INST0_APPL_CODE_ROM                   :>.
  .SPI_59_INST0_FAST_CODE_ROM                   :>.

  .SPI_59_INST1_PUBLIC_CODE_ROM                 :>. /* Instance 1 */
  .SPI_59_INST1_PRIVATE_CODE_ROM                :>.
  .SPI_59_INST1_APPL_CODE_ROM                   :>.
  .SPI_59_INST1_FAST_CODE_ROM                   :>.

  .SPI_59_INST2_PUBLIC_CODE_ROM                 :>. /* Instance 2 */
  .SPI_59_INST2_PRIVATE_CODE_ROM                :>.
  .SPI_59_INST2_APPL_CODE_ROM                   :>.
  .SPI_59_INST2_FAST_CODE_ROM                   :>.

  .SPI_59_INST3_PUBLIC_CODE_ROM                 :>. /* Instance 3 */
  .SPI_59_INST3_PRIVATE_CODE_ROM                :>.
  .SPI_59_INST3_APPL_CODE_ROM                   :>.
  .SPI_59_INST3_FAST_CODE_ROM                   :>.

  .SPI_59_INST4_PUBLIC_CODE_ROM                 :>. /* Instance 4 */
  .SPI_59_INST4_PRIVATE_CODE_ROM                :>.
  .SPI_59_INST4_APPL_CODE_ROM                   :>.
  .SPI_59_INST4_FAST_CODE_ROM                   :>.

  .SPI_59_INST5_PUBLIC_CODE_ROM                 :>. /* Instance 5 */
  .SPI_59_INST5_PRIVATE_CODE_ROM                :>.
  .SPI_59_INST5_APPL_CODE_ROM                   :>.
  .SPI_59_INST5_FAST_CODE_ROM                   :>.

  .SPI_59_INST6_PUBLIC_CODE_ROM                 :>. /* Instance 6 */
  .SPI_59_INST6_PRIVATE_CODE_ROM                :>.
  .SPI_59_INST6_APPL_CODE_ROM                   :>.
  .SPI_59_INST6_FAST_CODE_ROM                   :>.

  .SPI_59_INST7_PUBLIC_CODE_ROM                 :>. /* Instance 7 */
  .SPI_59_INST7_PRIVATE_CODE_ROM                :>.
  .SPI_59_INST7_APPL_CODE_ROM                   :>.
  .SPI_59_INST7_FAST_CODE_ROM                   :>.

  .WDG_PUBLIC_CODE_ROM                          :>.   /* Single core */
  .WDG_PRIVATE_CODE_ROM                         :>.
  .WDG_FAST_CODE_ROM                            :>.

  .WDG_59_INST0_PUBLIC_CODE_ROM                 :>.   /* Instance 0 */
  .WDG_59_INST0_PRIVATE_CODE_ROM                :>.
  .WDG_59_INST0_FAST_CODE_ROM                   :>.

  .WDG_59_INST1_PUBLIC_CODE_ROM                 :>.   /* Instance 1 */
  .WDG_59_INST1_PRIVATE_CODE_ROM                :>.
  .WDG_59_INST1_FAST_CODE_ROM                   :>.

  .WDG_59_INST2_PUBLIC_CODE_ROM                 :>.   /* Instance 2 */
  .WDG_59_INST2_PRIVATE_CODE_ROM                :>.
  .WDG_59_INST2_FAST_CODE_ROM                   :>.

  .WDG_59_INST3_PUBLIC_CODE_ROM                 :>.   /* Instance 3 */
  .WDG_59_INST3_PRIVATE_CODE_ROM                :>.
  .WDG_59_INST3_FAST_CODE_ROM                   :>.

  .CAN_PUBLIC_CODE_ROM                          :>.
  .CAN_PRIVATE_CODE_ROM                         :>.
  .CAN_APPL_CODE_ROM                            :>.
  .CAN_FAST_CODE_ROM                            :>.

  .CAN_59_INST0_PUBLIC_CODE_ROM                 :>.   /* Instance 0 */
  .CAN_59_INST0_PRIVATE_CODE_ROM                :>.
  .CAN_59_INST0_APPL_CODE_ROM                   :>.
  .CAN_59_INST0_FAST_CODE_ROM                   :>.

  .CAN_59_INST1_PUBLIC_CODE_ROM                 :>.   /* Instance 1 */
  .CAN_59_INST1_PRIVATE_CODE_ROM                :>.
  .CAN_59_INST1_APPL_CODE_ROM                   :>.
  .CAN_59_INST1_FAST_CODE_ROM                   :>.

  .ADC_PUBLIC_CODE_ROM                          :>.   /* Single core */
  .ADC_PRIVATE_CODE_ROM                         :>.
  .ADC_APPL_CODE_ROM                            :>.
  .ADC_FAST_CODE_ROM                            :>.

  .ADC_59_INST0_PUBLIC_CODE_ROM                 :>.   /* Instance 0 */
  .ADC_59_INST0_PRIVATE_CODE_ROM                :>.
  .ADC_59_INST0_APPL_CODE_ROM                   :>.
  .ADC_59_INST0_FAST_CODE_ROM                   :>.

  .ADC_59_INST1_PUBLIC_CODE_ROM                 :>.   /* Instance 1 */
  .ADC_59_INST1_PRIVATE_CODE_ROM                :>.
  .ADC_59_INST1_APPL_CODE_ROM                   :>.
  .ADC_59_INST1_FAST_CODE_ROM                   :>.

  .ADC_59_INST2_PUBLIC_CODE_ROM                 :>.   /* Instance 2 */
  .ADC_59_INST2_PRIVATE_CODE_ROM                :>.
  .ADC_59_INST2_APPL_CODE_ROM                   :>.
  .ADC_59_INST2_FAST_CODE_ROM                   :>.

  .LIN_PUBLIC_CODE_ROM                          :>.
  .LIN_PRIVATE_CODE_ROM                         :>.
  .LIN_APPL_CODE_ROM                            :>.
  .LIN_FAST_CODE_ROM                            :>.

  .FR_59_RENESAS_PUBLIC_CODE_ROM                :>.
  .FR_59_RENESAS_PRIVATE_CODE_ROM               :>.
  .FR_59_RENESAS_APPL_CODE_ROM                  :>.

  .MCU_PUBLIC_CODE_ROM                          :>.
  .MCU_PRIVATE_CODE_ROM                         :>.
  .MCU_APPL_CODE_ROM                            :>.
  .MCU_FAST_CODE_ROM                            :>.
  .MCU_CODE_RRAM_INTVEC   align(4)              :>.
  .MCU_CR_CODE_RRAM       align(4)              :>.
  .MCU_CR_CODE_ROM        align(4)              :>.

  .FLS_PUBLIC_CODE_ROM                          :>.
  .FLS_PRIVATE_CODE_ROM                         :>.
  .FLS_APPL_CODE_ROM                            :>.
  .FLS_FAST_CODE_ROM                            :>.
  .R_RFD_CODE_COMMON                align(4)    :>.       /* RFD Code area for Common Flash component located in ROM */
  .R_RFD_CODE_COMMON_RAM_NO_BGO     align(4)    :>.       /* RFD Code area for Common Flash component located in ROM when satisfied the BGO condtion */
  .R_RFD_CODE_DF                    align(4)    :>.       /* RFD Code area for Data Flash component located in ROM   */
  .R_RFD_ROSDATA_VERSION_COMMON                 :>.
  .R_RFD_ROSDATA_VERSION_DF                     :>.

  .ETH_PUBLIC_CODE_ROM                       :>.
  .ETH_PRIVATE_CODE_ROM                      :>.
  .ETH_FAST_CODE_ROM                         :>.

  .fixaddr              align(4)                :>.     /* ghs internal (compiler) */
  .fixtype              align(4)                :>.     /* ghs internal (compiler) */
  .secinfo              align(4)                :>.     /* ghs internal (runtime library) */
  .syscall              align(4)                :>.     /* ghs internal (linker) */

  .romdata              ROM(.data)              :>.     /* constant data to initialize variables (copied to RAM at startup)*/
  .romzdata             ROM(.zdata)             :>.     /* constant data to initialize variables in ZDA area (copied to RAM at startup)*/
  .romsdata             ROM(.sdata)             :>.     /* constant data to initialize variables in SDA area (copied to RAM at startup)*/
  .romtdata             ROM(.tdata)             :>.     /* constant data to initialize variables in TDA area (copied to RAM at startup)*/
  .romsldata            ROM(.sldata)            :>.     /* constant data to initialize variables in LSDA area (copied to GRAM at startup)*/

  .ROM.RAM_1BIT              ROM(.RAM_1BIT)               :>.  /* Single core */
  .ROM.RAM_8BIT              ROM(.RAM_8BIT)               :>.
  .ROM.RAM_16BIT             ROM(.RAM_16BIT)              :>.
  .ROM.RAM_32BIT             ROM(.RAM_32BIT)              :>.
  .ROM.RAM_UNSPECIFIED       ROM(.RAM_UNSPECIFIED)        :>.
  .ROM.RAM_INIT_PTR          ROM(.RAM_INIT_PTR)           :>.
  .ROM.FAST_RAM_1BIT         ROM(.FAST_RAM_1BIT)          :>.
  .ROM.FAST_RAM_8BIT         ROM(.FAST_RAM_8BIT)          :>.
  .ROM.FAST_RAM_16BIT        ROM(.FAST_RAM_16BIT)         :>.
  .ROM.FAST_RAM_32BIT        ROM(.FAST_RAM_32BIT)         :>.
  .ROM.FAST_RAM_UNSPECIFIED  ROM(.FAST_RAM_UNSPECIFIED)   :>.
  .ROM.FAST_RAM_INIT_PTR     ROM(.FAST_RAM_INIT_PTR)      :>.

  .ROM.RAM_1BIT_0              ROM(.RAM_1BIT_0)               :>.  /* Instance 0 */
  .ROM.RAM_8BIT_0              ROM(.RAM_8BIT_0)               :>.
  .ROM.RAM_16BIT_0             ROM(.RAM_16BIT_0)              :>.
  .ROM.RAM_32BIT_0             ROM(.RAM_32BIT_0)              :>.
  .ROM.RAM_UNSPECIFIED_0       ROM(.RAM_UNSPECIFIED_0)        :>.
  .ROM.RAM_INIT_PTR_0          ROM(.RAM_INIT_PTR_0)           :>.
  .ROM.FAST_RAM_1BIT_0         ROM(.FAST_RAM_1BIT_0)          :>.
  .ROM.FAST_RAM_8BIT_0         ROM(.FAST_RAM_8BIT_0)          :>.
  .ROM.FAST_RAM_16BIT_0        ROM(.FAST_RAM_16BIT_0)         :>.
  .ROM.FAST_RAM_32BIT_0        ROM(.FAST_RAM_32BIT_0)         :>.
  .ROM.FAST_RAM_UNSPECIFIED_0  ROM(.FAST_RAM_UNSPECIFIED_0)   :>.
  .ROM.FAST_RAM_INIT_PTR_0     ROM(.FAST_RAM_INIT_PTR_0)      :>.

  .ROM.RAM_1BIT_1              ROM(.RAM_1BIT_1)               :>.  /* Instance 1 */
  .ROM.RAM_8BIT_1              ROM(.RAM_8BIT_1)               :>.
  .ROM.RAM_16BIT_1             ROM(.RAM_16BIT_1)              :>.
  .ROM.RAM_32BIT_1             ROM(.RAM_32BIT_1)              :>.
  .ROM.RAM_UNSPECIFIED_1       ROM(.RAM_UNSPECIFIED_1)        :>.
  .ROM.RAM_INIT_PTR_1          ROM(.RAM_INIT_PTR_1)           :>.
  .ROM.FAST_RAM_1BIT_1         ROM(.FAST_RAM_1BIT_1)          :>.
  .ROM.FAST_RAM_8BIT_1         ROM(.FAST_RAM_8BIT_1)          :>.
  .ROM.FAST_RAM_16BIT_1        ROM(.FAST_RAM_16BIT_1)         :>.
  .ROM.FAST_RAM_32BIT_1        ROM(.FAST_RAM_32BIT_1)         :>.
  .ROM.FAST_RAM_UNSPECIFIED_1  ROM(.FAST_RAM_UNSPECIFIED_1)   :>.
  .ROM.FAST_RAM_INIT_PTR_1     ROM(.FAST_RAM_INIT_PTR_1)      :>.

  .ROM.RAM_1BIT_2              ROM(.RAM_1BIT_2)               :>.  /* Instance 2 */
  .ROM.RAM_8BIT_2              ROM(.RAM_8BIT_2)               :>.
  .ROM.RAM_16BIT_2             ROM(.RAM_16BIT_2)              :>.
  .ROM.RAM_32BIT_2             ROM(.RAM_32BIT_2)              :>.
  .ROM.RAM_UNSPECIFIED_2       ROM(.RAM_UNSPECIFIED_2)        :>.
  .ROM.RAM_INIT_PTR_2          ROM(.RAM_INIT_PTR_2)           :>.
  .ROM.FAST_RAM_1BIT_2         ROM(.FAST_RAM_1BIT_2)          :>.
  .ROM.FAST_RAM_8BIT_2         ROM(.FAST_RAM_8BIT_2)          :>.
  .ROM.FAST_RAM_16BIT_2        ROM(.FAST_RAM_16BIT_2)         :>.
  .ROM.FAST_RAM_32BIT_2        ROM(.FAST_RAM_32BIT_2)         :>.
  .ROM.FAST_RAM_UNSPECIFIED_2  ROM(.FAST_RAM_UNSPECIFIED_2)   :>.
  .ROM.FAST_RAM_INIT_PTR_2     ROM(.FAST_RAM_INIT_PTR_2)      :>.

  .ROM.RAM_1BIT_3              ROM(.RAM_1BIT_3)               :>.  /* Instance 3 */
  .ROM.RAM_8BIT_3              ROM(.RAM_8BIT_3)               :>.
  .ROM.RAM_16BIT_3             ROM(.RAM_16BIT_3)              :>.
  .ROM.RAM_32BIT_3             ROM(.RAM_32BIT_3)              :>.
  .ROM.RAM_UNSPECIFIED_3       ROM(.RAM_UNSPECIFIED_3)        :>.
  .ROM.RAM_INIT_PTR_3          ROM(.RAM_INIT_PTR_3)           :>.
  .ROM.FAST_RAM_1BIT_3         ROM(.FAST_RAM_1BIT_3)          :>.
  .ROM.FAST_RAM_8BIT_3         ROM(.FAST_RAM_8BIT_3)          :>.
  .ROM.FAST_RAM_16BIT_3        ROM(.FAST_RAM_16BIT_3)         :>.
  .ROM.FAST_RAM_32BIT_3        ROM(.FAST_RAM_32BIT_3)         :>.
  .ROM.FAST_RAM_UNSPECIFIED_3  ROM(.FAST_RAM_UNSPECIFIED_3)   :>.
  .ROM.FAST_RAM_INIT_PTR_3     ROM(.FAST_RAM_INIT_PTR_3)      :>.

  .ROM.RAM_1BIT_4              ROM(.RAM_1BIT_4)               :>.  /* Instance 4 */
  .ROM.RAM_8BIT_4              ROM(.RAM_8BIT_4)               :>.
  .ROM.RAM_16BIT_4             ROM(.RAM_16BIT_4)              :>.
  .ROM.RAM_32BIT_4             ROM(.RAM_32BIT_4)              :>.
  .ROM.RAM_UNSPECIFIED_4       ROM(.RAM_UNSPECIFIED_4)        :>.
  .ROM.RAM_INIT_PTR_4          ROM(.RAM_INIT_PTR_4)           :>.
  .ROM.FAST_RAM_1BIT_4         ROM(.FAST_RAM_1BIT_4)          :>.
  .ROM.FAST_RAM_8BIT_4         ROM(.FAST_RAM_8BIT_4)          :>.
  .ROM.FAST_RAM_16BIT_4        ROM(.FAST_RAM_16BIT_4)         :>.
  .ROM.FAST_RAM_32BIT_4        ROM(.FAST_RAM_32BIT_4)         :>.
  .ROM.FAST_RAM_UNSPECIFIED_4  ROM(.FAST_RAM_UNSPECIFIED_4)   :>.
  .ROM.FAST_RAM_INIT_PTR_4     ROM(.FAST_RAM_INIT_PTR_4)      :>.

  .ROM.RAM_1BIT_5              ROM(.RAM_1BIT_5)               :>.  /* Instance 5 */
  .ROM.RAM_8BIT_5              ROM(.RAM_8BIT_5)               :>.
  .ROM.RAM_16BIT_5             ROM(.RAM_16BIT_5)              :>.
  .ROM.RAM_32BIT_5             ROM(.RAM_32BIT_5)              :>.
  .ROM.RAM_UNSPECIFIED_5       ROM(.RAM_UNSPECIFIED_5)        :>.
  .ROM.RAM_INIT_PTR_5          ROM(.RAM_INIT_PTR_5)           :>.
  .ROM.FAST_RAM_1BIT_5         ROM(.FAST_RAM_1BIT_5)          :>.
  .ROM.FAST_RAM_8BIT_5         ROM(.FAST_RAM_8BIT_5)          :>.
  .ROM.FAST_RAM_16BIT_5        ROM(.FAST_RAM_16BIT_5)         :>.
  .ROM.FAST_RAM_32BIT_5        ROM(.FAST_RAM_32BIT_5)         :>.
  .ROM.FAST_RAM_UNSPECIFIED_5  ROM(.FAST_RAM_UNSPECIFIED_5)   :>.
  .ROM.FAST_RAM_INIT_PTR_5     ROM(.FAST_RAM_INIT_PTR_5)      :>.

  .ROM.RAM_1BIT_6              ROM(.RAM_1BIT_6)               :>.  /* Instance 6 */
  .ROM.RAM_8BIT_6              ROM(.RAM_8BIT_6)               :>.
  .ROM.RAM_16BIT_6             ROM(.RAM_16BIT_6)              :>.
  .ROM.RAM_32BIT_6             ROM(.RAM_32BIT_6)              :>.
  .ROM.RAM_UNSPECIFIED_6       ROM(.RAM_UNSPECIFIED_6)        :>.
  .ROM.RAM_INIT_PTR_6          ROM(.RAM_INIT_PTR_6)           :>.
  .ROM.FAST_RAM_1BIT_6         ROM(.FAST_RAM_1BIT_6)          :>.
  .ROM.FAST_RAM_8BIT_6         ROM(.FAST_RAM_8BIT_6)          :>.
  .ROM.FAST_RAM_16BIT_6        ROM(.FAST_RAM_16BIT_6)         :>.
  .ROM.FAST_RAM_32BIT_6        ROM(.FAST_RAM_32BIT_6)         :>.
  .ROM.FAST_RAM_UNSPECIFIED_6  ROM(.FAST_RAM_UNSPECIFIED_6)   :>.
  .ROM.FAST_RAM_INIT_PTR_6     ROM(.FAST_RAM_INIT_PTR_6)      :>.

  .ROM.RAM_1BIT_7              ROM(.RAM_1BIT_7)               :>.  /* Instance 7 */
  .ROM.RAM_8BIT_7              ROM(.RAM_8BIT_7)               :>.
  .ROM.RAM_16BIT_7             ROM(.RAM_16BIT_7)              :>.
  .ROM.RAM_32BIT_7             ROM(.RAM_32BIT_7)              :>.
  .ROM.RAM_UNSPECIFIED_7       ROM(.RAM_UNSPECIFIED_7)        :>.
  .ROM.RAM_INIT_PTR_7          ROM(.RAM_INIT_PTR_7)           :>.
  .ROM.FAST_RAM_1BIT_7         ROM(.FAST_RAM_1BIT_7)          :>.
  .ROM.FAST_RAM_8BIT_7         ROM(.FAST_RAM_8BIT_7)          :>.
  .ROM.FAST_RAM_16BIT_7        ROM(.FAST_RAM_16BIT_7)         :>.
  .ROM.FAST_RAM_32BIT_7        ROM(.FAST_RAM_32BIT_7)         :>.
  .ROM.FAST_RAM_UNSPECIFIED_7  ROM(.FAST_RAM_UNSPECIFIED_7)   :>.
  .ROM.FAST_RAM_INIT_PTR_7     ROM(.FAST_RAM_INIT_PTR_7)      :>.

  /* MCAL Driver Database area *****/
  .DIO_CFG_DBTOC_UNSPECIFIED      align(4)      :>dBaseROM
  .DIO_CFG_DATA_1BIT                            :>.
  .DIO_CFG_DATA_8BIT                            :>.
  .DIO_CFG_DATA_16BIT             align(4)      :>.
  .DIO_CFG_DATA_32BIT             align(4)      :>.
  .DIO_CFG_DATA_UNSPECIFIED       align(4)      :>.

  .GPT_CFG_DBTOC_UNSPECIFIED      align(4)      :>.  /* Single core */
  .GPT_CFG_DATA_1BIT                            :>.
  .GPT_CFG_DATA_8BIT                            :>.
  .GPT_CFG_DATA_16BIT             align(4)      :>.
  .GPT_CFG_DATA_32BIT             align(4)      :>.
  .GPT_CFG_DATA_UNSPECIFIED       align(4)      :>.

  .GPT_59_INST0_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 0 */
  .GPT_59_INST0_CFG_DATA_1BIT                          :>.
  .GPT_59_INST0_CFG_DATA_8BIT                          :>.
  .GPT_59_INST0_CFG_DATA_16BIT           align(4)      :>.
  .GPT_59_INST0_CFG_DATA_32BIT           align(4)      :>.
  .GPT_59_INST0_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .GPT_59_INST1_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 1 */
  .GPT_59_INST1_CFG_DATA_1BIT                          :>.
  .GPT_59_INST1_CFG_DATA_8BIT                          :>.
  .GPT_59_INST1_CFG_DATA_16BIT           align(4)      :>.
  .GPT_59_INST1_CFG_DATA_32BIT           align(4)      :>.
  .GPT_59_INST1_CFG_DATA_UNSPECIFIED     align(4)      :>.
  
  .GPT_59_INST2_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 2 */
  .GPT_59_INST2_CFG_DATA_1BIT                          :>.
  .GPT_59_INST2_CFG_DATA_8BIT                          :>.
  .GPT_59_INST2_CFG_DATA_16BIT           align(4)      :>.
  .GPT_59_INST2_CFG_DATA_32BIT           align(4)      :>.
  .GPT_59_INST2_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .GPT_59_INST3_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 3 */
  .GPT_59_INST3_CFG_DATA_1BIT                          :>.
  .GPT_59_INST3_CFG_DATA_8BIT                          :>.
  .GPT_59_INST3_CFG_DATA_16BIT           align(4)      :>.
  .GPT_59_INST3_CFG_DATA_32BIT           align(4)      :>.
  .GPT_59_INST3_CFG_DATA_UNSPECIFIED     align(4)      :>.
  
  .GPT_59_INST4_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 4 */
  .GPT_59_INST4_CFG_DATA_1BIT                          :>.
  .GPT_59_INST4_CFG_DATA_8BIT                          :>.
  .GPT_59_INST4_CFG_DATA_16BIT           align(4)      :>.
  .GPT_59_INST4_CFG_DATA_32BIT           align(4)      :>.
  .GPT_59_INST4_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .GPT_59_INST5_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 5 */
  .GPT_59_INST5_CFG_DATA_1BIT                          :>.
  .GPT_59_INST5_CFG_DATA_8BIT                          :>.
  .GPT_59_INST5_CFG_DATA_16BIT           align(4)      :>.
  .GPT_59_INST5_CFG_DATA_32BIT           align(4)      :>.
  .GPT_59_INST5_CFG_DATA_UNSPECIFIED     align(4)      :>.
  
  .GPT_59_INST6_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 6 */
  .GPT_59_INST6_CFG_DATA_1BIT                          :>.
  .GPT_59_INST6_CFG_DATA_8BIT                          :>.
  .GPT_59_INST6_CFG_DATA_16BIT           align(4)      :>.
  .GPT_59_INST6_CFG_DATA_32BIT           align(4)      :>.
  .GPT_59_INST6_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .GPT_59_INST7_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 7 */
  .GPT_59_INST7_CFG_DATA_1BIT                          :>.
  .GPT_59_INST7_CFG_DATA_8BIT                          :>.
  .GPT_59_INST7_CFG_DATA_16BIT           align(4)      :>.
  .GPT_59_INST7_CFG_DATA_32BIT           align(4)      :>.
  .GPT_59_INST7_CFG_DATA_UNSPECIFIED     align(4)      :>. 

  .ICU_CFG_DBTOC_UNSPECIFIED      align(4)      :>.  /* Single core */
  .ICU_CFG_DATA_1BIT                            :>.
  .ICU_CFG_DATA_8BIT                            :>.
  .ICU_CFG_DATA_16BIT             align(4)      :>.
  .ICU_CFG_DATA_32BIT             align(4)      :>.
  .ICU_CFG_DATA_UNSPECIFIED       align(4)      :>.

  .ICU_59_INST0_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 0 */
  .ICU_59_INST0_CFG_DATA_1BIT                          :>.
  .ICU_59_INST0_CFG_DATA_8BIT                          :>.
  .ICU_59_INST0_CFG_DATA_16BIT           align(4)      :>.
  .ICU_59_INST0_CFG_DATA_32BIT           align(4)      :>.
  .ICU_59_INST0_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .ICU_59_INST1_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 1 */
  .ICU_59_INST1_CFG_DATA_1BIT                          :>.
  .ICU_59_INST1_CFG_DATA_8BIT                          :>.
  .ICU_59_INST1_CFG_DATA_16BIT           align(4)      :>.
  .ICU_59_INST1_CFG_DATA_32BIT           align(4)      :>.
  .ICU_59_INST1_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .ICU_59_INST2_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 2 */
  .ICU_59_INST2_CFG_DATA_1BIT                          :>.
  .ICU_59_INST2_CFG_DATA_8BIT                          :>.
  .ICU_59_INST2_CFG_DATA_16BIT           align(4)      :>.
  .ICU_59_INST2_CFG_DATA_32BIT           align(4)      :>.
  .ICU_59_INST2_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .ICU_59_INST3_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 3 */
  .ICU_59_INST3_CFG_DATA_1BIT                          :>.
  .ICU_59_INST3_CFG_DATA_8BIT                          :>.
  .ICU_59_INST3_CFG_DATA_16BIT           align(4)      :>.
  .ICU_59_INST3_CFG_DATA_32BIT           align(4)      :>.
  .ICU_59_INST3_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .ICU_59_INST4_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 4 */
  .ICU_59_INST4_CFG_DATA_1BIT                          :>.
  .ICU_59_INST4_CFG_DATA_8BIT                          :>.
  .ICU_59_INST4_CFG_DATA_16BIT           align(4)      :>.
  .ICU_59_INST4_CFG_DATA_32BIT           align(4)      :>.
  .ICU_59_INST4_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .ICU_59_INST5_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 5 */
  .ICU_59_INST5_CFG_DATA_1BIT                          :>.
  .ICU_59_INST5_CFG_DATA_8BIT                          :>.
  .ICU_59_INST5_CFG_DATA_16BIT           align(4)      :>.
  .ICU_59_INST5_CFG_DATA_32BIT           align(4)      :>.
  .ICU_59_INST5_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .ICU_59_INST6_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 6 */
  .ICU_59_INST6_CFG_DATA_1BIT                          :>.
  .ICU_59_INST6_CFG_DATA_8BIT                          :>.
  .ICU_59_INST6_CFG_DATA_16BIT           align(4)      :>.
  .ICU_59_INST6_CFG_DATA_32BIT           align(4)      :>.
  .ICU_59_INST6_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .ICU_59_INST7_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 7 */
  .ICU_59_INST7_CFG_DATA_1BIT                          :>.
  .ICU_59_INST7_CFG_DATA_8BIT                          :>.
  .ICU_59_INST7_CFG_DATA_16BIT           align(4)      :>.
  .ICU_59_INST7_CFG_DATA_32BIT           align(4)      :>.
  .ICU_59_INST7_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .PORT_CFG_DBTOC_UNSPECIFIED     align(4)      :>.
  .PORT_CFG_DBCC_UNSPECIFIED      align(4)      :>.
  .PORT_CFG_DATA_1BIT                           :>.
  .PORT_CFG_DATA_8BIT                           :>.
  .PORT_CFG_DATA_16BIT            align(4)      :>.
  .PORT_CFG_DATA_32BIT            align(4)      :>.
  .PORT_CFG_DATA_UNSPECIFIED      align(4)      :>.

  .PWM_CFG_DBTOC_UNSPECIFIED      align(4)      :>.  /* Single core */
  .PWM_CFG_DATA_1BIT                            :>.
  .PWM_CFG_DATA_8BIT                            :>.
  .PWM_CFG_DATA_16BIT             align(4)      :>.
  .PWM_CFG_DATA_32BIT             align(4)      :>.
  .PWM_CFG_DATA_UNSPECIFIED       align(4)      :>.

  .PWM_59_INST0_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 0 */
  .PWM_59_INST0_CFG_DATA_1BIT                          :>.
  .PWM_59_INST0_CFG_DATA_8BIT                          :>.
  .PWM_59_INST0_CFG_DATA_16BIT           align(4)      :>.
  .PWM_59_INST0_CFG_DATA_32BIT           align(4)      :>.
  .PWM_59_INST0_CFG_DATA_UNSPECIFIED     align(4)      :>.
  
  .PWM_59_INST1_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 1 */
  .PWM_59_INST1_CFG_DATA_1BIT                          :>.
  .PWM_59_INST1_CFG_DATA_8BIT                          :>.
  .PWM_59_INST1_CFG_DATA_16BIT           align(4)      :>.
  .PWM_59_INST1_CFG_DATA_32BIT           align(4)      :>.
  .PWM_59_INST1_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .PWM_59_INST2_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 2 */
  .PWM_59_INST2_CFG_DATA_1BIT                          :>.
  .PWM_59_INST2_CFG_DATA_8BIT                          :>.
  .PWM_59_INST2_CFG_DATA_16BIT           align(4)      :>.
  .PWM_59_INST2_CFG_DATA_32BIT           align(4)      :>.
  .PWM_59_INST2_CFG_DATA_UNSPECIFIED     align(4)      :>.
  
  .PWM_59_INST3_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 3 */
  .PWM_59_INST3_CFG_DATA_1BIT                          :>.
  .PWM_59_INST3_CFG_DATA_8BIT                          :>.
  .PWM_59_INST3_CFG_DATA_16BIT           align(4)      :>.
  .PWM_59_INST3_CFG_DATA_32BIT           align(4)      :>.
  .PWM_59_INST3_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .PWM_59_INST4_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 4 */
  .PWM_59_INST4_CFG_DATA_1BIT                          :>.
  .PWM_59_INST4_CFG_DATA_8BIT                          :>.
  .PWM_59_INST4_CFG_DATA_16BIT           align(4)      :>.
  .PWM_59_INST4_CFG_DATA_32BIT           align(4)      :>.
  .PWM_59_INST4_CFG_DATA_UNSPECIFIED     align(4)      :>.
  
  .PWM_59_INST5_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 5 */
  .PWM_59_INST5_CFG_DATA_1BIT                          :>.
  .PWM_59_INST5_CFG_DATA_8BIT                          :>.
  .PWM_59_INST5_CFG_DATA_16BIT           align(4)      :>.
  .PWM_59_INST5_CFG_DATA_32BIT           align(4)      :>.
  .PWM_59_INST5_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .PWM_59_INST6_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 6 */
  .PWM_59_INST6_CFG_DATA_1BIT                          :>.
  .PWM_59_INST6_CFG_DATA_8BIT                          :>.
  .PWM_59_INST6_CFG_DATA_16BIT           align(4)      :>.
  .PWM_59_INST6_CFG_DATA_32BIT           align(4)      :>.
  .PWM_59_INST6_CFG_DATA_UNSPECIFIED     align(4)      :>.
  
  .PWM_59_INST7_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 7 */
  .PWM_59_INST7_CFG_DATA_1BIT                          :>.
  .PWM_59_INST7_CFG_DATA_8BIT                          :>.
  .PWM_59_INST7_CFG_DATA_16BIT           align(4)      :>.
  .PWM_59_INST7_CFG_DATA_32BIT           align(4)      :>.
  .PWM_59_INST7_CFG_DATA_UNSPECIFIED     align(4)      :>.
  
  .SPI_CFG_DBTOC_UNSPECIFIED      align(4)      :>.  /* Single core */
  .SPI_CFG_DATA_1BIT                            :>.
  .SPI_CFG_DATA_8BIT                            :>.
  .SPI_CFG_DATA_16BIT             align(4)      :>.
  .SPI_CFG_DATA_32BIT             align(4)      :>.
  .SPI_CFG_DATA_UNSPECIFIED       align(4)      :>.

  .SPI_59_INST0_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 0 */
  .SPI_59_INST0_CFG_DATA_1BIT                          :>.
  .SPI_59_INST0_CFG_DATA_8BIT                          :>.
  .SPI_59_INST0_CFG_DATA_16BIT           align(4)      :>.
  .SPI_59_INST0_CFG_DATA_32BIT           align(4)      :>.
  .SPI_59_INST0_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .SPI_59_INST1_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 1 */
  .SPI_59_INST1_CFG_DATA_1BIT                          :>.
  .SPI_59_INST1_CFG_DATA_8BIT                          :>.
  .SPI_59_INST1_CFG_DATA_16BIT           align(4)      :>.
  .SPI_59_INST1_CFG_DATA_32BIT           align(4)      :>.
  .SPI_59_INST1_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .SPI_59_INST2_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 2 */
  .SPI_59_INST2_CFG_DATA_1BIT                          :>.
  .SPI_59_INST2_CFG_DATA_8BIT                          :>.
  .SPI_59_INST2_CFG_DATA_16BIT           align(4)      :>.
  .SPI_59_INST2_CFG_DATA_32BIT           align(4)      :>.
  .SPI_59_INST2_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .SPI_59_INST3_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 3 */
  .SPI_59_INST3_CFG_DATA_1BIT                          :>.
  .SPI_59_INST3_CFG_DATA_8BIT                          :>.
  .SPI_59_INST3_CFG_DATA_16BIT           align(4)      :>.
  .SPI_59_INST3_CFG_DATA_32BIT           align(4)      :>.
  .SPI_59_INST3_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .SPI_59_INST4_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 4 */
  .SPI_59_INST4_CFG_DATA_1BIT                          :>.
  .SPI_59_INST4_CFG_DATA_8BIT                          :>.
  .SPI_59_INST4_CFG_DATA_16BIT           align(4)      :>.
  .SPI_59_INST4_CFG_DATA_32BIT           align(4)      :>.
  .SPI_59_INST4_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .SPI_59_INST5_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 5 */
  .SPI_59_INST5_CFG_DATA_1BIT                          :>.
  .SPI_59_INST5_CFG_DATA_8BIT                          :>.
  .SPI_59_INST5_CFG_DATA_16BIT           align(4)      :>.
  .SPI_59_INST5_CFG_DATA_32BIT           align(4)      :>.
  .SPI_59_INST5_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .SPI_59_INST6_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 6 */
  .SPI_59_INST6_CFG_DATA_1BIT                          :>.
  .SPI_59_INST6_CFG_DATA_8BIT                          :>.
  .SPI_59_INST6_CFG_DATA_16BIT           align(4)      :>.
  .SPI_59_INST6_CFG_DATA_32BIT           align(4)      :>.
  .SPI_59_INST6_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .SPI_59_INST7_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 7 */
  .SPI_59_INST7_CFG_DATA_1BIT                          :>.
  .SPI_59_INST7_CFG_DATA_8BIT                          :>.
  .SPI_59_INST7_CFG_DATA_16BIT           align(4)      :>.
  .SPI_59_INST7_CFG_DATA_32BIT           align(4)      :>.
  .SPI_59_INST7_CFG_DATA_UNSPECIFIED     align(4)      :>.

  .WDG_CFG_DBTOC_UNSPECIFIED      align(4)      :>.
  .WDG_59_INST0_CFG_DBTOC_UNSPECIFIED   align(4)      :>.
  .WDG_59_INST1_CFG_DBTOC_UNSPECIFIED   align(4)      :>.
  .WDG_59_INST2_CFG_DBTOC_UNSPECIFIED   align(4)      :>.
  .WDG_59_INST3_CFG_DBTOC_UNSPECIFIED   align(4)      :>.

  .FLS_CFG_DBTOC_UNSPECIFIED      align(4)      :>.
  .FLS_CFG_DBCC_UNSPECIFIED       align(4)      :>.
  .FLS_CFG_DATA_UNSPECIFIED       align(4)      :>.

  .CAN_CFG_DBTOC_UNSPECIFIED      align(4)      :>.
  .CAN_CFG_DBCC_UNSPECIFIED       align(4)      :>.
  .CAN_CFG_DATA_1BIT                            :>.
  .CAN_CFG_DATA_8BIT                            :>.
  .CAN_CFG_DATA_16BIT             align(4)      :>.
  .CAN_CFG_DATA_32BIT             align(4)      :>.
  .CAN_CFG_DATA_UNSPECIFIED       align(4)      :>.

  .CAN_59_INST0_CFG_DBTOC_UNSPECIFIED      align(4)      :>.
  .CAN_59_INST0_CFG_DBCC_UNSPECIFIED       align(4)      :>.
  .CAN_59_INST0_CFG_DATA_1BIT                            :>.
  .CAN_59_INST0_CFG_DATA_8BIT                            :>.
  .CAN_59_INST0_CFG_DATA_16BIT             align(4)      :>.
  .CAN_59_INST0_CFG_DATA_32BIT             align(4)      :>.
  .CAN_59_INST0_CFG_DATA_UNSPECIFIED       align(4)      :>.

  .CAN_59_INST1_CFG_DBTOC_UNSPECIFIED      align(4)      :>.
  .CAN_59_INST1_CFG_DBCC_UNSPECIFIED       align(4)      :>.
  .CAN_59_INST1_CFG_DATA_1BIT                            :>.
  .CAN_59_INST1_CFG_DATA_8BIT                            :>.
  .CAN_59_INST1_CFG_DATA_16BIT             align(4)      :>.
  .CAN_59_INST1_CFG_DATA_32BIT             align(4)      :>.
  .CAN_59_INST1_CFG_DATA_UNSPECIFIED       align(4)      :>.

  .LIN_CFG_DBTOC_UNSPECIFIED      align(4)      :>.
  .LIN_CFG_DATA_1BIT                            :>.
  .LIN_CFG_DATA_8BIT                            :>.
  .LIN_CFG_DATA_16BIT             align(4)      :>.
  .LIN_CFG_DATA_32BIT             align(4)      :>.
  .LIN_CFG_DATA_UNSPECIFIED       align(4)      :>.

  .FR_59_RENESAS_DBTOC_CFG_CONST_UNSPEC      align(4) :>.
  .FR_59_RENESAS_CFG_DBTOC_UNSPECIFIED       align(4) :>.
  .FR_59_RENESAS_CFG_DATA_UNSPECIFIED        align(4) :>.

  .ADC_CFG_DBTOC_UNSPECIFIED      align(4)      :>.  /* Single core */
  .ADC_CFG_DATA_1BIT                            :>.
  .ADC_CFG_DATA_8BIT                            :>.
  .ADC_CFG_DATA_16BIT             align(4)      :>.
  .ADC_CFG_DATA_32BIT             align(4)      :>.
  .ADC_CFG_DATA_UNSPECIFIED       align(4)      :>.
  .ADC_CFG_DATA_PTR               align(4)      :>.

  .ADC_59_INST0_CFG_DBTOC_UNSPECIFIED  align(4) :>.  /* Instance 0 */
  .ADC_59_INST0_CFG_DATA_1BIT                   :>.
  .ADC_59_INST0_CFG_DATA_8BIT                   :>.
  .ADC_59_INST0_CFG_DATA_16BIT         align(4) :>.
  .ADC_59_INST0_CFG_DATA_32BIT         align(4) :>.
  .ADC_59_INST0_CFG_DATA_UNSPECIFIED   align(4) :>.
  .ADC_59_INST0_CFG_DATA_PTR           align(4) :>.

  .ADC_59_INST1_CFG_DBTOC_UNSPECIFIED  align(4) :>.  /* Instance 1 */
  .ADC_59_INST1_CFG_DATA_1BIT                   :>.
  .ADC_59_INST1_CFG_DATA_8BIT                   :>.
  .ADC_59_INST1_CFG_DATA_16BIT         align(4) :>.
  .ADC_59_INST1_CFG_DATA_32BIT         align(4) :>.
  .ADC_59_INST1_CFG_DATA_UNSPECIFIED   align(4) :>.
  .ADC_59_INST1_CFG_DATA_PTR           align(4) :>.

  .ADC_59_INST2_CFG_DBTOC_UNSPECIFIED    align(4)      :>.  /* Instance 2 */
  .ADC_59_INST2_CFG_DATA_1BIT                          :>.
  .ADC_59_INST2_CFG_DATA_8BIT                          :>.
  .ADC_59_INST2_CFG_DATA_16BIT           align(4)      :>.
  .ADC_59_INST2_CFG_DATA_32BIT           align(4)      :>.
  .ADC_59_INST2_CFG_DATA_UNSPECIFIED     align(4)      :>.
  .ADC_59_INST2_CFG_DATA_PTR           align(4) :>.

  .MCU_CFG_DBTOC_UNSPECIFIED      align(4)      :>.
  .MCU_CFG_DATA_1BIT                            :>.
  .MCU_CFG_DATA_8BIT                            :>.
  .MCU_CFG_DATA_16BIT             align(4)      :>.
  .MCU_CFG_DATA_32BIT             align(4)      :>.
  .MCU_CFG_DATA_UNSPECIFIED       align(4)      :>.

  .ETH_CFG_DBTOC_UNSPECIFIED   align(4)      :>.
  .ETH_CFG_DATA_UNSPECIFIED    align(4)      :>.

  /* Start of internal RAM area (iRAM) */
  .data                        align(4)         :>iRAM_0   /* initialized data */
  .sdabase                     align(4)         :>.      /* initialize global pointer GP for SDA addressing */
  .zdata                       align(4)         :>.      /* initialized data in ZDA area */
  .sldata                      align(4)         :>.      /* initialized data in LSDA area */
  .sdata                       align(4)         :>.      /* initialized data in SDA area */
  .RAM_1BIT                    NOCLEAR          :>.      /* initialized data in SDA area */
  .RAM_8BIT                    NOCLEAR          :>.      /* initialized data in SDA area */
  .RAM_16BIT                   NOCLEAR align(4) :>.      /* initialized data in SDA area */
  .RAM_32BIT                   NOCLEAR align(4) :>.      /* initialized data in SDA area */
  .RAM_UNSPECIFIED             NOCLEAR align(4) :>.      /* initialized data in SDA area */
  .RAM_INIT_PTR                NOCLEAR align(4) :>.      /* initialized data in SDA area */
  .FAST_RAM_1BIT               NOCLEAR          :>.      /* initialized data in SDA area */
  .FAST_RAM_8BIT               NOCLEAR          :>.      /* initialized data in SDA area */
  .FAST_RAM_16BIT              NOCLEAR align(4) :>.      /* initialized data in SDA area */
  .FAST_RAM_32BIT              NOCLEAR align(4) :>.      /* initialized data in SDA area */
  .FAST_RAM_UNSPECIFIED        NOCLEAR align(4) :>.      /* initialized data in SDA area */
  .FAST_RAM_INIT_PTR           NOCLEAR align(4) :>.      /* initialized data in SDA area */

  .RAM_1BIT_0                  NOCLEAR          :>.      /* Instance 0 */
  .RAM_8BIT_0                  NOCLEAR          :>.
  .RAM_16BIT_0                 NOCLEAR align(4) :>.
  .RAM_32BIT_0                 NOCLEAR align(4) :>.
  .RAM_UNSPECIFIED_0           NOCLEAR align(4) :>.
  .RAM_INIT_PTR_0              NOCLEAR align(4) :>.
  .FAST_RAM_1BIT_0             NOCLEAR          :>.
  .FAST_RAM_8BIT_0             NOCLEAR          :>.
  .FAST_RAM_16BIT_0            NOCLEAR align(4) :>.
  .FAST_RAM_32BIT_0            NOCLEAR align(4) :>.
  .FAST_RAM_UNSPECIFIED_0      NOCLEAR align(4) :>.
  .FAST_RAM_INIT_PTR_0         NOCLEAR align(4) :>.

  .RAM_1BIT_1                  NOCLEAR          :>.      /* Instance 1 */
  .RAM_8BIT_1                  NOCLEAR          :>.
  .RAM_16BIT_1                 NOCLEAR align(4) :>.
  .RAM_32BIT_1                 NOCLEAR align(4) :>.
  .RAM_UNSPECIFIED_1           NOCLEAR align(4) :>.
  .RAM_INIT_PTR_1              NOCLEAR align(4) :>.
  .FAST_RAM_1BIT_1             NOCLEAR          :>.
  .FAST_RAM_8BIT_1             NOCLEAR          :>.
  .FAST_RAM_16BIT_1            NOCLEAR align(4) :>.
  .FAST_RAM_32BIT_1            NOCLEAR align(4) :>.
  .FAST_RAM_UNSPECIFIED_1      NOCLEAR align(4) :>.
  .FAST_RAM_INIT_PTR_1         NOCLEAR align(4) :>.

  .RAM_1BIT_2                  NOCLEAR          :>.      /* Instance 2 */
  .RAM_8BIT_2                  NOCLEAR          :>.
  .RAM_16BIT_2                 NOCLEAR align(4) :>.
  .RAM_32BIT_2                 NOCLEAR align(4) :>.
  .RAM_UNSPECIFIED_2           NOCLEAR align(4) :>.
  .RAM_INIT_PTR_2              NOCLEAR align(4) :>.
  .FAST_RAM_1BIT_2             NOCLEAR          :>.
  .FAST_RAM_8BIT_2             NOCLEAR          :>.
  .FAST_RAM_16BIT_2            NOCLEAR align(4) :>.
  .FAST_RAM_32BIT_2            NOCLEAR align(4) :>.
  .FAST_RAM_UNSPECIFIED_2      NOCLEAR align(4) :>.
  .FAST_RAM_INIT_PTR_2         NOCLEAR align(4) :>.

  .RAM_1BIT_3                  NOCLEAR          :>.      /* Instance 3 */
  .RAM_8BIT_3                  NOCLEAR          :>.
  .RAM_16BIT_3                 NOCLEAR align(4) :>.
  .RAM_32BIT_3                 NOCLEAR align(4) :>.
  .RAM_UNSPECIFIED_3           NOCLEAR align(4) :>.
  .RAM_INIT_PTR_3              NOCLEAR align(4) :>.
  .FAST_RAM_1BIT_3             NOCLEAR          :>.
  .FAST_RAM_8BIT_3             NOCLEAR          :>.
  .FAST_RAM_16BIT_3            NOCLEAR align(4) :>.
  .FAST_RAM_32BIT_3            NOCLEAR align(4) :>.
  .FAST_RAM_UNSPECIFIED_3      NOCLEAR align(4) :>.
  .FAST_RAM_INIT_PTR_3         NOCLEAR align(4) :>.

  .RAM_1BIT_4                  NOCLEAR          :>.      /* Instance 4 */
  .RAM_8BIT_4                  NOCLEAR          :>.
  .RAM_16BIT_4                 NOCLEAR align(4) :>.
  .RAM_32BIT_4                 NOCLEAR align(4) :>.
  .RAM_UNSPECIFIED_4           NOCLEAR align(4) :>.
  .RAM_INIT_PTR_4              NOCLEAR align(4) :>.
  .FAST_RAM_1BIT_4             NOCLEAR          :>.
  .FAST_RAM_8BIT_4             NOCLEAR          :>.
  .FAST_RAM_16BIT_4            NOCLEAR align(4) :>.
  .FAST_RAM_32BIT_4            NOCLEAR align(4) :>.
  .FAST_RAM_UNSPECIFIED_4      NOCLEAR align(4) :>.
  .FAST_RAM_INIT_PTR_4         NOCLEAR align(4) :>.

  .RAM_1BIT_5                  NOCLEAR          :>.      /* Instance 5 */
  .RAM_8BIT_5                  NOCLEAR          :>.
  .RAM_16BIT_5                 NOCLEAR align(4) :>.
  .RAM_32BIT_5                 NOCLEAR align(4) :>.
  .RAM_UNSPECIFIED_5           NOCLEAR align(4) :>.
  .RAM_INIT_PTR_5              NOCLEAR align(4) :>.
  .FAST_RAM_1BIT_5             NOCLEAR          :>.
  .FAST_RAM_8BIT_5             NOCLEAR          :>.
  .FAST_RAM_16BIT_5            NOCLEAR align(4) :>.
  .FAST_RAM_32BIT_5            NOCLEAR align(4) :>.
  .FAST_RAM_UNSPECIFIED_5      NOCLEAR align(4) :>.
  .FAST_RAM_INIT_PTR_5         NOCLEAR align(4) :>.

  .RAM_1BIT_6                  NOCLEAR          :>.      /* Instance 6 */
  .RAM_8BIT_6                  NOCLEAR          :>.
  .RAM_16BIT_6                 NOCLEAR align(4) :>.
  .RAM_32BIT_6                 NOCLEAR align(4) :>.
  .RAM_UNSPECIFIED_6           NOCLEAR align(4) :>.
  .RAM_INIT_PTR_6              NOCLEAR align(4) :>.
  .FAST_RAM_1BIT_6             NOCLEAR          :>.
  .FAST_RAM_8BIT_6             NOCLEAR          :>.
  .FAST_RAM_16BIT_6            NOCLEAR align(4) :>.
  .FAST_RAM_32BIT_6            NOCLEAR align(4) :>.
  .FAST_RAM_UNSPECIFIED_6      NOCLEAR align(4) :>.
  .FAST_RAM_INIT_PTR_6         NOCLEAR align(4) :>.

  .RAM_1BIT_7                  NOCLEAR          :>.      /* Instance 7 */
  .RAM_8BIT_7                  NOCLEAR          :>.
  .RAM_16BIT_7                 NOCLEAR align(4) :>.
  .RAM_32BIT_7                 NOCLEAR align(4) :>.
  .RAM_UNSPECIFIED_7           NOCLEAR align(4) :>.
  .RAM_INIT_PTR_7              NOCLEAR align(4) :>.
  .FAST_RAM_1BIT_7             NOCLEAR          :>.
  .FAST_RAM_8BIT_7             NOCLEAR          :>.
  .FAST_RAM_16BIT_7            NOCLEAR align(4) :>.
  .FAST_RAM_32BIT_7            NOCLEAR align(4) :>.
  .FAST_RAM_UNSPECIFIED_7      NOCLEAR align(4) :>.
  .FAST_RAM_INIT_PTR_7         NOCLEAR align(4) :>.

  .bss                         align(4)         :>.      /* zero initialized data */
  .zbss                        align(4)         :>.      /* zero initialized data in ZDA area */
  .slbss                       align(4)         :>.      /* zero initialized data in LSDA area */
  .sbss                        align(4)         :>.      /* zero initialized data in SDA area */
  .NOINIT_RAM_1BIT             NOCLEAR          :>.      /* no initialized data in SDA area */
  .NOINIT_RAM_8BIT             NOCLEAR          :>.      /* no initialized data in SDA area */
  .NOINIT_RAM_16BIT            NOCLEAR align(4) :>.      /* no initialized data in SDA area */
  .NOINIT_RAM_32BIT            NOCLEAR align(4) :>.      /* no initialized data in SDA area */
  .NOINIT_RAM_UNSPECIFIED      NOCLEAR align(4) :>.      /* no initialized data in SDA area */
  .NOINIT_RAM_PTR              NOCLEAR align(4) :>.      /* no initialized data in SDA area */
  .NOINIT_RAM_64BIT            NOCLEAR align(8) :>.      /* no initialized data in SDA area */

  .NOINIT_RAM_1BIT_0           NOCLEAR          :>.      /* Instance 0 */
  .NOINIT_RAM_8BIT_0           NOCLEAR          :>.
  .NOINIT_RAM_16BIT_0          NOCLEAR align(4) :>.
  .NOINIT_RAM_32BIT_0          NOCLEAR align(4) :>.
  .NOINIT_RAM_UNSPECIFIED_0    NOCLEAR align(4) :>.
  .NOINIT_RAM_PTR_0            NOCLEAR align(4) :>.
  .NOINIT_RAM_64BIT_0          NOCLEAR align(8) :>.

  .NOINIT_RAM_1BIT_1           NOCLEAR          :>.      /* Instance 1 */
  .NOINIT_RAM_8BIT_1           NOCLEAR          :>.
  .NOINIT_RAM_16BIT_1          NOCLEAR align(4) :>.
  .NOINIT_RAM_32BIT_1          NOCLEAR align(4) :>.
  .NOINIT_RAM_UNSPECIFIED_1    NOCLEAR align(4) :>.
  .NOINIT_RAM_PTR_1            NOCLEAR align(4) :>.
  .NOINIT_RAM_64BIT_1          NOCLEAR align(8) :>.

  .NOINIT_RAM_1BIT_2           NOCLEAR          :>.      /* Instance 2 */
  .NOINIT_RAM_8BIT_2           NOCLEAR          :>.
  .NOINIT_RAM_16BIT_2          NOCLEAR align(4) :>.
  .NOINIT_RAM_32BIT_2          NOCLEAR align(4) :>.
  .NOINIT_RAM_UNSPECIFIED_2    NOCLEAR align(4) :>.
  .NOINIT_RAM_PTR_2            NOCLEAR align(4) :>.
  .NOINIT_RAM_64BIT_2          NOCLEAR align(8) :>.

  .NOINIT_RAM_1BIT_3           NOCLEAR          :>.      /* Instance 3 */
  .NOINIT_RAM_8BIT_3           NOCLEAR          :>.
  .NOINIT_RAM_16BIT_3          NOCLEAR align(4) :>.
  .NOINIT_RAM_32BIT_3          NOCLEAR align(4) :>.
  .NOINIT_RAM_UNSPECIFIED_3    NOCLEAR align(4) :>.
  .NOINIT_RAM_PTR_3            NOCLEAR align(4) :>.
  .NOINIT_RAM_64BIT_3          NOCLEAR align(8) :>.

  .NOINIT_RAM_1BIT_4           NOCLEAR          :>.      /* Instance 4 */
  .NOINIT_RAM_8BIT_4           NOCLEAR          :>.
  .NOINIT_RAM_16BIT_4          NOCLEAR align(4) :>.
  .NOINIT_RAM_32BIT_4          NOCLEAR align(4) :>.
  .NOINIT_RAM_UNSPECIFIED_4    NOCLEAR align(4) :>.
  .NOINIT_RAM_PTR_4            NOCLEAR align(4) :>.
  .NOINIT_RAM_64BIT_4          NOCLEAR align(8) :>.

  .NOINIT_RAM_1BIT_5           NOCLEAR          :>.      /* Instance 5 */
  .NOINIT_RAM_8BIT_5           NOCLEAR          :>.
  .NOINIT_RAM_16BIT_5          NOCLEAR align(4) :>.
  .NOINIT_RAM_32BIT_5          NOCLEAR align(4) :>.
  .NOINIT_RAM_UNSPECIFIED_5    NOCLEAR align(4) :>.
  .NOINIT_RAM_PTR_5            NOCLEAR align(4) :>.
  .NOINIT_RAM_64BIT_5          NOCLEAR align(8) :>.

  .NOINIT_RAM_1BIT_6           NOCLEAR          :>.      /* Instance 6 */
  .NOINIT_RAM_8BIT_6           NOCLEAR          :>.
  .NOINIT_RAM_16BIT_6          NOCLEAR align(4) :>.
  .NOINIT_RAM_32BIT_6          NOCLEAR align(4) :>.
  .NOINIT_RAM_UNSPECIFIED_6    NOCLEAR align(4) :>.
  .NOINIT_RAM_PTR_6            NOCLEAR align(4) :>.
  .NOINIT_RAM_64BIT_6          NOCLEAR align(8) :>.

  .NOINIT_RAM_1BIT_7           NOCLEAR          :>.      /* Instance 7 */
  .NOINIT_RAM_8BIT_7           NOCLEAR          :>.
  .NOINIT_RAM_16BIT_7          NOCLEAR align(4) :>.
  .NOINIT_RAM_32BIT_7          NOCLEAR align(4) :>.
  .NOINIT_RAM_UNSPECIFIED_7    NOCLEAR align(4) :>.
  .NOINIT_RAM_PTR_7            NOCLEAR align(4) :>.
  .NOINIT_RAM_64BIT_7          NOCLEAR align(8) :>.

   /* MCAL Driver Configuration Ram area *****/
  .DIO_CFG_RAM_UNSPECIFIED     NOCLEAR          :>.      /* no initialized data in SDA area */
  
  .GPT_CFG_RAM_UNSPECIFIED     NOCLEAR          :>.      /* no initialized data in SDA area */  
  .GPT_59_INST0_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .GPT_59_INST1_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .GPT_59_INST2_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .GPT_59_INST3_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .GPT_59_INST4_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .GPT_59_INST5_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .GPT_59_INST6_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .GPT_59_INST7_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  
  .ICU_CFG_RAM_UNSPECIFIED     NOCLEAR          :>.      /* no initialized data in SDA area */
  .ICU_59_INST0_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .ICU_59_INST1_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .ICU_59_INST2_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .ICU_59_INST3_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .ICU_59_INST4_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .ICU_59_INST5_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .ICU_59_INST6_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .ICU_59_INST7_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .PORT_CFG_RAM_UNSPECIFIED    NOCLEAR          :>.      /* no initialized data in SDA area */
  .PWM_CFG_RAM_UNSPECIFIED     NOCLEAR          :>.      /* no initialized data in SDA area */
  .PWM_59_INST0_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .PWM_59_INST1_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .PWM_59_INST2_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .PWM_59_INST3_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .PWM_59_INST4_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .PWM_59_INST5_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .PWM_59_INST6_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .PWM_59_INST7_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .SPI_CFG_RAM_UNSPECIFIED     NOCLEAR          :>.      /* no initialized data in SDA area */
  .SPI_59_INST0_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .SPI_59_INST1_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .SPI_59_INST2_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .SPI_59_INST3_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .SPI_59_INST4_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .SPI_59_INST5_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .SPI_59_INST6_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .SPI_59_INST7_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .CAN_CFG_RAM_UNSPECIFIED     NOCLEAR          :>.      /* no initialized data in SDA area */
  .CAN_59_INST0_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .CAN_59_INST1_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .ADC_CFG_RAM_UNSPECIFIED     NOCLEAR          :>.      /* no initialized data in SDA area */
  .ADC_59_INST0_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .ADC_59_INST1_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .ADC_59_INST2_CFG_RAM_UNSPECIFIED   NOCLEAR   :>.      /* no initialized data in SDA area */
  .LIN_CFG_RAM_UNSPECIFIED     NOCLEAR          :>.      /* no initialized data in SDA area */
  .FR_59_RENESAS_CFG_RAM_UNSPECIFIED    NOCLEAR :>.      /* no initialized data in SDA area */
  .FR_59_RENESAS_VAR_POWER_ON_INIT      NOCLEAR :>.      /* no initialized data in SDA area */
  .MCU_CFG_RAM_UNSPECIFIED     NOCLEAR          :>.      /* no initialized data in SDA area */

  .FLS_BUFFER_CODE_RAM         align(4)         :>.      /* Temporary Buffer  */
  .FLS_USER_BUFFER_CODE_RAM    align(4)         :>.      /* Application Buffer  */
  .R_RFD_SBSS                  align(4)         :>.      /* Data without initialization value                */

  .ramtext  align(128)  MAX_SIZE(0x2000)        :>.      /* initialized and zero-initialized data in TDA area */
  .tdata    align(4)    MAX_SIZE(0x0100)        :>.      /* initialized and zero-initialized data in TDA area */
  .exec     align(128)                          :>.
  .mev_address                 align(32)        :>.      /* Mutual Exclusive Variable is used for Sync flags between multi core */
  .stack    align(4)    pad(0x0800)             :>.      /* definition of stack size */

  .heapbase align(4)                            :>.
  .heap     align(4)
            pad(addr(iRAM_0_TOP)-addr(.heapbase))
            NOCLEAR                             :>.      /* definition of heap size */

  .top_of_RAM           align(4)                :>iRAM_0_TOP

  /* Start of internal retention RAM area (iRAM_R) */
  .rcode    align(4) pad(0x2000)  :>iRAM_R   /* definition RRAM of code size */
  .rdata    align(4)              :>.        /* user defined segment for initialized data located in retention RAM */
  .MCU_CFG_BURAM_UNSPECIFIED      :>.
  .rbss     align(4)              :>.        /* user defined segment for zero initialized data located in retention RAM */
  .rsbss    align(4)              :>.        /* user defined segment for zero initialized data located in retention RAM */
  .rstack   align(4) pad(0x0800)  :>.        /* definition RRAM of stack size */
  .top_of_RAM_R align(4)          :>iRAM_R_TOP

  /* Start of Cluster RAM area (cRAM_0) */
  .ETH_PORT_RAM_0               align(32)        :>cRAM_0
  .INIT_RAM_PTR                 align(4)         :>.
  .INIT_RAM_PTR_0               align(4)         :>.
  .INIT_RAM_PTR_1               align(4)         :>.
  .INIT_RAM_PTR_2               align(4)         :>.
  .INIT_RAM_PTR_3               align(4)         :>.
  .INIT_RAM_PTR_4               align(4)         :>.
  .INIT_RAM_PTR_5               align(4)         :>.
  .INIT_RAM_PTR_6               align(4)         :>.
  .INIT_RAM_PTR_7               align(4)         :>.

  /* Start of Cluster RAM area (cRAM_2) */
  .ETH_PORT_RAM_1               align(32)        :>cRAM_2

  /*  Symbols for compiler references */
  ___ghs_romstart       = MEMADDR(iROM_0);
  ___ghs_romend         = MEMENDADDR(iROM_0);

  ___ghs_ramstart       = MEMADDR(iRAM_0);
  ___ghs_ramend         = MEMENDADDR(iRAM_0);

  ___ghs_rramstart      = MEMADDR(iRAM_R);
  ___ghs_rramend        = MEMENDADDR(iRAM_R);

  ___ghs_ram1start      = MEMADDR(iRAM_1);
  ___ghs_ram1end        = MEMENDADDR(iRAM_1);

  ___ghs_cram0start     = MEMADDR(cRAM_0);
  ___ghs_cram0end       = MEMENDADDR(cRAM_0);
  
  ___ghs_cram1start     = MEMADDR(cRAM_2);
  ___ghs_cram1end       = MEMENDADDR(cRAM_2);
}

/*===========================================================================*/
/*      End of File                                                          */
/*===========================================================================*/
